|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  | (N) |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | I |
|  |  |  | (N) |

|  |
| --- |
| SCHEDULE NO. 451 |
| LARGE CUSTOMER RETAIL WHEELING |
|  |

1. **TRANSMISSION SERVICE** (Continued)
2. Successor Tariffs. In the event that the Company transfers control of its transmission facilities to a Regional Transmission Organization, Customer shall take service under the rate schedules of such successor organization for the use of the Company’s Transmission System.
3. **DISTRIBUTION SERVICE**
4. Service Quality Standards and Distribution System Connection. The Company shall be obligated to maintain its Distribution System consistent with applicable standards, including service quality standards, required by the Commission. Each Customer, regardless of the voltage at which its distribution service is provided, shall be deemed to be connected to the Distribution System during the Term of its Schedule 451 Service Agreement. Except as otherwise provided in this Schedule, distribution service shall be provided under the terms and conditions set forth in the Company’s Electric Tariff Schedule 80 and Electric Tariff Schedule 85, as appropriate. Distribution service under this Schedule shall be provided on a non-discriminatory basis, which is comparable to the distribution service used by the Company to serve its Core Customers.
5. Service Voltages. Unless otherwise specified in the Schedule 451 Service Agreement, high voltage service is defined as three-phase delivery voltage of at least 100 kV. Primary voltage service is defined for purposes of this Schedule as three-phase delivery voltage of at least 600 Volts but less than 100 kV. Secondary voltage service is defined for purposes of this Schedule as three-phase delivery voltage of less than 600 Volts.

(Continued on Sheet No. 451-G)