|  |  |  |  |
| --- | --- | --- | --- |
| (T) |  |  |  |
|  |  |  |  |
|  |  |  |  |
| (T) |  |  |  |
|  |  |  |  |
| (M) |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| (M) |  |  |  |
|  |  |  |  |
| (T) |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| (T) |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| (K) |  |  |  |
| I |  |  |  |
| I | (O) |  |  |
| I | (O) |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| I |  |  |  |
| (K) |  |  |  |

|  |
| --- |
| SCHEDULE NO. 87T |
| Distribution System Transportation Service (Non-Exclusive Interruptible with Firm Option) |
| (Continued) |

1. **Rates and Charges: (Continued)**
2. The annual minimum load charge shall apply when the actual total interruptible therms delivered to the Customer in the last year are less than the annual contract volume. The deficiency volume shall be the greater of zero or the actual total interruptible therms delivered subtracted from the annual contract volume. The amount of the annual minimum load charge shall be equal to the tailblock of the total transportation service commodity charge, per therm, identified in item 4. above.
3. **Adjustments:** Rates in this schedule are subject to conditions adjustments as set forth in Schedule No. 1 and to adjustment by Supplemental Schedule Nos. 112, 119, 129 and 132 in this tariff and other adjusting and supplemental schedules, when applicable.
4. **Definitions; Required Volumes:**
   1. Firm use gas. Firm use gas shall be that mutually determined hourly and daily contracted volume of gas set forth in the service agreement, which Company will deliver to the Customer through the interruptible gas metering facilities at all times, including periods of curtailment of interruptible gas, except as provided for in paragraph 3 of Section 7 of this schedule and Rule No. 23 of this tariff. If firm use gas is contracted for, the daily contracted volume shall not be less than two therms per day. The hourly rate of delivery of firm use gas shall not be greater than 1/18th of the firm use per day contracted for or 1/9th of contracted firm use for those Customers whose operation is limited to twelve hours per day. Monthly firm use gas shall be the daily contracted volume times the number of days in the billing cycle.
   2. Interruptible gas. Interruptible gas shall be all gas used in excess of firm use gas as define above. The annual contract volume of interruptible gas shall not be less than 750,000 therms per year.

(M) Transferred from Sheet No. 187T-A

(K) Transferred to Sheet No. 187T-C (Continued on Sheet No. 187T-C)