


Cost Breakdown of the Manganes.e treatment at Laureldel Well Site.

Laureldel Site::

Total Cost $1$0,299.d@

AtecandAssociates $50,410.00



$&,ns.oa

$20;.000.00

,fit fi.I'tratfon system $9 JlOO.oo.

Crane Rental $16!H;OO.


FI DFowler (Pltirtibin) $7,J52;00 Fineline Chlorine analyzer $6QU0,.00 Chlotiti.ator $4;,000:.00

Labor $16,000.00

Build 12' *x* 14' pump .house t<> house new flltrntfon system..

.. •· ·• 4! • •. .• - , : , . • :• • •. •: •. .•. '• •. • -• •. •






Cost Breakdown ofthe Manganese treatment at Southwood 1 Well Site.

Southwo.od lSite:

# Total Cost: $174,2'.;t7Jl0

Atec and Associates ,$74,338.00:

Atec'Pilot Study $833;00



$8,815.00

$20,000 00


fit filtration s}rstem $91000,QO


Evergreen Pre Cast(Tanks) $16?395.00 II DFowler (Plumbin. ) $7,152..00 Fin\_elin¢ Chlorirt ana1yz-er $6,000 ()0 Chlotinatot $'4. ,000.00

Lappr $J6 00000

Build p1:itnp house install treatment $id drain .field fat manges.e tiltratfon system.

···· ······· ···· ···· • • • '•' • • • ··· ·






Cost Breakdown of the Manganese treatment at'f itM¢adows Site.

# Fir Meadows Site:

Total Cost: $255,.554.:00



$34,000.00

. . lectric $J2,000.00

Evergreen Pre Cast ('l'®l<s) $19r395.00

Crane Rental $1,694;00

H]) J?owler (Plum.bing) $7,152.0()


Fineline Chlorine analyzer$o,OQO,OO

2"d Chlodnator for recycled water· $4,000.00 L.abor $18;000;QQ.

Build pump house and drain field fortreatment system.

.• ,. • • • • • • \_:\_. •. • • - •' • I! • - · .. •. •

•




Cost Breakdown of the·Manganese treatment at Centennial Elementary

Well Site..

Centennial Site:

Total Cost: ·$1s,s·.$9.©

Atec andAssociates $680QO'.'OO



p'house·to fit fllttation system *$1,0bb..OO*

ectric $1.o;OO<tbo

Crane Rental $'1694•.00

Hb:Fowler (Plumbing) $7J.5:2.00 Firteline Chlorine analyzer $6 000.00 Chlorfo.ator $4,000.00

Labor 18,000:.0Q

Install filtration system in.existing building; build separation walls and chlorine room. install

two tanks and drain field f'or backwash. ·

