**Qwest Corporation d/b/a CenturyLink QC**

**Section 2**

**WN U-48** 1st Revised Sheet 58.2

**Access Service** Cancels Original Sheet 58.2

**Washington**

|  |  |
| --- | --- |
| 2.  General Regulations  2.4 Payment Arrangements And Credit Allowances  2.4.7 Ordering, Rating And Billing Of Access Services Where More Than One Exchange Telephone Company Is Involved  G. Examples - Switched Access provisioned by Direct-Trunked Transport and Tandem-Switched Transport (Cont’d)  3. Example 2 Layout – Terminating Switched Access, Tandem 3rd Party  a. Terminating Feature Group D Switched Access is ordered to an end office via DTT & TST. Terminating – Tandem 3rd Party rates would apply.  b. The premises of ordering customer, the serving wire center (SWC) of that premises, and the access tandem are in operating territory of Company A.  c. The customer orders a DS3 Entrance Facility from the customer's premises to the SWC with a 3/1 Mux in the SWC.  .  d. The customer orders a DS1 DTT to the AT.  e. The BP for TT is 57 for Company A.  f. Company B is not a CLOC ILEC.  g. The end office is in the operating territory of Company B.  h. The BP for transport is 43 for Company B. | (T) |

Advice No. 3725T

Issued by Qwest Corporation d/b/a CenturyLink QC Effective: July 3, 2018

By Phil Grate, Director – Washington (T)

**Qwest Corporation d/b/a CenturyLink QC**

**Section 6**

**WN U-48** 1st Revised Sheet 45

**Access Service** Cancels Original Sheet 45

**Washington**

|  |  |
| --- | --- |
| 6.  Switched Access Service  6.2 Provision And Description Of Switched Access Services  6.2.3 Feature Group C (FGC)  A. Description (Cont'd)  6. No access code is required for FGC switching. The number dialed by the customer's end user shall be a seven or ten-digit number for calls in the North American Numbering Plan (NANP). The form of the numbers dialed by the customer's end user is NXX-XXXX, 0 or 1 + NPA + NXX-XXXX.    7. FGC switching, when used in the terminating direction, may be used to access valid NXX codes in the LATA, community information services of an information provider, and other customer's services (by dialing the appropriate codes) when the services can be reached using valid NXX codes. When FGC is directly routed to an end office via DTT, only those valid NXX codes served by that office may be accessed. When FGC is routed through an access tandem, only those valid NXX codes served by end offices subtending the access tandem may be accessed.  Additionally, non-access charges will also be billed for calls from a FGC trunk to another customer's service in accordance with that customer's applicable service rates when the Company performs the billing function for that customer. Calls in the terminating direction will not be completed to 101XXXX, 950-XXXX (or 1+950-XXXX) access codes, local operator assistance (0- and 0+), Directory Assistance (1+NPA+555-1212) and service code 911. Calls will be completed to Directory Assistance (1+NPA+555-1212) when FGC switching is combined with Directory Assistance switching. The combination of FGC Switched Access Service with Directory Assistance Service is provided as set forth in Section 9, following. FGC may not be switched, in the terminating direction, to another Trunkside Switched Access Service.  The Company will establish a trunk group or groups for the customer at end office switches or access tandem switches where FGC switching is provided. When required by technical limitations, a separate trunk group will be established for each type of FGC switching arrangement provided. Different types of FGC or other switching arrangements may be combined in a single trunk group at the option of the Company.  8. The Company will provide 0+ and 0- intraLATA access from pay telephones utilizing Smart Public Access Lines via FGC for calls dialed as 0+ or 0- and/or 101XXXX 1+ in the following manner. 1+ interLATA sent-paid access from pay telephones utilizing Basic Public Access Lines Service shall be provided by FGD. | (C)  (C) |

Advice No. 3725T

Issued by Qwest Corporation d/b/a CenturyLink QC Effective: July 3, 2018

By Phil Grate, Director – Washington (T)

**Qwest Corporation d/b/a CenturyLink QC**

**Section 6**

**WN U-48** 2nd Revised Sheet 46

**Access Service** Cancels 1st Revised Sheet 46

**Washington**

|  |  |
| --- | --- |
| 6.  Switched Access Service  6.2 Provision And Description Of Switched Access Services  6.2.3 Feature Group C (FGC)  A.8. (Cont'd)  a. Smart Public Access Line (PAL)  For traffic originating from a Smart PAL, the customer to whom such calls are routed shall order FGC trunks from end offices to the customer’s premises via direct trunks or via Operator Access Tandems, with the Operator Trunk-Full Feature type of transport termination, as set forth in 6.3.2, following. The trunks must be dedicated, and the customer shall specify the number of trunks required at each end office from which the customer will receive 0+ or 0- traffic.  The customer is responsible for providing all other operator services signaling capabilities, as described in the Operator Services Systems Generic Requirements (OSSGR) Technical Reference FR-271 and the LATA Switching Systems Generic Requirements (LSSGR) Technical Reference FR-64.  When the Company provides Operator Services Signaling (OSS) between an Operator Access Tandem and the customer's premises, the customer will be required to order a separate and final trunk group from the Operator Access Tandem to the customer's premises for each Numbering Plan Area (NPA) within a LATA to identify the originating NPA. Also, the customer must order a separate trunk group for each type of coin control signaling that is utilized among the equal access end offices subtending an Operator Access Tandem.  The Company will not block 101XXXX 0+ or 0- calls and will route 101XXXX traffic in accordance to the end user request. It will be the responsibility of the 101XXXX 1+ dialed carrier to complete the casual 101XXXX intraLATA call or to provide a recorded message to the end user. | (C)  (C)  (C)  (D)  (D) |

Advice No. 3725T

Issued by Qwest Corporation d/b/a CenturyLink QC Effective: July 3, 2018

By Phil Grate, Director – Washington (T)

**Qwest Corporation d/b/a CenturyLink QC**

**Section 6**

**WN U-48** 1st Revised Sheet 139.1

**Access Service** Cancels Original Sheet 139.1

**Washington**

|  |  |
| --- | --- |
| 6.  Switched Access Service  6.8 Rates And Charges  6.8.1 Switched Transport  C. Tandem-Switched Transport Usage Rates (Cont’d)  **Rate Per Access Minute**  2. Tandem Switching Charge:  Originating $0.003306  Terminating – Tandem 3rd Party 0.002252  Terminating – Tandem End Office 0.000000 (R)  3. Common Transport Multiplexing:  Originating 0.000198  Terminating – Tandem 3rd Party 0.000036  Terminating – Tandem End Office 0.000000  **Monthly**  **Rate**  4. Access Tandem Trunk Port Charge,  per port $6.00 |  |

Advice No. 3725T

Issued by Qwest Corporation d/b/a CenturyLink QC Effective: July 3, 2018

By Phil Grate, Director – Washington