ENERGY EFFICIENT MEASURES:

 Financial assistance will be provided based on the results of a cost-effective analysis (Savings to Investment Ratio of 1.0 or greater) through the use of a U.S Department of Energy approved energy audit or priority list. The energy efficient measures eligible for funding must be installed in dwellings with permanently installed operable electric space heat except where noted. The installation of measures listed as “Always considered cost effective” under Major and Supplemental Measures are not dependent on audit results. The energy efficient measures that may be eligible for funding are listed as follows along with their estimated measure life where applicable:

(C)

(C)

(C)

(D)

(C)

Major Measures:

(1) Ceiling insulation up to R-49 for ceilings with less than R-30 in place. R-30 or better attics will not be further insulated: 45 years.

1. Floor insulation over unheated spaces up to R-30: 45 years.

(3) Wall insulation or exterior insulation sheathing up to R-26 for walls with no insulation installed (financing will not be available for the installation of urea-formaldehyde wall insulation): 45 years.

Nothing shall preclude the Company from providing a reimbursement for the installation of a greater R value of insulation for the above items that are determined to be cost effective (Savings to Investment Ratio of 1.0 or greater) through the audit process.

Supplemental Measures:

1. Attic ventilation, excluding power ventilators when installed with ceiling insulation (required if needed at the time ceiling insulation is installed). Whole house mechanical ventilation, and spot ventilation for kitchen and baths: Always considered cost effective.

(2) Ground cover and water pipe wrap when installed with floor insulation; other vapor barrier materials as required when installed with floor or ceiling insulation: Always considered cost effective.

(3) Forced air electric space heating duct insulation and sealing in unheated spaces: 20 years.

1. Weather stripping and/or caulking, including blower door assisted air sealing and duct sealing: Always considered cost effective.

(5) Thermal doors: 30 years.