ENERGY EFFICIENT MEASURES:

Financial assistance will be provided based on the results of a cost-effective analysis (Savings to Investment Ratio of 1.0 or greater) through the use of a U.S Department of Energy approved energy audit or priority list. The energy efficient measures eligible for funding must be installed in dwellings with permanently installed operable electric space heat except where noted. Each measure life used in the cost-effective analysis is included in the Washington Department of Commerce’s Weatherization Manual. The energy efficient measures that may be eligible for funding are listed as follows:

(C)

(D)

(C)

(D)

(C)

(D)

(D)

(D)

(D)

(D)(C)

(C)(D)

(D)(C)

Major Measures:

(1) Ceiling insulation up to R-49 for ceilings with less than R-30 in place, and vapor barrier materials required when installed with ceiling insulation. R-30 or better attics will not be further insulated.

1. Floor insulation over unheated spaces up to R-30, and ground cover and other vapor barrier materials as required when installed with floor insulation.

(3) Wall insulation or exterior insulation sheathing up to R-26 for walls with no insulation installed (financing will not be available for the installation of urea-formaldehyde wall insulation).

Nothing shall preclude the Company from providing a reimbursement for the installation of a greater R value of insulation for the above items that are determined to be cost effective (Savings to Investment Ratio of 1.0 or greater) through the audit process.

Supplemental Measures:

(1) Attic ventilation, excluding power ventilators when installed with ceiling insulation (required if needed at the time ceiling insulation is installed). Whole house mechanical ventilation, and spot ventilation for kitchen and baths.

(2) Forced air electric space heating duct insulation and sealing in unheated spaces.

1. Weather stripping and/or caulking, including blower door assisted air sealing.

(4) Thermal doors.