# Avista

**Allocation of Natural Gas Distribution Mains**

## Adjusted Plant in Service ($)

**Load Factor % Average**

|  |  |  |  |
| --- | --- | --- | --- |
| **(1 – Load Factor) % Peak** | | | |
|  | |  | |
|  | Allocated to all classes based on peak. | |  |

Large Main (>= 4”) is allocated to all classes on annual throughput.

Small Main (< 2”) is allocated to all classes except Schedules 131, 132, and 146 on annual throughput.

Medium Main (2-3”)

1/3 allocated to all classes on annual throughput.

2/3 allocated to all classes except Schedules 131, 132, and 146 on annual throughput.