{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["ControlPanel","Variables","ClassValues","EnergyCosts","ParticipationRate","ImpactInput","CEInput","DR","Results","Translator"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":48,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ControlPanel","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,2,1,4],[3,2,3,4],[2,2,2,4],[4,2,4,4]]}
[null,"Control Panel"]
[null,"Customer Class","Residential"]
[null,"Option","DLC Water Heating"]
[null,"Potential","Market Potential"]
[null,"State","ID"]
[]
[null,"Customer Class","Residential","General Service","Large General Service","Extra Large General Service"]
[null,"DLC Smart Thermostats - Cooling","x","x"]
[null,"DLC Smart Thermostats - Heating","x","x"]
[null,"DLC Central AC","x","x",null,null,null,null,"Key:"]
[null,"DLC Water Heating","x","x",null,null,null,null,"Input Tabs"]
[null,"CTA-2045 WH","x","x",null,null,null,null,"Calculation Tabs"]
[null,"DLC Electric Vehicle Charging","x",null,null,null,null,null,"Results Tabs"]
[null,"Ancillary Cooling","x","x",null,null,null,null,"Red text is user input"]
[null,"Ancillary Heating","x","x"]
[null,"Ancillary DLC WH","x","x"]
[null,"Ancillary WH","x","x"]
[null,"Ancillary EV","x"]
[null,"Ancillary Third Party",null,"x","x","x"]
[null,"Ancillary Battery Storage","x","x","x","x"]
[null,"DLC Smart Appliances","x","x"]
[null,"Third Party Contracts",null,"x","x","x"]
[null,"Time-of-Use Opt-in","x","x","x","x"]
[null,"Time-of-Use Opt-out"]
[null,"Variable Peak Pricing Rates","x","x","x","x"]
[null,"Real Time Pricing"]
[null,"Behavioral","x"]
[null,"Thermal Energy Storage",null,"x","x","x"]
[null,"Battery Energy Storage","x","x","x","x"]

{"sheet":"Variables","index":1,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[null,"Data Element","Value","Description"]
[null,"Discount Rate",5.21E-2,"The discount rate for future cash flows."]
[null,"Inflation Rate",2.1000000000000001E-2,"The inflation rate."]
[null,"Base Year",2022,"The base year for the forecast."]
[null,"Forecast End",2045,"The forecast's end year."]
[null,"Hierarchy Enabled?",true,"Toggle Hierarchy"]
[null,"Include Avoided Cost Savings?",false,"Set to True if you would like to run the model with Avoided Cost Savings"]
[null,"Select First CE Program?",false,"Set to True if you would like to record only the first year in which a program is cost effective."]
[null,"Minimum BC Ratio",1,"The minimum required BC Ratio in order to pass the economic screen."]
[null,"Max Shift Years",0,"Maximum number of start year shifts to forecast"]
[null,"Years Shifted",0,"Model automatically calculates impacts and cost-effectiveness for years following the start year."]
[null,"State","WA","Territory residing in Washington"]
[null,"State","ID","Territory residing in Idaho"]
[null,"Potential","Market Potential","The Market Potential or Opt-In case."]

{"sheet":"ClassValues","index":2,"n_rows":77,"n_cols":78,"rows_kept":77,"cut":false,"hidden":false,"merged":[]}
["Key","State","Customer Class","Data Element","Unit",{"$f":"YearBase","v":2022},{"$f":"F1+1","v":2023},{"$f":"G1+1","v":2024},2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,"Growth Rate","Notes",null,null,null,null,"Annual Average",null,"State","Customer Class","Data Element","Unit",2021,2022,2023,2024,2025,{"$f":"YearBase","v":2022},{"$f":"BP1+1","v":2023},{"$f":"BQ1+1","v":2024},2025,2026,"Change","Change","Change","Change","Change","Average Change"]
[{"$f":"B2&C2&D2","v":"WAAllSummer Peak Load"},"WA","All","Summer Peak Load","MW @meter",851.67781881214989,855.38436292133622,859.28516389702463,863.04920363371127,866.57607601177097,869.2570822329709,871.96299095981408,874.69365133610131,877.44892190272026,880.2286703364291,883.03277319731524,885.86111568465924,888.71359140093193,891.59010212367878,894.49055758503368,897.41487525863067,900.36298015367618,903.33480461595775,906.33028813557507,909.3493771611785,912.39202492051322,915.45819124707191,918.54784241266555,921.66095096572428,924.79749557515402,927.95746087957173,931.14083734175404,934.34762110813722,937.57781387320779,940.83142274863712,944.10846013700916,947.40894361000062,950.73289579087384,954.0803442411526,957.45132135134679,960.84586423560711,964.26401463018237,967.70581879556767,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","All","Summer Peak Load","MW @meter",837.50284860843283,851.67781881214989,855.38436292133622,859.28516389702463,863.04920363371127,845.41241664707911,849.05211346240594,852.67005616859456,856.15863246747824,859.44443628821352,{"$f":"(BK2-BP2)/BP2","v":-9.3558692572978455E-3},{"$f":"(BL2-BQ2)/BQ2","v":3.0925137669540856E-3},3.1833025366672144E-3,3.6518132399548666E-3,4.1942994721870476E-3,{"$f":"AVERAGE(BU2:BY2)","v":9.5321195169307366E-4}]
[{"$f":"B3&C3&D3","v":"WAAllWinter Peak Load"},"WA","All","Winter Peak Load","MW @meter",822.82237949453463,826.32673878462947,829.99806638675204,833.53485271596151,836.85248558769115,839.38559607345337,841.94293577357405,844.52435245837546,847.12970323718389,849.75885429845391,852.41168065852105,855.08806591871576,857.78790203056792,860.51108906885645,863.25753501224813,866.02715553129565,868.81987378355734,871.63562021561916,874.47433237179996,877.33595470933267,880.22043841981736,883.127741256749,886.05782736893275,889.01066713960165,891.98623703105545,894.98451943465466,898.00550252599749,901.04918012512201,904.11555156157362,907.20462154419158,910.31640003546261,913.45090213030539,916.60814793914392,919.7881624751418,922.99097554546415,926.21662164644806,929.46513986255627,932.73657376900178,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","All","Winter Peak Load","MW @meter",809.04232731201125,822.82237949453463,826.32673878462947,829.99806638675204,833.53485271596151,888.45727621567221,892.18461606634764,895.8885582403841,899.4622731106025,902.83145482666509,{"$f":"(BK3-BP3)/BP3","v":-8.9385219784482967E-2},{"$f":"(BL3-BQ3)/BQ3","v":-7.7744264273051381E-2},{"$f":"(BM3-BR3)/BR3","v":-7.7645616540053919E-2},{"$f":"(BN3-BS3)/BS3","v":-7.7228594017204291E-2},{"$f":"(BO3-BT3)/BT3","v":-7.6754749449893578E-2},{"$f":"AVERAGE(BU3:BY3)","v":-7.9751688812937233E-2}]
["WAAllSummer Peak Load @ Gen","WA","All","Summer Peak Load @ Gen","MW @generator",904.14117245097839,908.07603967729062,912.21712999308147,916.213034577548,919.95716229409618,922.803318498522,925.67591120293866,928.57478025840521,931.49977549192795,934.45075642915322,937.42759202626996,940.43016041083433,943.45834863122946,946.51205241449748,949.59117593227188,952.69563157456241,955.82533973114266,958.98022858030083,962.16023388472661,965.36529879430714,968.59537365561698,971.85041582789165,975.13038950528585,978.43526554521304,981.76502130258359,985.11964046975345,988.49911292200613,991.90343456839855,995.33260720779754,998.78663838995328,1002.265541281449,1005.7693345363767,1009.2980421715918,1012.8516934464077,1016.4303227465898,1020.0339694725207,1023.6626779314017,1027.3164972333748,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","All","Summer Peak Load @ Gen","MW @generator",889.09302408271242,904.14117245097839,908.07603967729062,912.21712999308147,916.213034577548,904.18440283110056,908.07712669776026,911.94658413753427,915.67768178339918,919.19191046867752,-1.6690598401316564E-2,-4.3343832049762649E-3,-4.2442666353141555E-3,-3.7792247852736155E-3,-3.2407551211048515E-3,-6.4578456295970909E-3]
["WAAllWinter Peak Load @ Gen","WA","All","Winter Peak Load @ Gen","MW @generator",873.50823807139807,877.22846589376275,881.12594727617602,884.88059964326487,888.40259869989302,891.0917487915782,893.80662061722626,896.54705256981151,899.31289295659451,902.10399972323876,904.92024018708605,907.7614907793087,910.62763679565103,913.51857215549808,916.43419916900268,919.3744283120235,922.33917800862457,925.32837442090135,928.34195124590292,931.37984951942769,934.44201742647817,937.52841011816486,940.63898953485909,943.77372423540123,946.93258923216854,950.11556583182949,953.32264148159902,956.55380962082961,959.80906953776662,963.08842623131386,966.39189027764724,969.71947770153224,973.07120985219524,976.44711328361063,979.84721963906486,983.27156553986936,986.72019247808987,990.19314671317238,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","All","Winter Peak Load @ Gen","MW @generator",858.87933467443122,873.50823807139807,877.22846589376275,881.12594727617602,884.88059964326487,950.2216857921627,954.20814552550542,958.16958100575835,961.99173594716842,965.59513885204819,-9.6127411617198497E-2,-8.4572645740373514E-2,-8.4474728395191212E-2,-8.4060793507100842E-2,-8.3590457284966391E-2,-8.656520730896608E-2]
["WAResidentialSummer Peak Load","WA","Residential","Summer Peak Load","MW @meter",508.94048538730942,511.93390612547415,515.19934807192931,518.39172527691858,521.32989892806063,523.40537333167742,525.48911043806436,527.58114314199338,529.68150446919435,531.79022757687619,533.90734575425051,536.03289242305732,538.16690113809216,540.30940558773625,542.46043959448798,544.62003711549721,546.78823224310099,548.96505920536197,551.15055236660862,553.34474622797768,555.54767542795912,557.75937474294244,559.97987908776611,562.20922351626859,564.44744322184181,566.69457353798646,568.95064993887001,571.21570803988675,573.4897835982199,575.77291251340625,578.06513082790264,580.36647472765515,582.67698054267032,584.99668474758857,587.32562396226001,589.66383495232276,592.01135462978311,594.36822005359829,596.73446843026147,599.1101371143892,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Summer Peak Load","MW @meter",498.87970176387404,508.94048538730942,511.93390612547415,515.19934807192931,518.39172527691858,525.21697511856826,528.06250447126308,530.90528315197218,533.6091203591144,536.10051296652182,-5.0145510526860927E-2,-3.621165851019871E-2,-3.573401438739772E-2,-3.4500482815577577E-2,-3.3032588593529498E-2,-3.7924850966712893E-2]
["WAResidentialWinter Peak Load","WA","Residential","Winter Peak Load","MW @meter",472.70065615274297,475.48092612084122,478.51384764120985,481.47890709867687,484.20786392695629,486.13555123143794,488.07091288121779,490.01397942874877,491.96478154811672,493.92335003552455,495.88971580977841,497.86390991277574,499.84596350999539,501.83590789098952,503.83377446987771,505.83959478584262,507.85340050362817,509.87522341403917,511.90509543444335,513.94304860927514,515.98911511054155,518.04332723833011,520.10571742131856,522.17631821728719,524.25516231363235,526.34228252788273,528.4377118082175,530.54148323398624,532.6536300162312,534.77418549821164,536.90318315593026,539.04065659866149,541.18663956948217,543.34116594580428,545.50426973990955,547.67598509948664,549.85634630817003,552.04538778608128,554.24314409037254,556.44964991577194,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Winter Peak Load","MW @meter",463.35626489923618,472.70065615274297,475.48092612084122,478.51384764120985,481.47890709867687,531.70376100280248,534.5844345730543,537.46232349865579,540.19955492925124,542.72171792520942,-0.12854431568184085,-0.11576053176657639,-0.11532231129122038,-0.11419059257855226,-0.11284385496983595,-0.11733232125760518]
["WAResidentialCustomer Population","WA","Residential","Customer Population","#",234948.21728845764,237104.15365298794,239413.17054642178,241597.52052238034,243801.79999848534,246026.19080685184,248270.87643858872,250536.04205893492,252821.87452253397,255128.56238884755,257456.29593770995,259805.26718502431,262175.66989860212,264567.69961414731,266981.55365138588,269417.43113034312,271875.53298776899,274356.06199371355,276859.22276825353,279385.22179837152,281934.26745498931,284506.57001015631,287102.34165439522,289721.79651420552,292365.15066972707,295032.6221725645,297724.43106377451,300440.79939201707,303181.95123187237,305948.11270232499,308739.51198541623,311556.37934506737,314398.94714607386,317267.44987327349,320162.12415088905,323083.20876204764,326030.94466847787,329005.57503038709,332007.34522651968,335036.50287439849,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Customer Population","#",233036.2725682153,234948.21728845764,237104.15365298794,239413.17054642178,241597.52052238034,231769.008925,233824.27949999998,235803.30007500001,237679.48731666664,239570.60258760458,5.4677872986261854E-3,4.806762543483719E-3,5.5166894508014916E-3,7.2942063672718745E-3,8.4606287786689952E-3,6.3092148877704531E-3]
["WAResidentialPer Customer Summer Peak (kW)","WA","Residential","Per Customer Summer Peak (kW)","kW @meter",2.1661815154888271,2.1591098183573423,2.1519256726606573,2.145683135141685,2.1383349053669805,2.1274376179834777,2.1165958648720009,2.10580936302126,2.095077830862234,2.0844009882608203,2.0737785565105242,2.0632102583251837,2.0526958178317281,2.0422349605629795,2.0318274134504879,2.0214729048174025,2.0111711643713801,2.0009219231975295,1.9907249137513907,1.9805798698519532,1.9704865266747047,1.9604446207447217,1.9504538899297879,1.9405140734335553,1.9306249117887342,1.92078614685032,1.9109975217888553,1.9012587810837265,1.8915696705164917,1.8819299371642464,1.8723393293930204,1.8627975968512092,1.8533044904630389,1.8438597624220654,1.8344631661847033,1.8251144564637931,1.8158133892221962,1.8065597216664253,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Per Customer Summer Peak (kW)","kW @meter",2.1407813310172132,2.1661815154888271,2.1591098183573423,2.1519256726606573,2.145683135141685,2.2661225396555391,2.2583732775760059,2.2514752040497803,2.2450785567715941,2.2377558313753632,-5.5310869754368316E-2,-4.0822198439281747E-2,-4.1024385045990409E-2,-4.1492037697286613E-2,-4.1145103921855823E-2,-4.3958918971756578E-2]
["WAResidentialPer Customer Winter Peak (kW)","WA","Residential","Per Customer Winter Peak (kW)","kW @meter",2.0119354877776527,2.0053673408721799,1.9986947524611096,1.9928967236817119,1.9860717350321635,1.9759504044554719,1.9658806537541873,1.9558622200692393,1.9458948418811286,1.9359782590030987,1.9261122125743473,1.9162964450532649,1.9065307002107159,1.8968147231233465,1.8871482601669336,1.8775310590097618,1.8679628686060368,1.8584434391893343,1.8489725222660767,1.8395498706090501,1.830175238250948,1.8208483804779518,1.811569053823342,1.8023370160611443,1.7931520261998051,1.7840138444759011,1.774922232347881,1.7658769524898392,1.7568777687853185,1.7479244463211481,1.7390167513813124,1.7301544514408469,1.7213373151597731,1.7125651123770551,1.7038376141045937,1.6951545925212494,1.6865158209668942,1.6779210739364954,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Per Customer Winter Peak (kW)","kW @meter",1.9883439594735224,2.0119354877776527,2.0053673408721799,1.9986947524611096,1.9928967236817119,2.2941106900744472,2.2862657193521017,2.2792824499390365,2.2728067997282793,2.2653936337065836,-0.13328333803762638,-0.11999052833289675,-0.12017602692206178,-0.12060508059899352,-0.12028678193953372,-0.12286835116622244]
["WAResidentialSaturation Central AC","WA","Residential","Saturation Central AC","%",0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.41058159019236529,0.43416548076018596,0.45910403482876017,0.4854750645468085,0.51336085160879863,0.54284840398656775,0.574029727407662,0.60700211242744695,0.64186843799069937,0.6787374924298385,0.71772431290136185,0.75895054431957887,0.80254481890757212,0.84864315754964303,0.89738939419752461,0.9489356246545736,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Saturation Central AC","%",0.31054202419477445,0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.36715460254415411,0.36891706095211718,0.37068797971879092,0.37246739945657742,0.37425536097283113,{"$f":"BK11-BP11","v":-5.6612578349379661E-2},{"$f":"BL11-BQ11","v":-4.053743933392262E-2},-2.3446165430639043E-2,-5.2799442912824235E-3,1.4023416763545626E-2,-2.2370542128335624E-2]
["WAResidentialSaturation Elec Space Heat","WA","Residential","Saturation Elec Space Heat","%",0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Saturation Elec Space Heat","%",0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.1834748890528064,0.18441133157179282,0.18535795289838183,0.18631485403231768,0.18728213698451929,{"$f":"BK12-BP12","v":0.22452511094719357},{"$f":"BL12-BQ12","v":0.22358866842820715},{"$f":"BM12-BR12","v":0.22264204710161814},{"$f":"BN12-BS12","v":0.2216851459676823},{"$f":"BO12-BT12","v":0.22071786301548069},0.22263176709203636]
["WAResidentialSaturation Elec Water Heat","WA","Residential","Saturation Elec Water Heat","%",0.50120862662826382,0.49441459619652989,0.48771266084667403,0.48110157220275923,0.47458009881095176,0.4681470259101369,0.46180115520564441,0.45554130464604092,0.44936630820294804,0.44327501565384531,0.43726629236781689,0.43133901909420302,0.42549209175411595,0.41972442123478221,0.41403493318667239,0.40842256782338127,0.40288627972422009,0.39742503763948522,0.39203782429836631,0.3867236362194581,0.38148148352384115,0.37631038975069608,0.37120939167541728,0.36617753913019213,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Saturation Elec Water Heat","%",0.50809601767245227,0.50120862662826382,0.49441459619652989,0.48771266084667403,0.48110157220275923,0.43462810835545662,0.41782274446955009,0.40102066420800586,0.38422187659632434,0.36742639068481409,7.346790931699565E-2,8.3385882158713731E-2,9.3393931988524026E-2,0.10349078425034969,0.11367518151794515,9.3482737846505654E-2]
[{"$f":"B14&C14&D14","v":"WAResidentialSaturation CTA-2045 Water Heat"},"WA","Residential","Saturation CTA-2045 Water Heat","%",1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0.09,0.11461034197302272,0.13922068394604545,0.16383102591906817,0.1884413678920909,0.21305170986511363,0.23766205183813635,0.26227239381115908,0.28688273578418183,0.31149307775720458,0.33610341973022734,0.36071376170325009,0.38532410367627284,0.4099344456492956,0.43454478762231835,0.45915512959534088,0.4741551295953409,0.48915512959534091,0.50415512959534092,0.51915512959534094,0.53415512959534095,0.54915512959534096,0.56415512959534098,0.57915512959534099,0.594155129595341,0.60915512959534102,0.62415512959534103,0.63915512959534104,0.65415512959534106,0.66915512959534107,0.68415512959534108,0.6991551295953411,0.71415512959534111,0.72915512959534112,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Saturation CTA-2045 Water Heat","%",0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,0,0,0,0,0]
["WAResidentialSaturation Elec Vehicles","WA","Residential","Saturation Elec Vehicles","%",1.3330979366300576E-2,1.561924184676035E-2,1.8300284560060061E-2,2.1441528229402231E-2,2.5121966344480925E-2,2.9434151626739111E-2,3.4486523471368408E-2,4.0406134894705785E-2,4.7341847562124749E-2,5.5468075242433468E-2,6.498916982618444E-2,7.614456020398494E-2,8.921477323322026E-2,0.10452848820365733,0.12247080220200145,0.1434929142262,0.16812347157787377,0.19698186386290012,0.23079379890706891,0.27040955227751162,0.31682534933430856,0.37120841751105021,0.43492633881911552,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Saturation Elec Vehicles","%",1.137795371941131E-2,1.3330979366300576E-2,1.561924184676035E-2,1.8300284560060061E-2,2.1441528229402231E-2,4.1827814066743669E-3,5.081675856541689E-3,6.1166687907630978E-3,7.2966063543678759E-3,8.6939684048043912E-3,7.1951723127369428E-3,8.2493035097588874E-3,9.5025730559972522E-3,1.1003678205692185E-2,1.274755982459784E-2,9.7396573817566216E-3]
["WAResidentialSaturation Appliances","WA","Residential","Saturation Appliances","%",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Saturation Appliances","%",1,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0]
["WAResidentialSaturation AMI","WA","Residential","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Residential","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0]
["WAGeneral ServiceSummer Peak Load","WA","General Service","Summer Peak Load","MW @meter",82.553243740473945,83.421170332733325,84.292125093702282,85.117770324181976,85.951544435321352,86.793527533401502,87.643800514242088,88.502445070983285,89.369543701944693,90.245179718561332,91.129437253398152,92.022401268243442,92.924157562282005,93.834792780348863,94.754394421264337,95.683050846251433,96.620851287435798,97.567885856429996,98.524245553001833,99.490022273828686,100.46530882133752,101.45019891263263,102.44478718851089,103.44916922256618,104.46344153038339,105.48770157882309,106.52204779539775,107.56657957774033,108.62139730316618,109.68660233832922,110.76229704897332,111.84858480977974,112.94557001431171,114.05335808505686,115.17205548356883,116.30176972070883,117.44260936698788,118.59468406301141,119.75810453002633,120.93298258057254,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Summer Peak Load","MW @meter",81.642473954875783,82.553243740473945,83.421170332733325,84.292125093702282,85.117770324181976,76.210413965382784,77.058981509049929,77.888486399050691,78.726949296335036,79.574467059858975,7.1277135326418967E-2,7.1299440037093695E-2,7.1033399023017432E-2,7.0689590376726577E-2,6.9661833363622971E-2,7.0792279625375917E-2]
["WAGeneral ServiceWinter Peak Load","WA","General Service","Winter Peak Load","MW @meter",82.118842438313337,82.982201936358436,83.848573668664372,84.669874292596916,85.499261022415155,86.33681354287495,87.182612324116178,88.036738629403644,88.899274522944637,89.770302877783223,90.649907383772543,91.538172555625664,92.435183741045677,93.341027128936062,94.255789757691844,95.179559523572692,96.112425189158202,97.054476391886908,98.00580365267912,98.966498384645021,99.936652901878347,100.91636042833701,101.90571510681099,102.90481200797882,103.91374713955318,104.93261745551681,105.96152086544929,107.00055624394582,108.0498234401289,109.10942328725358,110.17945761240755,111.26002924630684,112.351242033188,113.45320084079768,114.56601157048092,115.68978116736881,116.82461763066624,117.97063002404164,119.12792848611851,120.29662424107084,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Winter Peak Load","MW @meter",81.212865190995998,82.118842438313337,82.982201936358436,83.848573668664372,84.669874292596916,82.639789595947491,83.559945249457741,84.459430057526234,85.368628601534411,86.287645911796758,-1.7266796199847372E-2,-1.724633503339635E-2,-1.7490387043360839E-2,-1.7805778981937605E-2,-1.8748589118464644E-2,-1.7711577275401364E-2]
["WAGeneral ServiceCustomer Population","WA","General Service","Customer Population","#",23328.459694842724,23557.51011569651,23798.089664878378,24029.339658011177,24262.848778745582,24498.639096951942,24736.732898105609,24977.152685393194,25219.921181839469,25465.061332454974,25712.596306404663,25962.549499197703,26214.944534898681,26469.805268360407,26727.155787478529,26987.020415468171,27249.423713162832,27514.390481335704,27781.945763043714,28052.11484599442,28324.923264936075,28600.396804071002,28878.561499492564,29159.443641645936,29443.069777812922,29729.466714621049,30018.66152057716,30310.681528625759,30605.554338732371,30903.307820492111,31203.970115763768,31507.569641329574,31814.135091581014,32123.695441230822,32436.27994805152,32751.918155640677,33070.639896213179,33392.475293420801,33717.454765199313,34045.609026643382,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Customer Population","#",23118.118330148642,23328.459694842724,23557.51011569651,23798.089664878378,24029.339658011177,23462.974389129256,23718.391026690559,23969.724360023891,24223.735012487272,24480.4515041247,-1.4697883280322366E-2,-1.6440041460191818E-2,-1.7197287634014735E-2,-1.7571416934237208E-2,-1.8427431619776918E-2,-1.6866812185708607E-2]
["WAGeneral ServicePer Customer Summer Peak (kW)","WA","General Service","Per Customer Summer Peak (kW)","kW @meter",3.5387352967296071,3.5411709439169168,3.5419702287323513,3.5422434214002396,3.5425165947790713,3.5427897521132157,3.5430628965943209,3.5433360313619779,3.5436091595043728,3.5438822840589319,3.5441554080129598,3.5444285343042727,3.5447016658218211,3.5449748054063104,3.5452479558508077,3.5455211199013545,3.5457943002575538,3.5460674995731725,3.5463407204567154,3.5466139654720163,3.5468872371387961,3.5471605379332405,3.5474338702885526,3.5477072365955089,3.5479806392030055,3.5482540804186002,3.548527562509046,3.5488010877008227,3.5490746581806589,3.5493482760960493,3.549621943555763,3.5498956626303557,3.5501694353526694,3.5504432637183192,3.5507171496861902,3.5509910951789196,3.5512651020833705,3.5515391722511116,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Per Customer Summer Peak (kW)","kW @meter",3.5315362949935576,3.5387352967296071,3.5411709439169168,3.5419702287323513,3.5422434214002396,3.2481139305463422,3.2489126864606725,3.2494527358416838,3.2499921773315097,3.2505310225365536,8.7257519442842602E-2,8.9206032367913177E-2,8.9774565685341826E-2,8.9839616672732367E-2,8.9742997941317335E-2,8.9164146422029467E-2]
["WAGeneral ServicePer Customer Winter Peak (kW)","WA","General Service","Per Customer Winter Peak (kW)","kW @meter",3.5201142086748032,3.5225370393056479,3.5233321182249981,3.5236038733327701,3.5238756092529862,3.5241473292129419,3.5244190363874934,3.5246907338997095,3.5249624248215268,3.5252341121743869,3.5255057989298759,3.525777488010351,3.5260491822895603,3.5263208845932623,3.526592597699826,3.5268643243408433,3.5271360672017114,3.5274078289222324,3.5276796120971863,3.5279514192769144,3.5282232529678801,3.5284951156332385,3.5287670096933885,3.5290389375265274,3.5293109014691901,3.5295829038167912,3.529854946824158,3.5301270327060532,3.530399163637699,3.530671341755288,3.5309435691564959,3.5312158479009819,3.5314881800108893,3.5317605674713337,3.5320330122308929,3.5323055162020855,3.532578081261847,3.5328507092520023,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Per Customer Winter Peak (kW)","kW @meter",3.5129530886207654,3.5201142086748032,3.5225370393056479,3.5233321182249981,3.5236038733327701,3.5221361207399058,3.5230022624817527,3.523587872307183,3.5241728229576119,3.5247571270186007,-2.6072337366709417E-3,-8.1977063645570763E-4,-2.9822812417815814E-4,-2.3855377555185371E-4,-3.2718670940201731E-4,-8.5819459645173572E-4]
["WAGeneral ServiceSaturation Central AC","WA","General Service","Saturation Central AC","%",0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.41058159019236529,0.43416548076018596,0.45910403482876017,0.4854750645468085,0.51336085160879863,0.54284840398656775,0.574029727407662,0.60700211242744695,0.64186843799069937,0.6787374924298385,0.71772431290136185,0.75895054431957887,0.80254481890757212,0.84864315754964303,0.89738939419752461,0.9489356246545736,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Saturation Central AC","%",0.31054202419477445,0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.36715460254415411,0.36891706095211718,0.37068797971879092,0.37246739945657742,0.37425536097283113,{"$f":"BK23-BP23","v":-5.6612578349379661E-2},{"$f":"BL23-BQ23","v":-4.053743933392262E-2},{"$f":"BM23-BR23","v":-2.3446165430639043E-2},{"$f":"BN23-BS23","v":-5.2799442912824235E-3},{"$f":"BO23-BT23","v":1.4023416763545626E-2},-2.2370542128335624E-2]
["WAGeneral ServiceSaturation Elec Water Heat","WA","General Service","Saturation Elec Water Heat","%",0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Saturation Elec Water Heat","%",0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.45200000000000001,0.434,0.41600000000000004,0.39800000000000002,0.38,0.14889668805662698,0.166896688056627,0.18489668805662696,0.20289668805662697,0.22089668805662699,0.18489668805662698]
["WAGeneral ServiceSaturation CTA-2045 Water Heat","WA","General Service","Saturation CTA-2045 Water Heat","%",1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0.09,0.11413333333333334,0.13826666666666668,0.16240000000000002,0.18653333333333336,0.2106666666666667,0.23480000000000004,0.25893333333333335,0.28306666666666669,0.30720000000000003,0.33133333333333337,0.35546666666666671,0.37960000000000005,0.40373333333333339,0.42786666666666673,0.45200000000000001,0.47700000000000004,0.502,0.52700000000000002,0.55200000000000005,0.57700000000000007,0.60200000000000009,0.62700000000000011,0.65200000000000014,0.67700000000000016,0.70200000000000018,0.7270000000000002,0.75200000000000022,0.77700000000000025,0.80200000000000027,0.82700000000000029,0.85200000000000031,0.87700000000000033,0.90200000000000036,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Saturation CTA-2045 Water Heat","%",0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,0,0,0,0,0]
["WAGeneral ServiceSaturation Elec Space Heat","WA","General Service","Saturation Elec Space Heat","%",0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Saturation Elec Space Heat","%",0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0,0,0,0,0,0]
["WAGeneral ServiceSaturation AMI","WA","General Service","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","General Service","Saturation AMI","%",0.66659999999999997,1,1,1,1,0.66659999999999997,1,1,1,1,0,0,0,0,0,0]
["WALarge General ServiceSummer Peak Load","WA","Large General Service","Summer Peak Load","MW @meter",186.03550103573571,185.76191625793456,185.4747487703068,185.19597048279891,184.92607834795717,184.66478913940105,184.41182865796193,184.16693144396069,183.92984049865598,183.70030701457046,183.47809011441251,183.26295659831931,183.05468069915568,182.85304384561252,182.65783443285565,182.46884760048513,182.28588501757127,182.10875467454224,181.93727068170489,181.77125307418717,181.61052762309771,181.45492565270396,181.30428386343786,181.15844416054236,181.01725348817965,180.88056366882677,180.74823124779033,180.62011734267662,180.49608749765983,180.37601154239485,180.25976345542736,180.14722123195699,180.03826675581524,179.93278567552451,179.83066728430614,179.73180440391451,179.63609327217242,179.54343343409161,179.45372763646347,179.36688172580935,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Large General Service","Summer Peak Load","MW @meter",185.60117464252585,186.03550103573571,185.76191625793456,185.4747487703068,185.19597048279891,173.2793132666134,173.33231993013067,173.38543320846506,173.43881288634788,173.49246030055886,7.1109823461463148E-2,7.328801178410134E-2,7.1381331294359571E-2,6.9395861766223657E-2,6.745832160063242E-2,7.0526669981356024E-2]
["WALarge General ServiceWinter Peak Load","WA","Large General Service","Winter Peak Load","MW @meter",185.05656840709079,184.78442325271743,184.49876686174574,184.22145552629959,183.95298358392401,183.69306929859675,183.44143991400563,183.19783136734,182.96198801220501,182.73366235036679,182.5126147720479,182.29861330450052,182.09143336859293,181.89085754315445,181.69667533683133,181.50868296721421,181.32668314700553,181.15048487700207,180.97990324567607,180.81475923514398,180.65487953331984,180.50009635205535,180.35024725107684,180.20517496753368,180.06472725097922,179.92875670361167,179.79712062560685,179.66968086538054,179.54630367462349,179.4268595679566,179.3112231870598,179.19927316913106,179.09089201953796,178.98596598852882,178.88438495187231,178.78604229530268,178.69083480264703,178.5986625475187,178.50942878846271,178.42303986744298,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Large General Service","Winter Peak Load","MW @meter",184.62452747163189,185.05656840709079,184.78442325271743,184.49876686174574,184.22145552629959,187.89775890979547,187.95523739983807,188.01283149909463,188.0707144722922,188.12888776898598,-1.7420279289946005E-2,-1.5422124080431572E-2,-1.7171212308414948E-2,-1.8992577449226961E-2,-2.0769974717995136E-2,-1.7955233569202922E-2]
["WALarge General ServiceCustomer Population","WA","Large General Service","Customer Population","#",1846.9634442056276,1844.6790514454428,1842.4155174741772,1840.1646871637577,1837.9919875922317,1835.8947068625957,1833.8702272070641,1831.9160217198687,1830.0296512034643,1828.208761124198,1826.4510786736489,1824.7544099319675,1823.116637129674,1821.5357160044994,1820.0096732499703,1818.5366040525521,1817.1146697142772,1815.7420953578915,1814.4171677116549,1813.1382329710302,1811.9036947345921,1810.7120120115815,1809.5616972986147,1808.4513147231521,1807.3794782514053,1806.3448499584467,1805.3461383583647,1804.3820967923773,1803.4515218728945,1802.5532519815877,1801.686165819588,1800.8491810080106,1800.0412527370511,1799.2613724619739,1798.5085666443601,1797.7818955370494,1797.0804520112524,1796.4033604243778,1795.7497755271529,1795.118881408682,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Large General Service","Customer Population","#",1849.0530968634114,1846.9634442056276,1844.6790514454428,1842.4155174741772,1840.1646871637577,1844.0874340658961,1844.0894915813856,1844.0897459699784,1844.0900003586078,1844.090254747274,2.6927480258172169E-3,1.5584670035604009E-3,3.1956442290963466E-4,-9.0802666036087832E-4,-2.1287285551293829E-3,3.0680484735939829E-4]
["WALarge General ServicePer Customer Summer Peak (kW)","WA","Large General Service","Per Customer Summer Peak (kW)","kW @meter",100.72505853831282,100.70148306415489,100.66933708014993,100.64097619884289,100.61310364590338,100.58571902251362,100.55882140516358,100.53240937925645,100.50648107133128,100.48103417993133,100.45606600514726,100.4315734768669,100.40755318176356,100.38400138905695,100.36091407508052,100.33828694669054,100.31611546355184,100.29439485933587,100.27312016186684,100.25228621225122,100.23188768302613,100.21191909536157,100.19237483535161,100.17324916942822,100.15453625893183,100.1362301738717,100.11832490590869,100.10081438059171,100.08369246887969,100.0669529979785,100.05058976152326,100.03459652913358,100.01896705537065,100.00369508812277,99.988774376444852,99.974198677878789,99.959961765277512,99.946057433157293,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Large General Service","Per Customer Summer Peak (kW)","kW @meter",100.37633584312161,100.72505853831282,100.70148306415489,100.66933708014993,100.64097619884289,93.964803439152703,93.993442683462618,94.022231611762209,94.051164993368218,94.080243553120113,6.8233340243410615E-2,7.1617930598839294E-2,7.103906531353911E-2,7.0367784250714771E-2,6.9735498101877499E-2,7.0198723701676263E-2]
["WALarge General ServicePer Customer Winter Peak (kW)","WA","Large General Service","Per Customer Winter Peak (kW)","kW @meter",100.19503579654386,100.17158437828256,100.13960754883385,100.11139590459143,100.08367001909637,100.05642949562953,100.02967341554047,100.00340037167602,99.977608500433604,99.952295512466875,99.927458722073624,99.903095075296832,99.879201176771005,99.855773315347477,99.832807488532552,99.810299425773323,99.788244610626194,99.766638301843429,99.745475553413186,99.724751233588364,99.70446004293963,99.684596531467008,99.66515511480533,99.646130089557047,99.627515647786012,99.609305890705613,99.591494841592962,99.574076457961212,99.55704464302076,99.540393256459183,99.5241161245699,99.508207049757345,99.492659819446615,99.477468214425059,99.462626016640584,99.44812701648334,99.433965019573947,99.420133853082419,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Large General Service","Per Customer Winter Peak (kW)","kW @meter",99.848148106084395,100.19503579654386,100.17158437828256,100.13960754883385,100.11139590459143,101.89200112681922,101.9230564774047,101.95427413984193,101.98564844216895,102.01718017037531,-2.0059013446904049E-2,-1.6954168571700179E-2,-1.7485189086964666E-2,-1.8100986967611424E-2,-1.8681012968610734E-2,-1.825607420835821E-2]
["WALarge General ServiceSaturation AMI","WA","Large General Service","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Large General Service","Saturation AMI","%",0.66659999999999997,1,1,1,1,0.66659999999999997,1,1,1,1,{"$f":"BK33-BP33","v":0},{"$f":"BL33-BQ33","v":0},{"$f":"BM33-BR33","v":0},{"$f":"BN33-BS33","v":0},{"$f":"BO33-BT33","v":0},0]
["WAExtra Large General ServiceSummer Peak Load","WA","Extra Large General Service","Summer Peak Load","MW @meter",74.148588648630835,74.267370205194212,74.318941961086267,74.343737549811834,74.368554300431811,74.393392228490967,74.41825134954567,74.443131679163884,74.468033232925279,74.492956026421055,74.517900075254147,74.542865395039101,74.567852001402116,74.592859909981129,74.61788913642566,74.642939696396994,74.66801160556804,74.693104879623533,74.718219534259802,74.743355585184943,74.768513048118805,74.793691938792961,74.818892272950706,74.844114066347174,74.869357334749154,74.894622093935325,74.919908359696066,74.945216147833591,74.970545474161895,74.995896354506783,75.021268804705926,75.046662840608747,75.072078478076591,75.097515732982629,75.122974621211782,75.148455158660994,75.173957361238962,75.199481244866348,75.225026825475652,75.250594119011282,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Extra Large General Service","Summer Peak Load","MW @meter",71.379498247157116,74.148588648630835,74.267370205194212,74.318941961086267,74.343737549811834,70.705714296514657,70.598307551962321,70.490853409106592,70.383749925680902,70.276995961273911,9.5294129667773189E-3,5.0288473191165486E-2,5.3574564832828908E-2,5.5910519680474315E-2,5.7867322484570882E-2,4.5434058631163385E-2]
["WAExtra Large General ServiceWinter Peak Load","WA","Extra Large General Service","Winter Peak Load","MW @meter",82.946312496387492,83.079187474712441,83.136878215132072,83.164615798388155,83.192377054395664,83.220162000543723,83.247970654234493,83.275803032883061,83.303659153917621,83.331539034779283,83.359442692922244,83.387370145813733,83.415321410933998,83.443296505776402,83.471295447847282,83.499318254666136,83.527364943765477,83.555435532691021,83.583530039001445,83.611648480268641,83.639790874077605,83.66795723802646,83.696147589726436,83.724361946802006,83.752600326890715,83.780862747643354,83.809149226723846,83.837459781809315,83.865794430590114,83.894153190769757,83.922536080065058,83.950943116205977,83.979374316935804,84.007829700011058,84.036309283201419,84.06481308428998,84.093341121073024,84.121893411360176,84.150469972974335,84.179070823751729,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Extra Large General Service","Winter Peak Load","MW @meter",79.848669750147195,82.946312496387492,83.079187474712441,83.136878215132072,83.164615798388155,86.215966707126753,86.084998843997454,85.953973185107415,85.823375107524569,85.69320322067297,-7.3852874359213408E-2,-3.6460317009446262E-2,-3.3445640775720022E-2,-3.1302624594135298E-2,-2.9507444315896556E-2,-4.0913780210882308E-2]
["WAExtra Large General ServiceCustomer Population","WA","Extra Large General Service","Customer Population","#",22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,22,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Extra Large General Service","Customer Population","#",22,22,22,22,22,19.974360285601595,19.974359245138892,19.974359245138892,19.974359245138892,19.974359245138892,0.10141199444863204,0.10141205182109073,0.10141205182109073,0.10141205182109073,0.10141205182109073,0.10141204034659898]
["WAExtra Large General ServicePer Customer Summer Peak (kW)","WA","Extra Large General Service","Per Customer Summer Peak (kW)","kW @meter",3370.3903931195837,3375.7895547815551,3378.1337255039216,3379.2607977187199,3380.3888318378099,3381.5178285677712,3382.6477886157122,3383.7787126892676,3384.9106014966037,3386.0434557464118,3387.177276147916,3388.3120634108682,3389.4478182455505,3390.5845413627785,3391.7222334738935,3392.8608952907725,3394.00052752582,3395.1411308919787,3396.2827061027183,3397.425253872043,3398.5687749144913,3399.7132699451345,3400.8587396795774,3402.0051848339622,3403.1526061249619,3404.3010042697874,3405.450379986185,3406.6007339924358,3407.7520670073586,3408.9043797503082,3410.0576729411787,3411.2119473003972,3412.3672035489362,3413.523442408301,3414.6806646005357,3415.8388708482266,3416.9980618744985,3418.1582384030162,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Extra Large General Service","Per Customer Summer Peak (kW)","kW @meter",3244.5226475980508,3370.3903931195837,3375.7895547815551,3378.1337255039216,3379.2607977187199,3539.8237182836078,3534.4466716319648,3529.06706763381,3523.7050191139433,3518.3604689786007,-8.3422535749532428E-2,-4.641639661141958E-2,-4.3432870476736302E-2,-4.1311997690041173E-2,-3.9535366681817619E-2,-5.0823833441909418E-2]
["WAExtra Large General ServicePer Customer Winter Peak (kW)","WA","Extra Large General Service","Per Customer Winter Peak (kW)","kW @meter",3770.2869316539773,3776.3267033960201,3778.9490097787307,3780.2098090176432,3781.4716842907119,3782.7346363883507,3783.9986661015678,3785.2637742219572,3786.5299615417102,3787.7972288536039,3789.0655769510108,3790.3350066278972,3791.605518678818,3792.8771138989273,3794.1497930839673,3795.423557030279,3796.6984065347942,3797.9743423950463,3799.2513654091567,3800.5294763758475,3801.8086760944366,3803.0889653648392,3804.3703449875652,3805.6528157637276,3806.9363784950324,3808.2210339837889,3809.5067830329017,3810.7936264458781,3812.0815650268232,3813.3705995804435,3814.6607309120482,3815.9519598275442,3817.2442871334456,3818.5377136368661,3819.8322401455189,3821.1278674677264,3822.4245964124102,3823.7224277890987,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"WA","Extra Large General Service","Per Customer Winter Peak (kW)","kW @meter",3629.4849886430543,3770.2869316539773,3776.3267033960201,3778.9490097787307,3780.2098090176432,4316.3318111006056,4309.7752367174298,4303.2155439992803,4296.677257790443,4290.1603084728686,-0.15912743795348178,-0.12517782840906516,-0.1224407272226911,-0.12049502835545833,-0.11886513854694349,-0.12922123209752798]
["WAExtra Large General ServiceSaturation AMI","WA","Extra Large General Service","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WA","Extra Large General Service","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,{"$f":"BK39-BP39","v":0},{"$f":"BL39-BQ39","v":0},{"$f":"BM39-BR39","v":0},{"$f":"BN39-BS39","v":0},{"$f":"BO39-BT39","v":0},0]
[{"$f":"B40&C40&D40","v":"IDAllSummer Peak Load"},"ID","All","Summer Peak Load","MW @meter",438.21549320885822,440.39313532760963,442.84853569421364,445.36736659254308,447.79324058344417,450.10369386643009,452.45609274100667,454.85018785394919,457.28574815425509,459.76256041842873,462.28042879186552,464.8391743458339,467.43863464957781,470.0786633570695,472.75912980796346,475.47991864231227,478.2409294286233,481.04207630484473,483.88328763188446,486.76450565927985,489.68568620264369,492.6467983325295,495.64782407436576,498.68875811912284,501.76960754438738,504.89039154552671,508.05114117663794,511.25189910098737,514.49271935065156,517.77366709508544,521.0948184183477,524.45626010472324,527.85808943249458,531.30041397561536,534.78335141305365,538.30702934557564,541.87158511975053,545.47716565896371,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","All","Summer Peak Load","MW @meter",410.55982135933306,418.6462473384895,420.66294620148631,422.93297355727555,425.26338762102546,438.95445927879501,441.65147382920117,444.46826859585883,447.23544813379726,450.01260050286555,-6.4686979068659028E-2,-5.2089097068446374E-2,-5.3559104386859985E-2,-5.433932993891679E-2,-5.4996710879171254E-2,-5.5934244268410691E-2]
[{"$f":"B41&C41&D41","v":"IDAllWinter Peak Load"},"ID","All","Winter Peak Load","MW @meter",430.62460789418617,432.71035462612008,435.05967491706451,437.47119707241637,439.79566145529668,442.01160337413035,444.26915828872899,446.5680615103924,448.90806693948196,451.28894658026132,453.71049007215527,456.1725042369182,458.67481264121994,461.21725517417451,463.79968763934892,466.42198136080748,469.08402280275948,471.78571320239132,474.52696821547954,477.3077175743922,480.1279047580997,482.98748667382813,485.88643334999927,488.82472764011368,491.80236493724385,494.81935289881602,497.87571118136623,500.97147118497259,504.10667580706752,507.28137920535039,510.49564656952487,513.74955390159789,517.04318780448091,520.37664527865002,523.7500335266194,527.16346976500085,530.61708104392142,534.11100407358242,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","All","Winter Peak Load","MW @meter",422.25644689655996,430.62460789418617,432.71035462612008,435.05967491706451,437.47119707241637,469.84186438289805,472.67242486583802,475.62845242230026,478.53374663249582,481.4502844936062,-0.10127964554380005,-8.8957626380651647E-2,-9.0234504638242549E-2,-9.0848497146468768E-2,-9.1347100287722208E-2,-9.2533474799377041E-2]
["IDAllSummer Peak Load @ Gen","ID","All","Summer Peak Load @ Gen","MW @generator",465.20956759052393,467.52135246379044,470.12800549297725,472.80199637464375,475.37730420338437,477.83008140860221,480.3273880538527,482.86895942575251,485.45455024055724,488.08393414020401,490.75690320544447,493.47326748553729,496.23285454399183,499.035509019865,501.88109220413406,504.76948163067874,507.70057068142654,510.6742682052232,513.69049815000858,516.74919920789148,519.85032447272658,522.99384110981339,526.17973003734676,529.4079856192609,532.67861536912164,535.99163966473122,539.34709147311889,542.7450160856082,546.18547086265175,549.66852498814274,553.19425923291794,556.76276572717427,560.37414774153626,564.02851947651334,567.72600586009776,571.46674235326316,575.25087476312717,579.07855906355599,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","All","Summer Peak Load @ Gen","MW @generator",435.85030635506803,444.43485617454047,446.5757836874979,448.98564472840377,451.45961229848069,469.47000992384488,472.35451746438622,475.36713218808427,478.32668249603984,481.296898933546,-7.1612036675634469E-2,-5.9107429393751458E-2,-6.0566552777979503E-2,-6.1341001540048914E-2,-6.1993515231821651E-2,-6.2924107123847203E-2]
["IDAllWinter Peak Load @ Gen","ID","All","Winter Peak Load @ Gen","MW @generator",457.1510837404681,459.36531247108911,461.85935089195573,464.41942281207724,466.887074200943,469.23951814197682,471.63613843931472,474.07665409943263,476.56080386295406,479.08834568960549,481.6590562606001,484.27273049791239,486.92918109991916,489.6282380929037,492.36974839793288,495.15357541263324,497.97959860740951,500.84771313565869,503.7578294575531,506.70987297697479,509.70378369119868,512.73951585293594,515.81703764435929,518.93633086274474,522.0973906173781,525.30022503738314,528.54485499013845,531.8313138099669,535.15964703678287,538.5299121644,541.9421783982076,545.39652642193641,548.89304817323693,552.43184662781493,556.01303559185919,559.63673950252496,563.30309323622703,567.01224192451514,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","All","Winter Peak Load @ Gen","MW @generator",448.2674440253881,457.1510837404681,459.36531247108911,461.85935089195573,464.41942281207724,502.50466778919576,505.53200520410479,508.69353200246013,511.80079853742865,514.92009036749323,-0.10793377104819364,-9.5702984114929099E-2,-9.6970408365900859E-2,-9.7579854873596175E-2,-9.8074766357191798E-2,-9.9252356951962314E-2]
["IDResidentialSummer Peak Load","ID","Residential","Summer Peak Load","MW @meter",236.90154526645125,238.84989351865499,241.0939837101532,243.37492184960871,245.53676130931328,247.55746037099513,249.59478922235127,251.64888472191242,253.71988485451686,255.80792874057957,257.91315664543771,260.03570998877314,262.1757313541122,264.33336449840385,266.50875436167672,268.70204707677539,270.913389979177,273.14293161688863,275.39082176042592,277.65721141287418,279.94225282003191,282.24609948063818,284.56890615668379,286.91082888380754,289.27202498177809,291.65265306506183,294.05287305347804,296.47284618294145,298.91273501629348,301.37270345422235,303.85291674627319,306.35354150194883,308.87474570190182,311.41669870921868,313.97957128079685,316.56353557881545,319.16876518230021,321.79543509878397,324.44372177606266,327.11380311404838,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Summer Peak Load","MW @meter",212.70897756027284,217.33229939608256,219.1197043925317,221.17842157321516,223.27094287809112,243.47788507640936,245.6840190375697,247.99753854434124,250.24906629148958,252.49820502491471,-0.12637249377486781,-0.11539912018922006,-0.11644403537757801,-0.11616684589109715,-0.11575235611651043,-0.11802697026985469]
["IDResidentialWinter Peak Load","ID","Residential","Winter Peak Load","MW @meter",226.05814374462506,227.91731266125615,230.05868688705544,232.23522246524971,234.29811072030535,236.22631882226824,238.17039553910408,240.13047146508725,242.10667826924663,244.09914870421045,246.10801661512406,248.13341694864104,250.17548576198826,252.23436023210564,254.31017866486104,256.40308050434106,258.51320634221821,260.64069792719528,262.78569817452734,264.94835117562212,267.12880220771945,269.3271977436504,271.54368546167649,273.77841425541021,276.03153424381691,278.30319678129911,280.59355446786395,282.90276115937405,285.2309719778828,287.57834332205493,289.94503287767242,292.33119962822735,294.73700386560159,297.16260720083443,299.60817257497899,302.07386427004781,304.55984792004858,307.06629052211065,309.59336044770316,312.14122745394553,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Winter Peak Load","MW @meter",221.2491965469865,226.05814374462506,227.91731266125615,230.05868688705544,232.23522246524971,253.25346897899871,255.54817873681057,257.95458554643358,260.29651164082543,262.63595280311495,-0.12637249377486789,-0.11539912018922015,-0.11644403537757818,-0.11616684589109731,-0.11575235611651064,-0.11802697026985483]
["IDResidentialCustomer Population","ID","Residential","Customer Population","#",120796.68660000582,122376.50927373911,123964.58984604779,125479.12305934337,127012.16003130926,128563.92683099561,130134.65228944356,131724.56803342985,133333.90851962357,134962.91106916027,136611.81590263854,138280.86617554407,139970.3080141065,141680.39055159441,143411.36596505373,145163.48951249503,146937.01957053496,148732.21767249788,150549.34854698274,152388.68015690125,154250.48373899297,156135.03384382327,158042.60837626981,159973.48863650372,161927.95936147158,163906.30876688403,165908.82858971745,167935.81413123498,169987.56430053301,172064.38165861974,174166.57246303238,176294.44671299928,178448.31819515399,180628.50452980766,182835.32721778695,185069.1116878441,187330.18734464614,189618.88761735064,191935.55000877465,194280.51614516453,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Customer Population","#",119412.35391190391,120796.68660000582,122376.50927373911,123964.58984604779,125479.12305934337,117743.38551173623,119119.66690483596,120496.78023223074,121856.72650752288,123232.02135784015,1.4174625546174083E-2,1.4078445136264708E-2,1.5599827961258469E-2,1.7297882512827739E-2,1.8234722410160838E-2,1.5877100713337165E-2]
["IDResidentialPer Customer Summer Peak (kW)","ID","Residential","Per Customer Summer Peak (kW)","kW @meter",1.961159299434293,1.9517625967282761,1.9448617061498685,1.9395650520645444,1.9331752270710694,1.9255592643527693,1.9179733055820232,1.9104172325548827,1.9028909275330765,1.8953942732421769,1.8879271528697712,1.8804894500636433,1.8730810489299601,1.8657018340314646,1.858351690385678,1.8510305034631089,1.8437381591854667,1.8364745439238856,1.8292395444971536,1.8220330481699487,1.8148549426510832,1.8077051160917521,1.8005834570837922,1.7934898546579454,1.7864241982821292,1.779386377859715,1.7723762837278123,1.7653938066555597,1.7584388378424234,1.751511268916502,1.7446109919328365,1.7377378993717303,1.730891884137072,1.7240728395546678,1.7172806593705794,1.7105152377494679,1.7037764692729434,1.6970642489379251,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Per Customer Summer Peak (kW)","kW @meter",1.7812979192856229,1.7991577874626246,1.7905372991346862,1.7842064564396791,1.7793473323247457,2.0678688999658532,2.0624975322827699,2.0581258525446171,2.0536335864564714,2.0489658632776333,-0.13858276058262808,-0.12768002904162568,-0.13001564169610469,-0.13119532705037548,-0.13158761489641982,-0.13181227465343076]
["IDResidentialPer Customer Winter Peak (kW)","ID","Residential","Per Customer Winter Peak (kW)","kW @meter",1.871393579636597,1.8624269805852776,1.8558419559389212,1.8507877390521588,1.8446903876176064,1.837423020944287,1.8301842848849286,1.8229740666459844,1.815792253878272,1.8086387346752213,1.8015133975711299,1.7944161315394274,1.7873468259909455,1.780305370772195,1.7732916561636474,1.7663055728780275,1.7593470120586103,1.752415865277523,1.7455120245340576,1.7386353822529867,1.7317858312828873,1.7249632648944728,1.7181675767789273,1.7113986610462517,1.7046564122236114,1.6979407252536947,1.6912514954930755,1.6845886187105814,1.6779519910856706,1.6713415092068149,1.6647570700698868,1.6581985710765554,1.6516659100326876,1.645158985146755,1.63867769502825,1.632221938686103,1.6257916155271108,1.6193866253543681,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Per Customer Winter Peak (kW)","kW @meter",1.8528166416534457,1.871393579636597,1.8624269805852776,1.8558419559389212,1.8507877390521588,2.1508933846118716,2.1453063576895879,2.1407591559648607,2.1360865263745281,2.1312313951296376,-0.13858276058262822,-0.1276800290416257,-0.13001564169610483,-0.13119532705037557,-0.13158761489642004,-0.13181227465343087]
["IDResidentialSaturation Central AC","ID","Residential","Saturation Central AC","%",0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.41058159019236529,0.43416548076018596,0.45910403482876017,0.4854750645468085,0.51336085160879863,0.54284840398656775,0.574029727407662,0.60700211242744695,0.64186843799069937,0.6787374924298385,0.71772431290136185,0.75895054431957887,0.80254481890757212,0.84864315754964303,0.89738939419752461,0.9489356246545736,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Saturation Central AC","%",0.31054202419477445,0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.36715460254415411,0.36891706095211718,0.37068797971879092,0.37246739945657742,0.37425536097283113,{"$f":"BK49-BP49","v":-5.6612578349379661E-2},{"$f":"BL49-BQ49","v":-4.053743933392262E-2},{"$f":"BM49-BR49","v":-2.3446165430639043E-2},{"$f":"BN49-BS49","v":-5.2799442912824235E-3},{"$f":"BO49-BT49","v":1.4023416763545626E-2},-2.2370542128335624E-2]
["IDResidentialSaturation Elec Space Heat","ID","Residential","Saturation Elec Space Heat","%",0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Saturation Elec Space Heat","%",0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.40799999999999997,0.1834748890528064,0.18441133157179282,0.18535795289838183,0.18631485403231768,0.18728213698451929,{"$f":"BK50-BP50","v":0.22452511094719357},0.22358866842820715,0.22264204710161814,0.2216851459676823,0.22071786301548069,0.22263176709203636]
["IDResidentialSaturation Elec Water Heat","ID","Residential","Saturation Elec Water Heat","%",0.50120862662826382,0.49441459619652989,0.48771266084667403,0.48110157220275923,0.47458009881095176,0.4681470259101369,0.46180115520564441,0.45554130464604092,0.44936630820294804,0.44327501565384531,0.43726629236781689,0.43133901909420302,0.42549209175411595,0.41972442123478221,0.41403493318667239,0.40842256782338127,0.40288627972422009,0.39742503763948522,0.39203782429836631,0.3867236362194581,0.38148148352384115,0.37631038975069608,0.37120939167541728,0.36617753913019213,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Saturation Elec Water Heat","%",0.50809601767245227,0.50120862662826382,0.49441459619652989,0.48771266084667403,0.48110157220275923,0.43462810835545662,0.41782274446955009,0.40102066420800586,0.38422187659632434,0.36742639068481409,7.346790931699565E-2,8.3385882158713731E-2,9.3393931988524026E-2,0.10349078425034969,0.11367518151794515,9.3482737846505654E-2]
[{"$f":"B52&C52&D52","v":"IDResidentialSaturation CTA-2045 Water Heat"},"ID","Residential","Saturation CTA-2045 Water Heat","%",1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0.09,0.11461034197302272,0.13922068394604545,0.16383102591906817,0.1884413678920909,0.21305170986511363,0.23766205183813635,0.26227239381115908,0.28688273578418183,0.31149307775720458,0.33610341973022734,0.36071376170325009,0.38532410367627284,0.4099344456492956,0.43454478762231835,0.45915512959534088,0.4741551295953409,0.48915512959534091,0.50415512959534092,0.51915512959534094,0.53415512959534095,0.54915512959534096,0.56415512959534098,0.57915512959534099,0.594155129595341,0.60915512959534102,0.62415512959534103,0.63915512959534104,0.65415512959534106,0.66915512959534107,0.68415512959534108,0.6991551295953411,0.71415512959534111,0.72915512959534112,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Saturation CTA-2045 Water Heat","%",0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,0,0,0,0,0]
["IDResidentialSaturation Elec Vehicles","ID","Residential","Saturation Elec Vehicles","%",1.3330979366300576E-2,1.561924184676035E-2,1.8300284560060061E-2,2.1441528229402231E-2,2.5121966344480925E-2,2.9434151626739111E-2,3.4486523471368408E-2,4.0406134894705785E-2,4.7341847562124749E-2,5.5468075242433468E-2,6.498916982618444E-2,7.614456020398494E-2,8.921477323322026E-2,0.10452848820365733,0.12247080220200145,0.1434929142262,0.16812347157787377,0.19698186386290012,0.23079379890706891,0.27040955227751162,0.31682534933430856,0.37120841751105021,0.43492633881911552,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,0.50958144070903011,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Saturation Elec Vehicles","%",1.137795371941131E-2,1.3330979366300576E-2,1.561924184676035E-2,1.8300284560060061E-2,2.1441528229402231E-2,4.087237354027079E-3,4.9655990506155823E-3,5.9769504387502097E-3,7.1299355977857033E-3,8.4953787836358E-3,7.2907163653842307E-3,8.3653803156849942E-3,9.6422914080101403E-3,1.1170348962274358E-2,1.2946149445766431E-2,9.8829772994240318E-3]
["IDResidentialSaturation Appliances","ID","Residential","Saturation Appliances","%",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Saturation Appliances","%",1,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0]
["IDResidentialSaturation AMI","ID","Residential","Saturation AMI","%",0.33,0.66,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Residential","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0]
["IDGeneral ServiceSummer Peak Load","ID","General Service","Summer Peak Load","MW @meter",64.062731357610858,64.833292079521755,65.601135141161166,66.37815292410356,67.16445519758841,67.960153044420409,68.765358876688808,69.580186451674891,70.404750887949817,71.239168681665134,72.083557723038155,72.938037313034684,73.80272818025135,74.677752498000075,75.563233901596774,76.459297505857123,77.366069922801728,78.283679279573008,79.212255236566605,80.151929005779763,81.102833369379297,82.065102698491629,83.038872972217916,84.02428179687648,85.021468425475746,86.030573777420045,87.051740458451292,88.085112780829348,89.130836783753779,90.189060254030124,91.259932746983381,92.343605607621839,93.440231992054052,94.549966889162278,95.672967142535185,96.809391472663023,97.959400499398399,99.123156764685987,100.30082475556394,101.49257092744088,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Summer Peak Load","MW @meter",63.441015338733642,64.062731357610858,64.833292079521755,65.601135141161166,66.37815292410356,57.996059697866826,58.655299460287033,59.322074946058464,59.996472471215448,60.678579341205598,9.3884923721241853E-2,9.2189997273562016E-2,9.2903310251278931E-2,9.3416536657795521E-2,9.3930570635945926E-2,9.326506770796486E-2]
["IDGeneral ServiceWinter Peak Load","ID","General Service","Winter Peak Load","MW @meter",64.747964791613157,65.526767653039386,66.302823785316775,67.08815277435987,67.882865563531539,68.687074423810174,69.500892969677125,70.324436175194322,71.157820390274352,72.00116335714516,72.854584227011784,73.718203576917546,74.592143426806928,75.476527256792792,76.371480024630031,77.277128183398432,78.193599699397268,79.121024070253767,80.059532343248549,81.009257133860189,81.970332644531794,82.94289468366209,83.927080684823878,84.92302972621232,85.930882550326132,86.950781583884208,87.982870957980566,89.027296528480576,90.084205896661175,91.153748430098148,92.236075283803359,93.331339421614885,94.439695637843172,95.561300579176219,96.696312766846916,97.84489261906559,99.007202473721108,100.18340661135359,101.37367127840194,102.57816471072984,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Winter Peak Load","MW @meter",64.119598719053229,64.747964791613157,65.526767653039386,66.302823785316775,67.08815277435987,63.893422604237998,64.619697543557379,65.354274480619665,66.097248508555083,66.848715810516254,3.5398966841420957E-3,1.9849558715331088E-3,2.6393556319085467E-3,3.1101941669339581E-3,3.5817735754611036E-3,2.9712351859957622E-3]
["IDGeneral ServiceCustomer Population","ID","General Service","Customer Population","#",16897.112874999999,17097.860366666668,17300.107833333332,17504.793213773384,17711.94552951285,17921.594150432022,18133.76879892392,18348.49955410264,18565.816856062091,18785.751510185735,19008.334691508,19233.597949127921,19461.57321067563,19692.292786832397,19925.789375904784,20162.096068453597,20401.246351978283,20643.274115657448,20888.213655146152,21136.099677430644,21386.967305741266,21640.852084524191,21897.7899844727,22157.817407618721,22420.97119248534,22687.288619301016,22956.807415276271,23229.5657599435,23505.602290560815,23784.956107580518,24067.666780183114,24353.774351877568,24643.319346168621,24936.342772291959,25232.886131018091,25532.991420525661,25836.70114234514,26144.058307373663,26455.106441961852,26769.889594073586,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Customer Population","#",16714.928233333332,16897.112874999999,17097.860366666668,17300.107833333332,17504.793213773384,16755.458774999999,16953.609491666666,17154.118646606672,17357.014327975681,17562.324958469271,-2.418945503726858E-3,-3.3324240890671365E-3,-3.2795785722942385E-3,-3.2785877551894881E-3,-3.2758615292642602E-3,-3.1170794899083964E-3]
["IDGeneral ServicePer Customer Summer Peak (kW)","ID","General Service","Per Customer Summer Peak (kW)","kW @meter",3.7913418600874955,3.7918950493898205,3.7919494937923366,3.791998689357547,3.792042781843159,3.7920819138057622,3.7921162246630953,3.7921458507552503,3.792170925404843,3.792191578976166,3.7922079389333136,3.7922201298973186,3.7922282737022992,3.7922324894506283,3.7922328935671401,3.7922295998523845,3.792222719534958,3.7922123613228891,3.7921986314541254,3.7921816337461194,3.7921614696445296,3.7921382382710354,3.7921120364703098,3.7920829588561218,3.7920510978566226,3.7920165437587934,3.7919793847520795,3.7919397069712417,3.7918975945383968,3.7918531296043012,3.7918063923888616,3.7917574612208949,3.791706412577148,3.7916533211205921,3.7915982597379951,3.791541299576795,3.7914825100812712,3.7914219590280411,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Per Customer Summer Peak (kW)","kW @meter",3.7954703994611219,3.7913418600874955,3.7918950493898205,3.7919494937923366,3.791998689357547,3.4613232903177744,3.4597528915077529,3.4581826188892082,3.4566124874664856,3.4550425120077231,9.6537387905384103E-2,9.584180690871158E-2,9.6499366076798737E-2,9.7013190672014055E-2,9.7525913553526425E-2,9.6683533023286972E-2]
["IDGeneral ServicePer Customer Winter Peak (kW)","ID","General Service","Per Customer Winter Peak (kW)","kW @meter",3.8318951450818881,3.8324542514563902,3.8325092782119237,3.8325589999870755,3.8326035640986187,3.8326431146279694,3.8326777924841191,3.8327077354654921,3.832733078320762,3.832753952808635,3.8327704877565982,3.8327828091186671,3.8327910400321321,3.83279530087332,3.8327957093123781,3.8327923803671013,3.8327854264558172,3.8327749574493271,3.8327610807219306,3.8327439012015421,3.8327235214189117,3.8327000415559529,3.832673559493216,3.8326441708564887,3.8326119690625582,3.8325770453641419,3.832539488893985,3.8324993867081703,3.832456823828609,3.8324118832847662,3.8323646461546033,3.8323151916047649,3.8322635969300145,3.8322099375919412,3.8321542872569303,3.8320967178334331,3.8320372995085257,3.8319761007837827,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Per Customer Winter Peak (kW)","kW @meter",3.8360678445022756,3.8318951450818881,3.8324542514563902,3.8325092782119237,3.8325589999870755,3.8132899529776081,3.8115598672554287,3.8098299205565813,3.8081001294111334,3.8063705100889313,5.9732912538899251E-3,5.3351589728805994E-3,5.9384096853603522E-3,6.4097970040942111E-3,6.8801736007386965E-3,6.1073661033927574E-3]
["IDGeneral ServiceSaturation Central AC","ID","General Service","Saturation Central AC","%",0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.41058159019236529,0.43416548076018596,0.45910403482876017,0.4854750645468085,0.51336085160879863,0.54284840398656775,0.574029727407662,0.60700211242744695,0.64186843799069937,0.6787374924298385,0.71772431290136185,0.75895054431957887,0.80254481890757212,0.84864315754964303,0.89738939419752461,0.9489356246545736,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Saturation Central AC","%",0.31054202419477445,0.32837962161819456,0.34724181428815187,0.367187455165295,0.38827877773637676,0.36715460254415411,0.36891706095211718,0.37068797971879092,0.37246739945657742,0.37425536097283113,{"$f":"BK61-BP61","v":-5.6612578349379661E-2},{"$f":"BL61-BQ61","v":-4.053743933392262E-2},{"$f":"BM61-BR61","v":-2.3446165430639043E-2},{"$f":"BN61-BS61","v":-5.2799442912824235E-3},{"$f":"BO61-BT61","v":1.4023416763545626E-2},-2.2370542128335624E-2]
["IDGeneral ServiceSaturation Elec Water Heat","ID","General Service","Saturation Elec Water Heat","%",0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Saturation Elec Water Heat","%",0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.60089668805662699,0.45200000000000001,0.434,0.41600000000000004,0.39800000000000002,0.38,0.14889668805662698,0.166896688056627,0.18489668805662696,0.20289668805662697,0.22089668805662699,0.18489668805662698]
[{"$f":"B63&C63&D63","v":"IDGeneral ServiceSaturation CTA-2045 Water Heat"},"ID","General Service","Saturation CTA-2045 Water Heat","%",1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0.09,0.11413333333333334,0.13826666666666668,0.16240000000000002,0.18653333333333336,0.2106666666666667,0.23480000000000004,0.25893333333333335,0.28306666666666669,0.30720000000000003,0.33133333333333337,0.35546666666666671,0.37960000000000005,0.40373333333333339,0.42786666666666673,0.45200000000000001,0.47700000000000004,0.502,0.52700000000000002,0.55200000000000005,0.57700000000000007,0.60200000000000009,0.62700000000000011,0.65200000000000014,0.67700000000000016,0.70200000000000018,0.7270000000000002,0.75200000000000022,0.77700000000000025,0.80200000000000027,0.82700000000000029,0.85200000000000031,0.87700000000000033,0.90200000000000036,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Saturation CTA-2045 Water Heat","%",0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,1.7999999999999999E-2,3.5999999999999997E-2,5.3999999999999992E-2,7.1999999999999995E-2,0,0,0,0,0,0]
["IDGeneral ServiceSaturation Elec Space Heat","ID","General Service","Saturation Elec Space Heat","%",0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Saturation Elec Space Heat","%",0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0.14199999999999999,0,0,0,0,0,0]
["IDGeneral ServiceSaturation AMI","ID","General Service","Saturation AMI","%",0.33,0.66,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","General Service","Saturation AMI","%",0,0.33329999999999999,0.66659999999999997,1,1,0,0.33329999999999999,0.66659999999999997,1,1,0,0,0,0,0,0]
["IDLarge General ServiceSummer Peak Load","ID","Large General Service","Summer Peak Load","MW @meter",89.565400813779064,89.248360746515118,88.935823881652169,88.633164034181576,88.340066398923611,88.056226204414401,87.781348393103485,87.515147311744457,87.257346411653643,87.007677958522294,86.765882751478102,86.531709851100757,86.304916316106599,86.085266948425669,85.872534046404084,85.666497165872372,85.466942888829223,85.273664599498119,85.086462267521355,84.90514223806457,84.729517028611042,84.559405132232854,84.394630827132119,84.23502399225292,84.080419928770056,83.93065918726758,83.785587400425385,83.645055121038752,83.508917665200656,83.377034960482121,83.249271398951663,83.125495694879419,83.00558074697642,82.889403505024916,82.77684484075948,82.667789422863464,82.562125595949695,82.459745263398389,82.360543773929436,82.264419811789594,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Large General Service","Summer Peak Load","MW @meter",89.286477610896441,89.565400813779064,89.248360746515118,88.935823881652169,88.633164034181576,88.489376568156743,88.517245842181993,88.545411250858677,88.573874221483067,88.602636188535499,9.0078727374212023E-3,1.1841251516860728E-2,7.9388585554694534E-3,4.0864155864293655E-3,3.4454782565518046E-4,6.6437892443671877E-3]
["IDLarge General ServiceWinter Peak Load","ID","Large General Service","Winter Peak Load","MW @meter",90.523418148769366,90.202986929592242,89.887107080366562,89.581209895957286,89.284977203937771,88.998100972920753,88.720282989335189,88.451234544505255,88.190676131702844,87.938337152855908,87.693955634604919,87.457277953409218,87.228058569415182,87.006059768806509,86.791051414366834,86.582810703992308,86.381121936901195,86.185776287295099,85.996571585233966,85.813312104495509,85.635808357196026,85.463876894957153,85.297340116410055,85.136026080834966,84.979768327740587,84.82840570219409,84.681782185718021,84.539746732577285,84.402153111284122,84.26885975115448,84.139729593755376,84.014629949086938,83.893432356348185,83.776012449140794,83.662249824969081,83.552027918899398,83.445233881246381,83.34175845915766,83.241495881972853,83.14434375023626,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Large General Service","Winter Peak Load","MW @meter",90.241511502938195,90.523418148769366,90.202986929592242,89.887107080366562,89.581209895957286,97.487470054155281,97.518173231444308,97.549202656008248,97.5805599002788,97.6122465446023,{"$f":"(BK67-BP67)/BP67","v":-7.4327075543060894E-2},{"$f":"(BL67-BQ67)/BQ67","v":-7.1727708291601938E-2},{"$f":"(BM67-BR67)/BR67","v":-7.5307798796892964E-2},{"$f":"(BN67-BS67)/BS67","v":-7.884206472861463E-2},{"$f":"(BO67-BT67)/BT67","v":-8.2274887966802032E-2},{"$f":"AVERAGE(BU67:BY67)","v":-7.6495907065394483E-2}]
["IDLarge General ServiceCustomer Population","ID","Large General Service","Customer Population","#",1012.1453726702155,1010.4140805274671,1008.6298556587464,1006.9026431411656,1005.2306250146694,1003.6120412887391,1002.0451880939107,1000.5284158922353,999.06012774480268,997.63877763450864,996.26286884230467,994.93095237522391,993.64162544453325,992.39352999241305,991.18535126561608,990.01581643460906,988.88369325674535,987.78778878206549,986.72694810036603,985.70005312822059,984.70602143467977,983.74380510441517,982.8123896371161,981.91079288197955,981.03806400617748,980.19328249621628,979.37555719114005,978.58402534656227,977.81785172854279,977.07622773635876,976.35837055324725,975.66352232422889,974.99094936014831,974.33994136709464,973.709810700395,973.09989164239448,972.50953970326691,971.93813094411951,971.38506132168357,970.84974605389925,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Large General Service","Customer Population","#",1012.8661455050126,1012.1453726702155,1010.4140805274671,1008.6298556587464,1006.9026431411656,1114.5513149107471,1114.5512681715891,1114.5512214324328,1114.5511746932789,1114.551127954127,-9.123417472606675E-2,-9.1880829914059964E-2,-9.3434145423238205E-2,-9.5034953476839462E-2,-9.6584608918355477E-2,-9.3633742491711955E-2]
["IDLarge General ServicePer Customer Summer Peak (kW)","ID","Large General Service","Per Customer Summer Peak (kW)","kW @meter",88.490648904998665,88.328500628103612,88.174887331257196,88.025555040434426,87.880396996096749,87.739308200548621,87.602185446427896,87.468927340460979,87.339434322758237,87.213608681917236,87.091354566193317,86.972577990986622,86.857186842887828,86.7450908805137,86.636201732356028,86.530432891857416,86.427699709918585,86.32791938503297,86.231010951235007,86.136895264040376,86.045494984547062,85.956734561858482,85.870540213980377,85.78683990733721,85.705563335043664,85.626641894060896,85.550008661359058,85.475598369200995,85.403347379654917,85.333193658437338,85.265076748181102,85.198937741217975,85.134719251958202,85.072365388945187,85.011821726657587,84.953035277125622,84.895954461424751,84.840529081103952,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Large General Service","Per Customer Summer Peak (kW)","kW @meter",88.152297326887577,88.490648904998665,88.328500628103612,88.174887331257196,88.025555040434426,79.394618609590836,79.419626866867873,79.444900824799419,79.470441764020691,79.496250971612881,0.11030569666643399,0.11421637693333238,0.11182089361399392,0.1095306050151761,0.10729190326053556,0.11063309509789439]
["IDLarge General ServicePer Customer Winter Peak (kW)","ID","Large General Service","Per Customer Winter Peak (kW)","kW @meter",89.437170383887505,89.273287722300466,89.118031333367952,88.967101741333082,88.820391044726506,88.677793122767056,88.539203664156915,88.404520191090839,88.273642078757888,88.14647057060634,88.022908789633632,87.902861745953558,87.786236340885253,87.672941367797591,87.56288750993528,87.455987335441861,87.352155289786879,87.251307685795013,87.153362691465418,87.058240315761509,86.965862392542149,86.876152562796534,86.789036255336981,86.70444066609609,86.622294736165799,86.542529128709418,86.46507620486905,86.389869998785045,86.316846191835992,86.245942086201765,86.17709657784583,86.110250129006573,86.045344740281379,85.982323922382591,85.92113266763775,85.861717421302544,85.804026052749336,85.748007826590054,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Large General Service","Per Customer Winter Peak (kW)","kW @meter",89.095199699802379,89.437170383887505,89.273287722300466,89.118031333367952,88.967101741333082,87.467906367291889,87.495457603688308,87.523301558664116,87.551439643076662,87.579873274884747,1.860446191174649E-2,2.2192155265867711E-2,1.9994517259651019E-2,1.7893385838974856E-2,1.5839580654498954E-2,1.8904820186147808E-2]
["IDLarge General ServiceSaturation AMI","ID","Large General Service","Saturation AMI","%",0.33,0.66,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Large General Service","Saturation AMI","%",0,0.33329999999999999,0.66659999999999997,1,1,0,0.33329999999999999,0.66659999999999997,1,1,{"$f":"BK71-BP71","v":0},{"$f":"BL71-BQ71","v":0},{"$f":"BM71-BR71","v":0},{"$f":"BN71-BS71","v":0},{"$f":"BO71-BT71","v":0},0]
["IDExtra Large General ServiceSummer Peak Load","ID","Extra Large General Service","Summer Peak Load","MW @meter",47.685815771017019,47.461588982917768,47.217592961247107,46.981127784649225,46.751957677618876,46.529854246600102,46.314596248863111,46.105969368617444,45.903766000134716,45.707785037661793,45.517831671911559,45.333717192925334,45.155258799107663,44.982279412239912,44.814607498285831,44.65207689380734,44.494526637815341,44.34180080888494,44.193748367370574,44.05022300256131,43.911082984621444,43.776191021166902,43.645414118331928,43.518623446185877,43.395694208363516,43.276505515777281,43.160940264283298,43.048885016177785,42.940229885403596,42.834868426350894,42.732697526139397,42.633617300273158,42.537530991562306,42.444344872209555,42.353968148962181,42.266312871233723,42.181293842102271,42.098828532095354,42.018836995674128,41.941241790332391,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Extra Large General Service","Summer Peak Load","MW @meter",45.12335084943016,47.685815771017019,47.461588982917768,47.217592961247107,46.981127784649225,48.991137936362072,48.794909489162485,48.603243854600485,48.416035149609144,48.233179948209745,-7.8948708886003915E-2,-2.2729701310170474E-2,-2.348927316658219E-2,-2.4753001452075984E-2,-2.5958316762546205E-2,-3.517580031547575E-2]
["IDExtra Large General ServiceWinter Peak Load","ID","Extra Large General Service","Winter Peak Load","MW @meter",49.295081209178662,49.06328738223224,48.811057164325767,48.566611936849547,48.329707967521976,48.100109155131264,47.877586790612561,47.661919325605524,47.452892148258087,47.250297366049757,47.053933595414506,46.86360575795036,46.679124883009585,46.500307916469559,46.326977535490983,46.158961969075662,45.996094824242775,45.838214917647171,45.685166112469688,45.536797160414352,45.392961548652394,45.253517351558486,45.118327087088836,44.987257577656123,44.860179815360219,44.736968831438553,44.617503569803716,44.501666764540687,44.389344821239405,44.280427702042772,44.174808814293733,44.072384902668659,43.973055944688028,43.87672504949856,43.783298359824386,43.692684956988067,43.604796768905359,43.519548480960545,43.436857449672203,43.356643619062041,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Extra Large General Service","Winter Peak Load","MW @meter",46.646140127582022,49.295081209178662,49.06328738223224,48.811057164325767,48.566611936849547,55.207502745506055,54.986375354025789,54.770389739238773,54.559426582836537,54.353369335372712,-0.15507607104400201,-0.10350371538775092,-0.10420050659084197,-0.10535978434053242,-0.10646547710441921,-0.11492111089350932]
["IDExtra Large General ServiceCustomer Population","ID","Extra Large General Service","Customer Population","#",11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,11,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Extra Large General Service","Customer Population","#",11.083333333333334,11,11,11,11,11,11,11,11,11,7.5757575757576297E-3,0,0,0,0,1.515151515151526E-3]
["IDExtra Large General ServicePer Customer Summer Peak (kW)","ID","Extra Large General Service","Per Customer Summer Peak (kW)","kW @meter",4335.0741610015466,4314.6899075379788,4292.5084510224642,4271.0116167862925,4250.1779706926245,4229.9867496909183,4210.4178408057378,4191.4517607834041,4173.0696363758834,4155.2531852419806,4137.9846974465054,4121.247017538667,4105.0235271916063,4089.2981283854465,4074.0552271168935,4059.2797176188487,4044.9569670741221,4031.0728008077213,4017.6134879427796,4004.5657275055737,3991.9166349655857,3979.6537291969912,3967.7649198483568,3956.238495107807,3945.0631098512285,3934.2277741615708,3923.7218422075725,3913.5350014707074,3903.6572623094175,3894.0789478500815,3884.7906841944905,3875.7833909339238,3867.0482719602096,3858.5768065645052,3850.3607408147436,3842.3920792030658,3834.663076554752,3827.1662301904867,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Extra Large General Service","Per Customer Summer Peak (kW)","kW @meter",4071.2797758884349,4335.0741610015466,4314.6899075379788,4292.5084510224642,4271.0116167862925,4453.7398123965522,4435.900862651135,4418.4767140545891,4401.4577408735586,4384.8345407463412,-8.587390656355294E-2,-2.2729701310170592E-2,-2.3489273166582107E-2,-2.4753001452076005E-2,-2.5958316762546511E-2,-3.6560839850985634E-2]
["IDExtra Large General ServicePer Customer Winter Peak (kW)","ID","Extra Large General Service","Per Customer Winter Peak (kW)","kW @meter",4481.3710190162419,4460.2988529302038,4437.368833120524,4415.1465397135953,4393.6098152292707,4372.7371959210241,4352.5078900556873,4332.9017568732297,4313.899286205281,4295.4815787317966,4277.630326855864,4260.3277961773056,4243.5568075463261,4227.3007196790513,4211.5434123173627,4196.2692699159697,4181.4631658402523,4167.1104470588334,4153.1969193154255,4139.7088327649408,4126.6328680593087,4113.9561228689536,4101.6660988262583,4089.7506888778289,4078.1981650327471,4066.9971664944137,4056.1366881639742,4045.606069503699,4035.3949837490372,4025.4934274584339,4015.8917103903395,4006.5804456971509,3997.5505404261844,3988.7931863180511,3980.2998508931259,3972.0622688170974,3964.0724335368509,3956.3225891782313,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,"ID","Extra Large General Service","Per Customer Winter Peak (kW)","kW @meter",4208.6742972254451,4481.3710190162419,4460.2988529302038,4437.368833120524,4415.1465397135953,5018.8638859550956,4998.7613958205266,4979.1263399307973,4959.9478711669581,4941.2153941247925,-0.16142888253991181,-0.10350371538775099,-0.10420050659084189,-0.10535978434053253,-0.10646547710441928,-0.1161916731926913]
["IDExtra Large General ServiceSaturation AMI","ID","Extra Large General Service","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ID","Extra Large General Service","Saturation AMI","%",1,1,1,1,1,1,1,1,1,1,{"$f":"BK77-BP77","v":0},{"$f":"BL77-BQ77","v":0},{"$f":"BM77-BR77","v":0},{"$f":"BN77-BS77","v":0},{"$f":"BO77-BT77","v":0},0]

{"sheet":"EnergyCosts","index":3,"n_rows":15,"n_cols":50,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Key","State","Customer Class","Data Element","Unit",{"$f":"YearBase","v":2022},{"$f":"F1+1","v":2023},2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066]
[{"$f":"B2&C2&D2","v":"WAAllAvoided Capacity Costs"},"WA","All","Avoided Capacity Costs","$/kW @gen",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAAllAvoided Summer Energy Costs","WA","All","Avoided Summer Energy Costs","$/MWh @gen",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAAllAvoided Winter Energy Costs","WA","All","Avoided Winter Energy Costs","$/MWh @gen",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialLine Loss","WA","Residential","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]
["WAGeneral ServiceLine Loss","WA","General Service","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]
["WALarge General ServiceLine Loss","WA","Large General Service","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]
["WAExtra Large General ServiceLine Loss","WA","Extra Large General Service","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]
["IDAllAvoided Capacity Costs","ID","All","Avoided Capacity Costs","$/kW @gen",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDAllAvoided Summer Energy Costs","ID","All","Avoided Summer Energy Costs","$/MWh @gen",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDAllAvoided Winter Energy Costs","ID","All","Avoided Winter Energy Costs","$/MWh @gen",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialLine Loss","ID","Residential","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]
["IDGeneral ServiceLine Loss","ID","General Service","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]
["IDLarge General ServiceLine Loss","ID","Large General Service","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]
["IDExtra Large General ServiceLine Loss","ID","Extra Large General Service","Line Loss","T&D Loss %",6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2,6.1600000000000002E-2]

{"sheet":"ParticipationRate","index":4,"n_rows":225,"n_cols":33,"rows_kept":225,"cut":false,"hidden":false,"merged":[]}
["Key","State","Customer Class","Option","Data Element","Unit","Year 1","Year 2","Year 3","Year 4","Year 5","Year 6","Year 7","Year 8","Year 9","Year 10","Year 11","Year 12","Year 13","Year 14","Year 15","Year 16","Year 17","Year 18","Year 19","Year 20","Year 21","Year 22","Year 23","Year 24","Year 25","Comments from Input Generator"]
[{"$f":"B2&C2&D2&E2","v":"WAResidentialBehavioralMarket Potential"},"WA","Residential","Behavioral","Market Potential","% of Eligible Customers",0.05,0.1,0.17,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,"high rate based on PG&E rollout with six waves http://www.calmac.org/publications/DNVGL_PGE_HERs_2015_final_to_calmac.pdf --> PC study has high case at 0% --> shif to 25%?",1]
["WAResidentialBehavioralProgram Dropout Rate (Attrition)","WA","Residential","Behavioral","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"high rate based on PG&E rollout with six waves http://www.calmac.org/publications/DNVGL_PGE_HERs_2015_final_to_calmac.pdf --> PC study has high case at 0% --> shif to 25%?",1]
["WAResidentialDLC Electric Vehicle ChargingMarket Potential","WA","Residential","DLC Electric Vehicle Charging","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["WAResidentialDLC Electric Vehicle ChargingProgram Dropout Rate (Attrition)","WA","Residential","DLC Electric Vehicle Charging","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["WAResidentialDLC Central ACMarket Potential","WA","Residential","DLC Central AC","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["WAResidentialDLC Central ACProgram Dropout Rate (Attrition)","WA","Residential","DLC Central AC","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["WAGeneral ServiceDLC Central ACMarket Potential","WA","General Service","DLC Central AC","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["WAGeneral ServiceDLC Central ACProgram Dropout Rate (Attrition)","WA","General Service","DLC Central AC","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["WAResidentialDLC Water HeatingMarket Potential","WA","Residential","DLC Water Heating","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["WAResidentialDLC Water HeatingProgram Dropout Rate (Attrition)","WA","Residential","DLC Water Heating","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["WAGeneral ServiceDLC Water HeatingMarket Potential","WA","General Service","DLC Water Heating","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["WAGeneral ServiceDLC Water HeatingProgram Dropout Rate (Attrition)","WA","General Service","DLC Water Heating","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["WAResidentialCTA-2045 WHMarket Potential","WA","Residential","CTA-2045 WH","Market Potential","% of Eligible Customers",0.02,0.06,0.1,0.15000000000000002,0.2,0.25,0.32500000000000001,0.4,0.47500000000000003,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAResidentialCTA-2045 WHProgram Dropout Rate (Attrition)","WA","Residential","CTA-2045 WH","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAGeneral ServiceCTA-2045 WHMarket Potential","WA","General Service","CTA-2045 WH","Market Potential","% of Eligible Customers",0.02,0.06,0.1,0.15000000000000002,0.2,0.25,0.32500000000000001,0.4,0.47500000000000003,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAGeneral ServiceCTA-2045 WHProgram Dropout Rate (Attrition)","WA","General Service","CTA-2045 WH","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAResidentialDLC Smart Thermostats - CoolingMarket Potential","WA","Residential","DLC Smart Thermostats - Cooling","Market Potential","% of Eligible Customers",2.0000000000000004E-2,6.0000000000000012E-2,0.13999999999999999,0.18000000000000005,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAResidentialDLC Smart Thermostats - CoolingProgram Dropout Rate (Attrition)","WA","Residential","DLC Smart Thermostats - Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingMarket Potential","WA","General Service","DLC Smart Thermostats - Cooling","Market Potential","% of Eligible Customers",2.0000000000000004E-2,6.0000000000000012E-2,0.13999999999999999,0.18000000000000005,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingProgram Dropout Rate (Attrition)","WA","General Service","DLC Smart Thermostats - Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAResidentialDLC Smart Thermostats - HeatingMarket Potential","WA","Residential","DLC Smart Thermostats - Heating","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat",1]
["WAResidentialDLC Smart Thermostats - HeatingProgram Dropout Rate (Attrition)","WA","Residential","DLC Smart Thermostats - Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingMarket Potential","WA","General Service","DLC Smart Thermostats - Heating","Market Potential","% of Eligible Customers",3.0000000000000001E-3,9.0000000000000011E-3,2.0999999999999998E-2,2.7000000000000003E-2,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,"Dropping to 3% to compensate for higher space heating saturations",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingProgram Dropout Rate (Attrition)","WA","General Service","DLC Smart Thermostats - Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Dropping to 3% to compensate for higher space heating saturations",1]
["WAResidentialDLC Smart AppliancesMarket Potential","WA","Residential","DLC Smart Appliances","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["WAResidentialDLC Smart AppliancesProgram Dropout Rate (Attrition)","WA","Residential","DLC Smart Appliances","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["WAGeneral ServiceDLC Smart AppliancesMarket Potential","WA","General Service","DLC Smart Appliances","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["WAGeneral ServiceDLC Smart AppliancesProgram Dropout Rate (Attrition)","WA","General Service","DLC Smart Appliances","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["WAGeneral ServiceThird Party ContractsMarket Potential","WA","General Service","Third Party Contracts","Market Potential","% of Eligible Customers",3.7499999999999999E-2,7.4999999999999997E-2,0.1275,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,"MPSC Demand Response Market Assessment",1]
["WAGeneral ServiceThird Party ContractsProgram Dropout Rate (Attrition)","WA","General Service","Third Party Contracts","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"MPSC Demand Response Market Assessment",1]
["WALarge General ServiceThird Party ContractsMarket Potential","WA","Large General Service","Third Party Contracts","Market Potential","% of Eligible Customers",5.525E-2,0.1105,0.18784999999999999,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0,1]
["WALarge General ServiceThird Party ContractsProgram Dropout Rate (Attrition)","WA","Large General Service","Third Party Contracts","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0,1]
["WAExtra Large General ServiceThird Party ContractsMarket Potential","WA","Extra Large General Service","Third Party Contracts","Market Potential","% of Eligible Customers",5.2249999999999998E-2,0.1045,0.17764999999999997,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0,1]
["WAExtra Large General ServiceThird Party ContractsProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Third Party Contracts","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0,1]
["WAResidentialTime-of-Use Opt-inMarket Potential","WA","Residential","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle Analysis and Estimate",1]
["WAResidentialTime-of-Use Opt-inProgram Dropout Rate (Attrition)","WA","Residential","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle Analysis and Estimate",1]
["WAGeneral ServiceTime-of-Use Opt-inMarket Potential","WA","General Service","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["WAGeneral ServiceTime-of-Use Opt-inProgram Dropout Rate (Attrition)","WA","General Service","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["WALarge General ServiceTime-of-Use Opt-inMarket Potential","WA","Large General Service","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["WALarge General ServiceTime-of-Use Opt-inProgram Dropout Rate (Attrition)","WA","Large General Service","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["WAExtra Large General ServiceTime-of-Use Opt-inMarket Potential","WA","Extra Large General Service","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["WAExtra Large General ServiceTime-of-Use Opt-inProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["WAResidentialTime-of-Use Opt-outMarket Potential","WA","Residential","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["WAResidentialTime-of-Use Opt-outProgram Dropout Rate (Attrition)","WA","Residential","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
["WAGeneral ServiceTime-of-Use Opt-outMarket Potential","WA","General Service","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["WAGeneral ServiceTime-of-Use Opt-outProgram Dropout Rate (Attrition)","WA","General Service","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
["WALarge General ServiceTime-of-Use Opt-outMarket Potential","WA","Large General Service","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["WALarge General ServiceTime-of-Use Opt-outProgram Dropout Rate (Attrition)","WA","Large General Service","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
["WAExtra Large General ServiceTime-of-Use Opt-outMarket Potential","WA","Extra Large General Service","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["WAExtra Large General ServiceTime-of-Use Opt-outProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
["WAResidentialVariable Peak Pricing RatesMarket Potential","WA","Residential","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"High Case- OG&E's VPP Plus participation rate- should be 103000/400000 around 25%",1]
["WAResidentialVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","WA","Residential","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"High Case- OG&E's VPP Plus participation rate- should be 103000/400000 around 25%",1]
["WAGeneral ServiceVariable Peak Pricing RatesMarket Potential","WA","General Service","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"Brattle",1]
["WAGeneral ServiceVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","WA","General Service","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle",1]
["WALarge General ServiceVariable Peak Pricing RatesMarket Potential","WA","Large General Service","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0,1]
["WALarge General ServiceVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","WA","Large General Service","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesMarket Potential","WA","Extra Large General Service","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"High Case- OG&E's VPP Plus participation rate",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"High Case- OG&E's VPP Plus participation rate",1]
["WALarge General ServiceReal Time PricingMarket Potential","WA","Large General Service","Real Time Pricing","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["WALarge General ServiceReal Time PricingProgram Dropout Rate (Attrition)","WA","Large General Service","Real Time Pricing","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["WAExtra Large General ServiceReal Time PricingMarket Potential","WA","Extra Large General Service","Real Time Pricing","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["WAExtra Large General ServiceReal Time PricingProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Real Time Pricing","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["WAGeneral ServiceThermal Energy StorageMarket Potential","WA","General Service","Thermal Energy Storage","Market Potential","% of Eligible Customers",5.0000000000000001E-4,1.5000000000000002E-3,3.4999999999999996E-3,4.5000000000000005E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Don't expect much participation - 0.5%",1]
["WAGeneral ServiceThermal Energy StorageProgram Dropout Rate (Attrition)","WA","General Service","Thermal Energy Storage","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Don't expect much participation - 0.5%",1]
[{"$f":"B66&C66&D66&E66","v":"WALarge General ServiceThermal Energy StorageMarket Potential"},"WA","Large General Service","Thermal Energy Storage","Market Potential","% of Eligible Customers",1.5E-3,4.5000000000000005E-3,1.0499999999999999E-2,1.3500000000000002E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,"Low participation is 1/2 DLC CAC",1]
["WALarge General ServiceThermal Energy StorageProgram Dropout Rate (Attrition)","WA","Large General Service","Thermal Energy Storage","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Low participation is 1/2 DLC CAC",1]
["WAExtra Large General ServiceThermal Energy StorageMarket Potential","WA","Extra Large General Service","Thermal Energy Storage","Market Potential","% of Eligible Customers",1.5E-3,4.5000000000000005E-3,1.0499999999999999E-2,1.3500000000000002E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,"Low participation is 1/2 DLC CAC",1]
["WAExtra Large General ServiceThermal Energy StorageProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Thermal Energy Storage","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Low participation is 1/2 DLC CAC",1]
["WAResidentialBattery Energy StorageMarket Potential","WA","Residential","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["WAResidentialBattery Energy StorageProgram Dropout Rate (Attrition)","WA","Residential","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["WAGeneral ServiceBattery Energy StorageMarket Potential","WA","General Service","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["WAGeneral ServiceBattery Energy StorageProgram Dropout Rate (Attrition)","WA","General Service","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["WALarge General ServiceBattery Energy StorageMarket Potential","WA","Large General Service","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["WALarge General ServiceBattery Energy StorageProgram Dropout Rate (Attrition)","WA","Large General Service","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["WAExtra Large General ServiceBattery Energy StorageMarket Potential","WA","Extra Large General Service","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["WAExtra Large General ServiceBattery Energy StorageProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["WAResidentialAncillary ServicesMarket Potential","WA","Residential","Ancillary Services","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["WAResidentialAncillary ServicesProgram Dropout Rate (Attrition)","WA","Residential","Ancillary Services","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["WAGeneral ServiceAncillary ServicesMarket Potential","WA","General Service","Ancillary Services","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["WAGeneral ServiceAncillary ServicesProgram Dropout Rate (Attrition)","WA","General Service","Ancillary Services","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["WALarge General ServiceAncillary ServicesMarket Potential","WA","Large General Service","Ancillary Services","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["WALarge General ServiceAncillary ServicesProgram Dropout Rate (Attrition)","WA","Large General Service","Ancillary Services","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["WAExtra Large General ServiceAncillary ServicesMarket Potential","WA","Extra Large General Service","Ancillary Services","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["WAExtra Large General ServiceAncillary ServicesProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Ancillary Services","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["IDResidentialBehavioralMarket Potential","ID","Residential","Behavioral","Market Potential","% of Eligible Customers",0.05,0.1,0.17,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,"high rate based on PG&E rollout with six waves http://www.calmac.org/publications/DNVGL_PGE_HERs_2015_final_to_calmac.pdf --> PC study has high case at 0% --> shif to 25%?",1]
["IDResidentialBehavioralProgram Dropout Rate (Attrition)","ID","Residential","Behavioral","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"high rate based on PG&E rollout with six waves http://www.calmac.org/publications/DNVGL_PGE_HERs_2015_final_to_calmac.pdf --> PC study has high case at 0% --> shif to 25%?",1]
["IDResidentialDLC Electric Vehicle ChargingMarket Potential","ID","Residential","DLC Electric Vehicle Charging","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["IDResidentialDLC Electric Vehicle ChargingProgram Dropout Rate (Attrition)","ID","Residential","DLC Electric Vehicle Charging","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["IDResidentialDLC Central ACMarket Potential","ID","Residential","DLC Central AC","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["IDResidentialDLC Central ACProgram Dropout Rate (Attrition)","ID","Residential","DLC Central AC","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["IDGeneral ServiceDLC Central ACMarket Potential","ID","General Service","DLC Central AC","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["IDGeneral ServiceDLC Central ACProgram Dropout Rate (Attrition)","ID","General Service","DLC Central AC","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC DLC Switch cooling assumption- 5 yr ramp rate",1]
["IDResidentialDLC Water HeatingMarket Potential","ID","Residential","DLC Water Heating","Market Potential","% of Eligible Customers",1.4999999999999999E-2,4.5000000000000005E-2,0.105,0.13500000000000001,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["IDResidentialDLC Water HeatingProgram Dropout Rate (Attrition)","ID","Residential","DLC Water Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["IDGeneral ServiceDLC Water HeatingMarket Potential","ID","General Service","DLC Water Heating","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["IDGeneral ServiceDLC Water HeatingProgram Dropout Rate (Attrition)","ID","General Service","DLC Water Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["IDResidentialCTA-2045 WHMarket Potential","ID","Residential","CTA-2045 WH","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDResidentialCTA-2045 WHProgram Dropout Rate (Attrition)","ID","Residential","CTA-2045 WH","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDGeneral ServiceCTA-2045 WHMarket Potential","ID","General Service","CTA-2045 WH","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDGeneral ServiceCTA-2045 WHProgram Dropout Rate (Attrition)","ID","General Service","CTA-2045 WH","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDResidentialDLC Smart Thermostats - CoolingMarket Potential","ID","Residential","DLC Smart Thermostats - Cooling","Market Potential","% of Eligible Customers",2.0000000000000004E-2,6.0000000000000012E-2,0.13999999999999999,0.18000000000000005,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDResidentialDLC Smart Thermostats - CoolingProgram Dropout Rate (Attrition)","ID","Residential","DLC Smart Thermostats - Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingMarket Potential","ID","General Service","DLC Smart Thermostats - Cooling","Market Potential","% of Eligible Customers",2.0000000000000004E-2,6.0000000000000012E-2,0.13999999999999999,0.18000000000000005,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingProgram Dropout Rate (Attrition)","ID","General Service","DLC Smart Thermostats - Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDResidentialDLC Smart Thermostats - HeatingMarket Potential","ID","Residential","DLC Smart Thermostats - Heating","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat",1]
["IDResidentialDLC Smart Thermostats - HeatingProgram Dropout Rate (Attrition)","ID","Residential","DLC Smart Thermostats - Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingMarket Potential","ID","General Service","DLC Smart Thermostats - Heating","Market Potential","% of Eligible Customers",3.0000000000000001E-3,9.0000000000000011E-3,2.0999999999999998E-2,2.7000000000000003E-2,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,"Dropping to 3% to compensate for higher space heating saturations",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingProgram Dropout Rate (Attrition)","ID","General Service","DLC Smart Thermostats - Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Dropping to 3% to compensate for higher space heating saturations",1]
["IDResidentialDLC Smart AppliancesMarket Potential","ID","Residential","DLC Smart Appliances","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["IDResidentialDLC Smart AppliancesProgram Dropout Rate (Attrition)","ID","Residential","DLC Smart Appliances","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["IDGeneral ServiceDLC Smart AppliancesMarket Potential","ID","General Service","DLC Smart Appliances","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["IDGeneral ServiceDLC Smart AppliancesProgram Dropout Rate (Attrition)","ID","General Service","DLC Smart Appliances","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"2015 ISACA IT Risk Reward Barometer - US Consumer Results. October 2015. http://www.isaca.org/SiteCollectionDocuments/2015-risk-reward-survey/2015-isaca-risk-reward-consumer-summary-us_res_eng_1015.pdf",1]
["IDGeneral ServiceThird Party ContractsMarket Potential","ID","General Service","Third Party Contracts","Market Potential","% of Eligible Customers",3.7499999999999999E-2,7.4999999999999997E-2,0.1275,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,"MPSC Demand Response Market Assessment",1]
["IDGeneral ServiceThird Party ContractsProgram Dropout Rate (Attrition)","ID","General Service","Third Party Contracts","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"MPSC Demand Response Market Assessment",1]
["IDLarge General ServiceThird Party ContractsMarket Potential","ID","Large General Service","Third Party Contracts","Market Potential","% of Eligible Customers",5.525E-2,0.1105,0.18784999999999999,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0.221,0,1]
["IDLarge General ServiceThird Party ContractsProgram Dropout Rate (Attrition)","ID","Large General Service","Third Party Contracts","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0,1]
["IDExtra Large General ServiceThird Party ContractsMarket Potential","ID","Extra Large General Service","Third Party Contracts","Market Potential","% of Eligible Customers",5.2249999999999998E-2,0.1045,0.17764999999999997,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0.20899999999999999,0,1]
["IDExtra Large General ServiceThird Party ContractsProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Third Party Contracts","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0,1]
["IDResidentialTime-of-Use Opt-inMarket Potential","ID","Residential","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle Analysis and Estimate",1]
["IDResidentialTime-of-Use Opt-inProgram Dropout Rate (Attrition)","ID","Residential","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle Analysis and Estimate",1]
["IDGeneral ServiceTime-of-Use Opt-inMarket Potential","ID","General Service","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["IDGeneral ServiceTime-of-Use Opt-inProgram Dropout Rate (Attrition)","ID","General Service","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["IDLarge General ServiceTime-of-Use Opt-inMarket Potential","ID","Large General Service","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["IDLarge General ServiceTime-of-Use Opt-inProgram Dropout Rate (Attrition)","ID","Large General Service","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["IDExtra Large General ServiceTime-of-Use Opt-inMarket Potential","ID","Extra Large General Service","Time-of-Use Opt-in","Market Potential","% of Eligible Customers",1.2999999999999999E-2,3.9E-2,7.8E-2,0.11700000000000001,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,0.13,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["IDExtra Large General ServiceTime-of-Use Opt-inProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Time-of-Use Opt-in","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-in case as high, 75% of high as low case- Using low case -9.8%",1]
["IDResidentialTime-of-Use Opt-outMarket Potential","ID","Residential","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["IDResidentialTime-of-Use Opt-outProgram Dropout Rate (Attrition)","ID","Residential","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
[{"$f":"B130&C130&D130&E130","v":"IDGeneral ServiceTime-of-Use Opt-outMarket Potential"},"ID","General Service","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["IDGeneral ServiceTime-of-Use Opt-outProgram Dropout Rate (Attrition)","ID","General Service","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
["IDLarge General ServiceTime-of-Use Opt-outMarket Potential","ID","Large General Service","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["IDLarge General ServiceTime-of-Use Opt-outProgram Dropout Rate (Attrition)","ID","Large General Service","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
["IDExtra Large General ServiceTime-of-Use Opt-outMarket Potential","ID","Extra Large General Service","Time-of-Use Opt-out","Market Potential","% of Eligible Customers",1,0.85399999999999998,0.78900000000000003,0.75600000000000001,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,0.74,"Brattle opt-out case",1]
["IDExtra Large General ServiceTime-of-Use Opt-outProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Time-of-Use Opt-out","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle opt-out case",1]
["IDResidentialVariable Peak Pricing RatesMarket Potential","ID","Residential","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"High Case- OG&E's VPP Plus participation rate- should be 103000/400000 around 25%",1]
["IDResidentialVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","ID","Residential","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"High Case- OG&E's VPP Plus participation rate- should be 103000/400000 around 25%",1]
["IDGeneral ServiceVariable Peak Pricing RatesMarket Potential","ID","General Service","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"Brattle",1]
["IDGeneral ServiceVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","ID","General Service","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Brattle",1]
["IDLarge General ServiceVariable Peak Pricing RatesMarket Potential","ID","Large General Service","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","ID","Large General Service","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesMarket Potential","ID","Extra Large General Service","Variable Peak Pricing Rates","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"High Case- OG&E's VPP Plus participation rate",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Variable Peak Pricing Rates","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"High Case- OG&E's VPP Plus participation rate",1]
["IDLarge General ServiceReal Time PricingMarket Potential","ID","Large General Service","Real Time Pricing","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["IDLarge General ServiceReal Time PricingProgram Dropout Rate (Attrition)","ID","Large General Service","Real Time Pricing","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["IDExtra Large General ServiceReal Time PricingMarket Potential","ID","Extra Large General Service","Real Time Pricing","Market Potential","% of Eligible Customers",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},"",1]
["IDExtra Large General ServiceReal Time PricingProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Real Time Pricing","Program Dropout Rate (Attrition)","%","","","","","","","","","","","","","","","","","","","","","","","","","","",1]
["IDGeneral ServiceThermal Energy StorageMarket Potential","ID","General Service","Thermal Energy Storage","Market Potential","% of Eligible Customers",5.0000000000000001E-4,1.5000000000000002E-3,3.4999999999999996E-3,4.5000000000000005E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Don't expect much participation - 0.5%",1]
["IDGeneral ServiceThermal Energy StorageProgram Dropout Rate (Attrition)","ID","General Service","Thermal Energy Storage","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Don't expect much participation - 0.5%",1]
["IDLarge General ServiceThermal Energy StorageMarket Potential","ID","Large General Service","Thermal Energy Storage","Market Potential","% of Eligible Customers",1.5E-3,4.5000000000000005E-3,1.0499999999999999E-2,1.3500000000000002E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,"Low participation is 1/2 DLC CAC",1]
["IDLarge General ServiceThermal Energy StorageProgram Dropout Rate (Attrition)","ID","Large General Service","Thermal Energy Storage","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Low participation is 1/2 DLC CAC",1]
["IDExtra Large General ServiceThermal Energy StorageMarket Potential","ID","Extra Large General Service","Thermal Energy Storage","Market Potential","% of Eligible Customers",1.5E-3,4.5000000000000005E-3,1.0499999999999999E-2,1.3500000000000002E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,"Low participation is 1/2 DLC CAC",1]
["IDExtra Large General ServiceThermal Energy StorageProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Thermal Energy Storage","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Low participation is 1/2 DLC CAC",1]
["IDResidentialBattery Energy StorageMarket Potential","ID","Residential","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["IDResidentialBattery Energy StorageProgram Dropout Rate (Attrition)","ID","Residential","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["IDGeneral ServiceBattery Energy StorageMarket Potential","ID","General Service","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["IDGeneral ServiceBattery Energy StorageProgram Dropout Rate (Attrition)","ID","General Service","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["IDLarge General ServiceBattery Energy StorageMarket Potential","ID","Large General Service","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["IDLarge General ServiceBattery Energy StorageProgram Dropout Rate (Attrition)","ID","Large General Service","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["IDExtra Large General ServiceBattery Energy StorageMarket Potential","ID","Extra Large General Service","Battery Energy Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["IDExtra Large General ServiceBattery Energy StorageProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Battery Energy Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["IDResidentialAncillary CoolingMarket Potential","ID","Residential","Ancillary Cooling","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDResidentialAncillary CoolingProgram Dropout Rate (Attrition)","ID","Residential","Ancillary Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDGeneral ServiceAncillary CoolingMarket Potential","ID","General Service","Ancillary Cooling","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDGeneral ServiceAncillary CoolingProgram Dropout Rate (Attrition)","ID","General Service","Ancillary Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["IDResidentialAncillary HeatingMarket Potential","ID","Residential","Ancillary Heating","Market Potential","% of Eligible Customers",2.5000000000000005E-3,7.5000000000000015E-3,1.7499999999999998E-2,2.2500000000000006E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat= half for ancillary",1]
["IDResidentialAncillary HeatingProgram Dropout Rate (Attrition)","ID","Residential","Ancillary Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat= half for ancillary",1]
["IDGeneral ServiceAncillary HeatingMarket Potential","ID","General Service","Ancillary Heating","Market Potential","% of Eligible Customers",1.5E-3,4.5000000000000005E-3,1.0499999999999999E-2,1.3500000000000002E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,"Dropping to 3% to compensate for higher space heating saturations- half for ancillary",1]
["IDGeneral ServiceAncillary HeatingProgram Dropout Rate (Attrition)","ID","General Service","Ancillary Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Dropping to 3% to compensate for higher space heating saturations- half for ancillary",1]
["IDResidentialAncillary DLC WHMarket Potential","ID","Residential","Ancillary DLC WH","Market Potential","% of Eligible Customers",1.4999999999999999E-2,4.5000000000000005E-2,0.105,0.13500000000000001,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["IDResidentialAncillary DLC WHProgram Dropout Rate (Attrition)","ID","Residential","Ancillary DLC WH","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["IDGeneral ServiceAncillary DLC WHMarket Potential","ID","General Service","Ancillary DLC WH","Market Potential","% of Eligible Customers",5.000000000000001E-3,1.5000000000000003E-2,3.4999999999999996E-2,4.5000000000000012E-2,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["IDGeneral ServiceAncillary DLC WHProgram Dropout Rate (Attrition)","ID","General Service","Ancillary DLC WH","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["IDResidentialAncillary WHMarket Potential","ID","Residential","Ancillary WH","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDResidentialAncillary WHProgram Dropout Rate (Attrition)","ID","Residential","Ancillary WH","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDGeneral ServiceAncillary WHMarket Potential","ID","General Service","Ancillary WH","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDGeneral ServiceAncillary WHProgram Dropout Rate (Attrition)","ID","General Service","Ancillary WH","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["IDResidentialAncillary EVMarket Potential","ID","Residential","Ancillary EV","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["IDResidentialAncillary EVProgram Dropout Rate (Attrition)","ID","Residential","Ancillary EV","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["IDGeneral ServiceAncillary Third PartyMarket Potential","ID","General Service","Ancillary Third Party","Market Potential","% of Eligible Customers",7.4999999999999997E-3,1.4999999999999999E-2,2.5499999999999998E-2,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["IDGeneral ServiceAncillary Third PartyProgram Dropout Rate (Attrition)","ID","General Service","Ancillary Third Party","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["IDLarge General ServiceAncillary Third PartyMarket Potential","ID","Large General Service","Ancillary Third Party","Market Potential","% of Eligible Customers",1.1050000000000001E-2,2.2100000000000002E-2,3.7569999999999999E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["IDLarge General ServiceAncillary Third PartyProgram Dropout Rate (Attrition)","ID","Large General Service","Ancillary Third Party","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["IDExtra Large General ServiceAncillary Third PartyMarket Potential","ID","Extra Large General Service","Ancillary Third Party","Market Potential","% of Eligible Customers",1.0450000000000001E-2,2.0900000000000002E-2,3.5529999999999999E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["IDExtra Large General ServiceAncillary Third PartyProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Ancillary Third Party","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["IDResidentialAncillary Battery StorageMarket Potential","ID","Residential","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["IDResidentialAncillary Battery StorageProgram Dropout Rate (Attrition)","ID","Residential","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["IDGeneral ServiceAncillary Battery StorageMarket Potential","ID","General Service","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["IDGeneral ServiceAncillary Battery StorageProgram Dropout Rate (Attrition)","ID","General Service","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["IDLarge General ServiceAncillary Battery StorageMarket Potential","ID","Large General Service","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["IDLarge General ServiceAncillary Battery StorageProgram Dropout Rate (Attrition)","ID","Large General Service","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["IDExtra Large General ServiceAncillary Battery StorageMarket Potential","ID","Extra Large General Service","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["IDExtra Large General ServiceAncillary Battery StorageProgram Dropout Rate (Attrition)","ID","Extra Large General Service","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
[{"$f":"B194&C194&D194&E194","v":"WAResidentialAncillary CoolingMarket Potential"},"WA","Residential","Ancillary Cooling","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAResidentialAncillary CoolingProgram Dropout Rate (Attrition)","WA","Residential","Ancillary Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAGeneral ServiceAncillary CoolingMarket Potential","WA","General Service","Ancillary Cooling","Market Potential","% of Eligible Customers",1.0000000000000002E-2,3.0000000000000006E-2,6.9999999999999993E-2,9.0000000000000024E-2,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAGeneral ServiceAncillary CoolingProgram Dropout Rate (Attrition)","WA","General Service","Ancillary Cooling","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Smart Thermostat cooling assumption- 5 yr ramp rate",1]
["WAResidentialAncillary HeatingMarket Potential","WA","Residential","Ancillary Heating","Market Potential","% of Eligible Customers",2.5000000000000005E-3,7.5000000000000015E-3,1.7499999999999998E-2,2.2500000000000006E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat= half for ancillary",1]
["WAResidentialAncillary HeatingProgram Dropout Rate (Attrition)","WA","Residential","Ancillary Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Assuming maximum participation for combined DLC Cooling and Smart Therm is 25%, reduced from 30% to account for those program participants who may have intended to participate but were unable to correctly install their thermostat= half for ancillary",1]
["WAGeneral ServiceAncillary HeatingMarket Potential","WA","General Service","Ancillary Heating","Market Potential","% of Eligible Customers",1.5E-3,4.5000000000000005E-3,1.0499999999999999E-2,1.3500000000000002E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,"Dropping to 3% to compensate for higher space heating saturations- half for ancillary",1]
["WAGeneral ServiceAncillary HeatingProgram Dropout Rate (Attrition)","WA","General Service","Ancillary Heating","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Dropping to 3% to compensate for higher space heating saturations- half for ancillary",1]
["WAResidentialAncillary DLC WHMarket Potential","WA","Residential","Ancillary DLC WH","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["WAResidentialAncillary DLC WHProgram Dropout Rate (Attrition)","WA","Residential","Ancillary DLC WH","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Ensure population applies to the subset of customers participating in AC or Space Heating DLC",1]
["WAGeneral ServiceAncillary DLC WHMarket Potential","WA","General Service","Ancillary DLC WH","Market Potential","% of Eligible Customers",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["WAGeneral ServiceAncillary DLC WHProgram Dropout Rate (Attrition)","WA","General Service","Ancillary DLC WH","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"* Changed from 3% to reflect a Brattle Study to the left that estimates 5-10%",1]
["WAResidentialAncillary WHMarket Potential","WA","Residential","Ancillary WH","Market Potential","% of Eligible Customers",0.02,0.06,0.1,0.15000000000000002,0.2,0.25,0.32500000000000001,0.4,0.47500000000000003,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAResidentialAncillary WHProgram Dropout Rate (Attrition)","WA","Residential","Ancillary WH","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAGeneral ServiceAncillary WHMarket Potential","WA","General Service","Ancillary WH","Market Potential","% of Eligible Customers",0.02,0.06,0.1,0.15000000000000002,0.2,0.25,0.32500000000000001,0.4,0.47500000000000003,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAGeneral ServiceAncillary WHProgram Dropout Rate (Attrition)","WA","General Service","Ancillary WH","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"NWPC Electric Resistance Grid-Ready Summer/Winter Participation- 10 yr ramp rate",1]
["WAResidentialAncillary EVMarket Potential","WA","Residential","Ancillary EV","Market Potential","% of Eligible Customers",2.5000000000000001E-2,7.5000000000000011E-2,0.17499999999999999,0.22500000000000003,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,0.25,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["WAResidentialAncillary EVProgram Dropout Rate (Attrition)","WA","Residential","Ancillary EV","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Prelim Assumption: One Third of TOU Demand Rate w EV.  This participation rate will be throttled / scaled using the equipment saturation for EVs, which will be quite low.",1]
["WAGeneral ServiceAncillary Third PartyMarket Potential","WA","General Service","Ancillary Third Party","Market Potential","% of Eligible Customers",7.4999999999999997E-3,1.4999999999999999E-2,2.5499999999999998E-2,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["WAGeneral ServiceAncillary Third PartyProgram Dropout Rate (Attrition)","WA","General Service","Ancillary Third Party","Program Dropout Rate (Attrition)","%",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["WALarge General ServiceAncillary Third PartyMarket Potential","WA","Large General Service","Ancillary Third Party","Market Potential","% of Eligible Customers",1.1050000000000001E-2,2.2100000000000002E-2,3.7569999999999999E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,4.4200000000000003E-2,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["WALarge General ServiceAncillary Third PartyProgram Dropout Rate (Attrition)","WA","Large General Service","Ancillary Third Party","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["WAExtra Large General ServiceAncillary Third PartyMarket Potential","WA","Extra Large General Service","Ancillary Third Party","Market Potential","% of Eligible Customers",1.0450000000000001E-2,2.0900000000000002E-2,3.5529999999999999E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,4.1800000000000004E-2,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["WAExtra Large General ServiceAncillary Third PartyProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Ancillary Third Party","Program Dropout Rate (Attrition)","%",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,"Participation rate based on saturations of EMS systems within PAC commercial customers- if we have the breakout of their Market Profile then we can get closer to the correct number of eligible participants.",1]
["WAResidentialAncillary Battery StorageMarket Potential","WA","Residential","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["WAResidentialAncillary Battery StorageProgram Dropout Rate (Attrition)","WA","Residential","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"20% from MISO LRZ 7. Assuming half for high and half again for low. *halved again 9-14-17, as per discussion with Kelly - potential looked too high.  Pacificorp study didn't consider this program",1]
["WAGeneral ServiceAncillary Battery StorageMarket Potential","WA","General Service","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["WAGeneral ServiceAncillary Battery StorageProgram Dropout Rate (Attrition)","WA","General Service","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["WALarge General ServiceAncillary Battery StorageMarket Potential","WA","Large General Service","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["WALarge General ServiceAncillary Battery StorageProgram Dropout Rate (Attrition)","WA","Large General Service","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]
["WAExtra Large General ServiceAncillary Battery StorageMarket Potential","WA","Extra Large General Service","Ancillary Battery Storage","Market Potential","% of Eligible Customers",1E-4,2.9999999999999997E-4,5.0000000000000001E-4,8.0000000000000004E-4,1.1000000000000001E-3,1.4000000000000002E-3,1.7000000000000001E-3,2.1000000000000003E-3,2.5000000000000001E-3,2.8999999999999998E-3,3.3999999999999998E-3,3.8999999999999998E-3,4.3999999999999994E-3,4.9999999999999992E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,"Same as Residential",1]
["WAExtra Large General ServiceAncillary Battery StorageProgram Dropout Rate (Attrition)","WA","Extra Large General Service","Ancillary Battery Storage","Program Dropout Rate (Attrition)","%",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"Same as Residential",1]

{"sheet":"ImpactInput","index":5,"n_rows":561,"n_cols":9,"rows_kept":561,"cut":false,"hidden":false,"merged":[]}
["Key","State","Customer Class","Option","Data Element","Unit","Market Potential","Comments from Input Generator"]
[{"$f":"B2&C2&D2&E2","v":"WAResidentialBehavioralEvent Non-Performance Rate"},"WA","Residential","Behavioral","Event Non-Performance Rate","%",0,0,1]
[{"$f":"B3&C3&D3&E3","v":"WAResidentialBehavioralPer Customer Summer Peak Reduction (kW)"},"WA","Residential","Behavioral","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"hi participation case = 0.75% of low to account for lower potential customers ",1]
["WAResidentialBehavioralPer Customer Summer Peak Reduction (%)","WA","Residential","Behavioral","Per Customer Summer Peak Reduction (%)","% of Peak",0.02,"Opower documentation for BDR with Consumers and DTE",1]
["WAResidentialBehavioralPer Customer Winter Peak Reduction (kW)","WA","Residential","Behavioral","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Assume 50% of Summer impacts.",1]
["WAResidentialBehavioralPer Customer Winter Peak Reduction (%)","WA","Residential","Behavioral","Per Customer Winter Peak Reduction (%)","% of Peak",0.02,0,1]
["WAResidentialDLC Electric Vehicle ChargingEvent Non-Performance Rate","WA","Residential","DLC Electric Vehicle Charging","Event Non-Performance Rate","%",0,0,1]
["WAResidentialDLC Electric Vehicle ChargingPer Customer Summer Peak Reduction (kW)","WA","Residential","DLC Electric Vehicle Charging","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"Expecting 90% + load shift",1]
["WAResidentialDLC Electric Vehicle ChargingPer Customer Summer Peak Reduction (%)","WA","Residential","DLC Electric Vehicle Charging","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Electric Vehicle ChargingPer Customer Winter Peak Reduction (kW)","WA","Residential","DLC Electric Vehicle Charging","Per Customer Winter Peak Reduction (kW)","kW @meter",0.5,"Expecting 90% + load shift",1]
["WAResidentialDLC Electric Vehicle ChargingPer Customer Winter Peak Reduction (%)","WA","Residential","DLC Electric Vehicle Charging","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Central ACEvent Non-Performance Rate","WA","Residential","DLC Central AC","Event Non-Performance Rate","%",0,0,1]
["WAResidentialDLC Central ACPer Customer Summer Peak Reduction (kW)","WA","Residential","DLC Central AC","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"NWPC DLC Switch cooling assumption (east)",1]
["WAResidentialDLC Central ACPer Customer Summer Peak Reduction (%)","WA","Residential","DLC Central AC","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Central ACPer Customer Winter Peak Reduction (kW)","WA","Residential","DLC Central AC","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialDLC Central ACPer Customer Winter Peak Reduction (%)","WA","Residential","DLC Central AC","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Central ACEvent Non-Performance Rate","WA","General Service","DLC Central AC","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceDLC Central ACPer Customer Summer Peak Reduction (kW)","WA","General Service","DLC Central AC","Per Customer Summer Peak Reduction (kW)","kW @meter",1.25,"NWPC DLC Switch cooling assumption (east)",1]
["WAGeneral ServiceDLC Central ACPer Customer Summer Peak Reduction (%)","WA","General Service","DLC Central AC","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Central ACPer Customer Winter Peak Reduction (kW)","WA","General Service","DLC Central AC","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceDLC Central ACPer Customer Winter Peak Reduction (%)","WA","General Service","DLC Central AC","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Water HeatingEvent Non-Performance Rate","WA","Residential","DLC Water Heating","Event Non-Performance Rate","%",0,0,1]
["WAResidentialDLC Water HeatingPer Customer Summer Peak Reduction (kW)","WA","Residential","DLC Water Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAResidentialDLC Water HeatingPer Customer Summer Peak Reduction (%)","WA","Residential","DLC Water Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Water HeatingPer Customer Winter Peak Reduction (kW)","WA","Residential","DLC Water Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAResidentialDLC Water HeatingPer Customer Winter Peak Reduction (%)","WA","Residential","DLC Water Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Water HeatingEvent Non-Performance Rate","WA","General Service","DLC Water Heating","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceDLC Water HeatingPer Customer Summer Peak Reduction (kW)","WA","General Service","DLC Water Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAGeneral ServiceDLC Water HeatingPer Customer Summer Peak Reduction (%)","WA","General Service","DLC Water Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Water HeatingPer Customer Winter Peak Reduction (kW)","WA","General Service","DLC Water Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAGeneral ServiceDLC Water HeatingPer Customer Winter Peak Reduction (%)","WA","General Service","DLC Water Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialCTA-2045 WHEvent Non-Performance Rate","WA","Residential","CTA-2045 WH","Event Non-Performance Rate","%",0.03,"Ability for customers to easily override event- using 3% as placeholder",1]
["WAResidentialCTA-2045 WHPer Customer Summer Peak Reduction (kW)","WA","Residential","CTA-2045 WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["WAResidentialCTA-2045 WHPer Customer Summer Peak Reduction (%)","WA","Residential","CTA-2045 WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialCTA-2045 WHPer Customer Winter Peak Reduction (kW)","WA","Residential","CTA-2045 WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["WAResidentialCTA-2045 WHPer Customer Winter Peak Reduction (%)","WA","Residential","CTA-2045 WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Duke Energy produced PPT of pilot but no impacts",1]
["WAGeneral ServiceCTA-2045 WHEvent Non-Performance Rate","WA","General Service","CTA-2045 WH","Event Non-Performance Rate","%",0.03,0,1]
["WAGeneral ServiceCTA-2045 WHPer Customer Summer Peak Reduction (kW)","WA","General Service","CTA-2045 WH","Per Customer Summer Peak Reduction (kW)","kW @meter",1.26,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["WAGeneral ServiceCTA-2045 WHPer Customer Summer Peak Reduction (%)","WA","General Service","CTA-2045 WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceCTA-2045 WHPer Customer Winter Peak Reduction (kW)","WA","General Service","CTA-2045 WH","Per Customer Winter Peak Reduction (kW)","kW @meter",1.26,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["WAGeneral ServiceCTA-2045 WHPer Customer Winter Peak Reduction (%)","WA","General Service","CTA-2045 WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Smart Thermostats - CoolingEvent Non-Performance Rate","WA","Residential","DLC Smart Thermostats - Cooling","Event Non-Performance Rate","%",0,0,1]
["WAResidentialDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (kW)","WA","Residential","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
["WAResidentialDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (%)","WA","Residential","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (kW)","WA","Residential","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (%)","WA","Residential","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingEvent Non-Performance Rate","WA","General Service","DLC Smart Thermostats - Cooling","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (kW)","WA","General Service","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",1.25,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (%)","WA","General Service","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (kW)","WA","General Service","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (%)","WA","General Service","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Smart Thermostats - HeatingEvent Non-Performance Rate","WA","Residential","DLC Smart Thermostats - Heating","Event Non-Performance Rate","%",0,0,1]
["WAResidentialDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (kW)","WA","Residential","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (%)","WA","Residential","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (kW)","WA","Residential","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",1.0900000000000001,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["WAResidentialDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (%)","WA","Residential","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingEvent Non-Performance Rate","WA","General Service","DLC Smart Thermostats - Heating","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (kW)","WA","General Service","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (%)","WA","General Service","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (kW)","WA","General Service","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",1.35,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (%)","WA","General Service","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Pacificorp Assumptions",1]
["WAResidentialDLC Smart AppliancesEvent Non-Performance Rate","WA","Residential","DLC Smart Appliances","Event Non-Performance Rate","%",0,0,1]
["WAResidentialDLC Smart AppliancesPer Customer Summer Peak Reduction (kW)","WA","Residential","DLC Smart Appliances","Per Customer Summer Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["WAResidentialDLC Smart AppliancesPer Customer Summer Peak Reduction (%)","WA","Residential","DLC Smart Appliances","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialDLC Smart AppliancesPer Customer Winter Peak Reduction (kW)","WA","Residential","DLC Smart Appliances","Per Customer Winter Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["WAResidentialDLC Smart AppliancesPer Customer Winter Peak Reduction (%)","WA","Residential","DLC Smart Appliances","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
[{"$f":"B67&C67&D67&E67","v":"WAGeneral ServiceDLC Smart AppliancesEvent Non-Performance Rate"},"WA","General Service","DLC Smart Appliances","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceDLC Smart AppliancesPer Customer Summer Peak Reduction (kW)","WA","General Service","DLC Smart Appliances","Per Customer Summer Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["WAGeneral ServiceDLC Smart AppliancesPer Customer Summer Peak Reduction (%)","WA","General Service","DLC Smart Appliances","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceDLC Smart AppliancesPer Customer Winter Peak Reduction (kW)","WA","General Service","DLC Smart Appliances","Per Customer Winter Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["WAGeneral ServiceDLC Smart AppliancesPer Customer Winter Peak Reduction (%)","WA","General Service","DLC Smart Appliances","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceThird Party ContractsEvent Non-Performance Rate","WA","General Service","Third Party Contracts","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceThird Party ContractsPer Customer Summer Peak Reduction (kW)","WA","General Service","Third Party Contracts","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceThird Party ContractsPer Customer Summer Peak Reduction (%)","WA","General Service","Third Party Contracts","Per Customer Summer Peak Reduction (%)","% of Peak",0.1,"Michigan Demand Response Market Assessment- Capacity Bidding",1]
["WAGeneral ServiceThird Party ContractsPer Customer Winter Peak Reduction (kW)","WA","General Service","Third Party Contracts","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceThird Party ContractsPer Customer Winter Peak Reduction (%)","WA","General Service","Third Party Contracts","Per Customer Winter Peak Reduction (%)","% of Peak",0.1,"Michigan Demand Response Market Assessment- Capacity Bidding",1]
["WALarge General ServiceThird Party ContractsEvent Non-Performance Rate","WA","Large General Service","Third Party Contracts","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceThird Party ContractsPer Customer Summer Peak Reduction (kW)","WA","Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceThird Party ContractsPer Customer Summer Peak Reduction (%)","WA","Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["WALarge General ServiceThird Party ContractsPer Customer Winter Peak Reduction (kW)","WA","Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceThird Party ContractsPer Customer Winter Peak Reduction (%)","WA","Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["WAExtra Large General ServiceThird Party ContractsEvent Non-Performance Rate","WA","Extra Large General Service","Third Party Contracts","Event Non-Performance Rate","%",0,0,1]
["WAExtra Large General ServiceThird Party ContractsPer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceThird Party ContractsPer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["WAExtra Large General ServiceThird Party ContractsPer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceThird Party ContractsPer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["WAResidentialTime-of-Use Opt-inEvent Non-Performance Rate","WA","Residential","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,"None - should be in eval'd number.",1]
["WAResidentialTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","WA","Residential","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","WA","Residential","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",5.7000000000000002E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WAResidentialTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","WA","Residential","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","WA","Residential","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",2.8500000000000001E-2,"Assume 50% of Summer impacts. Brattle Analysis and Estimate - Negative impacts in Winter set to zero in Eastern states.",1]
["WAGeneral ServiceTime-of-Use Opt-inEvent Non-Performance Rate","WA","General Service","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","WA","General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","WA","General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",2E-3,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WAGeneral ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","WA","General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","WA","General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",1E-3,"Assume 50% of Summer impacts.",1]
["WALarge General ServiceTime-of-Use Opt-inEvent Non-Performance Rate","WA","Large General Service","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","WA","Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","WA","Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",2.5999999999999999E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WALarge General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","WA","Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","WA","Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",1.2999999999999999E-2,"Assume 50% of Summer impacts.",1]
["WAExtra Large General ServiceTime-of-Use Opt-inEvent Non-Performance Rate","WA","Extra Large General Service","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",3.1E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WAExtra Large General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",1.55E-2,"Assume 50% of Summer impacts.",1]
["WAResidentialTime-of-Use Opt-outEvent Non-Performance Rate","WA","Residential","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,"None - should be in eval'd number.",1]
["WAResidentialTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)","WA","Residential","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","WA","Residential","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",3.4000000000000002E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WAResidentialTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","WA","Residential","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","WA","Residential","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1.7000000000000001E-2,"Assume 50% of Summer impacts. Brattle Analysis and Estimate - Negative impacts in Winter set to zero in Eastern states.",1]
["WAGeneral ServiceTime-of-Use Opt-outEvent Non-Performance Rate","WA","General Service","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)","WA","General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","WA","General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",2E-3,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WAGeneral ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","WA","General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","WA","General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1E-3,"Assume 50% of Summer impacts.",1]
["WALarge General ServiceTime-of-Use Opt-outEvent Non-Performance Rate","WA","Large General Service","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)","WA","Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","WA","Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",2.5999999999999999E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WALarge General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","WA","Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","WA","Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1.2999999999999999E-2,"Assume 50% of Summer impacts.",1]
["WAExtra Large General ServiceTime-of-Use Opt-outEvent Non-Performance Rate","WA","Extra Large General Service","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",3.1E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["WAExtra Large General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1.55E-2,"Assume 50% of Summer impacts.",1]
["WAResidentialVariable Peak Pricing RatesEvent Non-Performance Rate","WA","Residential","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["WAResidentialVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","WA","Residential","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","WA","Residential","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.1,"OG&E 2017 Smart Hours Study - Res 10% impacts for VPP only",1]
["WAResidentialVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","WA","Residential","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
[{"$f":"B131&C131&D131&E131","v":"WAResidentialVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)"},"WA","Residential","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",7.5000000000000011E-2,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesEvent Non-Performance Rate","WA","General Service","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","WA","General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","WA","General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.04,"OG&E 2017 Smart Hours Study - 4% for an average CPE day for VPP only customers without a smart thermostat",1]
["WAGeneral ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","WA","General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)","WA","General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",0.03,0,1]
["WALarge General ServiceVariable Peak Pricing RatesEvent Non-Performance Rate","WA","Large General Service","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","WA","Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","WA","Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.04,"OG&E 2017 Smart Hours Study - 4% for an average CPE day for VPP only customers without a smart thermostat",1]
["WALarge General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","WA","Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)","WA","Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",0.03,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesEvent Non-Performance Rate","WA","Extra Large General Service","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.04,"OG&E 2017 Smart Hours Study - 4% for an average CPE day for VPP only customers without a smart thermostat",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",0.03,0,1]
["WALarge General ServiceReal Time PricingEvent Non-Performance Rate","WA","Large General Service","Real Time Pricing","Event Non-Performance Rate","%","","",1]
["WALarge General ServiceReal Time PricingPer Customer Summer Peak Reduction (kW)","WA","Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["WALarge General ServiceReal Time PricingPer Customer Summer Peak Reduction (%)","WA","Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
["WALarge General ServiceReal Time PricingPer Customer Winter Peak Reduction (kW)","WA","Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["WALarge General ServiceReal Time PricingPer Customer Winter Peak Reduction (%)","WA","Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["WAExtra Large General ServiceReal Time PricingEvent Non-Performance Rate","WA","Extra Large General Service","Real Time Pricing","Event Non-Performance Rate","%","","",1]
["WAExtra Large General ServiceReal Time PricingPer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["WAExtra Large General ServiceReal Time PricingPer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
["WAExtra Large General ServiceReal Time PricingPer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["WAExtra Large General ServiceReal Time PricingPer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["WAGeneral ServiceThermal Energy StorageEvent Non-Performance Rate","WA","General Service","Thermal Energy Storage","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceThermal Energy StoragePer Customer Summer Peak Reduction (kW)","WA","General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",1.68,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["WAGeneral ServiceThermal Energy StoragePer Customer Summer Peak Reduction (%)","WA","General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceThermal Energy StoragePer Customer Winter Peak Reduction (kW)","WA","General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Removed Winter Impacts",1]
["WAGeneral ServiceThermal Energy StoragePer Customer Winter Peak Reduction (%)","WA","General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WALarge General ServiceThermal Energy StorageEvent Non-Performance Rate","WA","Large General Service","Thermal Energy Storage","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (kW)","WA","Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",8.4,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["WALarge General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (%)","WA","Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WALarge General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (kW)","WA","Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["WALarge General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (%)","WA","Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAExtra Large General ServiceThermal Energy StorageEvent Non-Performance Rate","WA","Extra Large General Service","Thermal Energy Storage","Event Non-Performance Rate","%",0,0,1]
["WAExtra Large General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",8.4,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["WAExtra Large General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAExtra Large General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["WAExtra Large General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialBattery Energy StorageEvent Non-Performance Rate","WA","Residential","Battery Energy Storage","Event Non-Performance Rate","%",0,0,1]
["WAResidentialBattery Energy StoragePer Customer Summer Peak Reduction (kW)","WA","Residential","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAResidentialBattery Energy StoragePer Customer Summer Peak Reduction (%)","WA","Residential","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialBattery Energy StoragePer Customer Winter Peak Reduction (kW)","WA","Residential","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAResidentialBattery Energy StoragePer Customer Winter Peak Reduction (%)","WA","Residential","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceBattery Energy StorageEvent Non-Performance Rate","WA","General Service","Battery Energy Storage","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceBattery Energy StoragePer Customer Summer Peak Reduction (kW)","WA","General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAGeneral ServiceBattery Energy StoragePer Customer Summer Peak Reduction (%)","WA","General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceBattery Energy StoragePer Customer Winter Peak Reduction (kW)","WA","General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAGeneral ServiceBattery Energy StoragePer Customer Winter Peak Reduction (%)","WA","General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WALarge General ServiceBattery Energy StorageEvent Non-Performance Rate","WA","Large General Service","Battery Energy Storage","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (kW)","WA","Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["WALarge General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (%)","WA","Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WALarge General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (kW)","WA","Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["WALarge General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (%)","WA","Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAExtra Large General ServiceBattery Energy StorageEvent Non-Performance Rate","WA","Extra Large General Service","Battery Energy Storage","Event Non-Performance Rate","%",0,"Pacificorp: ",1]
["WAExtra Large General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Calculated",1]
["WAExtra Large General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,"MISO Res LoadMAP DSM Programs.xlsx (LRZ7) ",1]
["WAExtra Large General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"None",1]
["WAExtra Large General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,"None",1]
["WAResidentialAncillary ServicesEvent Non-Performance Rate","WA","Residential","Ancillary Services","Event Non-Performance Rate","%","","",1]
["WAResidentialAncillary ServicesPer Customer Summer Peak Reduction (kW)","WA","Residential","Ancillary Services","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["WAResidentialAncillary ServicesPer Customer Summer Peak Reduction (%)","WA","Residential","Ancillary Services","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
[{"$f":"B195&C195&D195&E195","v":"WAResidentialAncillary ServicesPer Customer Winter Peak Reduction (kW)"},"WA","Residential","Ancillary Services","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["WAResidentialAncillary ServicesPer Customer Winter Peak Reduction (%)","WA","Residential","Ancillary Services","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["WAGeneral ServiceAncillary ServicesEvent Non-Performance Rate","WA","General Service","Ancillary Services","Event Non-Performance Rate","%","","",1]
["WAGeneral ServiceAncillary ServicesPer Customer Summer Peak Reduction (kW)","WA","General Service","Ancillary Services","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["WAGeneral ServiceAncillary ServicesPer Customer Summer Peak Reduction (%)","WA","General Service","Ancillary Services","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
["WAGeneral ServiceAncillary ServicesPer Customer Winter Peak Reduction (kW)","WA","General Service","Ancillary Services","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["WAGeneral ServiceAncillary ServicesPer Customer Winter Peak Reduction (%)","WA","General Service","Ancillary Services","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["WALarge General ServiceAncillary ServicesEvent Non-Performance Rate","WA","Large General Service","Ancillary Services","Event Non-Performance Rate","%","","",1]
["WALarge General ServiceAncillary ServicesPer Customer Summer Peak Reduction (kW)","WA","Large General Service","Ancillary Services","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["WALarge General ServiceAncillary ServicesPer Customer Summer Peak Reduction (%)","WA","Large General Service","Ancillary Services","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
["WALarge General ServiceAncillary ServicesPer Customer Winter Peak Reduction (kW)","WA","Large General Service","Ancillary Services","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["WALarge General ServiceAncillary ServicesPer Customer Winter Peak Reduction (%)","WA","Large General Service","Ancillary Services","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["WAExtra Large General ServiceAncillary ServicesEvent Non-Performance Rate","WA","Extra Large General Service","Ancillary Services","Event Non-Performance Rate","%","","",1]
["WAExtra Large General ServiceAncillary ServicesPer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Ancillary Services","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["WAExtra Large General ServiceAncillary ServicesPer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Ancillary Services","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
["WAExtra Large General ServiceAncillary ServicesPer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Ancillary Services","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["WAExtra Large General ServiceAncillary ServicesPer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Ancillary Services","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["IDResidentialBehavioralEvent Non-Performance Rate","ID","Residential","Behavioral","Event Non-Performance Rate","%",0,0,1]
["IDResidentialBehavioralPer Customer Summer Peak Reduction (kW)","ID","Residential","Behavioral","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"hi participation case = 0.75% of low to account for lower potential customers ",1]
["IDResidentialBehavioralPer Customer Summer Peak Reduction (%)","ID","Residential","Behavioral","Per Customer Summer Peak Reduction (%)","% of Peak",0.02,"Opower documentation for BDR with Consumers and DTE",1]
["IDResidentialBehavioralPer Customer Winter Peak Reduction (kW)","ID","Residential","Behavioral","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Assume 50% of Summer impacts.",1]
["IDResidentialBehavioralPer Customer Winter Peak Reduction (%)","ID","Residential","Behavioral","Per Customer Winter Peak Reduction (%)","% of Peak",0.02,0,1]
["IDResidentialDLC Electric Vehicle ChargingEvent Non-Performance Rate","ID","Residential","DLC Electric Vehicle Charging","Event Non-Performance Rate","%",0,0,1]
["IDResidentialDLC Electric Vehicle ChargingPer Customer Summer Peak Reduction (kW)","ID","Residential","DLC Electric Vehicle Charging","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"Expecting 90% + load shift",1]
["IDResidentialDLC Electric Vehicle ChargingPer Customer Summer Peak Reduction (%)","ID","Residential","DLC Electric Vehicle Charging","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Electric Vehicle ChargingPer Customer Winter Peak Reduction (kW)","ID","Residential","DLC Electric Vehicle Charging","Per Customer Winter Peak Reduction (kW)","kW @meter",0.5,"Expecting 90% + load shift",1]
["IDResidentialDLC Electric Vehicle ChargingPer Customer Winter Peak Reduction (%)","ID","Residential","DLC Electric Vehicle Charging","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Central ACEvent Non-Performance Rate","ID","Residential","DLC Central AC","Event Non-Performance Rate","%",0,0,1]
["IDResidentialDLC Central ACPer Customer Summer Peak Reduction (kW)","ID","Residential","DLC Central AC","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"NWPC DLC Switch cooling assumption (east)",1]
["IDResidentialDLC Central ACPer Customer Summer Peak Reduction (%)","ID","Residential","DLC Central AC","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Central ACPer Customer Winter Peak Reduction (kW)","ID","Residential","DLC Central AC","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialDLC Central ACPer Customer Winter Peak Reduction (%)","ID","Residential","DLC Central AC","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Central ACEvent Non-Performance Rate","ID","General Service","DLC Central AC","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceDLC Central ACPer Customer Summer Peak Reduction (kW)","ID","General Service","DLC Central AC","Per Customer Summer Peak Reduction (kW)","kW @meter",1.25,"NWPC DLC Switch cooling assumption (east)",1]
["IDGeneral ServiceDLC Central ACPer Customer Summer Peak Reduction (%)","ID","General Service","DLC Central AC","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Central ACPer Customer Winter Peak Reduction (kW)","ID","General Service","DLC Central AC","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceDLC Central ACPer Customer Winter Peak Reduction (%)","ID","General Service","DLC Central AC","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Water HeatingEvent Non-Performance Rate","ID","Residential","DLC Water Heating","Event Non-Performance Rate","%",0,0,1]
["IDResidentialDLC Water HeatingPer Customer Summer Peak Reduction (kW)","ID","Residential","DLC Water Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDResidentialDLC Water HeatingPer Customer Summer Peak Reduction (%)","ID","Residential","DLC Water Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Water HeatingPer Customer Winter Peak Reduction (kW)","ID","Residential","DLC Water Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",0.5,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDResidentialDLC Water HeatingPer Customer Winter Peak Reduction (%)","ID","Residential","DLC Water Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Water HeatingEvent Non-Performance Rate","ID","General Service","DLC Water Heating","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceDLC Water HeatingPer Customer Summer Peak Reduction (kW)","ID","General Service","DLC Water Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",1.26,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDGeneral ServiceDLC Water HeatingPer Customer Summer Peak Reduction (%)","ID","General Service","DLC Water Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Water HeatingPer Customer Winter Peak Reduction (kW)","ID","General Service","DLC Water Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",1.26,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDGeneral ServiceDLC Water HeatingPer Customer Winter Peak Reduction (%)","ID","General Service","DLC Water Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialCTA-2045 WHEvent Non-Performance Rate","ID","Residential","CTA-2045 WH","Event Non-Performance Rate","%",0,"Ability for customers to easily override event- using 3% as placeholder",1]
["IDResidentialCTA-2045 WHPer Customer Summer Peak Reduction (kW)","ID","Residential","CTA-2045 WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["IDResidentialCTA-2045 WHPer Customer Summer Peak Reduction (%)","ID","Residential","CTA-2045 WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialCTA-2045 WHPer Customer Winter Peak Reduction (kW)","ID","Residential","CTA-2045 WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["IDResidentialCTA-2045 WHPer Customer Winter Peak Reduction (%)","ID","Residential","CTA-2045 WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Duke Energy produced PPT of pilot but no impacts",1]
["IDGeneral ServiceCTA-2045 WHEvent Non-Performance Rate","ID","General Service","CTA-2045 WH","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceCTA-2045 WHPer Customer Summer Peak Reduction (kW)","ID","General Service","CTA-2045 WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["IDGeneral ServiceCTA-2045 WHPer Customer Summer Peak Reduction (%)","ID","General Service","CTA-2045 WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceCTA-2045 WHPer Customer Winter Peak Reduction (kW)","ID","General Service","CTA-2045 WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["IDGeneral ServiceCTA-2045 WHPer Customer Winter Peak Reduction (%)","ID","General Service","CTA-2045 WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingEvent Non-Performance Rate","ID","Residential","DLC Smart Thermostats - Cooling","Event Non-Performance Rate","%",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (kW)","ID","Residential","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
["IDResidentialDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (%)","ID","Residential","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (kW)","ID","Residential","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (%)","ID","Residential","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingEvent Non-Performance Rate","ID","General Service","DLC Smart Thermostats - Cooling","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (kW)","ID","General Service","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",1.25,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
[{"$f":"B259&C259&D259&E259","v":"IDGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Summer Peak Reduction (%)"},"ID","General Service","DLC Smart Thermostats - Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (kW)","ID","General Service","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Winter Peak Reduction (%)","ID","General Service","DLC Smart Thermostats - Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Smart Thermostats - HeatingEvent Non-Performance Rate","ID","Residential","DLC Smart Thermostats - Heating","Event Non-Performance Rate","%",0,0,1]
["IDResidentialDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (kW)","ID","Residential","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (%)","ID","Residential","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (kW)","ID","Residential","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",1.0900000000000001,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["IDResidentialDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (%)","ID","Residential","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingEvent Non-Performance Rate","ID","General Service","DLC Smart Thermostats - Heating","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (kW)","ID","General Service","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Summer Peak Reduction (%)","ID","General Service","DLC Smart Thermostats - Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (kW)","ID","General Service","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",1.35,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Winter Peak Reduction (%)","ID","General Service","DLC Smart Thermostats - Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Pacificorp Assumptions",1]
["IDResidentialDLC Smart AppliancesEvent Non-Performance Rate","ID","Residential","DLC Smart Appliances","Event Non-Performance Rate","%",0,0,1]
["IDResidentialDLC Smart AppliancesPer Customer Summer Peak Reduction (kW)","ID","Residential","DLC Smart Appliances","Per Customer Summer Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["IDResidentialDLC Smart AppliancesPer Customer Summer Peak Reduction (%)","ID","Residential","DLC Smart Appliances","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialDLC Smart AppliancesPer Customer Winter Peak Reduction (kW)","ID","Residential","DLC Smart Appliances","Per Customer Winter Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["IDResidentialDLC Smart AppliancesPer Customer Winter Peak Reduction (%)","ID","Residential","DLC Smart Appliances","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Smart AppliancesEvent Non-Performance Rate","ID","General Service","DLC Smart Appliances","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceDLC Smart AppliancesPer Customer Summer Peak Reduction (kW)","ID","General Service","DLC Smart Appliances","Per Customer Summer Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["IDGeneral ServiceDLC Smart AppliancesPer Customer Summer Peak Reduction (%)","ID","General Service","DLC Smart Appliances","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceDLC Smart AppliancesPer Customer Winter Peak Reduction (kW)","ID","General Service","DLC Smart Appliances","Per Customer Winter Peak Reduction (kW)","kW @meter",0.14000000000000001,"Ghatikar, Rish. Demand Response Automation in Appliance and Equipment. Lawrence Berkley National Laboratory, 2015. Web. http://docketpublic.energy.ca.gov/PublicDocuments/15-IEPR-05/TN205072_20150618T110004_Demand_Response_Automation_in_Appliances_and_Equipment.pptx kw @ meter values= 0.14 for summer and winter",1]
["IDGeneral ServiceDLC Smart AppliancesPer Customer Winter Peak Reduction (%)","ID","General Service","DLC Smart Appliances","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceThird Party ContractsEvent Non-Performance Rate","ID","General Service","Third Party Contracts","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceThird Party ContractsPer Customer Summer Peak Reduction (kW)","ID","General Service","Third Party Contracts","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceThird Party ContractsPer Customer Summer Peak Reduction (%)","ID","General Service","Third Party Contracts","Per Customer Summer Peak Reduction (%)","% of Peak",0.1,"Michigan Demand Response Market Assessment- Capacity Bidding",1]
["IDGeneral ServiceThird Party ContractsPer Customer Winter Peak Reduction (kW)","ID","General Service","Third Party Contracts","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceThird Party ContractsPer Customer Winter Peak Reduction (%)","ID","General Service","Third Party Contracts","Per Customer Winter Peak Reduction (%)","% of Peak",0.1,"Michigan Demand Response Market Assessment- Capacity Bidding",1]
["IDLarge General ServiceThird Party ContractsEvent Non-Performance Rate","ID","Large General Service","Third Party Contracts","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceThird Party ContractsPer Customer Summer Peak Reduction (kW)","ID","Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceThird Party ContractsPer Customer Summer Peak Reduction (%)","ID","Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["IDLarge General ServiceThird Party ContractsPer Customer Winter Peak Reduction (kW)","ID","Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceThird Party ContractsPer Customer Winter Peak Reduction (%)","ID","Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["IDExtra Large General ServiceThird Party ContractsEvent Non-Performance Rate","ID","Extra Large General Service","Third Party Contracts","Event Non-Performance Rate","%",0,0,1]
["IDExtra Large General ServiceThird Party ContractsPer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceThird Party ContractsPer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Third Party Contracts","Per Customer Summer Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["IDExtra Large General ServiceThird Party ContractsPer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceThird Party ContractsPer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Third Party Contracts","Per Customer Winter Peak Reduction (%)","% of Peak",0.21,"weighted average from impacts in the following report: Impact Estimates from Aggregator Programs in California (Source: 2012 Statewide Load Impact Evaluation of California Aggregator Demand Response Programs Volume 1: Ex post and Ex ante Load Impacts; Christensen Associates Energy Consulting; April 1, 2013).",1]
["IDResidentialTime-of-Use Opt-inEvent Non-Performance Rate","ID","Residential","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,"None - should be in eval'd number.",1]
["IDResidentialTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","ID","Residential","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","ID","Residential","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",5.7000000000000002E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDResidentialTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","ID","Residential","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","ID","Residential","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",2.8500000000000001E-2,"Assume 50% of Summer impacts. Brattle Analysis and Estimate - Negative impacts in Winter set to zero in Eastern states.",1]
["IDGeneral ServiceTime-of-Use Opt-inEvent Non-Performance Rate","ID","General Service","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","ID","General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","ID","General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",2E-3,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDGeneral ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","ID","General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","ID","General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",1E-3,"Assume 50% of Summer impacts.",1]
["IDLarge General ServiceTime-of-Use Opt-inEvent Non-Performance Rate","ID","Large General Service","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","ID","Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","ID","Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",2.5999999999999999E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDLarge General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","ID","Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","ID","Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",1.2999999999999999E-2,"Assume 50% of Summer impacts.",1]
["IDExtra Large General ServiceTime-of-Use Opt-inEvent Non-Performance Rate","ID","Extra Large General Service","Time-of-Use Opt-in","Event Non-Performance Rate","%",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inPer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Time-of-Use Opt-in","Per Customer Summer Peak Reduction (%)","% of Peak",3.1E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDExtra Large General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inPer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Time-of-Use Opt-in","Per Customer Winter Peak Reduction (%)","% of Peak",1.55E-2,"Assume 50% of Summer impacts.",1]
["IDResidentialTime-of-Use Opt-outEvent Non-Performance Rate","ID","Residential","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,"None - should be in eval'd number.",1]
["IDResidentialTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)","ID","Residential","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","ID","Residential","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",3.4000000000000002E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDResidentialTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","ID","Residential","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","ID","Residential","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1.7000000000000001E-2,"Assume 50% of Summer impacts. Brattle Analysis and Estimate - Negative impacts in Winter set to zero in Eastern states.",1]
["IDGeneral ServiceTime-of-Use Opt-outEvent Non-Performance Rate","ID","General Service","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,0,1]
[{"$f":"B323&C323&D323&E323","v":"IDGeneral ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)"},"ID","General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","ID","General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",2E-3,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDGeneral ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","ID","General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","ID","General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1E-3,"Assume 50% of Summer impacts.",1]
["IDLarge General ServiceTime-of-Use Opt-outEvent Non-Performance Rate","ID","Large General Service","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)","ID","Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","ID","Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",2.5999999999999999E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDLarge General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","ID","Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","ID","Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1.2999999999999999E-2,"Assume 50% of Summer impacts.",1]
["IDExtra Large General ServiceTime-of-Use Opt-outEvent Non-Performance Rate","ID","Extra Large General Service","Time-of-Use Opt-out","Event Non-Performance Rate","%",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outPer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Time-of-Use Opt-out","Per Customer Summer Peak Reduction (%)","% of Peak",3.1E-2,"Brattle Analysis and Estimate - Pacificorp 2019 opt-in and opt-out scenarios",1]
["IDExtra Large General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outPer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Time-of-Use Opt-out","Per Customer Winter Peak Reduction (%)","% of Peak",1.55E-2,"Assume 50% of Summer impacts.",1]
["IDResidentialVariable Peak Pricing RatesEvent Non-Performance Rate","ID","Residential","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["IDResidentialVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","ID","Residential","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","ID","Residential","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.1,"OG&E 2017 Smart Hours Study - Res 10% impacts for VPP only",1]
["IDResidentialVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","ID","Residential","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)","ID","Residential","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",7.5000000000000011E-2,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesEvent Non-Performance Rate","ID","General Service","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","ID","General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","ID","General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.04,"OG&E 2017 Smart Hours Study - 4% for an average CPE day for VPP only customers without a smart thermostat",1]
["IDGeneral ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","ID","General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)","ID","General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",0.03,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesEvent Non-Performance Rate","ID","Large General Service","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","ID","Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","ID","Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.04,"OG&E 2017 Smart Hours Study - 4% for an average CPE day for VPP only customers without a smart thermostat",1]
["IDLarge General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","ID","Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)","ID","Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",0.03,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesEvent Non-Performance Rate","ID","Extra Large General Service","Variable Peak Pricing Rates","Event Non-Performance Rate","%",0,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesPer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Summer Peak Reduction (%)","% of Peak",0.04,"OG&E 2017 Smart Hours Study - 4% for an average CPE day for VPP only customers without a smart thermostat",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesPer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Winter Peak Reduction (%)","% of Peak",0.03,0,1]
["IDLarge General ServiceReal Time PricingEvent Non-Performance Rate","ID","Large General Service","Real Time Pricing","Event Non-Performance Rate","%","","",1]
["IDLarge General ServiceReal Time PricingPer Customer Summer Peak Reduction (kW)","ID","Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["IDLarge General ServiceReal Time PricingPer Customer Summer Peak Reduction (%)","ID","Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
["IDLarge General ServiceReal Time PricingPer Customer Winter Peak Reduction (kW)","ID","Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["IDLarge General ServiceReal Time PricingPer Customer Winter Peak Reduction (%)","ID","Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["IDExtra Large General ServiceReal Time PricingEvent Non-Performance Rate","ID","Extra Large General Service","Real Time Pricing","Event Non-Performance Rate","%","","",1]
["IDExtra Large General ServiceReal Time PricingPer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (kW)","kW @meter","","",1]
["IDExtra Large General ServiceReal Time PricingPer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Real Time Pricing","Per Customer Summer Peak Reduction (%)","% of Peak","","",1]
["IDExtra Large General ServiceReal Time PricingPer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (kW)","kW @meter","","",1]
["IDExtra Large General ServiceReal Time PricingPer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Real Time Pricing","Per Customer Winter Peak Reduction (%)","% of Peak","","",1]
["IDGeneral ServiceThermal Energy StorageEvent Non-Performance Rate","ID","General Service","Thermal Energy Storage","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceThermal Energy StoragePer Customer Summer Peak Reduction (kW)","ID","General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",1.68,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["IDGeneral ServiceThermal Energy StoragePer Customer Summer Peak Reduction (%)","ID","General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceThermal Energy StoragePer Customer Winter Peak Reduction (kW)","ID","General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Removed Winter Impacts",1]
["IDGeneral ServiceThermal Energy StoragePer Customer Winter Peak Reduction (%)","ID","General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDLarge General ServiceThermal Energy StorageEvent Non-Performance Rate","ID","Large General Service","Thermal Energy Storage","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (kW)","ID","Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",8.4,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["IDLarge General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (%)","ID","Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDLarge General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (kW)","ID","Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["IDLarge General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (%)","ID","Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDExtra Large General ServiceThermal Energy StorageEvent Non-Performance Rate","ID","Extra Large General Service","Thermal Energy Storage","Event Non-Performance Rate","%",0,0,1]
["IDExtra Large General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",8.4,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["IDExtra Large General ServiceThermal Energy StoragePer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Thermal Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDExtra Large General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"Ice Energy - Ice Bear Tech Specifications, https://www.ice-energy.com/wp-content/uploads/2016/03/ICE-BEAR-30-Product-Sheet.pdf",1]
["IDExtra Large General ServiceThermal Energy StoragePer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Thermal Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialBattery Energy StorageEvent Non-Performance Rate","ID","Residential","Battery Energy Storage","Event Non-Performance Rate","%",0,0,1]
["IDResidentialBattery Energy StoragePer Customer Summer Peak Reduction (kW)","ID","Residential","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDResidentialBattery Energy StoragePer Customer Summer Peak Reduction (%)","ID","Residential","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialBattery Energy StoragePer Customer Winter Peak Reduction (kW)","ID","Residential","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDResidentialBattery Energy StoragePer Customer Winter Peak Reduction (%)","ID","Residential","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
[{"$f":"B387&C387&D387&E387","v":"IDGeneral ServiceBattery Energy StorageEvent Non-Performance Rate"},"ID","General Service","Battery Energy Storage","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceBattery Energy StoragePer Customer Summer Peak Reduction (kW)","ID","General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDGeneral ServiceBattery Energy StoragePer Customer Summer Peak Reduction (%)","ID","General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceBattery Energy StoragePer Customer Winter Peak Reduction (kW)","ID","General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDGeneral ServiceBattery Energy StoragePer Customer Winter Peak Reduction (%)","ID","General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDLarge General ServiceBattery Energy StorageEvent Non-Performance Rate","ID","Large General Service","Battery Energy Storage","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (kW)","ID","Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["IDLarge General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (%)","ID","Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDLarge General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (kW)","ID","Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["IDLarge General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (%)","ID","Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDExtra Large General ServiceBattery Energy StorageEvent Non-Performance Rate","ID","Extra Large General Service","Battery Energy Storage","Event Non-Performance Rate","%",0,"Pacificorp: ",1]
["IDExtra Large General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Calculated",1]
["IDExtra Large General ServiceBattery Energy StoragePer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Battery Energy Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,"MISO Res LoadMAP DSM Programs.xlsx (LRZ7) ",1]
["IDExtra Large General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"None",1]
["IDExtra Large General ServiceBattery Energy StoragePer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Battery Energy Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,"None",1]
["IDResidentialAncillary CoolingEvent Non-Performance Rate","ID","Residential","Ancillary Cooling","Event Non-Performance Rate","%",0,0,1]
["IDResidentialAncillary CoolingPer Customer Summer Peak Reduction (kW)","ID","Residential","Ancillary Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",0.25,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
["IDResidentialAncillary CoolingPer Customer Summer Peak Reduction (%)","ID","Residential","Ancillary Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary CoolingPer Customer Winter Peak Reduction (kW)","ID","Residential","Ancillary Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialAncillary CoolingPer Customer Winter Peak Reduction (%)","ID","Residential","Ancillary Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary CoolingEvent Non-Performance Rate","ID","General Service","Ancillary Cooling","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceAncillary CoolingPer Customer Summer Peak Reduction (kW)","ID","General Service","Ancillary Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",0.625,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
["IDGeneral ServiceAncillary CoolingPer Customer Summer Peak Reduction (%)","ID","General Service","Ancillary Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary CoolingPer Customer Winter Peak Reduction (kW)","ID","General Service","Ancillary Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceAncillary CoolingPer Customer Winter Peak Reduction (%)","ID","General Service","Ancillary Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary HeatingEvent Non-Performance Rate","ID","Residential","Ancillary Heating","Event Non-Performance Rate","%",0,0,1]
["IDResidentialAncillary HeatingPer Customer Summer Peak Reduction (kW)","ID","Residential","Ancillary Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDResidentialAncillary HeatingPer Customer Summer Peak Reduction (%)","ID","Residential","Ancillary Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary HeatingPer Customer Winter Peak Reduction (kW)","ID","Residential","Ancillary Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",0.54500000000000004,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["IDResidentialAncillary HeatingPer Customer Winter Peak Reduction (%)","ID","Residential","Ancillary Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary HeatingEvent Non-Performance Rate","ID","General Service","Ancillary Heating","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceAncillary HeatingPer Customer Summer Peak Reduction (kW)","ID","General Service","Ancillary Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceAncillary HeatingPer Customer Summer Peak Reduction (%)","ID","General Service","Ancillary Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary HeatingPer Customer Winter Peak Reduction (kW)","ID","General Service","Ancillary Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",0.67500000000000004,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["IDGeneral ServiceAncillary HeatingPer Customer Winter Peak Reduction (%)","ID","General Service","Ancillary Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Pacificorp Assumptions",1]
["IDResidentialAncillary WHEvent Non-Performance Rate","ID","Residential","Ancillary WH","Event Non-Performance Rate","%",0,"Ability for customers to easily override event- using 3% as placeholder",1]
["IDResidentialAncillary WHPer Customer Summer Peak Reduction (kW)","ID","Residential","Ancillary WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["IDResidentialAncillary WHPer Customer Summer Peak Reduction (%)","ID","Residential","Ancillary WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary WHPer Customer Winter Peak Reduction (kW)","ID","Residential","Ancillary WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["IDResidentialAncillary WHPer Customer Winter Peak Reduction (%)","ID","Residential","Ancillary WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Duke Energy produced PPT of pilot but no impacts",1]
["IDGeneral ServiceAncillary WHEvent Non-Performance Rate","ID","General Service","Ancillary WH","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceAncillary WHPer Customer Summer Peak Reduction (kW)","ID","General Service","Ancillary WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["IDGeneral ServiceAncillary WHPer Customer Summer Peak Reduction (%)","ID","General Service","Ancillary WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary WHPer Customer Winter Peak Reduction (kW)","ID","General Service","Ancillary WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["IDGeneral ServiceAncillary WHPer Customer Winter Peak Reduction (%)","ID","General Service","Ancillary WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary DLC WHEvent Non-Performance Rate","ID","Residential","Ancillary DLC WH","Event Non-Performance Rate","%",0,0,1]
["IDResidentialAncillary DLC WHPer Customer Summer Peak Reduction (kW)","ID","Residential","Ancillary DLC WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDResidentialAncillary DLC WHPer Customer Summer Peak Reduction (%)","ID","Residential","Ancillary DLC WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary DLC WHPer Customer Winter Peak Reduction (kW)","ID","Residential","Ancillary DLC WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0.5,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDResidentialAncillary DLC WHPer Customer Winter Peak Reduction (%)","ID","Residential","Ancillary DLC WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary DLC WHEvent Non-Performance Rate","ID","General Service","Ancillary DLC WH","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceAncillary DLC WHPer Customer Summer Peak Reduction (kW)","ID","General Service","Ancillary DLC WH","Per Customer Summer Peak Reduction (kW)","kW @meter",1.26,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDGeneral ServiceAncillary DLC WHPer Customer Summer Peak Reduction (%)","ID","General Service","Ancillary DLC WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary DLC WHPer Customer Winter Peak Reduction (kW)","ID","General Service","Ancillary DLC WH","Per Customer Winter Peak Reduction (kW)","kW @meter",1.26,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["IDGeneral ServiceAncillary DLC WHPer Customer Winter Peak Reduction (%)","ID","General Service","Ancillary DLC WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary EVEvent Non-Performance Rate","ID","Residential","Ancillary EV","Event Non-Performance Rate","%",0,0,1]
["IDResidentialAncillary EVPer Customer Summer Peak Reduction (kW)","ID","Residential","Ancillary EV","Per Customer Summer Peak Reduction (kW)","kW @meter",0.25,"Expecting 90% + load shift",1]
["IDResidentialAncillary EVPer Customer Summer Peak Reduction (%)","ID","Residential","Ancillary EV","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary EVPer Customer Winter Peak Reduction (kW)","ID","Residential","Ancillary EV","Per Customer Winter Peak Reduction (kW)","kW @meter",0.25,"Expecting 90% + load shift",1]
["IDResidentialAncillary EVPer Customer Winter Peak Reduction (%)","ID","Residential","Ancillary EV","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary Third PartyEvent Non-Performance Rate","ID","General Service","Ancillary Third Party","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceAncillary Third PartyPer Customer Summer Peak Reduction (kW)","ID","General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDGeneral ServiceAncillary Third PartyPer Customer Summer Peak Reduction (%)","ID","General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (%)","% of Peak",7.4999999999999997E-2,"75% of impact for ancillary",1]
["IDGeneral ServiceAncillary Third PartyPer Customer Winter Peak Reduction (kW)","ID","General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
[{"$f":"B451&C451&D451&E451","v":"IDGeneral ServiceAncillary Third PartyPer Customer Winter Peak Reduction (%)"},"ID","General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (%)","% of Peak",7.4999999999999997E-2,"75% of impact for ancillary",1]
["IDLarge General ServiceAncillary Third PartyEvent Non-Performance Rate","ID","Large General Service","Ancillary Third Party","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (kW)","ID","Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (%)","ID","Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["IDLarge General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (kW)","ID","Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDLarge General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (%)","ID","Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["IDExtra Large General ServiceAncillary Third PartyEvent Non-Performance Rate","ID","Extra Large General Service","Ancillary Third Party","Event Non-Performance Rate","%",0,0,1]
["IDExtra Large General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["IDExtra Large General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["IDExtra Large General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["IDResidentialAncillary Battery StorageEvent Non-Performance Rate","ID","Residential","Ancillary Battery Storage","Event Non-Performance Rate","%",0,0,1]
["IDResidentialAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","ID","Residential","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDResidentialAncillary Battery StoragePer Customer Summer Peak Reduction (%)","ID","Residential","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDResidentialAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","ID","Residential","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDResidentialAncillary Battery StoragePer Customer Winter Peak Reduction (%)","ID","Residential","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary Battery StorageEvent Non-Performance Rate","ID","General Service","Ancillary Battery Storage","Event Non-Performance Rate","%",0,0,1]
["IDGeneral ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","ID","General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDGeneral ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (%)","ID","General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDGeneral ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","ID","General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["IDGeneral ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (%)","ID","General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDLarge General ServiceAncillary Battery StorageEvent Non-Performance Rate","ID","Large General Service","Ancillary Battery Storage","Event Non-Performance Rate","%",0,0,1]
["IDLarge General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","ID","Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["IDLarge General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (%)","ID","Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["IDLarge General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","ID","Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["IDLarge General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (%)","ID","Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["IDExtra Large General ServiceAncillary Battery StorageEvent Non-Performance Rate","ID","Extra Large General Service","Ancillary Battery Storage","Event Non-Performance Rate","%",0,"Pacificorp: ",1]
["IDExtra Large General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","ID","Extra Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Calculated",1]
["IDExtra Large General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (%)","ID","Extra Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,"MISO Res LoadMAP DSM Programs.xlsx (LRZ7) ",1]
["IDExtra Large General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","ID","Extra Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"None",1]
["IDExtra Large General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (%)","ID","Extra Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,"None",1]
["WAResidentialAncillary CoolingEvent Non-Performance Rate","WA","Residential","Ancillary Cooling","Event Non-Performance Rate","%",0,0,1]
["WAResidentialAncillary CoolingPer Customer Summer Peak Reduction (kW)","WA","Residential","Ancillary Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",0.25,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
["WAResidentialAncillary CoolingPer Customer Summer Peak Reduction (%)","WA","Residential","Ancillary Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary CoolingPer Customer Winter Peak Reduction (kW)","WA","Residential","Ancillary Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialAncillary CoolingPer Customer Winter Peak Reduction (%)","WA","Residential","Ancillary Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary CoolingEvent Non-Performance Rate","WA","General Service","Ancillary Cooling","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceAncillary CoolingPer Customer Summer Peak Reduction (kW)","WA","General Service","Ancillary Cooling","Per Customer Summer Peak Reduction (kW)","kW @meter",0.625,"NWPC DLC Switch cooling assumption (east)- Thermostat impact was 1.27 kW but didn't seem right so we defaulted to DLC Central AC",1]
["WAGeneral ServiceAncillary CoolingPer Customer Summer Peak Reduction (%)","WA","General Service","Ancillary Cooling","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary CoolingPer Customer Winter Peak Reduction (kW)","WA","General Service","Ancillary Cooling","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceAncillary CoolingPer Customer Winter Peak Reduction (%)","WA","General Service","Ancillary Cooling","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary HeatingEvent Non-Performance Rate","WA","Residential","Ancillary Heating","Event Non-Performance Rate","%",0,0,1]
["WAResidentialAncillary HeatingPer Customer Summer Peak Reduction (kW)","WA","Residential","Ancillary Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAResidentialAncillary HeatingPer Customer Summer Peak Reduction (%)","WA","Residential","Ancillary Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary HeatingPer Customer Winter Peak Reduction (kW)","WA","Residential","Ancillary Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",0.54500000000000004,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["WAResidentialAncillary HeatingPer Customer Winter Peak Reduction (%)","WA","Residential","Ancillary Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary HeatingEvent Non-Performance Rate","WA","General Service","Ancillary Heating","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceAncillary HeatingPer Customer Summer Peak Reduction (kW)","WA","General Service","Ancillary Heating","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceAncillary HeatingPer Customer Summer Peak Reduction (%)","WA","General Service","Ancillary Heating","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary HeatingPer Customer Winter Peak Reduction (kW)","WA","General Service","Ancillary Heating","Per Customer Winter Peak Reduction (kW)","kW @meter",0.67500000000000004,"NWPC Smart thermostat heating assumption- general service uses 0.54 (switch to thermostat impact ratio) of eastern switch impact",1]
["WAGeneral ServiceAncillary HeatingPer Customer Winter Peak Reduction (%)","WA","General Service","Ancillary Heating","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Pacificorp Assumptions",1]
["WAResidentialAncillary WHEvent Non-Performance Rate","WA","Residential","Ancillary WH","Event Non-Performance Rate","%",0.03,"Ability for customers to easily override event- using 3% as placeholder",1]
["WAResidentialAncillary WHPer Customer Summer Peak Reduction (kW)","WA","Residential","Ancillary WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["WAResidentialAncillary WHPer Customer Summer Peak Reduction (%)","WA","Residential","Ancillary WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary WHPer Customer Winter Peak Reduction (kW)","WA","Residential","Ancillary WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0.5,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact",1]
["WAResidentialAncillary WHPer Customer Winter Peak Reduction (%)","WA","Residential","Ancillary WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,"Duke Energy produced PPT of pilot but no impacts",1]
["WAGeneral ServiceAncillary WHEvent Non-Performance Rate","WA","General Service","Ancillary WH","Event Non-Performance Rate","%",0.03,0,1]
["WAGeneral ServiceAncillary WHPer Customer Summer Peak Reduction (kW)","WA","General Service","Ancillary WH","Per Customer Summer Peak Reduction (kW)","kW @meter",1.26,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["WAGeneral ServiceAncillary WHPer Customer Summer Peak Reduction (%)","WA","General Service","Ancillary WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary WHPer Customer Winter Peak Reduction (kW)","WA","General Service","Ancillary WH","Per Customer Winter Peak Reduction (kW)","kW @meter",1.26,"NWPC Electric Resistance Grid-Ready Summer/Winter Impact- General service used 2.56x of res",1]
["WAGeneral ServiceAncillary WHPer Customer Winter Peak Reduction (%)","WA","General Service","Ancillary WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary DLC WHEvent Non-Performance Rate","WA","Residential","Ancillary DLC WH","Event Non-Performance Rate","%",0,0,1]
["WAResidentialAncillary DLC WHPer Customer Summer Peak Reduction (kW)","WA","Residential","Ancillary DLC WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAResidentialAncillary DLC WHPer Customer Summer Peak Reduction (%)","WA","Residential","Ancillary DLC WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
[{"$f":"B515&C515&D515&E515","v":"WAResidentialAncillary DLC WHPer Customer Winter Peak Reduction (kW)"},"WA","Residential","Ancillary DLC WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAResidentialAncillary DLC WHPer Customer Winter Peak Reduction (%)","WA","Residential","Ancillary DLC WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary DLC WHEvent Non-Performance Rate","WA","General Service","Ancillary DLC WH","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceAncillary DLC WHPer Customer Summer Peak Reduction (kW)","WA","General Service","Ancillary DLC WH","Per Customer Summer Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAGeneral ServiceAncillary DLC WHPer Customer Summer Peak Reduction (%)","WA","General Service","Ancillary DLC WH","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary DLC WHPer Customer Winter Peak Reduction (kW)","WA","General Service","Ancillary DLC WH","Per Customer Winter Peak Reduction (kW)","kW @meter",0,"7th Plan, pg 25 from Cadmnus Report, Commercial: Res value multiplied by the CAC DLC ratio  (small C&I impact /Res impact)",1]
["WAGeneral ServiceAncillary DLC WHPer Customer Winter Peak Reduction (%)","WA","General Service","Ancillary DLC WH","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary EVEvent Non-Performance Rate","WA","Residential","Ancillary EV","Event Non-Performance Rate","%",0,0,1]
["WAResidentialAncillary EVPer Customer Summer Peak Reduction (kW)","WA","Residential","Ancillary EV","Per Customer Summer Peak Reduction (kW)","kW @meter",0.25,"Expecting 90% + load shift",1]
["WAResidentialAncillary EVPer Customer Summer Peak Reduction (%)","WA","Residential","Ancillary EV","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary EVPer Customer Winter Peak Reduction (kW)","WA","Residential","Ancillary EV","Per Customer Winter Peak Reduction (kW)","kW @meter",0.25,"Expecting 90% + load shift",1]
["WAResidentialAncillary EVPer Customer Winter Peak Reduction (%)","WA","Residential","Ancillary EV","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary Third PartyEvent Non-Performance Rate","WA","General Service","Ancillary Third Party","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceAncillary Third PartyPer Customer Summer Peak Reduction (kW)","WA","General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceAncillary Third PartyPer Customer Summer Peak Reduction (%)","WA","General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (%)","% of Peak",7.4999999999999997E-2,"75% of impact for ancillary",1]
["WAGeneral ServiceAncillary Third PartyPer Customer Winter Peak Reduction (kW)","WA","General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAGeneral ServiceAncillary Third PartyPer Customer Winter Peak Reduction (%)","WA","General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (%)","% of Peak",7.4999999999999997E-2,"75% of impact for ancillary",1]
["WALarge General ServiceAncillary Third PartyEvent Non-Performance Rate","WA","Large General Service","Ancillary Third Party","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (kW)","WA","Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (%)","WA","Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["WALarge General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (kW)","WA","Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WALarge General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (%)","WA","Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["WAExtra Large General ServiceAncillary Third PartyEvent Non-Performance Rate","WA","Extra Large General Service","Ancillary Third Party","Event Non-Performance Rate","%",0,0,1]
["WAExtra Large General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceAncillary Third PartyPer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Ancillary Third Party","Per Customer Summer Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["WAExtra Large General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (kW)","kW @meter",0,0,1]
["WAExtra Large General ServiceAncillary Third PartyPer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Ancillary Third Party","Per Customer Winter Peak Reduction (%)","% of Peak",0.1575,"75% of impact for ancillary",1]
["WAResidentialAncillary Battery StorageEvent Non-Performance Rate","WA","Residential","Ancillary Battery Storage","Event Non-Performance Rate","%",0,0,1]
["WAResidentialAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","WA","Residential","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAResidentialAncillary Battery StoragePer Customer Summer Peak Reduction (%)","WA","Residential","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAResidentialAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","WA","Residential","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAResidentialAncillary Battery StoragePer Customer Winter Peak Reduction (%)","WA","Residential","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary Battery StorageEvent Non-Performance Rate","WA","General Service","Ancillary Battery Storage","Event Non-Performance Rate","%",0,0,1]
["WAGeneral ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","WA","General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAGeneral ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (%)","WA","General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WAGeneral ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","WA","General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",2,"Typical battery size for segment",1]
["WAGeneral ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (%)","WA","General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WALarge General ServiceAncillary Battery StorageEvent Non-Performance Rate","WA","Large General Service","Ancillary Battery Storage","Event Non-Performance Rate","%",0,0,1]
["WALarge General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","WA","Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["WALarge General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (%)","WA","Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,0,1]
["WALarge General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","WA","Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"Typical battery size for segment",1]
["WALarge General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (%)","WA","Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,0,1]
["WAExtra Large General ServiceAncillary Battery StorageEvent Non-Performance Rate","WA","Extra Large General Service","Ancillary Battery Storage","Event Non-Performance Rate","%",0,"Pacificorp: ",1]
["WAExtra Large General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (kW)","WA","Extra Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (kW)","kW @meter",15,"Calculated",1]
["WAExtra Large General ServiceAncillary Battery StoragePer Customer Summer Peak Reduction (%)","WA","Extra Large General Service","Ancillary Battery Storage","Per Customer Summer Peak Reduction (%)","% of Peak",0,"MISO Res LoadMAP DSM Programs.xlsx (LRZ7) ",1]
["WAExtra Large General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (kW)","WA","Extra Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (kW)","kW @meter",15,"None",1]
["WAExtra Large General ServiceAncillary Battery StoragePer Customer Winter Peak Reduction (%)","WA","Extra Large General Service","Ancillary Battery Storage","Per Customer Winter Peak Reduction (%)","% of Peak",0,"None",1]

{"sheet":"CEInput","index":6,"n_rows":1581,"n_cols":9,"rows_kept":1581,"cut":false,"hidden":false,"merged":[]}
["Key","State","Customer Class","Option","Data Element","Unit","Market Potential","Comments from Input Generator"]
[{"$f":"B2&C2&D2&E2","v":"WAResidentialBehavioralSummer DR Event Hours"},"WA","Residential","Behavioral","Summer DR Event Hours","hours/year",40,"8 hour event window x 5 events, Consumers Energy 7am-8pm 8 hr window",1]
["WAResidentialBehavioralWinter DR Event Hours","WA","Residential","Behavioral","Winter DR Event Hours","hours/year",40,"8 hour event window x 5 events, Consumers Energy 7am-8pm 8 hr window",1]
["WAResidentialBehavioralAnnual O&M Cost","WA","Residential","Behavioral","Annual O&M Cost","$/participant/year",3.25,"Oracle interview on 8/30, estimation of admin cost per household - KM heard 3 - 3.5 all inclusive- Implementation Cost",1]
["WAResidentialBehavioralAnnual Program Administration Cost","WA","Residential","Behavioral","Annual Program Administration Cost","$/yr",39633.409935479009,0,1]
["WAResidentialBehavioralCost of Equip + Install","WA","Residential","Behavioral","Cost of Equip + Install","$/tech",0,0,1]
["WAResidentialBehavioralCost of Equip + Install (per kW basis)","WA","Residential","Behavioral","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialBehavioralDe-rate","WA","Residential","Behavioral","De-rate","capacity equivalence factor",1,"Impact Reduced to reflect diminished savings program pulls in participants who are not \"high\" users",1]
["WAResidentialBehavioralNet to Gross Ratio (free ridership)","WA","Residential","Behavioral","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialBehavioralPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Behavioral","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,0,1]
["WAResidentialBehavioralPer Participant Annual Incentive","WA","Residential","Behavioral","Per Participant Annual Incentive","$/participant/year",0,"No Incentive for Behavioral DR - Brattle  PGE Potential Study 2016 - ",1]
["WAResidentialBehavioralPer kW Annual Incentive","WA","Residential","Behavioral","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialBehavioralProgram Development Cost","WA","Residential","Behavioral","Program Development Cost","$/program",66055.683225798348,0,1]
["WAResidentialBehavioralProgram Life","WA","Residential","Behavioral","Program Life","years",1,"MISO Res LoadMAP DSM Programs.xlsx (LRZ7) - Lifetime",1]
["WAResidentialBehavioralProgram Start Year","WA","Residential","Behavioral","Program Start Year","year",2022,0,1]
["WAResidentialDLC Electric Vehicle ChargingSummer DR Event Hours","WA","Residential","DLC Electric Vehicle Charging","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["WAResidentialDLC Electric Vehicle ChargingWinter DR Event Hours","WA","Residential","DLC Electric Vehicle Charging","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["WAResidentialDLC Electric Vehicle ChargingAnnual O&M Cost","WA","Residential","DLC Electric Vehicle Charging","Annual O&M Cost","$/participant/year",5,"Average subscription fees for EE and DR program management",1]
["WAResidentialDLC Electric Vehicle ChargingAnnual Program Administration Cost","WA","Residential","DLC Electric Vehicle Charging","Annual Program Administration Cost","$/yr",58962.721128592144,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Electric Vehicle ChargingCost of Equip + Install","WA","Residential","DLC Electric Vehicle Charging","Cost of Equip + Install","$/tech",700,"ppt from Kurtis email 2-5 indicates utility incentives are ~$1200 for charging equipment. Research indicates this is approx cost of equipment. (see Dave email to VN 3-15)",1]
["WAResidentialDLC Electric Vehicle ChargingCost of Equip + Install (per kW basis)","WA","Residential","DLC Electric Vehicle Charging","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialDLC Electric Vehicle ChargingDe-rate","WA","Residential","DLC Electric Vehicle Charging","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialDLC Electric Vehicle ChargingNet to Gross Ratio (free ridership)","WA","Residential","DLC Electric Vehicle Charging","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialDLC Electric Vehicle ChargingPer Customer Annual Marketing/Recruitment Cost","WA","Residential","DLC Electric Vehicle Charging","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,"Assumption $50 for RAP C&I, MAP = RAPx1.2",1]
["WAResidentialDLC Electric Vehicle ChargingPer Participant Annual Incentive","WA","Residential","DLC Electric Vehicle Charging","Per Participant Annual Incentive","$/participant/year",0,"Avista would provide a rate based charger or give a rebate on it, with no further incentives",1]
["WAResidentialDLC Electric Vehicle ChargingPer kW Annual Incentive","WA","Residential","DLC Electric Vehicle Charging","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialDLC Electric Vehicle ChargingProgram Development Cost","WA","Residential","DLC Electric Vehicle Charging","Program Development Cost","$/program",49135.600940493452,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Electric Vehicle ChargingProgram Life","WA","Residential","DLC Electric Vehicle Charging","Program Life","years",8,0,1]
["WAResidentialDLC Electric Vehicle ChargingProgram Start Year","WA","Residential","DLC Electric Vehicle Charging","Program Start Year","year",2024,"Technology won’t be available for mass market till 2024",1]
["WAResidentialDLC Central ACSummer DR Event Hours","WA","Residential","DLC Central AC","Summer DR Event Hours","hours/year",50,"Current PC Cool Keeper program allows for max 100 hours of curtailment.  ",1]
["WAResidentialDLC Central ACWinter DR Event Hours","WA","Residential","DLC Central AC","Winter DR Event Hours","hours/year",0,0,1]
["WAResidentialDLC Central ACAnnual O&M Cost","WA","Residential","DLC Central AC","Annual O&M Cost","$/participant/year",13,"Assume 5% of equipment + install costs.",1]
["WAResidentialDLC Central ACAnnual Program Administration Cost","WA","Residential","DLC Central AC","Annual Program Administration Cost","$/yr",47453.015095025105,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Central ACCost of Equip + Install","WA","Residential","DLC Central AC","Cost of Equip + Install","$/tech",260,"$100 installation cost. Idaho Power at 10,000 quantity pays $160 per switch.  I believe Avista volumes would be the same or less per order, making the cost $160 or greater.",1]
["WAResidentialDLC Central ACCost of Equip + Install (per kW basis)","WA","Residential","DLC Central AC","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialDLC Central ACDe-rate","WA","Residential","DLC Central AC","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialDLC Central ACNet to Gross Ratio (free ridership)","WA","Residential","DLC Central AC","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialDLC Central ACPer Customer Annual Marketing/Recruitment Cost","WA","Residential","DLC Central AC","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["WAResidentialDLC Central ACPer Participant Annual Incentive","WA","Residential","DLC Central AC","Per Participant Annual Incentive","$/participant/year",20,"$20 is the incentive level per participating unit. No. of units per average participant is 1.059",1]
["WAResidentialDLC Central ACPer kW Annual Incentive","WA","Residential","DLC Central AC","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialDLC Central ACProgram Development Cost","WA","Residential","DLC Central AC","Program Development Cost","$/program",39544.179245854255,0,1]
["WAResidentialDLC Central ACProgram Life","WA","Residential","DLC Central AC","Program Life","years",8,0,1]
["WAResidentialDLC Central ACProgram Start Year","WA","Residential","DLC Central AC","Program Start Year","year",2022,0,1]
["WAGeneral ServiceDLC Central ACSummer DR Event Hours","WA","General Service","DLC Central AC","Summer DR Event Hours","hours/year",50,"Current PC Cool Keeper program allows for max 100 hours of curtailment.  ",1]
["WAGeneral ServiceDLC Central ACWinter DR Event Hours","WA","General Service","DLC Central AC","Winter DR Event Hours","hours/year",0,0,1]
["WAGeneral ServiceDLC Central ACAnnual O&M Cost","WA","General Service","DLC Central AC","Annual O&M Cost","$/participant/year",13,"Assume 5% of equipment + install costs.",1]
["WAGeneral ServiceDLC Central ACAnnual Program Administration Cost","WA","General Service","DLC Central AC","Annual Program Administration Cost","$/yr",9818.9532780170521,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceDLC Central ACCost of Equip + Install","WA","General Service","DLC Central AC","Cost of Equip + Install","$/tech",260,"$100 installation cost. Idaho Power at 10,000 quantity pays $160 per switch.  I believe Avista volumes would be the same or less per order, making the cost $160 or greater.",1]
["WAGeneral ServiceDLC Central ACCost of Equip + Install (per kW basis)","WA","General Service","DLC Central AC","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceDLC Central ACDe-rate","WA","General Service","DLC Central AC","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceDLC Central ACNet to Gross Ratio (free ridership)","WA","General Service","DLC Central AC","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceDLC Central ACPer Customer Annual Marketing/Recruitment Cost","WA","General Service","DLC Central AC","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"25% Higher than Residential",1]
["WAGeneral ServiceDLC Central ACPer Participant Annual Incentive","WA","General Service","DLC Central AC","Per Participant Annual Incentive","$/participant/year",38,"Assumed participants have less than 5.5 tons of AC unit. Incentive level provided by PacifiCorp.",1]
["WAGeneral ServiceDLC Central ACPer kW Annual Incentive","WA","General Service","DLC Central AC","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceDLC Central ACProgram Development Cost","WA","General Service","DLC Central AC","Program Development Cost","$/program",8182.4610650142104,0,1]
["WAGeneral ServiceDLC Central ACProgram Life","WA","General Service","DLC Central AC","Program Life","years",8,0,1]
["WAGeneral ServiceDLC Central ACProgram Start Year","WA","General Service","DLC Central AC","Program Start Year","year",2022,0,1]
["WAResidentialDLC Water HeatingSummer DR Event Hours","WA","Residential","DLC Water Heating","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["WAResidentialDLC Water HeatingWinter DR Event Hours","WA","Residential","DLC Water Heating","Winter DR Event Hours","hours/year",0,"Split 50 hrs summer, and 50 hrs winter",1]
["WAResidentialDLC Water HeatingAnnual O&M Cost","WA","Residential","DLC Water Heating","Annual O&M Cost","$/participant/year",0,"Assume 5% of equipment + install costs.",1]
["WAResidentialDLC Water HeatingAnnual Program Administration Cost","WA","Residential","DLC Water Heating","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Water HeatingCost of Equip + Install","WA","Residential","DLC Water Heating","Cost of Equip + Install","$/tech",0,"Assumed $160 cost for water heater switch (same as cooling switch cost), plus $200 installation cost. Cost of Permit and License is $100 for res and $125 for C&I",1]
["WAResidentialDLC Water HeatingCost of Equip + Install (per kW basis)","WA","Residential","DLC Water Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialDLC Water HeatingDe-rate","WA","Residential","DLC Water Heating","De-rate","capacity equivalence factor",0,0,1]
["WAResidentialDLC Water HeatingNet to Gross Ratio (free ridership)","WA","Residential","DLC Water Heating","Net to Gross Ratio (free ridership)","ratio",0,0,1]
[{"$f":"B66&C66&D66&E66","v":"WAResidentialDLC Water HeatingPer Customer Annual Marketing/Recruitment Cost"},"WA","Residential","DLC Water Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as DLC CAC",1]
["WAResidentialDLC Water HeatingPer Participant Annual Incentive","WA","Residential","DLC Water Heating","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["WAResidentialDLC Water HeatingPer kW Annual Incentive","WA","Residential","DLC Water Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialDLC Water HeatingProgram Development Cost","WA","Residential","DLC Water Heating","Program Development Cost","$/program",0,0,1]
["WAResidentialDLC Water HeatingProgram Life","WA","Residential","DLC Water Heating","Program Life","years",0,0,1]
["WAResidentialDLC Water HeatingProgram Start Year","WA","Residential","DLC Water Heating","Program Start Year","year",0,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["WAGeneral ServiceDLC Water HeatingSummer DR Event Hours","WA","General Service","DLC Water Heating","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["WAGeneral ServiceDLC Water HeatingWinter DR Event Hours","WA","General Service","DLC Water Heating","Winter DR Event Hours","hours/year",0,"Split 50 hrs summer, and 50 hrs winter",1]
["WAGeneral ServiceDLC Water HeatingAnnual O&M Cost","WA","General Service","DLC Water Heating","Annual O&M Cost","$/participant/year",0,"Assume 5% of equipment + install costs.",1]
["WAGeneral ServiceDLC Water HeatingAnnual Program Administration Cost","WA","General Service","DLC Water Heating","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceDLC Water HeatingCost of Equip + Install","WA","General Service","DLC Water Heating","Cost of Equip + Install","$/tech",0,"Assumed $160 cost for water heater switch (same as cooling switch cost), plus $200 installation cost. Cost of Permit and License is $100 for res and $125 for C&I",1]
["WAGeneral ServiceDLC Water HeatingCost of Equip + Install (per kW basis)","WA","General Service","DLC Water Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceDLC Water HeatingDe-rate","WA","General Service","DLC Water Heating","De-rate","capacity equivalence factor",0,0,1]
["WAGeneral ServiceDLC Water HeatingNet to Gross Ratio (free ridership)","WA","General Service","DLC Water Heating","Net to Gross Ratio (free ridership)","ratio",0,0,1]
["WAGeneral ServiceDLC Water HeatingPer Customer Annual Marketing/Recruitment Cost","WA","General Service","DLC Water Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as DLC CAC",1]
["WAGeneral ServiceDLC Water HeatingPer Participant Annual Incentive","WA","General Service","DLC Water Heating","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["WAGeneral ServiceDLC Water HeatingPer kW Annual Incentive","WA","General Service","DLC Water Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceDLC Water HeatingProgram Development Cost","WA","General Service","DLC Water Heating","Program Development Cost","$/program",0,"No startup costs; Framework already exists for current programs",1]
["WAGeneral ServiceDLC Water HeatingProgram Life","WA","General Service","DLC Water Heating","Program Life","years",0,0,1]
["WAGeneral ServiceDLC Water HeatingProgram Start Year","WA","General Service","DLC Water Heating","Program Start Year","year",0,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["WAResidentialCTA-2045 WHSummer DR Event Hours","WA","Residential","CTA-2045 WH","Summer DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAResidentialCTA-2045 WHWinter DR Event Hours","WA","Residential","CTA-2045 WH","Winter DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAResidentialCTA-2045 WHAnnual O&M Cost","WA","Residential","CTA-2045 WH","Annual O&M Cost","$/participant/year",0,0,1]
["WAResidentialCTA-2045 WHAnnual Program Administration Cost","WA","Residential","CTA-2045 WH","Annual Program Administration Cost","$/yr",81900,"Share of Cost as noted in table at right",1]
["WAResidentialCTA-2045 WHCost of Equip + Install","WA","Residential","CTA-2045 WH","Cost of Equip + Install","$/tech",170,"$150 for module and comms, 20% of customers will need help provisioning these (an additional $100 for these customers)- average customer will be $170",1]
["WAResidentialCTA-2045 WHCost of Equip + Install (per kW basis)","WA","Residential","CTA-2045 WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialCTA-2045 WHDe-rate","WA","Residential","CTA-2045 WH","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialCTA-2045 WHNet to Gross Ratio (free ridership)","WA","Residential","CTA-2045 WH","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialCTA-2045 WHPer Customer Annual Marketing/Recruitment Cost","WA","Residential","CTA-2045 WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Same as Smart Thermostats",1]
["WAResidentialCTA-2045 WHPer Participant Annual Incentive","WA","Residential","CTA-2045 WH","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["WAResidentialCTA-2045 WHPer kW Annual Incentive","WA","Residential","CTA-2045 WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialCTA-2045 WHProgram Development Cost","WA","Residential","CTA-2045 WH","Program Development Cost","$/program",68250,0,1]
["WAResidentialCTA-2045 WHProgram Life","WA","Residential","CTA-2045 WH","Program Life","years",8,0,1]
["WAResidentialCTA-2045 WHProgram Start Year","WA","Residential","CTA-2045 WH","Program Start Year","year",2022,0,1]
["WAGeneral ServiceCTA-2045 WHSummer DR Event Hours","WA","General Service","CTA-2045 WH","Summer DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAGeneral ServiceCTA-2045 WHWinter DR Event Hours","WA","General Service","CTA-2045 WH","Winter DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAGeneral ServiceCTA-2045 WHAnnual O&M Cost","WA","General Service","CTA-2045 WH","Annual O&M Cost","$/participant/year",0,0,1]
["WAGeneral ServiceCTA-2045 WHAnnual Program Administration Cost","WA","General Service","CTA-2045 WH","Annual Program Administration Cost","$/yr",8100,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceCTA-2045 WHCost of Equip + Install","WA","General Service","CTA-2045 WH","Cost of Equip + Install","$/tech",170,"$150 for module and comms, 20% of customers will need help provisioning these (an additional $100 install cost for these customers)- average customer will be $170",1]
["WAGeneral ServiceCTA-2045 WHCost of Equip + Install (per kW basis)","WA","General Service","CTA-2045 WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceCTA-2045 WHDe-rate","WA","General Service","CTA-2045 WH","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceCTA-2045 WHNet to Gross Ratio (free ridership)","WA","General Service","CTA-2045 WH","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceCTA-2045 WHPer Customer Annual Marketing/Recruitment Cost","WA","General Service","CTA-2045 WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Same as Smart Thermostats",1]
["WAGeneral ServiceCTA-2045 WHPer Participant Annual Incentive","WA","General Service","CTA-2045 WH","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["WAGeneral ServiceCTA-2045 WHPer kW Annual Incentive","WA","General Service","CTA-2045 WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceCTA-2045 WHProgram Development Cost","WA","General Service","CTA-2045 WH","Program Development Cost","$/program",6750,"No startup costs; Framework already exists for current programs",1]
["WAGeneral ServiceCTA-2045 WHProgram Life","WA","General Service","CTA-2045 WH","Program Life","years",8,0,1]
["WAGeneral ServiceCTA-2045 WHProgram Start Year","WA","General Service","CTA-2045 WH","Program Start Year","year",2022,0,1]
["WAResidentialDLC Smart Thermostats - CoolingSummer DR Event Hours","WA","Residential","DLC Smart Thermostats - Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAResidentialDLC Smart Thermostats - CoolingWinter DR Event Hours","WA","Residential","DLC Smart Thermostats - Cooling","Winter DR Event Hours","hours/year",0,0,1]
["WAResidentialDLC Smart Thermostats - CoolingAnnual O&M Cost","WA","Residential","DLC Smart Thermostats - Cooling","Annual O&M Cost","$/participant/year",44,"Pacificorp:Assume 5% of equipment+install costs",1]
["WAResidentialDLC Smart Thermostats - CoolingAnnual Program Administration Cost","WA","Residential","DLC Smart Thermostats - Cooling","Annual Program Administration Cost","$/yr",47453.015095025105,0,1]
["WAResidentialDLC Smart Thermostats - CoolingCost of Equip + Install","WA","Residential","DLC Smart Thermostats - Cooling","Cost of Equip + Install","$/tech",0,"BYOT",1]
["WAResidentialDLC Smart Thermostats - CoolingCost of Equip + Install (per kW basis)","WA","Residential","DLC Smart Thermostats - Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialDLC Smart Thermostats - CoolingDe-rate","WA","Residential","DLC Smart Thermostats - Cooling","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialDLC Smart Thermostats - CoolingNet to Gross Ratio (free ridership)","WA","Residential","DLC Smart Thermostats - Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialDLC Smart Thermostats - CoolingPer Customer Annual Marketing/Recruitment Cost","WA","Residential","DLC Smart Thermostats - Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["WAResidentialDLC Smart Thermostats - CoolingPer Participant Annual Incentive","WA","Residential","DLC Smart Thermostats - Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["WAResidentialDLC Smart Thermostats - CoolingPer kW Annual Incentive","WA","Residential","DLC Smart Thermostats - Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialDLC Smart Thermostats - CoolingProgram Development Cost","WA","Residential","DLC Smart Thermostats - Cooling","Program Development Cost","$/program",39544.179245854255,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Smart Thermostats - CoolingProgram Life","WA","Residential","DLC Smart Thermostats - Cooling","Program Life","years",10,0,1]
["WAResidentialDLC Smart Thermostats - CoolingProgram Start Year","WA","Residential","DLC Smart Thermostats - Cooling","Program Start Year","year",2022,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingSummer DR Event Hours","WA","General Service","DLC Smart Thermostats - Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingWinter DR Event Hours","WA","General Service","DLC Smart Thermostats - Cooling","Winter DR Event Hours","hours/year",0,0,1]
[{"$f":"B130&C130&D130&E130","v":"WAGeneral ServiceDLC Smart Thermostats - CoolingAnnual O&M Cost"},"WA","General Service","DLC Smart Thermostats - Cooling","Annual O&M Cost","$/participant/year",44,"Average subscription fees for EE and DR program management",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingAnnual Program Administration Cost","WA","General Service","DLC Smart Thermostats - Cooling","Annual Program Administration Cost","$/yr",9818.9532780170521,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingCost of Equip + Install","WA","General Service","DLC Smart Thermostats - Cooling","Cost of Equip + Install","$/tech",0,"Bring Your Own Thermostat program",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingCost of Equip + Install (per kW basis)","WA","General Service","DLC Smart Thermostats - Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingDe-rate","WA","General Service","DLC Smart Thermostats - Cooling","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingNet to Gross Ratio (free ridership)","WA","General Service","DLC Smart Thermostats - Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Annual Marketing/Recruitment Cost","WA","General Service","DLC Smart Thermostats - Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingPer Participant Annual Incentive","WA","General Service","DLC Smart Thermostats - Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingPer kW Annual Incentive","WA","General Service","DLC Smart Thermostats - Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingProgram Development Cost","WA","General Service","DLC Smart Thermostats - Cooling","Program Development Cost","$/program",8182.4610650142104,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingProgram Life","WA","General Service","DLC Smart Thermostats - Cooling","Program Life","years",10,0,1]
["WAGeneral ServiceDLC Smart Thermostats - CoolingProgram Start Year","WA","General Service","DLC Smart Thermostats - Cooling","Program Start Year","year",2022,0,1]
["WAResidentialDLC Smart Thermostats - HeatingSummer DR Event Hours","WA","Residential","DLC Smart Thermostats - Heating","Summer DR Event Hours","hours/year",0,0,1]
["WAResidentialDLC Smart Thermostats - HeatingWinter DR Event Hours","WA","Residential","DLC Smart Thermostats - Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAResidentialDLC Smart Thermostats - HeatingAnnual O&M Cost","WA","Residential","DLC Smart Thermostats - Heating","Annual O&M Cost","$/participant/year",44,"Pacificorp:Assume 5% of equipment+install costs",1]
["WAResidentialDLC Smart Thermostats - HeatingAnnual Program Administration Cost","WA","Residential","DLC Smart Thermostats - Heating","Annual Program Administration Cost","$/yr",49622.070954138835,0,1]
["WAResidentialDLC Smart Thermostats - HeatingCost of Equip + Install","WA","Residential","DLC Smart Thermostats - Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["WAResidentialDLC Smart Thermostats - HeatingCost of Equip + Install (per kW basis)","WA","Residential","DLC Smart Thermostats - Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialDLC Smart Thermostats - HeatingDe-rate","WA","Residential","DLC Smart Thermostats - Heating","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialDLC Smart Thermostats - HeatingNet to Gross Ratio (free ridership)","WA","Residential","DLC Smart Thermostats - Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialDLC Smart Thermostats - HeatingPer Customer Annual Marketing/Recruitment Cost","WA","Residential","DLC Smart Thermostats - Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["WAResidentialDLC Smart Thermostats - HeatingPer Participant Annual Incentive","WA","Residential","DLC Smart Thermostats - Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["WAResidentialDLC Smart Thermostats - HeatingPer kW Annual Incentive","WA","Residential","DLC Smart Thermostats - Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialDLC Smart Thermostats - HeatingProgram Development Cost","WA","Residential","DLC Smart Thermostats - Heating","Program Development Cost","$/program",41351.725795115701,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Smart Thermostats - HeatingProgram Life","WA","Residential","DLC Smart Thermostats - Heating","Program Life","years",10,0,1]
["WAResidentialDLC Smart Thermostats - HeatingProgram Start Year","WA","Residential","DLC Smart Thermostats - Heating","Program Start Year","year",2022,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingSummer DR Event Hours","WA","General Service","DLC Smart Thermostats - Heating","Summer DR Event Hours","hours/year",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingWinter DR Event Hours","WA","General Service","DLC Smart Thermostats - Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingAnnual O&M Cost","WA","General Service","DLC Smart Thermostats - Heating","Annual O&M Cost","$/participant/year",44,"Average subscription fees for EE and DR program management",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingAnnual Program Administration Cost","WA","General Service","DLC Smart Thermostats - Heating","Annual Program Administration Cost","$/yr",7889.4814253694949,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingCost of Equip + Install","WA","General Service","DLC Smart Thermostats - Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingCost of Equip + Install (per kW basis)","WA","General Service","DLC Smart Thermostats - Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingDe-rate","WA","General Service","DLC Smart Thermostats - Heating","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingNet to Gross Ratio (free ridership)","WA","General Service","DLC Smart Thermostats - Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Annual Marketing/Recruitment Cost","WA","General Service","DLC Smart Thermostats - Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingPer Participant Annual Incentive","WA","General Service","DLC Smart Thermostats - Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingPer kW Annual Incentive","WA","General Service","DLC Smart Thermostats - Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingProgram Development Cost","WA","General Service","DLC Smart Thermostats - Heating","Program Development Cost","$/program",6574.5678544745788,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingProgram Life","WA","General Service","DLC Smart Thermostats - Heating","Program Life","years",10,0,1]
["WAGeneral ServiceDLC Smart Thermostats - HeatingProgram Start Year","WA","General Service","DLC Smart Thermostats - Heating","Program Start Year","year",2022,0,1]
["WAResidentialDLC Smart AppliancesSummer DR Event Hours","WA","Residential","DLC Smart Appliances","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["WAResidentialDLC Smart AppliancesWinter DR Event Hours","WA","Residential","DLC Smart Appliances","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["WAResidentialDLC Smart AppliancesAnnual O&M Cost","WA","Residential","DLC Smart Appliances","Annual O&M Cost","$/participant/year",0,0,1]
["WAResidentialDLC Smart AppliancesAnnual Program Administration Cost","WA","Residential","DLC Smart Appliances","Annual Program Administration Cost","$/yr",52263.179834532872,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Smart AppliancesCost of Equip + Install","WA","Residential","DLC Smart Appliances","Cost of Equip + Install","$/tech",300,"Google research revealed devices range anywhere between $150 -400. Need wifi hub or some sort to connect devices. See email between Dave & Victoria 5-9-16",1]
["WAResidentialDLC Smart AppliancesCost of Equip + Install (per kW basis)","WA","Residential","DLC Smart Appliances","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialDLC Smart AppliancesDe-rate","WA","Residential","DLC Smart Appliances","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialDLC Smart AppliancesNet to Gross Ratio (free ridership)","WA","Residential","DLC Smart Appliances","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialDLC Smart AppliancesPer Customer Annual Marketing/Recruitment Cost","WA","Residential","DLC Smart Appliances","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
["WAResidentialDLC Smart AppliancesPer Participant Annual Incentive","WA","Residential","DLC Smart Appliances","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WAResidentialDLC Smart AppliancesPer kW Annual Incentive","WA","Residential","DLC Smart Appliances","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialDLC Smart AppliancesProgram Development Cost","WA","Residential","DLC Smart Appliances","Program Development Cost","$/program",43552.649862110731,"Share of Cost as noted in table at right",1]
["WAResidentialDLC Smart AppliancesProgram Life","WA","Residential","DLC Smart Appliances","Program Life","years",8,0,1]
["WAResidentialDLC Smart AppliancesProgram Start Year","WA","Residential","DLC Smart Appliances","Program Start Year","year",2022,0,1]
["WAGeneral ServiceDLC Smart AppliancesSummer DR Event Hours","WA","General Service","DLC Smart Appliances","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["WAGeneral ServiceDLC Smart AppliancesWinter DR Event Hours","WA","General Service","DLC Smart Appliances","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["WAGeneral ServiceDLC Smart AppliancesAnnual O&M Cost","WA","General Service","DLC Smart Appliances","Annual O&M Cost","$/participant/year",0,0,1]
["WAGeneral ServiceDLC Smart AppliancesAnnual Program Administration Cost","WA","General Service","DLC Smart Appliances","Annual Program Administration Cost","$/yr",5540.0973728168119,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceDLC Smart AppliancesCost of Equip + Install","WA","General Service","DLC Smart Appliances","Cost of Equip + Install","$/tech",300,"Google research revealed devices range anywhere between $150 -400. Need wifi hub or some sort to connect devices. See email between Dave & Victoria 5-9-16",1]
["WAGeneral ServiceDLC Smart AppliancesCost of Equip + Install (per kW basis)","WA","General Service","DLC Smart Appliances","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceDLC Smart AppliancesDe-rate","WA","General Service","DLC Smart Appliances","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceDLC Smart AppliancesNet to Gross Ratio (free ridership)","WA","General Service","DLC Smart Appliances","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceDLC Smart AppliancesPer Customer Annual Marketing/Recruitment Cost","WA","General Service","DLC Smart Appliances","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
["WAGeneral ServiceDLC Smart AppliancesPer Participant Annual Incentive","WA","General Service","DLC Smart Appliances","Per Participant Annual Incentive","$/participant/year",0,0,1]
[{"$f":"B194&C194&D194&E194","v":"WAGeneral ServiceDLC Smart AppliancesPer kW Annual Incentive"},"WA","General Service","DLC Smart Appliances","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceDLC Smart AppliancesProgram Development Cost","WA","General Service","DLC Smart Appliances","Program Development Cost","$/program",4616.7478106806766,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceDLC Smart AppliancesProgram Life","WA","General Service","DLC Smart Appliances","Program Life","years",8,0,1]
["WAGeneral ServiceDLC Smart AppliancesProgram Start Year","WA","General Service","DLC Smart Appliances","Program Start Year","year",2022,0,1]
["WAGeneral ServiceThird Party ContractsSummer DR Event Hours","WA","General Service","Third Party Contracts","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAGeneral ServiceThird Party ContractsWinter DR Event Hours","WA","General Service","Third Party Contracts","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAGeneral ServiceThird Party ContractsAnnual O&M Cost","WA","General Service","Third Party Contracts","Annual O&M Cost","$/participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["WAGeneral ServiceThird Party ContractsAnnual Program Administration Cost","WA","General Service","Third Party Contracts","Annual Program Administration Cost","$/yr",0,0,1]
["WAGeneral ServiceThird Party ContractsCost of Equip + Install","WA","General Service","Third Party Contracts","Cost of Equip + Install","$/tech",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["WAGeneral ServiceThird Party ContractsCost of Equip + Install (per kW basis)","WA","General Service","Third Party Contracts","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceThird Party ContractsDe-rate","WA","General Service","Third Party Contracts","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceThird Party ContractsNet to Gross Ratio (free ridership)","WA","General Service","Third Party Contracts","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceThird Party ContractsPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Third Party Contracts","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["WAGeneral ServiceThird Party ContractsPer Participant Annual Incentive","WA","General Service","Third Party Contracts","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WAGeneral ServiceThird Party ContractsPer kW Annual Incentive","WA","General Service","Third Party Contracts","Per kW Annual Incentive","$/kW @meter/year",0,"MPSC Demand Response Market Assessment",1]
["WAGeneral ServiceThird Party ContractsAnnual O&M Cost per MW","WA","General Service","Third Party Contracts","Annual O&M Cost per MW","$/MW @meter",80000,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["WAGeneral ServiceThird Party ContractsProgram Development Cost","WA","General Service","Third Party Contracts","Program Development Cost","$/program",0,0,1]
["WAGeneral ServiceThird Party ContractsProgram Life","WA","General Service","Third Party Contracts","Program Life","years",3,0,1]
["WAGeneral ServiceThird Party ContractsProgram Start Year","WA","General Service","Third Party Contracts","Program Start Year","year",2022,0,1]
["WALarge General ServiceThird Party ContractsSummer DR Event Hours","WA","Large General Service","Third Party Contracts","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WALarge General ServiceThird Party ContractsWinter DR Event Hours","WA","Large General Service","Third Party Contracts","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WALarge General ServiceThird Party ContractsAnnual O&M Cost","WA","Large General Service","Third Party Contracts","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceThird Party ContractsAnnual Program Administration Cost","WA","Large General Service","Third Party Contracts","Annual Program Administration Cost","$/yr",0,0,1]
["WALarge General ServiceThird Party ContractsCost of Equip + Install","WA","Large General Service","Third Party Contracts","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceThird Party ContractsCost of Equip + Install (per kW basis)","WA","Large General Service","Third Party Contracts","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceThird Party ContractsDe-rate","WA","Large General Service","Third Party Contracts","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceThird Party ContractsNet to Gross Ratio (free ridership)","WA","Large General Service","Third Party Contracts","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceThird Party ContractsPer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Third Party Contracts","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceThird Party ContractsPer Participant Annual Incentive","WA","Large General Service","Third Party Contracts","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WALarge General ServiceThird Party ContractsPer kW Annual Incentive","WA","Large General Service","Third Party Contracts","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["WALarge General ServiceThird Party ContractsAnnual O&M Cost per MW","WA","Large General Service","Third Party Contracts","Annual O&M Cost per MW","$/MW @meter",80000,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceThird Party ContractsProgram Development Cost","WA","Large General Service","Third Party Contracts","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
["WALarge General ServiceThird Party ContractsProgram Life","WA","Large General Service","Third Party Contracts","Program Life","years",3,0,1]
["WALarge General ServiceThird Party ContractsProgram Start Year","WA","Large General Service","Third Party Contracts","Program Start Year","year",2022,0,1]
["WAExtra Large General ServiceThird Party ContractsSummer DR Event Hours","WA","Extra Large General Service","Third Party Contracts","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAExtra Large General ServiceThird Party ContractsWinter DR Event Hours","WA","Extra Large General Service","Third Party Contracts","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAExtra Large General ServiceThird Party ContractsAnnual O&M Cost","WA","Extra Large General Service","Third Party Contracts","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceThird Party ContractsAnnual Program Administration Cost","WA","Extra Large General Service","Third Party Contracts","Annual Program Administration Cost","$/yr",0,0,1]
["WAExtra Large General ServiceThird Party ContractsCost of Equip + Install","WA","Extra Large General Service","Third Party Contracts","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceThird Party ContractsCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Third Party Contracts","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceThird Party ContractsDe-rate","WA","Extra Large General Service","Third Party Contracts","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceThird Party ContractsNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Third Party Contracts","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceThird Party ContractsPer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Third Party Contracts","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceThird Party ContractsPer Participant Annual Incentive","WA","Extra Large General Service","Third Party Contracts","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WAExtra Large General ServiceThird Party ContractsPer kW Annual Incentive","WA","Extra Large General Service","Third Party Contracts","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["WAExtra Large General ServiceThird Party ContractsAnnual O&M Cost per MW","WA","Extra Large General Service","Third Party Contracts","Annual O&M Cost per MW","$/MW @meter",80000,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceThird Party ContractsProgram Development Cost","WA","Extra Large General Service","Third Party Contracts","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
["WAExtra Large General ServiceThird Party ContractsProgram Life","WA","Extra Large General Service","Third Party Contracts","Program Life","years",3,0,1]
["WAExtra Large General ServiceThird Party ContractsProgram Start Year","WA","Extra Large General Service","Third Party Contracts","Program Start Year","year",2022,0,1]
["WAResidentialTime-of-Use Opt-inSummer DR Event Hours","WA","Residential","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["WAResidentialTime-of-Use Opt-inWinter DR Event Hours","WA","Residential","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WAResidentialTime-of-Use Opt-inAnnual O&M Cost","WA","Residential","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["WAResidentialTime-of-Use Opt-inAnnual Program Administration Cost","WA","Residential","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",47916.738281110811,0,1]
["WAResidentialTime-of-Use Opt-inCost of Equip + Install","WA","Residential","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["WAResidentialTime-of-Use Opt-inCost of Equip + Install (per kW basis)","WA","Residential","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialTime-of-Use Opt-inDe-rate","WA","Residential","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialTime-of-Use Opt-inNet to Gross Ratio (free ridership)","WA","Residential","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["WAResidentialTime-of-Use Opt-inPer Participant Annual Incentive","WA","Residential","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAResidentialTime-of-Use Opt-inPer kW Annual Incentive","WA","Residential","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialTime-of-Use Opt-inProgram Development Cost","WA","Residential","Time-of-Use Opt-in","Program Development Cost","$/program",39930.615234259014,0,1]
["WAResidentialTime-of-Use Opt-inProgram Life","WA","Residential","Time-of-Use Opt-in","Program Life","years",10,0,1]
["WAResidentialTime-of-Use Opt-inProgram Start Year","WA","Residential","Time-of-Use Opt-in","Program Start Year","year",2022,0,1]
["WAGeneral ServiceTime-of-Use Opt-inSummer DR Event Hours","WA","General Service","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
[{"$f":"B258&C258&D258&E258","v":"WAGeneral ServiceTime-of-Use Opt-inWinter DR Event Hours"},"WA","General Service","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WAGeneral ServiceTime-of-Use Opt-inAnnual O&M Cost","WA","General Service","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-inAnnual Program Administration Cost","WA","General Service","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",290.94608430387308,0,1]
["WAGeneral ServiceTime-of-Use Opt-inCost of Equip + Install","WA","General Service","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-inCost of Equip + Install (per kW basis)","WA","General Service","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-inDe-rate","WA","General Service","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceTime-of-Use Opt-inNet to Gross Ratio (free ridership)","WA","General Service","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["WAGeneral ServiceTime-of-Use Opt-inPer Participant Annual Incentive","WA","General Service","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAGeneral ServiceTime-of-Use Opt-inPer kW Annual Incentive","WA","General Service","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-inProgram Development Cost","WA","General Service","Time-of-Use Opt-in","Program Development Cost","$/program",242.45507025322755,0,1]
["WAGeneral ServiceTime-of-Use Opt-inProgram Life","WA","General Service","Time-of-Use Opt-in","Program Life","years",10,0,1]
["WAGeneral ServiceTime-of-Use Opt-inProgram Start Year","WA","General Service","Time-of-Use Opt-in","Program Start Year","year",2022,0,1]
["WALarge General ServiceTime-of-Use Opt-inSummer DR Event Hours","WA","Large General Service","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["WALarge General ServiceTime-of-Use Opt-inWinter DR Event Hours","WA","Large General Service","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WALarge General ServiceTime-of-Use Opt-inAnnual O&M Cost","WA","Large General Service","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["WALarge General ServiceTime-of-Use Opt-inAnnual Program Administration Cost","WA","Large General Service","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",7130.0131599480765,0,1]
["WALarge General ServiceTime-of-Use Opt-inCost of Equip + Install","WA","Large General Service","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["WALarge General ServiceTime-of-Use Opt-inCost of Equip + Install (per kW basis)","WA","Large General Service","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WALarge General ServiceTime-of-Use Opt-inDe-rate","WA","Large General Service","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceTime-of-Use Opt-inNet to Gross Ratio (free ridership)","WA","Large General Service","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["WALarge General ServiceTime-of-Use Opt-inPer Participant Annual Incentive","WA","Large General Service","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WALarge General ServiceTime-of-Use Opt-inPer kW Annual Incentive","WA","Large General Service","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WALarge General ServiceTime-of-Use Opt-inProgram Development Cost","WA","Large General Service","Time-of-Use Opt-in","Program Development Cost","$/program",5941.6776332900636,0,1]
["WALarge General ServiceTime-of-Use Opt-inProgram Life","WA","Large General Service","Time-of-Use Opt-in","Program Life","years",10,0,1]
["WALarge General ServiceTime-of-Use Opt-inProgram Start Year","WA","Large General Service","Time-of-Use Opt-in","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["WAExtra Large General ServiceTime-of-Use Opt-inSummer DR Event Hours","WA","Extra Large General Service","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["WAExtra Large General ServiceTime-of-Use Opt-inWinter DR Event Hours","WA","Extra Large General Service","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WAExtra Large General ServiceTime-of-Use Opt-inAnnual O&M Cost","WA","Extra Large General Service","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inAnnual Program Administration Cost","WA","Extra Large General Service","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",3774.9711255850957,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inCost of Equip + Install","WA","Extra Large General Service","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inDe-rate","WA","Extra Large General Service","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["WAExtra Large General ServiceTime-of-Use Opt-inPer Participant Annual Incentive","WA","Extra Large General Service","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAExtra Large General ServiceTime-of-Use Opt-inPer kW Annual Incentive","WA","Extra Large General Service","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inProgram Development Cost","WA","Extra Large General Service","Time-of-Use Opt-in","Program Development Cost","$/program",3145.809271320913,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inProgram Life","WA","Extra Large General Service","Time-of-Use Opt-in","Program Life","years",10,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-inProgram Start Year","WA","Extra Large General Service","Time-of-Use Opt-in","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["WAResidentialTime-of-Use Opt-outSummer DR Event Hours","WA","Residential","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["WAResidentialTime-of-Use Opt-outWinter DR Event Hours","WA","Residential","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WAResidentialTime-of-Use Opt-outAnnual O&M Cost","WA","Residential","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["WAResidentialTime-of-Use Opt-outAnnual Program Administration Cost","WA","Residential","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",42357.865197275212,0,1]
["WAResidentialTime-of-Use Opt-outCost of Equip + Install","WA","Residential","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["WAResidentialTime-of-Use Opt-outCost of Equip + Install (per kW basis)","WA","Residential","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialTime-of-Use Opt-outDe-rate","WA","Residential","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialTime-of-Use Opt-outNet to Gross Ratio (free ridership)","WA","Residential","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["WAResidentialTime-of-Use Opt-outPer Participant Annual Incentive","WA","Residential","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAResidentialTime-of-Use Opt-outPer kW Annual Incentive","WA","Residential","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialTime-of-Use Opt-outProgram Development Cost","WA","Residential","Time-of-Use Opt-out","Program Development Cost","$/program",35298.220997729346,0,1]
["WAResidentialTime-of-Use Opt-outProgram Life","WA","Residential","Time-of-Use Opt-out","Program Life","years",10,0,1]
["WAResidentialTime-of-Use Opt-outProgram Start Year","WA","Residential","Time-of-Use Opt-out","Program Start Year","year",2022,0,1]
["WAGeneral ServiceTime-of-Use Opt-outSummer DR Event Hours","WA","General Service","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["WAGeneral ServiceTime-of-Use Opt-outWinter DR Event Hours","WA","General Service","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WAGeneral ServiceTime-of-Use Opt-outAnnual O&M Cost","WA","General Service","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-outAnnual Program Administration Cost","WA","General Service","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",431.1766871772752,0,1]
["WAGeneral ServiceTime-of-Use Opt-outCost of Equip + Install","WA","General Service","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-outCost of Equip + Install (per kW basis)","WA","General Service","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-outDe-rate","WA","General Service","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceTime-of-Use Opt-outNet to Gross Ratio (free ridership)","WA","General Service","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
[{"$f":"B322&C322&D322&E322","v":"WAGeneral ServiceTime-of-Use Opt-outPer Participant Annual Incentive"},"WA","General Service","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAGeneral ServiceTime-of-Use Opt-outPer kW Annual Incentive","WA","General Service","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceTime-of-Use Opt-outProgram Development Cost","WA","General Service","Time-of-Use Opt-out","Program Development Cost","$/program",359.31390598106265,0,1]
["WAGeneral ServiceTime-of-Use Opt-outProgram Life","WA","General Service","Time-of-Use Opt-out","Program Life","years",10,0,1]
["WAGeneral ServiceTime-of-Use Opt-outProgram Start Year","WA","General Service","Time-of-Use Opt-out","Program Start Year","year",2022,0,1]
["WALarge General ServiceTime-of-Use Opt-outSummer DR Event Hours","WA","Large General Service","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["WALarge General ServiceTime-of-Use Opt-outWinter DR Event Hours","WA","Large General Service","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WALarge General ServiceTime-of-Use Opt-outAnnual O&M Cost","WA","Large General Service","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["WALarge General ServiceTime-of-Use Opt-outAnnual Program Administration Cost","WA","Large General Service","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",10566.54692979438,0,1]
["WALarge General ServiceTime-of-Use Opt-outCost of Equip + Install","WA","Large General Service","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["WALarge General ServiceTime-of-Use Opt-outCost of Equip + Install (per kW basis)","WA","Large General Service","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WALarge General ServiceTime-of-Use Opt-outDe-rate","WA","Large General Service","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceTime-of-Use Opt-outNet to Gross Ratio (free ridership)","WA","Large General Service","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["WALarge General ServiceTime-of-Use Opt-outPer Participant Annual Incentive","WA","Large General Service","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WALarge General ServiceTime-of-Use Opt-outPer kW Annual Incentive","WA","Large General Service","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WALarge General ServiceTime-of-Use Opt-outProgram Development Cost","WA","Large General Service","Time-of-Use Opt-out","Program Development Cost","$/program",8805.4557748286497,0,1]
["WALarge General ServiceTime-of-Use Opt-outProgram Life","WA","Large General Service","Time-of-Use Opt-out","Program Life","years",10,0,1]
["WALarge General ServiceTime-of-Use Opt-outProgram Start Year","WA","Large General Service","Time-of-Use Opt-out","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["WAExtra Large General ServiceTime-of-Use Opt-outSummer DR Event Hours","WA","Extra Large General Service","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["WAExtra Large General ServiceTime-of-Use Opt-outWinter DR Event Hours","WA","Extra Large General Service","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["WAExtra Large General ServiceTime-of-Use Opt-outAnnual O&M Cost","WA","Extra Large General Service","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outAnnual Program Administration Cost","WA","Extra Large General Service","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",5594.4370174772739,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outCost of Equip + Install","WA","Extra Large General Service","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outDe-rate","WA","Extra Large General Service","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["WAExtra Large General ServiceTime-of-Use Opt-outPer Participant Annual Incentive","WA","Extra Large General Service","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAExtra Large General ServiceTime-of-Use Opt-outPer kW Annual Incentive","WA","Extra Large General Service","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outProgram Development Cost","WA","Extra Large General Service","Time-of-Use Opt-out","Program Development Cost","$/program",4662.0308478977286,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outProgram Life","WA","Extra Large General Service","Time-of-Use Opt-out","Program Life","years",10,0,1]
["WAExtra Large General ServiceTime-of-Use Opt-outProgram Start Year","WA","Extra Large General Service","Time-of-Use Opt-out","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["WAResidentialVariable Peak Pricing RatesSummer DR Event Hours","WA","Residential","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",80,"Top 60 summer system hours ",1]
["WAResidentialVariable Peak Pricing RatesWinter DR Event Hours","WA","Residential","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",80,"Using summer hours except for UT",1]
["WAResidentialVariable Peak Pricing RatesAnnual O&M Cost","WA","Residential","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
["WAResidentialVariable Peak Pricing RatesAnnual Program Administration Cost","WA","Residential","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",46572.590233996452,0,1]
["WAResidentialVariable Peak Pricing RatesCost of Equip + Install","WA","Residential","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,"Assume zero, but would be $470 w tech costs included.  Based on PacifiCorp estimate: $270 for PCT, plus $200 for installation",1]
["WAResidentialVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","WA","Residential","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialVariable Peak Pricing RatesDe-rate","WA","Residential","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","WA","Residential","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
["WAResidentialVariable Peak Pricing RatesPer Participant Annual Incentive","WA","Residential","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAResidentialVariable Peak Pricing RatesPer kW Annual Incentive","WA","Residential","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialVariable Peak Pricing RatesProgram Development Cost","WA","Residential","Variable Peak Pricing Rates","Program Development Cost","$/program",38810.491861663715,0,1]
["WAResidentialVariable Peak Pricing RatesProgram Life","WA","Residential","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["WAResidentialVariable Peak Pricing RatesProgram Start Year","WA","Residential","Variable Peak Pricing Rates","Program Start Year","year",2022,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesSummer DR Event Hours","WA","General Service","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",40,"Top 40 summer system hours ",1]
["WAGeneral ServiceVariable Peak Pricing RatesWinter DR Event Hours","WA","General Service","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",40,"Using summer hours except for UT",1]
["WAGeneral ServiceVariable Peak Pricing RatesAnnual O&M Cost","WA","General Service","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesAnnual Program Administration Cost","WA","General Service","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",3256.639093562208,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesCost of Equip + Install","WA","General Service","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,"Assume zero, but would be $470 w tech costs included.  Based on PacifiCorp estimate: $270 for PCT, plus $200 for installation",1]
["WAGeneral ServiceVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","WA","General Service","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesDe-rate","WA","General Service","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","WA","General Service","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesPer Participant Annual Incentive","WA","General Service","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAGeneral ServiceVariable Peak Pricing RatesPer kW Annual Incentive","WA","General Service","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesProgram Development Cost","WA","General Service","Variable Peak Pricing Rates","Program Development Cost","$/program",2713.8659113018398,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesProgram Life","WA","General Service","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["WAGeneral ServiceVariable Peak Pricing RatesProgram Start Year","WA","General Service","Variable Peak Pricing Rates","Program Start Year","year",2022,0,1]
["WALarge General ServiceVariable Peak Pricing RatesSummer DR Event Hours","WA","Large General Service","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",40,"Top 40 summer system hours ",1]
["WALarge General ServiceVariable Peak Pricing RatesWinter DR Event Hours","WA","Large General Service","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",40,"Using summer hours except for UT",1]
["WALarge General ServiceVariable Peak Pricing RatesAnnual O&M Cost","WA","Large General Service","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
[{"$f":"B386&C386&D386&E386","v":"WALarge General ServiceVariable Peak Pricing RatesAnnual Program Administration Cost"},"WA","Large General Service","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",6139.0913318201347,0,1]
["WALarge General ServiceVariable Peak Pricing RatesCost of Equip + Install","WA","Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,"No equipment cost because assuming they have their own technology (like a Energy Management System etc) to control their processes",1]
["WALarge General ServiceVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","WA","Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"Currently zero, but $360/kW if tech costs included. Based on Auto-DR tech enablement costs. $300/kW is incentive level offered by SCE for Auto-DR participants, and is expected to cover a large fraction of costs. 20% adder included to recognize some additional expenses on the part of the customer. ",1]
["WALarge General ServiceVariable Peak Pricing RatesDe-rate","WA","Large General Service","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","WA","Large General Service","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",200,"Assumed 4X Residential recruitment costs",1]
["WALarge General ServiceVariable Peak Pricing RatesPer Participant Annual Incentive","WA","Large General Service","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WALarge General ServiceVariable Peak Pricing RatesPer kW Annual Incentive","WA","Large General Service","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WALarge General ServiceVariable Peak Pricing RatesProgram Development Cost","WA","Large General Service","Variable Peak Pricing Rates","Program Development Cost","$/program",5115.9094431834455,0,1]
["WALarge General ServiceVariable Peak Pricing RatesProgram Life","WA","Large General Service","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["WALarge General ServiceVariable Peak Pricing RatesProgram Start Year","WA","Large General Service","Variable Peak Pricing Rates","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesSummer DR Event Hours","WA","Extra Large General Service","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",40,"Top 40 summer system hours ",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesWinter DR Event Hours","WA","Extra Large General Service","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",40,"Using summer hours except for UT",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesAnnual O&M Cost","WA","Extra Large General Service","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesAnnual Program Administration Cost","WA","Extra Large General Service","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",2698.5466637379527,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesCost of Equip + Install","WA","Extra Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"Currently zero, but $360/kW if tech costs included. Based on Auto-DR tech enablement costs. $300/kW is incentive level offered by SCE for Auto-DR participants, and is expected to cover a large fraction of costs. 20% adder included to recognize some additional expenses on the part of the customer. ",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesDe-rate","WA","Extra Large General Service","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",400,"Assumed 2X Large C&I recruitment costs",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesPer Participant Annual Incentive","WA","Extra Large General Service","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["WAExtra Large General ServiceVariable Peak Pricing RatesPer kW Annual Incentive","WA","Extra Large General Service","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesProgram Development Cost","WA","Extra Large General Service","Variable Peak Pricing Rates","Program Development Cost","$/program",2248.7888864482939,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesProgram Life","WA","Extra Large General Service","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["WAExtra Large General ServiceVariable Peak Pricing RatesProgram Start Year","WA","Extra Large General Service","Variable Peak Pricing Rates","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["WALarge General ServiceReal Time PricingSummer DR Event Hours","WA","Large General Service","Real Time Pricing","Summer DR Event Hours","hours/year","","",1]
["WALarge General ServiceReal Time PricingWinter DR Event Hours","WA","Large General Service","Real Time Pricing","Winter DR Event Hours","hours/year","","",1]
["WALarge General ServiceReal Time PricingAnnual O&M Cost","WA","Large General Service","Real Time Pricing","Annual O&M Cost","$/participant/year","","",1]
["WALarge General ServiceReal Time PricingAnnual Program Administration Cost","WA","Large General Service","Real Time Pricing","Annual Program Administration Cost","$/yr","","",1]
["WALarge General ServiceReal Time PricingCost of Equip + Install","WA","Large General Service","Real Time Pricing","Cost of Equip + Install","$/tech","","",1]
["WALarge General ServiceReal Time PricingCost of Equip + Install (per kW basis)","WA","Large General Service","Real Time Pricing","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["WALarge General ServiceReal Time PricingDe-rate","WA","Large General Service","Real Time Pricing","De-rate","capacity equivalence factor","","",1]
["WALarge General ServiceReal Time PricingNet to Gross Ratio (free ridership)","WA","Large General Service","Real Time Pricing","Net to Gross Ratio (free ridership)","ratio","","",1]
["WALarge General ServiceReal Time PricingPer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Real Time Pricing","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["WALarge General ServiceReal Time PricingPer Participant Annual Incentive","WA","Large General Service","Real Time Pricing","Per Participant Annual Incentive","$/participant/year","","",1]
["WALarge General ServiceReal Time PricingPer kW Annual Incentive","WA","Large General Service","Real Time Pricing","Per kW Annual Incentive","$/kW @meter/year","","",1]
["WALarge General ServiceReal Time PricingProgram Development Cost","WA","Large General Service","Real Time Pricing","Program Development Cost","$/program","","",1]
["WALarge General ServiceReal Time PricingProgram Life","WA","Large General Service","Real Time Pricing","Program Life","years","","",1]
["WALarge General ServiceReal Time PricingProgram Start Year","WA","Large General Service","Real Time Pricing","Program Start Year","year","","",1]
["WAExtra Large General ServiceReal Time PricingSummer DR Event Hours","WA","Extra Large General Service","Real Time Pricing","Summer DR Event Hours","hours/year","","",1]
["WAExtra Large General ServiceReal Time PricingWinter DR Event Hours","WA","Extra Large General Service","Real Time Pricing","Winter DR Event Hours","hours/year","","",1]
["WAExtra Large General ServiceReal Time PricingAnnual O&M Cost","WA","Extra Large General Service","Real Time Pricing","Annual O&M Cost","$/participant/year","","",1]
["WAExtra Large General ServiceReal Time PricingAnnual Program Administration Cost","WA","Extra Large General Service","Real Time Pricing","Annual Program Administration Cost","$/yr","","",1]
["WAExtra Large General ServiceReal Time PricingCost of Equip + Install","WA","Extra Large General Service","Real Time Pricing","Cost of Equip + Install","$/tech","","",1]
["WAExtra Large General ServiceReal Time PricingCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Real Time Pricing","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["WAExtra Large General ServiceReal Time PricingDe-rate","WA","Extra Large General Service","Real Time Pricing","De-rate","capacity equivalence factor","","",1]
["WAExtra Large General ServiceReal Time PricingNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Real Time Pricing","Net to Gross Ratio (free ridership)","ratio","","",1]
["WAExtra Large General ServiceReal Time PricingPer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Real Time Pricing","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["WAExtra Large General ServiceReal Time PricingPer Participant Annual Incentive","WA","Extra Large General Service","Real Time Pricing","Per Participant Annual Incentive","$/participant/year","","",1]
["WAExtra Large General ServiceReal Time PricingPer kW Annual Incentive","WA","Extra Large General Service","Real Time Pricing","Per kW Annual Incentive","$/kW @meter/year","","",1]
["WAExtra Large General ServiceReal Time PricingProgram Development Cost","WA","Extra Large General Service","Real Time Pricing","Program Development Cost","$/program","","",1]
["WAExtra Large General ServiceReal Time PricingProgram Life","WA","Extra Large General Service","Real Time Pricing","Program Life","years","","",1]
["WAExtra Large General ServiceReal Time PricingProgram Start Year","WA","Extra Large General Service","Real Time Pricing","Program Start Year","year","","",1]
["WAGeneral ServiceThermal Energy StorageSummer DR Event Hours","WA","General Service","Thermal Energy Storage","Summer DR Event Hours","hours/year",36,"Same as TOU, six hours on peak period each summer",1]
["WAGeneral ServiceThermal Energy StorageWinter DR Event Hours","WA","General Service","Thermal Energy Storage","Winter DR Event Hours","hours/year",0,0,1]
["WAGeneral ServiceThermal Energy StorageAnnual O&M Cost","WA","General Service","Thermal Energy Storage","Annual O&M Cost","$/participant/year",84,"Assumption of 5% equipment costs",1]
["WAGeneral ServiceThermal Energy StorageAnnual Program Administration Cost","WA","General Service","Thermal Energy Storage","Annual Program Administration Cost","$/yr",27189.08625134463,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceThermal Energy StorageCost of Equip + Install","WA","General Service","Thermal Energy Storage","Cost of Equip + Install","$/tech",0,0,1]
["WAGeneral ServiceThermal Energy StorageCost of Equip + Install (per kW basis)","WA","General Service","Thermal Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",1680,"Utility Dive Article, Ice Energy Implementer cost",1]
["WAGeneral ServiceThermal Energy StorageDe-rate","WA","General Service","Thermal Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceThermal Energy StorageNet to Gross Ratio (free ridership)","WA","General Service","Thermal Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceThermal Energy StoragePer Customer Annual Marketing/Recruitment Cost","WA","General Service","Thermal Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",100,"Assumption $100 for RAP C&I, MAP = RAPx1.2",1]
["WAGeneral ServiceThermal Energy StoragePer Participant Annual Incentive","WA","General Service","Thermal Energy Storage","Per Participant Annual Incentive","$/participant/year",0,"No incentive. Program purchases & installs unit.",1]
["WAGeneral ServiceThermal Energy StoragePer kW Annual Incentive","WA","General Service","Thermal Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
[{"$f":"B450&C450&D450&E450","v":"WAGeneral ServiceThermal Energy StorageProgram Development Cost"},"WA","General Service","Thermal Energy Storage","Program Development Cost","$/program",22657.571876120524,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceThermal Energy StorageProgram Life","WA","General Service","Thermal Energy Storage","Program Life","years",20,0,1]
["WAGeneral ServiceThermal Energy StorageProgram Start Year","WA","General Service","Thermal Energy Storage","Program Start Year","year",2022,0,1]
["WALarge General ServiceThermal Energy StorageSummer DR Event Hours","WA","Large General Service","Thermal Energy Storage","Summer DR Event Hours","hours/year",36,"Same as TOU, six hours on peak period each summer",1]
["WALarge General ServiceThermal Energy StorageWinter DR Event Hours","WA","Large General Service","Thermal Energy Storage","Winter DR Event Hours","hours/year",0,0,1]
["WALarge General ServiceThermal Energy StorageAnnual O&M Cost","WA","Large General Service","Thermal Energy Storage","Annual O&M Cost","$/participant/year",420,"Assumption of 5% equipment costs",1]
["WALarge General ServiceThermal Energy StorageAnnual Program Administration Cost","WA","Large General Service","Thermal Energy Storage","Annual Program Administration Cost","$/yr",26505.0278124326,"Share of Cost as noted in table at right",1]
["WALarge General ServiceThermal Energy StorageCost of Equip + Install","WA","Large General Service","Thermal Energy Storage","Cost of Equip + Install","$/tech",0,0,1]
["WALarge General ServiceThermal Energy StorageCost of Equip + Install (per kW basis)","WA","Large General Service","Thermal Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",8400,"Utility Dive Article, Ice Energy Implementer cost",1]
["WALarge General ServiceThermal Energy StorageDe-rate","WA","Large General Service","Thermal Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceThermal Energy StorageNet to Gross Ratio (free ridership)","WA","Large General Service","Thermal Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceThermal Energy StoragePer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Thermal Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",100,"Assumption $100 for RAP C&I, MAP = RAPx1.2",1]
["WALarge General ServiceThermal Energy StoragePer Participant Annual Incentive","WA","Large General Service","Thermal Energy Storage","Per Participant Annual Incentive","$/participant/year",0,"No incentive. Program purchases & installs unit.",1]
["WALarge General ServiceThermal Energy StoragePer kW Annual Incentive","WA","Large General Service","Thermal Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WALarge General ServiceThermal Energy StorageProgram Development Cost","WA","Large General Service","Thermal Energy Storage","Program Development Cost","$/program",22087.523177027168,"Share of Cost as noted in table at right",1]
["WALarge General ServiceThermal Energy StorageProgram Life","WA","Large General Service","Thermal Energy Storage","Program Life","years",20,0,1]
["WALarge General ServiceThermal Energy StorageProgram Start Year","WA","Large General Service","Thermal Energy Storage","Program Start Year","year",2022,0,1]
["WAExtra Large General ServiceThermal Energy StorageSummer DR Event Hours","WA","Extra Large General Service","Thermal Energy Storage","Summer DR Event Hours","hours/year",36,"Same as TOU, six hours on peak period each summer",1]
["WAExtra Large General ServiceThermal Energy StorageWinter DR Event Hours","WA","Extra Large General Service","Thermal Energy Storage","Winter DR Event Hours","hours/year",0,0,1]
["WAExtra Large General ServiceThermal Energy StorageAnnual O&M Cost","WA","Extra Large General Service","Thermal Energy Storage","Annual O&M Cost","$/participant/year",420,"Assumption of 5% equipment costs",1]
["WAExtra Large General ServiceThermal Energy StorageAnnual Program Administration Cost","WA","Extra Large General Service","Thermal Energy Storage","Annual Program Administration Cost","$/yr",287.0900290859567,"Share of Cost as noted in table at right",1]
["WAExtra Large General ServiceThermal Energy StorageCost of Equip + Install","WA","Extra Large General Service","Thermal Energy Storage","Cost of Equip + Install","$/tech",0,0,1]
["WAExtra Large General ServiceThermal Energy StorageCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Thermal Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",8400,"Utility Dive Article, Ice Energy Implementer cost",1]
["WAExtra Large General ServiceThermal Energy StorageDe-rate","WA","Extra Large General Service","Thermal Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceThermal Energy StorageNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Thermal Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceThermal Energy StoragePer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Thermal Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",100,"Assumption $100 for RAP C&I, MAP = RAPx1.2",1]
["WAExtra Large General ServiceThermal Energy StoragePer Participant Annual Incentive","WA","Extra Large General Service","Thermal Energy Storage","Per Participant Annual Incentive","$/participant/year",0,"No incentive. Program purchases & installs unit.",1]
["WAExtra Large General ServiceThermal Energy StoragePer kW Annual Incentive","WA","Extra Large General Service","Thermal Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAExtra Large General ServiceThermal Energy StorageProgram Development Cost","WA","Extra Large General Service","Thermal Energy Storage","Program Development Cost","$/program",239.24169090496389,"Share of Cost as noted in table at right",1]
["WAExtra Large General ServiceThermal Energy StorageProgram Life","WA","Extra Large General Service","Thermal Energy Storage","Program Life","years",20,0,1]
["WAExtra Large General ServiceThermal Energy StorageProgram Start Year","WA","Extra Large General Service","Thermal Energy Storage","Program Start Year","year",2022,0,1]
["WAResidentialBattery Energy StorageSummer DR Event Hours","WA","Residential","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["WAResidentialBattery Energy StorageWinter DR Event Hours","WA","Residential","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WAResidentialBattery Energy StorageAnnual O&M Cost","WA","Residential","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WAResidentialBattery Energy StorageAnnual Program Administration Cost","WA","Residential","Battery Energy Storage","Annual Program Administration Cost","$/yr",49838.915828113793,"half FTE @ $150,000",1]
["WAResidentialBattery Energy StorageCost of Equip + Install","WA","Residential","Battery Energy Storage","Cost of Equip + Install","$/tech",6912,"Lazard's cost - avg. of hi/low case for Residential Lithium-Ion Batteries - low=$1,662, hi=$2,178 ",1]
["WAResidentialBattery Energy StorageCost of Equip + Install (per kW basis)","WA","Residential","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialBattery Energy StorageDe-rate","WA","Residential","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialBattery Energy StorageNet to Gross Ratio (free ridership)","WA","Residential","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","WA","Residential","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["WAResidentialBattery Energy StoragePer Participant Annual Incentive","WA","Residential","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WAResidentialBattery Energy StoragePer kW Annual Incentive","WA","Residential","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialBattery Energy StorageProgram Development Cost","WA","Residential","Battery Energy Storage","Program Development Cost","$/program",27688.286571174332,0,1]
["WAResidentialBattery Energy StorageProgram Life","WA","Residential","Battery Energy Storage","Program Life","years",15,"NREL",1]
["WAResidentialBattery Energy StorageProgram Start Year","WA","Residential","Battery Energy Storage","Program Start Year","year",2022,0,1]
["WAGeneral ServiceBattery Energy StorageSummer DR Event Hours","WA","General Service","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["WAGeneral ServiceBattery Energy StorageWinter DR Event Hours","WA","General Service","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WAGeneral ServiceBattery Energy StorageAnnual O&M Cost","WA","General Service","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WAGeneral ServiceBattery Energy StorageAnnual Program Administration Cost","WA","General Service","Battery Energy Storage","Annual Program Administration Cost","$/yr",5283.1160966009629,"half FTE @ $150,000",1]
["WAGeneral ServiceBattery Energy StorageCost of Equip + Install","WA","General Service","Battery Energy Storage","Cost of Equip + Install","$/tech",6542.4,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["WAGeneral ServiceBattery Energy StorageCost of Equip + Install (per kW basis)","WA","General Service","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceBattery Energy StorageDe-rate","WA","General Service","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceBattery Energy StorageNet to Gross Ratio (free ridership)","WA","General Service","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","WA","General Service","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["WAGeneral ServiceBattery Energy StoragePer Participant Annual Incentive","WA","General Service","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WAGeneral ServiceBattery Energy StoragePer kW Annual Incentive","WA","General Service","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceBattery Energy StorageProgram Development Cost","WA","General Service","Battery Energy Storage","Program Development Cost","$/program",2935.0644981116461,0,1]
["WAGeneral ServiceBattery Energy StorageProgram Life","WA","General Service","Battery Energy Storage","Program Life","years",15,"NREL",1]
["WAGeneral ServiceBattery Energy StorageProgram Start Year","WA","General Service","Battery Energy Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["WALarge General ServiceBattery Energy StorageSummer DR Event Hours","WA","Large General Service","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["WALarge General ServiceBattery Energy StorageWinter DR Event Hours","WA","Large General Service","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WALarge General ServiceBattery Energy StorageAnnual O&M Cost","WA","Large General Service","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WALarge General ServiceBattery Energy StorageAnnual Program Administration Cost","WA","Large General Service","Battery Energy Storage","Annual Program Administration Cost","$/yr",2575.0982909510931,"half FTE @ $150,000",1]
["WALarge General ServiceBattery Energy StorageCost of Equip + Install","WA","Large General Service","Battery Energy Storage","Cost of Equip + Install","$/tech",49068,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
[{"$f":"B514&C514&D514&E514","v":"WALarge General ServiceBattery Energy StorageCost of Equip + Install (per kW basis)"},"WA","Large General Service","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WALarge General ServiceBattery Energy StorageDe-rate","WA","Large General Service","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceBattery Energy StorageNet to Gross Ratio (free ridership)","WA","Large General Service","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["WALarge General ServiceBattery Energy StoragePer Participant Annual Incentive","WA","Large General Service","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WALarge General ServiceBattery Energy StoragePer kW Annual Incentive","WA","Large General Service","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WALarge General ServiceBattery Energy StorageProgram Development Cost","WA","Large General Service","Battery Energy Storage","Program Development Cost","$/program",1430.610161639496,0,1]
["WALarge General ServiceBattery Energy StorageProgram Life","WA","Large General Service","Battery Energy Storage","Program Life","years",15,"NREL",1]
["WALarge General ServiceBattery Energy StorageProgram Start Year","WA","Large General Service","Battery Energy Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["WAExtra Large General ServiceBattery Energy StorageSummer DR Event Hours","WA","Extra Large General Service","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["WAExtra Large General ServiceBattery Energy StorageWinter DR Event Hours","WA","Extra Large General Service","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WAExtra Large General ServiceBattery Energy StorageAnnual O&M Cost","WA","Extra Large General Service","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WAExtra Large General ServiceBattery Energy StorageAnnual Program Administration Cost","WA","Extra Large General Service","Battery Energy Storage","Annual Program Administration Cost","$/yr",27.892256838212912,"Calculated",1]
["WAExtra Large General ServiceBattery Energy StorageCost of Equip + Install","WA","Extra Large General Service","Battery Energy Storage","Cost of Equip + Install","$/tech",49068,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["WAExtra Large General ServiceBattery Energy StorageCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAExtra Large General ServiceBattery Energy StorageDe-rate","WA","Extra Large General Service","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceBattery Energy StorageNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["WAExtra Large General ServiceBattery Energy StoragePer Participant Annual Incentive","WA","Extra Large General Service","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WAExtra Large General ServiceBattery Energy StoragePer kW Annual Incentive","WA","Extra Large General Service","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAExtra Large General ServiceBattery Energy StorageProgram Development Cost","WA","Extra Large General Service","Battery Energy Storage","Program Development Cost","$/program",15.495698243451619,"Calculated",1]
["WAExtra Large General ServiceBattery Energy StorageProgram Life","WA","Extra Large General Service","Battery Energy Storage","Program Life","years",15,"NREL",1]
["WAExtra Large General ServiceBattery Energy StorageProgram Start Year","WA","Extra Large General Service","Battery Energy Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["WAResidentialAncillary ServicesSummer DR Event Hours","WA","Residential","Ancillary Services","Summer DR Event Hours","hours/year","","",1]
["WAResidentialAncillary ServicesWinter DR Event Hours","WA","Residential","Ancillary Services","Winter DR Event Hours","hours/year","","",1]
["WAResidentialAncillary ServicesAnnual O&M Cost","WA","Residential","Ancillary Services","Annual O&M Cost","$/participant/year","","",1]
["WAResidentialAncillary ServicesAnnual Program Administration Cost","WA","Residential","Ancillary Services","Annual Program Administration Cost","$/yr","","",1]
["WAResidentialAncillary ServicesCost of Equip + Install","WA","Residential","Ancillary Services","Cost of Equip + Install","$/tech","","",1]
["WAResidentialAncillary ServicesCost of Equip + Install (per kW basis)","WA","Residential","Ancillary Services","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["WAResidentialAncillary ServicesDe-rate","WA","Residential","Ancillary Services","De-rate","capacity equivalence factor","","",1]
["WAResidentialAncillary ServicesNet to Gross Ratio (free ridership)","WA","Residential","Ancillary Services","Net to Gross Ratio (free ridership)","ratio","","",1]
["WAResidentialAncillary ServicesPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Ancillary Services","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["WAResidentialAncillary ServicesPer Participant Annual Incentive","WA","Residential","Ancillary Services","Per Participant Annual Incentive","$/participant/year","","",1]
["WAResidentialAncillary ServicesPer kW Annual Incentive","WA","Residential","Ancillary Services","Per kW Annual Incentive","$/kW @meter/year","","",1]
["WAResidentialAncillary ServicesProgram Development Cost","WA","Residential","Ancillary Services","Program Development Cost","$/program","","",1]
["WAResidentialAncillary ServicesProgram Life","WA","Residential","Ancillary Services","Program Life","years","","",1]
["WAResidentialAncillary ServicesProgram Start Year","WA","Residential","Ancillary Services","Program Start Year","year","","",1]
["WAGeneral ServiceAncillary ServicesSummer DR Event Hours","WA","General Service","Ancillary Services","Summer DR Event Hours","hours/year","","",1]
["WAGeneral ServiceAncillary ServicesWinter DR Event Hours","WA","General Service","Ancillary Services","Winter DR Event Hours","hours/year","","",1]
["WAGeneral ServiceAncillary ServicesAnnual O&M Cost","WA","General Service","Ancillary Services","Annual O&M Cost","$/participant/year","","",1]
["WAGeneral ServiceAncillary ServicesAnnual Program Administration Cost","WA","General Service","Ancillary Services","Annual Program Administration Cost","$/yr","","",1]
["WAGeneral ServiceAncillary ServicesCost of Equip + Install","WA","General Service","Ancillary Services","Cost of Equip + Install","$/tech","","",1]
["WAGeneral ServiceAncillary ServicesCost of Equip + Install (per kW basis)","WA","General Service","Ancillary Services","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["WAGeneral ServiceAncillary ServicesDe-rate","WA","General Service","Ancillary Services","De-rate","capacity equivalence factor","","",1]
["WAGeneral ServiceAncillary ServicesNet to Gross Ratio (free ridership)","WA","General Service","Ancillary Services","Net to Gross Ratio (free ridership)","ratio","","",1]
["WAGeneral ServiceAncillary ServicesPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Ancillary Services","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["WAGeneral ServiceAncillary ServicesPer Participant Annual Incentive","WA","General Service","Ancillary Services","Per Participant Annual Incentive","$/participant/year","","",1]
["WAGeneral ServiceAncillary ServicesPer kW Annual Incentive","WA","General Service","Ancillary Services","Per kW Annual Incentive","$/kW @meter/year","","",1]
["WAGeneral ServiceAncillary ServicesProgram Development Cost","WA","General Service","Ancillary Services","Program Development Cost","$/program","","",1]
["WAGeneral ServiceAncillary ServicesProgram Life","WA","General Service","Ancillary Services","Program Life","years","","",1]
["WAGeneral ServiceAncillary ServicesProgram Start Year","WA","General Service","Ancillary Services","Program Start Year","year","","",1]
["WALarge General ServiceAncillary ServicesSummer DR Event Hours","WA","Large General Service","Ancillary Services","Summer DR Event Hours","hours/year","","",1]
["WALarge General ServiceAncillary ServicesWinter DR Event Hours","WA","Large General Service","Ancillary Services","Winter DR Event Hours","hours/year","","",1]
["WALarge General ServiceAncillary ServicesAnnual O&M Cost","WA","Large General Service","Ancillary Services","Annual O&M Cost","$/participant/year","","",1]
["WALarge General ServiceAncillary ServicesAnnual Program Administration Cost","WA","Large General Service","Ancillary Services","Annual Program Administration Cost","$/yr","","",1]
["WALarge General ServiceAncillary ServicesCost of Equip + Install","WA","Large General Service","Ancillary Services","Cost of Equip + Install","$/tech","","",1]
["WALarge General ServiceAncillary ServicesCost of Equip + Install (per kW basis)","WA","Large General Service","Ancillary Services","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["WALarge General ServiceAncillary ServicesDe-rate","WA","Large General Service","Ancillary Services","De-rate","capacity equivalence factor","","",1]
["WALarge General ServiceAncillary ServicesNet to Gross Ratio (free ridership)","WA","Large General Service","Ancillary Services","Net to Gross Ratio (free ridership)","ratio","","",1]
["WALarge General ServiceAncillary ServicesPer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Ancillary Services","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["WALarge General ServiceAncillary ServicesPer Participant Annual Incentive","WA","Large General Service","Ancillary Services","Per Participant Annual Incentive","$/participant/year","","",1]
["WALarge General ServiceAncillary ServicesPer kW Annual Incentive","WA","Large General Service","Ancillary Services","Per kW Annual Incentive","$/kW @meter/year","","",1]
["WALarge General ServiceAncillary ServicesProgram Development Cost","WA","Large General Service","Ancillary Services","Program Development Cost","$/program","","",1]
["WALarge General ServiceAncillary ServicesProgram Life","WA","Large General Service","Ancillary Services","Program Life","years","","",1]
[{"$f":"B578&C578&D578&E578","v":"WALarge General ServiceAncillary ServicesProgram Start Year"},"WA","Large General Service","Ancillary Services","Program Start Year","year","","",1]
["WAExtra Large General ServiceAncillary ServicesSummer DR Event Hours","WA","Extra Large General Service","Ancillary Services","Summer DR Event Hours","hours/year","","",1]
["WAExtra Large General ServiceAncillary ServicesWinter DR Event Hours","WA","Extra Large General Service","Ancillary Services","Winter DR Event Hours","hours/year","","",1]
["WAExtra Large General ServiceAncillary ServicesAnnual O&M Cost","WA","Extra Large General Service","Ancillary Services","Annual O&M Cost","$/participant/year","","",1]
["WAExtra Large General ServiceAncillary ServicesAnnual Program Administration Cost","WA","Extra Large General Service","Ancillary Services","Annual Program Administration Cost","$/yr","","",1]
["WAExtra Large General ServiceAncillary ServicesCost of Equip + Install","WA","Extra Large General Service","Ancillary Services","Cost of Equip + Install","$/tech","","",1]
["WAExtra Large General ServiceAncillary ServicesCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Ancillary Services","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["WAExtra Large General ServiceAncillary ServicesDe-rate","WA","Extra Large General Service","Ancillary Services","De-rate","capacity equivalence factor","","",1]
["WAExtra Large General ServiceAncillary ServicesNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Ancillary Services","Net to Gross Ratio (free ridership)","ratio","","",1]
["WAExtra Large General ServiceAncillary ServicesPer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Ancillary Services","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["WAExtra Large General ServiceAncillary ServicesPer Participant Annual Incentive","WA","Extra Large General Service","Ancillary Services","Per Participant Annual Incentive","$/participant/year","","",1]
["WAExtra Large General ServiceAncillary ServicesPer kW Annual Incentive","WA","Extra Large General Service","Ancillary Services","Per kW Annual Incentive","$/kW @meter/year","","",1]
["WAExtra Large General ServiceAncillary ServicesProgram Development Cost","WA","Extra Large General Service","Ancillary Services","Program Development Cost","$/program","","",1]
["WAExtra Large General ServiceAncillary ServicesProgram Life","WA","Extra Large General Service","Ancillary Services","Program Life","years","","",1]
["WAExtra Large General ServiceAncillary ServicesProgram Start Year","WA","Extra Large General Service","Ancillary Services","Program Start Year","year","","",1]
["IDResidentialBehavioralSummer DR Event Hours","ID","Residential","Behavioral","Summer DR Event Hours","hours/year",40,"8 hour event window x 5 events, Consumers Energy 7am-8pm 8 hr window",1]
["IDResidentialBehavioralWinter DR Event Hours","ID","Residential","Behavioral","Winter DR Event Hours","hours/year",40,"8 hour event window x 5 events, Consumers Energy 7am-8pm 8 hr window",1]
["IDResidentialBehavioralAnnual O&M Cost","ID","Residential","Behavioral","Annual O&M Cost","$/participant/year",3.25,"Oracle interview on 8/30, estimation of admin cost per household - KM heard 3 - 3.5 all inclusive- Implementation Cost",1]
["IDResidentialBehavioralAnnual Program Administration Cost","ID","Residential","Behavioral","Annual Program Administration Cost","$/yr",20366.590064520991,0,1]
["IDResidentialBehavioralCost of Equip + Install","ID","Residential","Behavioral","Cost of Equip + Install","$/tech",0,0,1]
["IDResidentialBehavioralCost of Equip + Install (per kW basis)","ID","Residential","Behavioral","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialBehavioralDe-rate","ID","Residential","Behavioral","De-rate","capacity equivalence factor",1,"Impact Reduced to reflect diminished savings program pulls in participants who are not \"high\" users",1]
["IDResidentialBehavioralNet to Gross Ratio (free ridership)","ID","Residential","Behavioral","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialBehavioralPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Behavioral","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,0,1]
["IDResidentialBehavioralPer Participant Annual Incentive","ID","Residential","Behavioral","Per Participant Annual Incentive","$/participant/year",0,"No Incentive for Behavioral DR - Brattle  PGE Potential Study 2016 - ",1]
["IDResidentialBehavioralPer kW Annual Incentive","ID","Residential","Behavioral","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialBehavioralProgram Development Cost","ID","Residential","Behavioral","Program Development Cost","$/program",33944.316774201652,0,1]
["IDResidentialBehavioralProgram Life","ID","Residential","Behavioral","Program Life","years",1,"MISO Res LoadMAP DSM Programs.xlsx (LRZ7) - Lifetime",1]
["IDResidentialBehavioralProgram Start Year","ID","Residential","Behavioral","Program Start Year","year",2022,0,1]
["IDResidentialDLC Electric Vehicle ChargingSummer DR Event Hours","ID","Residential","DLC Electric Vehicle Charging","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["IDResidentialDLC Electric Vehicle ChargingWinter DR Event Hours","ID","Residential","DLC Electric Vehicle Charging","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["IDResidentialDLC Electric Vehicle ChargingAnnual O&M Cost","ID","Residential","DLC Electric Vehicle Charging","Annual O&M Cost","$/participant/year",5,"Average subscription fees for EE and DR program management",1]
["IDResidentialDLC Electric Vehicle ChargingAnnual Program Administration Cost","ID","Residential","DLC Electric Vehicle Charging","Annual Program Administration Cost","$/yr",31037.278871407852,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Electric Vehicle ChargingCost of Equip + Install","ID","Residential","DLC Electric Vehicle Charging","Cost of Equip + Install","$/tech",700,"ppt from Kurtis email 2-5 indicates utility incentives are ~$1200 for charging equipment. Research indicates this is approx cost of equipment. (see Dave email to VN 3-15)",1]
["IDResidentialDLC Electric Vehicle ChargingCost of Equip + Install (per kW basis)","ID","Residential","DLC Electric Vehicle Charging","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialDLC Electric Vehicle ChargingDe-rate","ID","Residential","DLC Electric Vehicle Charging","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialDLC Electric Vehicle ChargingNet to Gross Ratio (free ridership)","ID","Residential","DLC Electric Vehicle Charging","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialDLC Electric Vehicle ChargingPer Customer Annual Marketing/Recruitment Cost","ID","Residential","DLC Electric Vehicle Charging","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,"Assumption $50 for RAP C&I, MAP = RAPx1.2",1]
["IDResidentialDLC Electric Vehicle ChargingPer Participant Annual Incentive","ID","Residential","DLC Electric Vehicle Charging","Per Participant Annual Incentive","$/participant/year",0,"Avista would provide a rate based charger or give a rebate on it, with no further incentives",1]
["IDResidentialDLC Electric Vehicle ChargingPer kW Annual Incentive","ID","Residential","DLC Electric Vehicle Charging","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialDLC Electric Vehicle ChargingProgram Development Cost","ID","Residential","DLC Electric Vehicle Charging","Program Development Cost","$/program",25864.399059506544,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Electric Vehicle ChargingProgram Life","ID","Residential","DLC Electric Vehicle Charging","Program Life","years",8,0,1]
["IDResidentialDLC Electric Vehicle ChargingProgram Start Year","ID","Residential","DLC Electric Vehicle Charging","Program Start Year","year",2024,"Technology won’t be available for mass market till 2024",1]
["IDResidentialDLC Central ACSummer DR Event Hours","ID","Residential","DLC Central AC","Summer DR Event Hours","hours/year",50,"Current PC Cool Keeper program allows for max 100 hours of curtailment.  ",1]
["IDResidentialDLC Central ACWinter DR Event Hours","ID","Residential","DLC Central AC","Winter DR Event Hours","hours/year",0,0,1]
["IDResidentialDLC Central ACAnnual O&M Cost","ID","Residential","DLC Central AC","Annual O&M Cost","$/participant/year",13,"Assume 5% of equipment + install costs.",1]
["IDResidentialDLC Central ACAnnual Program Administration Cost","ID","Residential","DLC Central AC","Annual Program Administration Cost","$/yr",25562.612843506638,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Central ACCost of Equip + Install","ID","Residential","DLC Central AC","Cost of Equip + Install","$/tech",260,"$100 installation cost. Idaho Power at 10,000 quantity pays $160 per switch.  I believe Avista volumes would be the same or less per order, making the cost $160 or greater.",1]
["IDResidentialDLC Central ACCost of Equip + Install (per kW basis)","ID","Residential","DLC Central AC","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialDLC Central ACDe-rate","ID","Residential","DLC Central AC","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialDLC Central ACNet to Gross Ratio (free ridership)","ID","Residential","DLC Central AC","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialDLC Central ACPer Customer Annual Marketing/Recruitment Cost","ID","Residential","DLC Central AC","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["IDResidentialDLC Central ACPer Participant Annual Incentive","ID","Residential","DLC Central AC","Per Participant Annual Incentive","$/participant/year",20,"$20 is the incentive level per participating unit. No. of units per average participant is 1.059",1]
["IDResidentialDLC Central ACPer kW Annual Incentive","ID","Residential","DLC Central AC","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialDLC Central ACProgram Development Cost","ID","Residential","DLC Central AC","Program Development Cost","$/program",21302.177369588866,0,1]
["IDResidentialDLC Central ACProgram Life","ID","Residential","DLC Central AC","Program Life","years",8,0,1]
["IDResidentialDLC Central ACProgram Start Year","ID","Residential","DLC Central AC","Program Start Year","year",2022,0,1]
["IDGeneral ServiceDLC Central ACSummer DR Event Hours","ID","General Service","DLC Central AC","Summer DR Event Hours","hours/year",50,"Current PC Cool Keeper program allows for max 100 hours of curtailment.  ",1]
["IDGeneral ServiceDLC Central ACWinter DR Event Hours","ID","General Service","DLC Central AC","Winter DR Event Hours","hours/year",0,0,1]
["IDGeneral ServiceDLC Central ACAnnual O&M Cost","ID","General Service","DLC Central AC","Annual O&M Cost","$/participant/year",13,"Assume 5% of equipment + install costs.",1]
["IDGeneral ServiceDLC Central ACAnnual Program Administration Cost","ID","General Service","DLC Central AC","Annual Program Administration Cost","$/yr",7165.4187834512149,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceDLC Central ACCost of Equip + Install","ID","General Service","DLC Central AC","Cost of Equip + Install","$/tech",260,"$100 installation cost. Idaho Power at 10,000 quantity pays $160 per switch.  I believe Avista volumes would be the same or less per order, making the cost $160 or greater.",1]
["IDGeneral ServiceDLC Central ACCost of Equip + Install (per kW basis)","ID","General Service","DLC Central AC","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceDLC Central ACDe-rate","ID","General Service","DLC Central AC","De-rate","capacity equivalence factor",1,0,1]
[{"$f":"B642&C642&D642&E642","v":"IDGeneral ServiceDLC Central ACNet to Gross Ratio (free ridership)"},"ID","General Service","DLC Central AC","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceDLC Central ACPer Customer Annual Marketing/Recruitment Cost","ID","General Service","DLC Central AC","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"25% Higher than Residential",1]
["IDGeneral ServiceDLC Central ACPer Participant Annual Incentive","ID","General Service","DLC Central AC","Per Participant Annual Incentive","$/participant/year",38,"Assumed participants have less than 5.5 tons of AC unit. Incentive level provided by PacifiCorp.",1]
["IDGeneral ServiceDLC Central ACPer kW Annual Incentive","ID","General Service","DLC Central AC","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceDLC Central ACProgram Development Cost","ID","General Service","DLC Central AC","Program Development Cost","$/program",5971.1823195426796,0,1]
["IDGeneral ServiceDLC Central ACProgram Life","ID","General Service","DLC Central AC","Program Life","years",8,0,1]
["IDGeneral ServiceDLC Central ACProgram Start Year","ID","General Service","DLC Central AC","Program Start Year","year",2022,0,1]
["IDResidentialDLC Water HeatingSummer DR Event Hours","ID","Residential","DLC Water Heating","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["IDResidentialDLC Water HeatingWinter DR Event Hours","ID","Residential","DLC Water Heating","Winter DR Event Hours","hours/year",50,"Split 50 hrs summer, and 50 hrs winter",1]
["IDResidentialDLC Water HeatingAnnual O&M Cost","ID","Residential","DLC Water Heating","Annual O&M Cost","$/participant/year",23,"Assume 5% of equipment + install costs.",1]
["IDResidentialDLC Water HeatingAnnual Program Administration Cost","ID","Residential","DLC Water Heating","Annual Program Administration Cost","$/yr",81900,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Water HeatingCost of Equip + Install","ID","Residential","DLC Water Heating","Cost of Equip + Install","$/tech",460,"Assumed $160 cost for water heater switch (same as cooling switch cost), plus $200 installation cost. Cost of Permit and License is $100 for res and $125 for C&I",1]
["IDResidentialDLC Water HeatingCost of Equip + Install (per kW basis)","ID","Residential","DLC Water Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialDLC Water HeatingDe-rate","ID","Residential","DLC Water Heating","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialDLC Water HeatingNet to Gross Ratio (free ridership)","ID","Residential","DLC Water Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialDLC Water HeatingPer Customer Annual Marketing/Recruitment Cost","ID","Residential","DLC Water Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Same as DLC CAC",1]
["IDResidentialDLC Water HeatingPer Participant Annual Incentive","ID","Residential","DLC Water Heating","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["IDResidentialDLC Water HeatingPer kW Annual Incentive","ID","Residential","DLC Water Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialDLC Water HeatingProgram Development Cost","ID","Residential","DLC Water Heating","Program Development Cost","$/program",68250,0,1]
["IDResidentialDLC Water HeatingProgram Life","ID","Residential","DLC Water Heating","Program Life","years",8,0,1]
["IDResidentialDLC Water HeatingProgram Start Year","ID","Residential","DLC Water Heating","Program Start Year","year",2022,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["IDGeneral ServiceDLC Water HeatingSummer DR Event Hours","ID","General Service","DLC Water Heating","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["IDGeneral ServiceDLC Water HeatingWinter DR Event Hours","ID","General Service","DLC Water Heating","Winter DR Event Hours","hours/year",50,"Split 50 hrs summer, and 50 hrs winter",1]
["IDGeneral ServiceDLC Water HeatingAnnual O&M Cost","ID","General Service","DLC Water Heating","Annual O&M Cost","$/participant/year",24.25,"Assume 5% of equipment + install costs.",1]
["IDGeneral ServiceDLC Water HeatingAnnual Program Administration Cost","ID","General Service","DLC Water Heating","Annual Program Administration Cost","$/yr",8100,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceDLC Water HeatingCost of Equip + Install","ID","General Service","DLC Water Heating","Cost of Equip + Install","$/tech",485,"Assumed $160 cost for water heater switch (same as cooling switch cost), plus $200 installation cost. Cost of Permit and License is $100 for res and $125 for C&I",1]
["IDGeneral ServiceDLC Water HeatingCost of Equip + Install (per kW basis)","ID","General Service","DLC Water Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceDLC Water HeatingDe-rate","ID","General Service","DLC Water Heating","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceDLC Water HeatingNet to Gross Ratio (free ridership)","ID","General Service","DLC Water Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceDLC Water HeatingPer Customer Annual Marketing/Recruitment Cost","ID","General Service","DLC Water Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Same as DLC CAC",1]
["IDGeneral ServiceDLC Water HeatingPer Participant Annual Incentive","ID","General Service","DLC Water Heating","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["IDGeneral ServiceDLC Water HeatingPer kW Annual Incentive","ID","General Service","DLC Water Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceDLC Water HeatingProgram Development Cost","ID","General Service","DLC Water Heating","Program Development Cost","$/program",6750,"No startup costs; Framework already exists for current programs",1]
["IDGeneral ServiceDLC Water HeatingProgram Life","ID","General Service","DLC Water Heating","Program Life","years",8,0,1]
["IDGeneral ServiceDLC Water HeatingProgram Start Year","ID","General Service","DLC Water Heating","Program Start Year","year",2022,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["IDResidentialCTA-2045 WHSummer DR Event Hours","ID","Residential","CTA-2045 WH","Summer DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDResidentialCTA-2045 WHWinter DR Event Hours","ID","Residential","CTA-2045 WH","Winter DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDResidentialCTA-2045 WHAnnual O&M Cost","ID","Residential","CTA-2045 WH","Annual O&M Cost","$/participant/year",0,0,1]
["IDResidentialCTA-2045 WHAnnual Program Administration Cost","ID","Residential","CTA-2045 WH","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["IDResidentialCTA-2045 WHCost of Equip + Install","ID","Residential","CTA-2045 WH","Cost of Equip + Install","$/tech",0,"$150 for module and comms, 20% of customers will need help provisioning these (an additional $100 for these customers)- average customer will be $170",1]
["IDResidentialCTA-2045 WHCost of Equip + Install (per kW basis)","ID","Residential","CTA-2045 WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialCTA-2045 WHDe-rate","ID","Residential","CTA-2045 WH","De-rate","capacity equivalence factor",0,0,1]
["IDResidentialCTA-2045 WHNet to Gross Ratio (free ridership)","ID","Residential","CTA-2045 WH","Net to Gross Ratio (free ridership)","ratio",0,0,1]
["IDResidentialCTA-2045 WHPer Customer Annual Marketing/Recruitment Cost","ID","Residential","CTA-2045 WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as Smart Thermostats",1]
["IDResidentialCTA-2045 WHPer Participant Annual Incentive","ID","Residential","CTA-2045 WH","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["IDResidentialCTA-2045 WHPer kW Annual Incentive","ID","Residential","CTA-2045 WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialCTA-2045 WHProgram Development Cost","ID","Residential","CTA-2045 WH","Program Development Cost","$/program",0,0,1]
["IDResidentialCTA-2045 WHProgram Life","ID","Residential","CTA-2045 WH","Program Life","years",0,0,1]
["IDResidentialCTA-2045 WHProgram Start Year","ID","Residential","CTA-2045 WH","Program Start Year","year",0,0,1]
["IDGeneral ServiceCTA-2045 WHSummer DR Event Hours","ID","General Service","CTA-2045 WH","Summer DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDGeneral ServiceCTA-2045 WHWinter DR Event Hours","ID","General Service","CTA-2045 WH","Winter DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDGeneral ServiceCTA-2045 WHAnnual O&M Cost","ID","General Service","CTA-2045 WH","Annual O&M Cost","$/participant/year",0,0,1]
["IDGeneral ServiceCTA-2045 WHAnnual Program Administration Cost","ID","General Service","CTA-2045 WH","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceCTA-2045 WHCost of Equip + Install","ID","General Service","CTA-2045 WH","Cost of Equip + Install","$/tech",0,"$150 for module and comms, 20% of customers will need help provisioning these (an additional $100 install cost for these customers)- average customer will be $170",1]
["IDGeneral ServiceCTA-2045 WHCost of Equip + Install (per kW basis)","ID","General Service","CTA-2045 WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceCTA-2045 WHDe-rate","ID","General Service","CTA-2045 WH","De-rate","capacity equivalence factor",0,0,1]
["IDGeneral ServiceCTA-2045 WHNet to Gross Ratio (free ridership)","ID","General Service","CTA-2045 WH","Net to Gross Ratio (free ridership)","ratio",0,0,1]
["IDGeneral ServiceCTA-2045 WHPer Customer Annual Marketing/Recruitment Cost","ID","General Service","CTA-2045 WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as Smart Thermostats",1]
["IDGeneral ServiceCTA-2045 WHPer Participant Annual Incentive","ID","General Service","CTA-2045 WH","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["IDGeneral ServiceCTA-2045 WHPer kW Annual Incentive","ID","General Service","CTA-2045 WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceCTA-2045 WHProgram Development Cost","ID","General Service","CTA-2045 WH","Program Development Cost","$/program",0,"No startup costs; Framework already exists for current programs",1]
["IDGeneral ServiceCTA-2045 WHProgram Life","ID","General Service","CTA-2045 WH","Program Life","years",0,0,1]
["IDGeneral ServiceCTA-2045 WHProgram Start Year","ID","General Service","CTA-2045 WH","Program Start Year","year",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingSummer DR Event Hours","ID","Residential","DLC Smart Thermostats - Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
[{"$f":"B706&C706&D706&E706","v":"IDResidentialDLC Smart Thermostats - CoolingWinter DR Event Hours"},"ID","Residential","DLC Smart Thermostats - Cooling","Winter DR Event Hours","hours/year",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingAnnual O&M Cost","ID","Residential","DLC Smart Thermostats - Cooling","Annual O&M Cost","$/participant/year",44,"Pacificorp:Assume 5% of equipment+install costs",1]
["IDResidentialDLC Smart Thermostats - CoolingAnnual Program Administration Cost","ID","Residential","DLC Smart Thermostats - Cooling","Annual Program Administration Cost","$/yr",25562.612843506638,0,1]
["IDResidentialDLC Smart Thermostats - CoolingCost of Equip + Install","ID","Residential","DLC Smart Thermostats - Cooling","Cost of Equip + Install","$/tech",0,"BYOT",1]
["IDResidentialDLC Smart Thermostats - CoolingCost of Equip + Install (per kW basis)","ID","Residential","DLC Smart Thermostats - Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingDe-rate","ID","Residential","DLC Smart Thermostats - Cooling","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialDLC Smart Thermostats - CoolingNet to Gross Ratio (free ridership)","ID","Residential","DLC Smart Thermostats - Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialDLC Smart Thermostats - CoolingPer Customer Annual Marketing/Recruitment Cost","ID","Residential","DLC Smart Thermostats - Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["IDResidentialDLC Smart Thermostats - CoolingPer Participant Annual Incentive","ID","Residential","DLC Smart Thermostats - Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["IDResidentialDLC Smart Thermostats - CoolingPer kW Annual Incentive","ID","Residential","DLC Smart Thermostats - Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialDLC Smart Thermostats - CoolingProgram Development Cost","ID","Residential","DLC Smart Thermostats - Cooling","Program Development Cost","$/program",21302.177369588866,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Smart Thermostats - CoolingProgram Life","ID","Residential","DLC Smart Thermostats - Cooling","Program Life","years",10,0,1]
["IDResidentialDLC Smart Thermostats - CoolingProgram Start Year","ID","Residential","DLC Smart Thermostats - Cooling","Program Start Year","year",2022,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingSummer DR Event Hours","ID","General Service","DLC Smart Thermostats - Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingWinter DR Event Hours","ID","General Service","DLC Smart Thermostats - Cooling","Winter DR Event Hours","hours/year",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingAnnual O&M Cost","ID","General Service","DLC Smart Thermostats - Cooling","Annual O&M Cost","$/participant/year",44,"Average subscription fees for EE and DR program management",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingAnnual Program Administration Cost","ID","General Service","DLC Smart Thermostats - Cooling","Annual Program Administration Cost","$/yr",7165.4187834512149,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingCost of Equip + Install","ID","General Service","DLC Smart Thermostats - Cooling","Cost of Equip + Install","$/tech",0,"Bring Your Own Thermostat program",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingCost of Equip + Install (per kW basis)","ID","General Service","DLC Smart Thermostats - Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingDe-rate","ID","General Service","DLC Smart Thermostats - Cooling","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingNet to Gross Ratio (free ridership)","ID","General Service","DLC Smart Thermostats - Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingPer Customer Annual Marketing/Recruitment Cost","ID","General Service","DLC Smart Thermostats - Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingPer Participant Annual Incentive","ID","General Service","DLC Smart Thermostats - Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingPer kW Annual Incentive","ID","General Service","DLC Smart Thermostats - Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingProgram Development Cost","ID","General Service","DLC Smart Thermostats - Cooling","Program Development Cost","$/program",5971.1823195426796,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingProgram Life","ID","General Service","DLC Smart Thermostats - Cooling","Program Life","years",10,0,1]
["IDGeneral ServiceDLC Smart Thermostats - CoolingProgram Start Year","ID","General Service","DLC Smart Thermostats - Cooling","Program Start Year","year",2022,0,1]
["IDResidentialDLC Smart Thermostats - HeatingSummer DR Event Hours","ID","Residential","DLC Smart Thermostats - Heating","Summer DR Event Hours","hours/year",0,0,1]
["IDResidentialDLC Smart Thermostats - HeatingWinter DR Event Hours","ID","Residential","DLC Smart Thermostats - Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["IDResidentialDLC Smart Thermostats - HeatingAnnual O&M Cost","ID","Residential","DLC Smart Thermostats - Heating","Annual O&M Cost","$/participant/year",44,"Pacificorp:Assume 5% of equipment+install costs",1]
["IDResidentialDLC Smart Thermostats - HeatingAnnual Program Administration Cost","ID","Residential","DLC Smart Thermostats - Heating","Annual Program Administration Cost","$/yr",26731.068315754954,0,1]
["IDResidentialDLC Smart Thermostats - HeatingCost of Equip + Install","ID","Residential","DLC Smart Thermostats - Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["IDResidentialDLC Smart Thermostats - HeatingCost of Equip + Install (per kW basis)","ID","Residential","DLC Smart Thermostats - Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialDLC Smart Thermostats - HeatingDe-rate","ID","Residential","DLC Smart Thermostats - Heating","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialDLC Smart Thermostats - HeatingNet to Gross Ratio (free ridership)","ID","Residential","DLC Smart Thermostats - Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialDLC Smart Thermostats - HeatingPer Customer Annual Marketing/Recruitment Cost","ID","Residential","DLC Smart Thermostats - Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["IDResidentialDLC Smart Thermostats - HeatingPer Participant Annual Incentive","ID","Residential","DLC Smart Thermostats - Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["IDResidentialDLC Smart Thermostats - HeatingPer kW Annual Incentive","ID","Residential","DLC Smart Thermostats - Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialDLC Smart Thermostats - HeatingProgram Development Cost","ID","Residential","DLC Smart Thermostats - Heating","Program Development Cost","$/program",22275.890263129128,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Smart Thermostats - HeatingProgram Life","ID","Residential","DLC Smart Thermostats - Heating","Program Life","years",10,0,1]
["IDResidentialDLC Smart Thermostats - HeatingProgram Start Year","ID","Residential","DLC Smart Thermostats - Heating","Program Start Year","year",2022,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingSummer DR Event Hours","ID","General Service","DLC Smart Thermostats - Heating","Summer DR Event Hours","hours/year",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingWinter DR Event Hours","ID","General Service","DLC Smart Thermostats - Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingAnnual O&M Cost","ID","General Service","DLC Smart Thermostats - Heating","Annual O&M Cost","$/participant/year",44,"Average subscription fees for EE and DR program management",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingAnnual Program Administration Cost","ID","General Service","DLC Smart Thermostats - Heating","Annual Program Administration Cost","$/yr",5757.3793047367071,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingCost of Equip + Install","ID","General Service","DLC Smart Thermostats - Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingCost of Equip + Install (per kW basis)","ID","General Service","DLC Smart Thermostats - Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingDe-rate","ID","General Service","DLC Smart Thermostats - Heating","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingNet to Gross Ratio (free ridership)","ID","General Service","DLC Smart Thermostats - Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingPer Customer Annual Marketing/Recruitment Cost","ID","General Service","DLC Smart Thermostats - Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingPer Participant Annual Incentive","ID","General Service","DLC Smart Thermostats - Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingPer kW Annual Incentive","ID","General Service","DLC Smart Thermostats - Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingProgram Development Cost","ID","General Service","DLC Smart Thermostats - Heating","Program Development Cost","$/program",4797.8160872805893,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingProgram Life","ID","General Service","DLC Smart Thermostats - Heating","Program Life","years",10,0,1]
["IDGeneral ServiceDLC Smart Thermostats - HeatingProgram Start Year","ID","General Service","DLC Smart Thermostats - Heating","Program Start Year","year",2022,0,1]
["IDResidentialDLC Smart AppliancesSummer DR Event Hours","ID","Residential","DLC Smart Appliances","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["IDResidentialDLC Smart AppliancesWinter DR Event Hours","ID","Residential","DLC Smart Appliances","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["IDResidentialDLC Smart AppliancesAnnual O&M Cost","ID","Residential","DLC Smart Appliances","Annual O&M Cost","$/participant/year",0,0,1]
["IDResidentialDLC Smart AppliancesAnnual Program Administration Cost","ID","Residential","DLC Smart Appliances","Annual Program Administration Cost","$/yr",28153.81550372317,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Smart AppliancesCost of Equip + Install","ID","Residential","DLC Smart Appliances","Cost of Equip + Install","$/tech",300,"Google research revealed devices range anywhere between $150 -400. Need wifi hub or some sort to connect devices. See email between Dave & Victoria 5-9-16",1]
["IDResidentialDLC Smart AppliancesCost of Equip + Install (per kW basis)","ID","Residential","DLC Smart Appliances","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialDLC Smart AppliancesDe-rate","ID","Residential","DLC Smart Appliances","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialDLC Smart AppliancesNet to Gross Ratio (free ridership)","ID","Residential","DLC Smart Appliances","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialDLC Smart AppliancesPer Customer Annual Marketing/Recruitment Cost","ID","Residential","DLC Smart Appliances","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
[{"$f":"B770&C770&D770&E770","v":"IDResidentialDLC Smart AppliancesPer Participant Annual Incentive"},"ID","Residential","DLC Smart Appliances","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDResidentialDLC Smart AppliancesPer kW Annual Incentive","ID","Residential","DLC Smart Appliances","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialDLC Smart AppliancesProgram Development Cost","ID","Residential","DLC Smart Appliances","Program Development Cost","$/program",23461.512919769306,"Share of Cost as noted in table at right",1]
["IDResidentialDLC Smart AppliancesProgram Life","ID","Residential","DLC Smart Appliances","Program Life","years",8,0,1]
["IDResidentialDLC Smart AppliancesProgram Start Year","ID","Residential","DLC Smart Appliances","Program Start Year","year",2022,0,1]
["IDGeneral ServiceDLC Smart AppliancesSummer DR Event Hours","ID","General Service","DLC Smart Appliances","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["IDGeneral ServiceDLC Smart AppliancesWinter DR Event Hours","ID","General Service","DLC Smart Appliances","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["IDGeneral ServiceDLC Smart AppliancesAnnual O&M Cost","ID","General Service","DLC Smart Appliances","Annual O&M Cost","$/participant/year",0,0,1]
["IDGeneral ServiceDLC Smart AppliancesAnnual Program Administration Cost","ID","General Service","DLC Smart Appliances","Annual Program Administration Cost","$/yr",4042.9072889271533,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceDLC Smart AppliancesCost of Equip + Install","ID","General Service","DLC Smart Appliances","Cost of Equip + Install","$/tech",300,"Google research revealed devices range anywhere between $150 -400. Need wifi hub or some sort to connect devices. See email between Dave & Victoria 5-9-16",1]
["IDGeneral ServiceDLC Smart AppliancesCost of Equip + Install (per kW basis)","ID","General Service","DLC Smart Appliances","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceDLC Smart AppliancesDe-rate","ID","General Service","DLC Smart Appliances","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceDLC Smart AppliancesNet to Gross Ratio (free ridership)","ID","General Service","DLC Smart Appliances","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceDLC Smart AppliancesPer Customer Annual Marketing/Recruitment Cost","ID","General Service","DLC Smart Appliances","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
["IDGeneral ServiceDLC Smart AppliancesPer Participant Annual Incentive","ID","General Service","DLC Smart Appliances","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDGeneral ServiceDLC Smart AppliancesPer kW Annual Incentive","ID","General Service","DLC Smart Appliances","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceDLC Smart AppliancesProgram Development Cost","ID","General Service","DLC Smart Appliances","Program Development Cost","$/program",3369.0894074392945,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceDLC Smart AppliancesProgram Life","ID","General Service","DLC Smart Appliances","Program Life","years",8,0,1]
["IDGeneral ServiceDLC Smart AppliancesProgram Start Year","ID","General Service","DLC Smart Appliances","Program Start Year","year",2022,0,1]
["IDGeneral ServiceThird Party ContractsSummer DR Event Hours","ID","General Service","Third Party Contracts","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDGeneral ServiceThird Party ContractsWinter DR Event Hours","ID","General Service","Third Party Contracts","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDGeneral ServiceThird Party ContractsAnnual O&M Cost","ID","General Service","Third Party Contracts","Annual O&M Cost","$/participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["IDGeneral ServiceThird Party ContractsAnnual Program Administration Cost","ID","General Service","Third Party Contracts","Annual Program Administration Cost","$/yr",0,0,1]
["IDGeneral ServiceThird Party ContractsCost of Equip + Install","ID","General Service","Third Party Contracts","Cost of Equip + Install","$/tech",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["IDGeneral ServiceThird Party ContractsCost of Equip + Install (per kW basis)","ID","General Service","Third Party Contracts","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceThird Party ContractsDe-rate","ID","General Service","Third Party Contracts","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceThird Party ContractsNet to Gross Ratio (free ridership)","ID","General Service","Third Party Contracts","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceThird Party ContractsPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Third Party Contracts","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["IDGeneral ServiceThird Party ContractsPer Participant Annual Incentive","ID","General Service","Third Party Contracts","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDGeneral ServiceThird Party ContractsPer kW Annual Incentive","ID","General Service","Third Party Contracts","Per kW Annual Incentive","$/kW @meter/year",0,"MPSC Demand Response Market Assessment",1]
["IDGeneral ServiceThird Party ContractsAnnual O&M Cost per MW","ID","General Service","Third Party Contracts","Annual O&M Cost per MW","$/MW @meter",80000,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["IDGeneral ServiceThird Party ContractsProgram Development Cost","ID","General Service","Third Party Contracts","Program Development Cost","$/program",0,0,1]
["IDGeneral ServiceThird Party ContractsProgram Life","ID","General Service","Third Party Contracts","Program Life","years",3,0,1]
["IDGeneral ServiceThird Party ContractsProgram Start Year","ID","General Service","Third Party Contracts","Program Start Year","year",2022,0,1]
["IDLarge General ServiceThird Party ContractsSummer DR Event Hours","ID","Large General Service","Third Party Contracts","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDLarge General ServiceThird Party ContractsWinter DR Event Hours","ID","Large General Service","Third Party Contracts","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDLarge General ServiceThird Party ContractsAnnual O&M Cost","ID","Large General Service","Third Party Contracts","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceThird Party ContractsAnnual Program Administration Cost","ID","Large General Service","Third Party Contracts","Annual Program Administration Cost","$/yr",0,0,1]
["IDLarge General ServiceThird Party ContractsCost of Equip + Install","ID","Large General Service","Third Party Contracts","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceThird Party ContractsCost of Equip + Install (per kW basis)","ID","Large General Service","Third Party Contracts","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceThird Party ContractsDe-rate","ID","Large General Service","Third Party Contracts","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceThird Party ContractsNet to Gross Ratio (free ridership)","ID","Large General Service","Third Party Contracts","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceThird Party ContractsPer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Third Party Contracts","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceThird Party ContractsPer Participant Annual Incentive","ID","Large General Service","Third Party Contracts","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDLarge General ServiceThird Party ContractsPer kW Annual Incentive","ID","Large General Service","Third Party Contracts","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["IDLarge General ServiceThird Party ContractsAnnual O&M Cost per MW","ID","Large General Service","Third Party Contracts","Annual O&M Cost per MW","$/MW @meter",80000,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceThird Party ContractsProgram Development Cost","ID","Large General Service","Third Party Contracts","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
["IDLarge General ServiceThird Party ContractsProgram Life","ID","Large General Service","Third Party Contracts","Program Life","years",3,0,1]
["IDLarge General ServiceThird Party ContractsProgram Start Year","ID","Large General Service","Third Party Contracts","Program Start Year","year",2022,0,1]
["IDExtra Large General ServiceThird Party ContractsSummer DR Event Hours","ID","Extra Large General Service","Third Party Contracts","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDExtra Large General ServiceThird Party ContractsWinter DR Event Hours","ID","Extra Large General Service","Third Party Contracts","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDExtra Large General ServiceThird Party ContractsAnnual O&M Cost","ID","Extra Large General Service","Third Party Contracts","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceThird Party ContractsAnnual Program Administration Cost","ID","Extra Large General Service","Third Party Contracts","Annual Program Administration Cost","$/yr",0,0,1]
["IDExtra Large General ServiceThird Party ContractsCost of Equip + Install","ID","Extra Large General Service","Third Party Contracts","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceThird Party ContractsCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Third Party Contracts","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceThird Party ContractsDe-rate","ID","Extra Large General Service","Third Party Contracts","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceThird Party ContractsNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Third Party Contracts","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceThird Party ContractsPer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Third Party Contracts","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceThird Party ContractsPer Participant Annual Incentive","ID","Extra Large General Service","Third Party Contracts","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDExtra Large General ServiceThird Party ContractsPer kW Annual Incentive","ID","Extra Large General Service","Third Party Contracts","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["IDExtra Large General ServiceThird Party ContractsAnnual O&M Cost per MW","ID","Extra Large General Service","Third Party Contracts","Annual O&M Cost per MW","$/MW @meter",80000,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceThird Party ContractsProgram Development Cost","ID","Extra Large General Service","Third Party Contracts","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
["IDExtra Large General ServiceThird Party ContractsProgram Life","ID","Extra Large General Service","Third Party Contracts","Program Life","years",3,0,1]
["IDExtra Large General ServiceThird Party ContractsProgram Start Year","ID","Extra Large General Service","Third Party Contracts","Program Start Year","year",2022,0,1]
[{"$f":"B834&C834&D834&E834","v":"IDResidentialTime-of-Use Opt-inSummer DR Event Hours"},"ID","Residential","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDResidentialTime-of-Use Opt-inWinter DR Event Hours","ID","Residential","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDResidentialTime-of-Use Opt-inAnnual O&M Cost","ID","Residential","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["IDResidentialTime-of-Use Opt-inAnnual Program Administration Cost","ID","Residential","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",24623.179468762242,0,1]
["IDResidentialTime-of-Use Opt-inCost of Equip + Install","ID","Residential","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["IDResidentialTime-of-Use Opt-inCost of Equip + Install (per kW basis)","ID","Residential","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialTime-of-Use Opt-inDe-rate","ID","Residential","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialTime-of-Use Opt-inNet to Gross Ratio (free ridership)","ID","Residential","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDResidentialTime-of-Use Opt-inPer Participant Annual Incentive","ID","Residential","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDResidentialTime-of-Use Opt-inPer kW Annual Incentive","ID","Residential","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialTime-of-Use Opt-inProgram Development Cost","ID","Residential","Time-of-Use Opt-in","Program Development Cost","$/program",20519.316223968533,0,1]
["IDResidentialTime-of-Use Opt-inProgram Life","ID","Residential","Time-of-Use Opt-in","Program Life","years",10,0,1]
["IDResidentialTime-of-Use Opt-inProgram Start Year","ID","Residential","Time-of-Use Opt-in","Program Start Year","year",2022,0,1]
["IDGeneral ServiceTime-of-Use Opt-inSummer DR Event Hours","ID","General Service","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDGeneral ServiceTime-of-Use Opt-inWinter DR Event Hours","ID","General Service","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDGeneral ServiceTime-of-Use Opt-inAnnual O&M Cost","ID","General Service","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-inAnnual Program Administration Cost","ID","General Service","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",227.30184158655646,0,1]
["IDGeneral ServiceTime-of-Use Opt-inCost of Equip + Install","ID","General Service","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-inCost of Equip + Install (per kW basis)","ID","General Service","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-inDe-rate","ID","General Service","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceTime-of-Use Opt-inNet to Gross Ratio (free ridership)","ID","General Service","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",72,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDGeneral ServiceTime-of-Use Opt-inPer Participant Annual Incentive","ID","General Service","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDGeneral ServiceTime-of-Use Opt-inPer kW Annual Incentive","ID","General Service","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-inProgram Development Cost","ID","General Service","Time-of-Use Opt-in","Program Development Cost","$/program",189.41820132213039,0,1]
["IDGeneral ServiceTime-of-Use Opt-inProgram Life","ID","General Service","Time-of-Use Opt-in","Program Life","years",10,0,1]
["IDGeneral ServiceTime-of-Use Opt-inProgram Start Year","ID","General Service","Time-of-Use Opt-in","Program Start Year","year",2022,0,1]
["IDLarge General ServiceTime-of-Use Opt-inSummer DR Event Hours","ID","Large General Service","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDLarge General ServiceTime-of-Use Opt-inWinter DR Event Hours","ID","Large General Service","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDLarge General ServiceTime-of-Use Opt-inAnnual O&M Cost","ID","Large General Service","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-inAnnual Program Administration Cost","ID","Large General Service","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",3700.986910928867,0,1]
["IDLarge General ServiceTime-of-Use Opt-inCost of Equip + Install","ID","Large General Service","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-inCost of Equip + Install (per kW basis)","ID","Large General Service","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-inDe-rate","ID","Large General Service","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceTime-of-Use Opt-inNet to Gross Ratio (free ridership)","ID","Large General Service","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",72,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDLarge General ServiceTime-of-Use Opt-inPer Participant Annual Incentive","ID","Large General Service","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDLarge General ServiceTime-of-Use Opt-inPer kW Annual Incentive","ID","Large General Service","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-inProgram Development Cost","ID","Large General Service","Time-of-Use Opt-in","Program Development Cost","$/program",3084.1557591073893,0,1]
["IDLarge General ServiceTime-of-Use Opt-inProgram Life","ID","Large General Service","Time-of-Use Opt-in","Program Life","years",10,0,1]
["IDLarge General ServiceTime-of-Use Opt-inProgram Start Year","ID","Large General Service","Time-of-Use Opt-in","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["IDExtra Large General ServiceTime-of-Use Opt-inSummer DR Event Hours","ID","Extra Large General Service","Time-of-Use Opt-in","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDExtra Large General ServiceTime-of-Use Opt-inWinter DR Event Hours","ID","Extra Large General Service","Time-of-Use Opt-in","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDExtra Large General ServiceTime-of-Use Opt-inAnnual O&M Cost","ID","Extra Large General Service","Time-of-Use Opt-in","Annual O&M Cost","$/participant/year",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inAnnual Program Administration Cost","ID","Extra Large General Service","Time-of-Use Opt-in","Annual Program Administration Cost","$/yr",2335.8631277744703,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inCost of Equip + Install","ID","Extra Large General Service","Time-of-Use Opt-in","Cost of Equip + Install","$/tech",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Time-of-Use Opt-in","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inDe-rate","ID","Extra Large General Service","Time-of-Use Opt-in","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Time-of-Use Opt-in","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inPer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Time-of-Use Opt-in","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",72,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDExtra Large General ServiceTime-of-Use Opt-inPer Participant Annual Incentive","ID","Extra Large General Service","Time-of-Use Opt-in","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDExtra Large General ServiceTime-of-Use Opt-inPer kW Annual Incentive","ID","Extra Large General Service","Time-of-Use Opt-in","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inProgram Development Cost","ID","Extra Large General Service","Time-of-Use Opt-in","Program Development Cost","$/program",1946.5526064787255,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inProgram Life","ID","Extra Large General Service","Time-of-Use Opt-in","Program Life","years",10,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-inProgram Start Year","ID","Extra Large General Service","Time-of-Use Opt-in","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["IDResidentialTime-of-Use Opt-outSummer DR Event Hours","ID","Residential","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDResidentialTime-of-Use Opt-outWinter DR Event Hours","ID","Residential","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDResidentialTime-of-Use Opt-outAnnual O&M Cost","ID","Residential","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["IDResidentialTime-of-Use Opt-outAnnual Program Administration Cost","ID","Residential","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",21766.617555379384,0,1]
["IDResidentialTime-of-Use Opt-outCost of Equip + Install","ID","Residential","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["IDResidentialTime-of-Use Opt-outCost of Equip + Install (per kW basis)","ID","Residential","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialTime-of-Use Opt-outDe-rate","ID","Residential","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialTime-of-Use Opt-outNet to Gross Ratio (free ridership)","ID","Residential","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
[{"$f":"B898&C898&D898&E898","v":"IDResidentialTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost"},"ID","Residential","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDResidentialTime-of-Use Opt-outPer Participant Annual Incentive","ID","Residential","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDResidentialTime-of-Use Opt-outPer kW Annual Incentive","ID","Residential","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialTime-of-Use Opt-outProgram Development Cost","ID","Residential","Time-of-Use Opt-out","Program Development Cost","$/program",18138.847962816155,0,1]
["IDResidentialTime-of-Use Opt-outProgram Life","ID","Residential","Time-of-Use Opt-out","Program Life","years",10,0,1]
["IDResidentialTime-of-Use Opt-outProgram Start Year","ID","Residential","Time-of-Use Opt-out","Program Start Year","year",2022,0,1]
["IDGeneral ServiceTime-of-Use Opt-outSummer DR Event Hours","ID","General Service","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDGeneral ServiceTime-of-Use Opt-outWinter DR Event Hours","ID","General Service","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDGeneral ServiceTime-of-Use Opt-outAnnual O&M Cost","ID","General Service","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-outAnnual Program Administration Cost","ID","General Service","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",336.85710285148031,0,1]
["IDGeneral ServiceTime-of-Use Opt-outCost of Equip + Install","ID","General Service","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-outCost of Equip + Install (per kW basis)","ID","General Service","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-outDe-rate","ID","General Service","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceTime-of-Use Opt-outNet to Gross Ratio (free ridership)","ID","General Service","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",72,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDGeneral ServiceTime-of-Use Opt-outPer Participant Annual Incentive","ID","General Service","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDGeneral ServiceTime-of-Use Opt-outPer kW Annual Incentive","ID","General Service","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceTime-of-Use Opt-outProgram Development Cost","ID","General Service","Time-of-Use Opt-out","Program Development Cost","$/program",280.71425237623362,0,1]
["IDGeneral ServiceTime-of-Use Opt-outProgram Life","ID","General Service","Time-of-Use Opt-out","Program Life","years",10,0,1]
["IDGeneral ServiceTime-of-Use Opt-outProgram Start Year","ID","General Service","Time-of-Use Opt-out","Program Start Year","year",2022,0,1]
["IDLarge General ServiceTime-of-Use Opt-outSummer DR Event Hours","ID","Large General Service","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDLarge General ServiceTime-of-Use Opt-outWinter DR Event Hours","ID","Large General Service","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDLarge General ServiceTime-of-Use Opt-outAnnual O&M Cost","ID","Large General Service","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-outAnnual Program Administration Cost","ID","Large General Service","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",5484.7937869962361,0,1]
["IDLarge General ServiceTime-of-Use Opt-outCost of Equip + Install","ID","Large General Service","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-outCost of Equip + Install (per kW basis)","ID","Large General Service","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-outDe-rate","ID","Large General Service","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceTime-of-Use Opt-outNet to Gross Ratio (free ridership)","ID","Large General Service","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",72,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDLarge General ServiceTime-of-Use Opt-outPer Participant Annual Incentive","ID","Large General Service","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDLarge General ServiceTime-of-Use Opt-outPer kW Annual Incentive","ID","Large General Service","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDLarge General ServiceTime-of-Use Opt-outProgram Development Cost","ID","Large General Service","Time-of-Use Opt-out","Program Development Cost","$/program",4570.66148916353,0,1]
["IDLarge General ServiceTime-of-Use Opt-outProgram Life","ID","Large General Service","Time-of-Use Opt-out","Program Life","years",10,0,1]
["IDLarge General ServiceTime-of-Use Opt-outProgram Start Year","ID","Large General Service","Time-of-Use Opt-out","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["IDExtra Large General ServiceTime-of-Use Opt-outSummer DR Event Hours","ID","Extra Large General Service","Time-of-Use Opt-out","Summer DR Event Hours","hours/year",528,"Six hours on-peak period each summer weekday",1]
["IDExtra Large General ServiceTime-of-Use Opt-outWinter DR Event Hours","ID","Extra Large General Service","Time-of-Use Opt-out","Winter DR Event Hours","hours/year",528,"Six hours on-peak period each winter weekday too, except for Utah",1]
["IDExtra Large General ServiceTime-of-Use Opt-outAnnual O&M Cost","ID","Extra Large General Service","Time-of-Use Opt-out","Annual O&M Cost","$/participant/year",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outAnnual Program Administration Cost","ID","Extra Large General Service","Time-of-Use Opt-out","Annual Program Administration Cost","$/yr",3461.7057230487599,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outCost of Equip + Install","ID","Extra Large General Service","Time-of-Use Opt-out","Cost of Equip + Install","$/tech",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Time-of-Use Opt-out","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outDe-rate","ID","Extra Large General Service","Time-of-Use Opt-out","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Time-of-Use Opt-out","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outPer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Time-of-Use Opt-out","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",72,"1.5x standatd $50 marketing cost because it involves more education on kW rate blocks",1]
["IDExtra Large General ServiceTime-of-Use Opt-outPer Participant Annual Incentive","ID","Extra Large General Service","Time-of-Use Opt-out","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDExtra Large General ServiceTime-of-Use Opt-outPer kW Annual Incentive","ID","Extra Large General Service","Time-of-Use Opt-out","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outProgram Development Cost","ID","Extra Large General Service","Time-of-Use Opt-out","Program Development Cost","$/program",2884.7547692072999,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outProgram Life","ID","Extra Large General Service","Time-of-Use Opt-out","Program Life","years",10,0,1]
["IDExtra Large General ServiceTime-of-Use Opt-outProgram Start Year","ID","Extra Large General Service","Time-of-Use Opt-out","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["IDResidentialVariable Peak Pricing RatesSummer DR Event Hours","ID","Residential","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",80,"Top 60 summer system hours ",1]
["IDResidentialVariable Peak Pricing RatesWinter DR Event Hours","ID","Residential","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",80,"Using summer hours except for UT",1]
["IDResidentialVariable Peak Pricing RatesAnnual O&M Cost","ID","Residential","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
["IDResidentialVariable Peak Pricing RatesAnnual Program Administration Cost","ID","Residential","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",23932.45635646455,0,1]
["IDResidentialVariable Peak Pricing RatesCost of Equip + Install","ID","Residential","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,"Assume zero, but would be $470 w tech costs included.  Based on PacifiCorp estimate: $270 for PCT, plus $200 for installation",1]
["IDResidentialVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","ID","Residential","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialVariable Peak Pricing RatesDe-rate","ID","Residential","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","ID","Residential","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
["IDResidentialVariable Peak Pricing RatesPer Participant Annual Incentive","ID","Residential","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDResidentialVariable Peak Pricing RatesPer kW Annual Incentive","ID","Residential","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialVariable Peak Pricing RatesProgram Development Cost","ID","Residential","Variable Peak Pricing Rates","Program Development Cost","$/program",19943.713630387127,0,1]
["IDResidentialVariable Peak Pricing RatesProgram Life","ID","Residential","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["IDResidentialVariable Peak Pricing RatesProgram Start Year","ID","Residential","Variable Peak Pricing Rates","Program Start Year","year",2022,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesSummer DR Event Hours","ID","General Service","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",40,"Top 40 summer system hours ",1]
["IDGeneral ServiceVariable Peak Pricing RatesWinter DR Event Hours","ID","General Service","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",40,"Using summer hours except for UT",1]
[{"$f":"B962&C962&D962&E962","v":"IDGeneral ServiceVariable Peak Pricing RatesAnnual O&M Cost"},"ID","General Service","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesAnnual Program Administration Cost","ID","General Service","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",2544.2516785217658,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesCost of Equip + Install","ID","General Service","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,"Assume zero, but would be $470 w tech costs included.  Based on PacifiCorp estimate: $270 for PCT, plus $200 for installation",1]
["IDGeneral ServiceVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","ID","General Service","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesDe-rate","ID","General Service","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","ID","General Service","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesPer Participant Annual Incentive","ID","General Service","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDGeneral ServiceVariable Peak Pricing RatesPer kW Annual Incentive","ID","General Service","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesProgram Development Cost","ID","General Service","Variable Peak Pricing Rates","Program Development Cost","$/program",2120.2097321014717,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesProgram Life","ID","General Service","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["IDGeneral ServiceVariable Peak Pricing RatesProgram Start Year","ID","General Service","Variable Peak Pricing Rates","Program Start Year","year",2022,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesSummer DR Event Hours","ID","Large General Service","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",40,"Top 40 summer system hours ",1]
["IDLarge General ServiceVariable Peak Pricing RatesWinter DR Event Hours","ID","Large General Service","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",40,"Using summer hours except for UT",1]
["IDLarge General ServiceVariable Peak Pricing RatesAnnual O&M Cost","ID","Large General Service","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesAnnual Program Administration Cost","ID","Large General Service","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",3186.6275916142417,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesCost of Equip + Install","ID","Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,"No equipment cost because assuming they have their own technology (like a Energy Management System etc) to control their processes",1]
["IDLarge General ServiceVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","ID","Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"Currently zero, but $360/kW if tech costs included. Based on Auto-DR tech enablement costs. $300/kW is incentive level offered by SCE for Auto-DR participants, and is expected to cover a large fraction of costs. 20% adder included to recognize some additional expenses on the part of the customer. ",1]
["IDLarge General ServiceVariable Peak Pricing RatesDe-rate","ID","Large General Service","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","ID","Large General Service","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",200,"Assumed 4X Residential recruitment costs",1]
["IDLarge General ServiceVariable Peak Pricing RatesPer Participant Annual Incentive","ID","Large General Service","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDLarge General ServiceVariable Peak Pricing RatesPer kW Annual Incentive","ID","Large General Service","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesProgram Development Cost","ID","Large General Service","Variable Peak Pricing Rates","Program Development Cost","$/program",2655.522993011868,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesProgram Life","ID","Large General Service","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["IDLarge General ServiceVariable Peak Pricing RatesProgram Start Year","ID","Large General Service","Variable Peak Pricing Rates","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesSummer DR Event Hours","ID","Extra Large General Service","Variable Peak Pricing Rates","Summer DR Event Hours","hours/year",40,"Top 40 summer system hours ",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesWinter DR Event Hours","ID","Extra Large General Service","Variable Peak Pricing Rates","Winter DR Event Hours","hours/year",40,"Using summer hours except for UT",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesAnnual O&M Cost","ID","Extra Large General Service","Variable Peak Pricing Rates","Annual O&M Cost","$/participant/year",0,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesAnnual Program Administration Cost","ID","Extra Large General Service","Variable Peak Pricing Rates","Annual Program Administration Cost","$/yr",1669.7970502826836,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesCost of Equip + Install","ID","Extra Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install","$/tech",0,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Variable Peak Pricing Rates","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"Currently zero, but $360/kW if tech costs included. Based on Auto-DR tech enablement costs. $300/kW is incentive level offered by SCE for Auto-DR participants, and is expected to cover a large fraction of costs. 20% adder included to recognize some additional expenses on the part of the customer. ",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesDe-rate","ID","Extra Large General Service","Variable Peak Pricing Rates","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Variable Peak Pricing Rates","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesPer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Variable Peak Pricing Rates","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",400,"Assumed 2X Large C&I recruitment costs",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesPer Participant Annual Incentive","ID","Extra Large General Service","Variable Peak Pricing Rates","Per Participant Annual Incentive","$/participant/year",0,"Incentive built into rate design",1]
["IDExtra Large General ServiceVariable Peak Pricing RatesPer kW Annual Incentive","ID","Extra Large General Service","Variable Peak Pricing Rates","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesProgram Development Cost","ID","Extra Large General Service","Variable Peak Pricing Rates","Program Development Cost","$/program",1391.4975419022362,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesProgram Life","ID","Extra Large General Service","Variable Peak Pricing Rates","Program Life","years",10,0,1]
["IDExtra Large General ServiceVariable Peak Pricing RatesProgram Start Year","ID","Extra Large General Service","Variable Peak Pricing Rates","Program Start Year","year",2022,"Metering capability exists in this class, but need 2 years before program can be implemented and ramp up.",1]
["IDLarge General ServiceReal Time PricingSummer DR Event Hours","ID","Large General Service","Real Time Pricing","Summer DR Event Hours","hours/year","","",1]
["IDLarge General ServiceReal Time PricingWinter DR Event Hours","ID","Large General Service","Real Time Pricing","Winter DR Event Hours","hours/year","","",1]
["IDLarge General ServiceReal Time PricingAnnual O&M Cost","ID","Large General Service","Real Time Pricing","Annual O&M Cost","$/participant/year","","",1]
["IDLarge General ServiceReal Time PricingAnnual Program Administration Cost","ID","Large General Service","Real Time Pricing","Annual Program Administration Cost","$/yr","","",1]
["IDLarge General ServiceReal Time PricingCost of Equip + Install","ID","Large General Service","Real Time Pricing","Cost of Equip + Install","$/tech","","",1]
["IDLarge General ServiceReal Time PricingCost of Equip + Install (per kW basis)","ID","Large General Service","Real Time Pricing","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["IDLarge General ServiceReal Time PricingDe-rate","ID","Large General Service","Real Time Pricing","De-rate","capacity equivalence factor","","",1]
["IDLarge General ServiceReal Time PricingNet to Gross Ratio (free ridership)","ID","Large General Service","Real Time Pricing","Net to Gross Ratio (free ridership)","ratio","","",1]
["IDLarge General ServiceReal Time PricingPer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Real Time Pricing","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["IDLarge General ServiceReal Time PricingPer Participant Annual Incentive","ID","Large General Service","Real Time Pricing","Per Participant Annual Incentive","$/participant/year","","",1]
["IDLarge General ServiceReal Time PricingPer kW Annual Incentive","ID","Large General Service","Real Time Pricing","Per kW Annual Incentive","$/kW @meter/year","","",1]
["IDLarge General ServiceReal Time PricingProgram Development Cost","ID","Large General Service","Real Time Pricing","Program Development Cost","$/program","","",1]
["IDLarge General ServiceReal Time PricingProgram Life","ID","Large General Service","Real Time Pricing","Program Life","years","","",1]
["IDLarge General ServiceReal Time PricingProgram Start Year","ID","Large General Service","Real Time Pricing","Program Start Year","year","","",1]
["IDExtra Large General ServiceReal Time PricingSummer DR Event Hours","ID","Extra Large General Service","Real Time Pricing","Summer DR Event Hours","hours/year","","",1]
["IDExtra Large General ServiceReal Time PricingWinter DR Event Hours","ID","Extra Large General Service","Real Time Pricing","Winter DR Event Hours","hours/year","","",1]
["IDExtra Large General ServiceReal Time PricingAnnual O&M Cost","ID","Extra Large General Service","Real Time Pricing","Annual O&M Cost","$/participant/year","","",1]
["IDExtra Large General ServiceReal Time PricingAnnual Program Administration Cost","ID","Extra Large General Service","Real Time Pricing","Annual Program Administration Cost","$/yr","","",1]
["IDExtra Large General ServiceReal Time PricingCost of Equip + Install","ID","Extra Large General Service","Real Time Pricing","Cost of Equip + Install","$/tech","","",1]
["IDExtra Large General ServiceReal Time PricingCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Real Time Pricing","Cost of Equip + Install (per kW basis)","$/kW @meter","","",1]
["IDExtra Large General ServiceReal Time PricingDe-rate","ID","Extra Large General Service","Real Time Pricing","De-rate","capacity equivalence factor","","",1]
["IDExtra Large General ServiceReal Time PricingNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Real Time Pricing","Net to Gross Ratio (free ridership)","ratio","","",1]
["IDExtra Large General ServiceReal Time PricingPer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Real Time Pricing","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year","","",1]
["IDExtra Large General ServiceReal Time PricingPer Participant Annual Incentive","ID","Extra Large General Service","Real Time Pricing","Per Participant Annual Incentive","$/participant/year","","",1]
[{"$f":"B1026&C1026&D1026&E1026","v":"IDExtra Large General ServiceReal Time PricingPer kW Annual Incentive"},"ID","Extra Large General Service","Real Time Pricing","Per kW Annual Incentive","$/kW @meter/year","","",1]
["IDExtra Large General ServiceReal Time PricingProgram Development Cost","ID","Extra Large General Service","Real Time Pricing","Program Development Cost","$/program","","",1]
["IDExtra Large General ServiceReal Time PricingProgram Life","ID","Extra Large General Service","Real Time Pricing","Program Life","years","","",1]
["IDExtra Large General ServiceReal Time PricingProgram Start Year","ID","Extra Large General Service","Real Time Pricing","Program Start Year","year","","",1]
["IDGeneral ServiceThermal Energy StorageSummer DR Event Hours","ID","General Service","Thermal Energy Storage","Summer DR Event Hours","hours/year",36,"Same as TOU, six hours on peak period each summer",1]
["IDGeneral ServiceThermal Energy StorageWinter DR Event Hours","ID","General Service","Thermal Energy Storage","Winter DR Event Hours","hours/year",0,0,1]
["IDGeneral ServiceThermal Energy StorageAnnual O&M Cost","ID","General Service","Thermal Energy Storage","Annual O&M Cost","$/participant/year",84,"Assumption of 5% equipment costs",1]
["IDGeneral ServiceThermal Energy StorageAnnual Program Administration Cost","ID","General Service","Thermal Energy Storage","Annual Program Administration Cost","$/yr",19841.339887667156,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceThermal Energy StorageCost of Equip + Install","ID","General Service","Thermal Energy Storage","Cost of Equip + Install","$/tech",0,0,1]
["IDGeneral ServiceThermal Energy StorageCost of Equip + Install (per kW basis)","ID","General Service","Thermal Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",1680,"Utility Dive Article, Ice Energy Implementer cost",1]
["IDGeneral ServiceThermal Energy StorageDe-rate","ID","General Service","Thermal Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceThermal Energy StorageNet to Gross Ratio (free ridership)","ID","General Service","Thermal Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceThermal Energy StoragePer Customer Annual Marketing/Recruitment Cost","ID","General Service","Thermal Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",100,"Assumption $100 for RAP C&I, MAP = RAPx1.2",1]
["IDGeneral ServiceThermal Energy StoragePer Participant Annual Incentive","ID","General Service","Thermal Energy Storage","Per Participant Annual Incentive","$/participant/year",0,"No incentive. Program purchases & installs unit.",1]
["IDGeneral ServiceThermal Energy StoragePer kW Annual Incentive","ID","General Service","Thermal Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceThermal Energy StorageProgram Development Cost","ID","General Service","Thermal Energy Storage","Program Development Cost","$/program",16534.449906389294,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceThermal Energy StorageProgram Life","ID","General Service","Thermal Energy Storage","Program Life","years",20,0,1]
["IDGeneral ServiceThermal Energy StorageProgram Start Year","ID","General Service","Thermal Energy Storage","Program Start Year","year",2022,0,1]
["IDLarge General ServiceThermal Energy StorageSummer DR Event Hours","ID","Large General Service","Thermal Energy Storage","Summer DR Event Hours","hours/year",36,"Same as TOU, six hours on peak period each summer",1]
["IDLarge General ServiceThermal Energy StorageWinter DR Event Hours","ID","Large General Service","Thermal Energy Storage","Winter DR Event Hours","hours/year",0,0,1]
["IDLarge General ServiceThermal Energy StorageAnnual O&M Cost","ID","Large General Service","Thermal Energy Storage","Annual O&M Cost","$/participant/year",420,"Assumption of 5% equipment costs",1]
["IDLarge General ServiceThermal Energy StorageAnnual Program Administration Cost","ID","Large General Service","Thermal Energy Storage","Annual Program Administration Cost","$/yr",16019.353810473196,"Share of Cost as noted in table at right",1]
["IDLarge General ServiceThermal Energy StorageCost of Equip + Install","ID","Large General Service","Thermal Energy Storage","Cost of Equip + Install","$/tech",0,0,1]
["IDLarge General ServiceThermal Energy StorageCost of Equip + Install (per kW basis)","ID","Large General Service","Thermal Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",8400,"Utility Dive Article, Ice Energy Implementer cost",1]
["IDLarge General ServiceThermal Energy StorageDe-rate","ID","Large General Service","Thermal Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceThermal Energy StorageNet to Gross Ratio (free ridership)","ID","Large General Service","Thermal Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceThermal Energy StoragePer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Thermal Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",100,"Assumption $100 for RAP C&I, MAP = RAPx1.2",1]
["IDLarge General ServiceThermal Energy StoragePer Participant Annual Incentive","ID","Large General Service","Thermal Energy Storage","Per Participant Annual Incentive","$/participant/year",0,"No incentive. Program purchases & installs unit.",1]
["IDLarge General ServiceThermal Energy StoragePer kW Annual Incentive","ID","Large General Service","Thermal Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDLarge General ServiceThermal Energy StorageProgram Development Cost","ID","Large General Service","Thermal Energy Storage","Program Development Cost","$/program",13349.461508727663,"Share of Cost as noted in table at right",1]
["IDLarge General ServiceThermal Energy StorageProgram Life","ID","Large General Service","Thermal Energy Storage","Program Life","years",20,0,1]
["IDLarge General ServiceThermal Energy StorageProgram Start Year","ID","Large General Service","Thermal Energy Storage","Program Start Year","year",2022,0,1]
["IDExtra Large General ServiceThermal Energy StorageSummer DR Event Hours","ID","Extra Large General Service","Thermal Energy Storage","Summer DR Event Hours","hours/year",36,"Same as TOU, six hours on peak period each summer",1]
["IDExtra Large General ServiceThermal Energy StorageWinter DR Event Hours","ID","Extra Large General Service","Thermal Energy Storage","Winter DR Event Hours","hours/year",0,0,1]
["IDExtra Large General ServiceThermal Energy StorageAnnual O&M Cost","ID","Extra Large General Service","Thermal Energy Storage","Annual O&M Cost","$/participant/year",420,"Assumption of 5% equipment costs",1]
["IDExtra Large General ServiceThermal Energy StorageAnnual Program Administration Cost","ID","Extra Large General Service","Thermal Energy Storage","Annual Program Administration Cost","$/yr",158.10220899647004,"Share of Cost as noted in table at right",1]
["IDExtra Large General ServiceThermal Energy StorageCost of Equip + Install","ID","Extra Large General Service","Thermal Energy Storage","Cost of Equip + Install","$/tech",0,0,1]
["IDExtra Large General ServiceThermal Energy StorageCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Thermal Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",8400,"Utility Dive Article, Ice Energy Implementer cost",1]
["IDExtra Large General ServiceThermal Energy StorageDe-rate","ID","Extra Large General Service","Thermal Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceThermal Energy StorageNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Thermal Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceThermal Energy StoragePer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Thermal Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",100,"Assumption $100 for RAP C&I, MAP = RAPx1.2",1]
["IDExtra Large General ServiceThermal Energy StoragePer Participant Annual Incentive","ID","Extra Large General Service","Thermal Energy Storage","Per Participant Annual Incentive","$/participant/year",0,"No incentive. Program purchases & installs unit.",1]
["IDExtra Large General ServiceThermal Energy StoragePer kW Annual Incentive","ID","Extra Large General Service","Thermal Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDExtra Large General ServiceThermal Energy StorageProgram Development Cost","ID","Extra Large General Service","Thermal Energy Storage","Program Development Cost","$/program",131.7518408303917,"Share of Cost as noted in table at right",1]
["IDExtra Large General ServiceThermal Energy StorageProgram Life","ID","Extra Large General Service","Thermal Energy Storage","Program Life","years",20,0,1]
["IDExtra Large General ServiceThermal Energy StorageProgram Start Year","ID","Extra Large General Service","Thermal Energy Storage","Program Start Year","year",2022,0,1]
["IDResidentialBattery Energy StorageSummer DR Event Hours","ID","Residential","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDResidentialBattery Energy StorageWinter DR Event Hours","ID","Residential","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDResidentialBattery Energy StorageAnnual O&M Cost","ID","Residential","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDResidentialBattery Energy StorageAnnual Program Administration Cost","ID","Residential","Battery Energy Storage","Annual Program Administration Cost","$/yr",26847.881157877229,"half FTE @ $150,000",1]
["IDResidentialBattery Energy StorageCost of Equip + Install","ID","Residential","Battery Energy Storage","Cost of Equip + Install","$/tech",6912,"Lazard's cost - avg. of hi/low case for Residential Lithium-Ion Batteries - low=$1,662, hi=$2,178 ",1]
["IDResidentialBattery Energy StorageCost of Equip + Install (per kW basis)","ID","Residential","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialBattery Energy StorageDe-rate","ID","Residential","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialBattery Energy StorageNet to Gross Ratio (free ridership)","ID","Residential","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","ID","Residential","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDResidentialBattery Energy StoragePer Participant Annual Incentive","ID","Residential","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDResidentialBattery Energy StoragePer kW Annual Incentive","ID","Residential","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialBattery Energy StorageProgram Development Cost","ID","Residential","Battery Energy Storage","Program Development Cost","$/program",14915.489532154017,0,1]
["IDResidentialBattery Energy StorageProgram Life","ID","Residential","Battery Energy Storage","Program Life","years",15,"NREL",1]
["IDResidentialBattery Energy StorageProgram Start Year","ID","Residential","Battery Energy Storage","Program Start Year","year",2022,0,1]
["IDGeneral ServiceBattery Energy StorageSummer DR Event Hours","ID","General Service","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDGeneral ServiceBattery Energy StorageWinter DR Event Hours","ID","General Service","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDGeneral ServiceBattery Energy StorageAnnual O&M Cost","ID","General Service","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDGeneral ServiceBattery Energy StorageAnnual Program Administration Cost","ID","General Service","Battery Energy Storage","Annual Program Administration Cost","$/yr",3855.3742177886193,"half FTE @ $150,000",1]
[{"$f":"B1090&C1090&D1090&E1090","v":"IDGeneral ServiceBattery Energy StorageCost of Equip + Install"},"ID","General Service","Battery Energy Storage","Cost of Equip + Install","$/tech",6542.4,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["IDGeneral ServiceBattery Energy StorageCost of Equip + Install (per kW basis)","ID","General Service","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceBattery Energy StorageDe-rate","ID","General Service","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceBattery Energy StorageNet to Gross Ratio (free ridership)","ID","General Service","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","ID","General Service","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDGeneral ServiceBattery Energy StoragePer Participant Annual Incentive","ID","General Service","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDGeneral ServiceBattery Energy StoragePer kW Annual Incentive","ID","General Service","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceBattery Energy StorageProgram Development Cost","ID","General Service","Battery Energy Storage","Program Development Cost","$/program",2141.8745654381219,0,1]
["IDGeneral ServiceBattery Energy StorageProgram Life","ID","General Service","Battery Energy Storage","Program Life","years",15,"NREL",1]
["IDGeneral ServiceBattery Energy StorageProgram Start Year","ID","General Service","Battery Energy Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["IDLarge General ServiceBattery Energy StorageSummer DR Event Hours","ID","Large General Service","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDLarge General ServiceBattery Energy StorageWinter DR Event Hours","ID","Large General Service","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDLarge General ServiceBattery Energy StorageAnnual O&M Cost","ID","Large General Service","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDLarge General ServiceBattery Energy StorageAnnual Program Administration Cost","ID","Large General Service","Battery Energy Storage","Annual Program Administration Cost","$/yr",1556.3617179130367,"half FTE @ $150,000",1]
["IDLarge General ServiceBattery Energy StorageCost of Equip + Install","ID","Large General Service","Battery Energy Storage","Cost of Equip + Install","$/tech",49068,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["IDLarge General ServiceBattery Energy StorageCost of Equip + Install (per kW basis)","ID","Large General Service","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDLarge General ServiceBattery Energy StorageDe-rate","ID","Large General Service","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceBattery Energy StorageNet to Gross Ratio (free ridership)","ID","Large General Service","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDLarge General ServiceBattery Energy StoragePer Participant Annual Incentive","ID","Large General Service","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDLarge General ServiceBattery Energy StoragePer kW Annual Incentive","ID","Large General Service","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDLarge General ServiceBattery Energy StorageProgram Development Cost","ID","Large General Service","Battery Energy Storage","Program Development Cost","$/program",864.64539884057604,0,1]
["IDLarge General ServiceBattery Energy StorageProgram Life","ID","Large General Service","Battery Energy Storage","Program Life","years",15,"NREL",1]
["IDLarge General ServiceBattery Energy StorageProgram Start Year","ID","Large General Service","Battery Energy Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["IDExtra Large General ServiceBattery Energy StorageSummer DR Event Hours","ID","Extra Large General Service","Battery Energy Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDExtra Large General ServiceBattery Energy StorageWinter DR Event Hours","ID","Extra Large General Service","Battery Energy Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDExtra Large General ServiceBattery Energy StorageAnnual O&M Cost","ID","Extra Large General Service","Battery Energy Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDExtra Large General ServiceBattery Energy StorageAnnual Program Administration Cost","ID","Extra Large General Service","Battery Energy Storage","Annual Program Administration Cost","$/yr",15.36043391704847,"Calculated",1]
["IDExtra Large General ServiceBattery Energy StorageCost of Equip + Install","ID","Extra Large General Service","Battery Energy Storage","Cost of Equip + Install","$/tech",49068,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["IDExtra Large General ServiceBattery Energy StorageCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Battery Energy Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDExtra Large General ServiceBattery Energy StorageDe-rate","ID","Extra Large General Service","Battery Energy Storage","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceBattery Energy StorageNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Battery Energy Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceBattery Energy StoragePer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Battery Energy Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDExtra Large General ServiceBattery Energy StoragePer Participant Annual Incentive","ID","Extra Large General Service","Battery Energy Storage","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDExtra Large General ServiceBattery Energy StoragePer kW Annual Incentive","ID","Extra Large General Service","Battery Energy Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDExtra Large General ServiceBattery Energy StorageProgram Development Cost","ID","Extra Large General Service","Battery Energy Storage","Program Development Cost","$/program",8.5335743983602619,"Calculated",1]
["IDExtra Large General ServiceBattery Energy StorageProgram Life","ID","Extra Large General Service","Battery Energy Storage","Program Life","years",15,"NREL",1]
["IDExtra Large General ServiceBattery Energy StorageProgram Start Year","ID","Extra Large General Service","Battery Energy Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["IDResidentialAncillary CoolingSummer DR Event Hours","ID","Residential","Ancillary Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["IDResidentialAncillary CoolingWinter DR Event Hours","ID","Residential","Ancillary Cooling","Winter DR Event Hours","hours/year",0,0,1]
["IDResidentialAncillary CoolingAnnual O&M Cost","ID","Residential","Ancillary Cooling","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["IDResidentialAncillary CoolingAnnual Program Administration Cost","ID","Residential","Ancillary Cooling","Annual Program Administration Cost","$/yr",12781.306421753319,"Half for Ancillary- tied to participation reduction from parent program",1]
["IDResidentialAncillary CoolingCost of Equip + Install","ID","Residential","Ancillary Cooling","Cost of Equip + Install","$/tech",0,"BYOT",1]
["IDResidentialAncillary CoolingCost of Equip + Install (per kW basis)","ID","Residential","Ancillary Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialAncillary CoolingDe-rate","ID","Residential","Ancillary Cooling","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialAncillary CoolingNet to Gross Ratio (free ridership)","ID","Residential","Ancillary Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialAncillary CoolingPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Ancillary Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["IDResidentialAncillary CoolingPer Participant Annual Incentive","ID","Residential","Ancillary Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC. Adding $20 to account for ancillary service option",1]
["IDResidentialAncillary CoolingPer kW Annual Incentive","ID","Residential","Ancillary Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialAncillary CoolingProgram Development Cost","ID","Residential","Ancillary Cooling","Program Development Cost","$/program",10651.088684794433,"Half for Ancillary- tied to participation reduction from parent program",1]
["IDResidentialAncillary CoolingProgram Life","ID","Residential","Ancillary Cooling","Program Life","years",10,0,1]
["IDResidentialAncillary CoolingProgram Start Year","ID","Residential","Ancillary Cooling","Program Start Year","year",2022,0,1]
["IDGeneral ServiceAncillary CoolingSummer DR Event Hours","ID","General Service","Ancillary Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["IDGeneral ServiceAncillary CoolingWinter DR Event Hours","ID","General Service","Ancillary Cooling","Winter DR Event Hours","hours/year",0,0,1]
["IDGeneral ServiceAncillary CoolingAnnual O&M Cost","ID","General Service","Ancillary Cooling","Annual O&M Cost","$/participant/year",0,"Average subscription fees for EE and DR program management",1]
["IDGeneral ServiceAncillary CoolingAnnual Program Administration Cost","ID","General Service","Ancillary Cooling","Annual Program Administration Cost","$/yr",3582.7093917256075,"Half for Ancillary- tied to participation reduction from parent program",1]
["IDGeneral ServiceAncillary CoolingCost of Equip + Install","ID","General Service","Ancillary Cooling","Cost of Equip + Install","$/tech",0,"Bring Your Own Thermostat program",1]
["IDGeneral ServiceAncillary CoolingCost of Equip + Install (per kW basis)","ID","General Service","Ancillary Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceAncillary CoolingDe-rate","ID","General Service","Ancillary Cooling","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceAncillary CoolingNet to Gross Ratio (free ridership)","ID","General Service","Ancillary Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceAncillary CoolingPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Ancillary Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["IDGeneral ServiceAncillary CoolingPer Participant Annual Incentive","ID","General Service","Ancillary Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC. Adding $20 to account for ancillary service option",1]
["IDGeneral ServiceAncillary CoolingPer kW Annual Incentive","ID","General Service","Ancillary Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceAncillary CoolingProgram Development Cost","ID","General Service","Ancillary Cooling","Program Development Cost","$/program",2985.5911597713398,"Half for Ancillary- tied to participation reduction from parent program",1]
[{"$f":"B1154&C1154&D1154&E1154","v":"IDGeneral ServiceAncillary CoolingProgram Life"},"ID","General Service","Ancillary Cooling","Program Life","years",10,0,1]
["IDGeneral ServiceAncillary CoolingProgram Start Year","ID","General Service","Ancillary Cooling","Program Start Year","year",2022,0,1]
["IDResidentialAncillary HeatingSummer DR Event Hours","ID","Residential","Ancillary Heating","Summer DR Event Hours","hours/year",0,0,1]
["IDResidentialAncillary HeatingWinter DR Event Hours","ID","Residential","Ancillary Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["IDResidentialAncillary HeatingAnnual O&M Cost","ID","Residential","Ancillary Heating","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["IDResidentialAncillary HeatingAnnual Program Administration Cost","ID","Residential","Ancillary Heating","Annual Program Administration Cost","$/yr",13365.534157877477,"Half for Ancillary- tied to participation reduction from parent program",1]
["IDResidentialAncillary HeatingCost of Equip + Install","ID","Residential","Ancillary Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["IDResidentialAncillary HeatingCost of Equip + Install (per kW basis)","ID","Residential","Ancillary Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialAncillary HeatingDe-rate","ID","Residential","Ancillary Heating","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialAncillary HeatingNet to Gross Ratio (free ridership)","ID","Residential","Ancillary Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialAncillary HeatingPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Ancillary Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["IDResidentialAncillary HeatingPer Participant Annual Incentive","ID","Residential","Ancillary Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["IDResidentialAncillary HeatingPer kW Annual Incentive","ID","Residential","Ancillary Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialAncillary HeatingProgram Development Cost","ID","Residential","Ancillary Heating","Program Development Cost","$/program",11137.945131564564,"Half for Ancillary- tied to participation reduction from parent program",1]
["IDResidentialAncillary HeatingProgram Life","ID","Residential","Ancillary Heating","Program Life","years",10,0,1]
["IDResidentialAncillary HeatingProgram Start Year","ID","Residential","Ancillary Heating","Program Start Year","year",2022,0,1]
["IDGeneral ServiceAncillary HeatingSummer DR Event Hours","ID","General Service","Ancillary Heating","Summer DR Event Hours","hours/year",0,0,1]
["IDGeneral ServiceAncillary HeatingWinter DR Event Hours","ID","General Service","Ancillary Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["IDGeneral ServiceAncillary HeatingAnnual O&M Cost","ID","General Service","Ancillary Heating","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["IDGeneral ServiceAncillary HeatingAnnual Program Administration Cost","ID","General Service","Ancillary Heating","Annual Program Administration Cost","$/yr",2878.6896523683536,"Half for Ancillary- tied to participation reduction from parent program",1]
["IDGeneral ServiceAncillary HeatingCost of Equip + Install","ID","General Service","Ancillary Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["IDGeneral ServiceAncillary HeatingCost of Equip + Install (per kW basis)","ID","General Service","Ancillary Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceAncillary HeatingDe-rate","ID","General Service","Ancillary Heating","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceAncillary HeatingNet to Gross Ratio (free ridership)","ID","General Service","Ancillary Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceAncillary HeatingPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Ancillary Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["IDGeneral ServiceAncillary HeatingPer Participant Annual Incentive","ID","General Service","Ancillary Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["IDGeneral ServiceAncillary HeatingPer kW Annual Incentive","ID","General Service","Ancillary Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceAncillary HeatingProgram Development Cost","ID","General Service","Ancillary Heating","Program Development Cost","$/program",2398.9080436402946,"Half for Ancillary- tied to participation reduction from parent program",1]
["IDGeneral ServiceAncillary HeatingProgram Life","ID","General Service","Ancillary Heating","Program Life","years",10,0,1]
["IDGeneral ServiceAncillary HeatingProgram Start Year","ID","General Service","Ancillary Heating","Program Start Year","year",2022,0,1]
["IDResidentialAncillary WHSummer DR Event Hours","ID","Residential","Ancillary WH","Summer DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDResidentialAncillary WHWinter DR Event Hours","ID","Residential","Ancillary WH","Winter DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDResidentialAncillary WHAnnual O&M Cost","ID","Residential","Ancillary WH","Annual O&M Cost","$/participant/year",0,0,1]
["IDResidentialAncillary WHAnnual Program Administration Cost","ID","Residential","Ancillary WH","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["IDResidentialAncillary WHCost of Equip + Install","ID","Residential","Ancillary WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["IDResidentialAncillary WHCost of Equip + Install (per kW basis)","ID","Residential","Ancillary WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialAncillary WHDe-rate","ID","Residential","Ancillary WH","De-rate","capacity equivalence factor",0,0,1]
["IDResidentialAncillary WHNet to Gross Ratio (free ridership)","ID","Residential","Ancillary WH","Net to Gross Ratio (free ridership)","ratio",0,0,1]
["IDResidentialAncillary WHPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Ancillary WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as Smart Thermostats",1]
["IDResidentialAncillary WHPer Participant Annual Incentive","ID","Residential","Ancillary WH","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["IDResidentialAncillary WHPer kW Annual Incentive","ID","Residential","Ancillary WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialAncillary WHProgram Development Cost","ID","Residential","Ancillary WH","Program Development Cost","$/program",0,0,1]
["IDResidentialAncillary WHProgram Life","ID","Residential","Ancillary WH","Program Life","years",0,0,1]
["IDResidentialAncillary WHProgram Start Year","ID","Residential","Ancillary WH","Program Start Year","year",0,0,1]
["IDGeneral ServiceAncillary WHSummer DR Event Hours","ID","General Service","Ancillary WH","Summer DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDGeneral ServiceAncillary WHWinter DR Event Hours","ID","General Service","Ancillary WH","Winter DR Event Hours","hours/year",0,"25 total events around 3 hrs ea.",1]
["IDGeneral ServiceAncillary WHAnnual O&M Cost","ID","General Service","Ancillary WH","Annual O&M Cost","$/participant/year",0,0,1]
["IDGeneral ServiceAncillary WHAnnual Program Administration Cost","ID","General Service","Ancillary WH","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceAncillary WHCost of Equip + Install","ID","General Service","Ancillary WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["IDGeneral ServiceAncillary WHCost of Equip + Install (per kW basis)","ID","General Service","Ancillary WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceAncillary WHDe-rate","ID","General Service","Ancillary WH","De-rate","capacity equivalence factor",0,0,1]
["IDGeneral ServiceAncillary WHNet to Gross Ratio (free ridership)","ID","General Service","Ancillary WH","Net to Gross Ratio (free ridership)","ratio",0,0,1]
["IDGeneral ServiceAncillary WHPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Ancillary WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as Smart Thermostats",1]
["IDGeneral ServiceAncillary WHPer Participant Annual Incentive","ID","General Service","Ancillary WH","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["IDGeneral ServiceAncillary WHPer kW Annual Incentive","ID","General Service","Ancillary WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceAncillary WHProgram Development Cost","ID","General Service","Ancillary WH","Program Development Cost","$/program",0,"No startup costs; Framework already exists for current programs",1]
["IDGeneral ServiceAncillary WHProgram Life","ID","General Service","Ancillary WH","Program Life","years",0,0,1]
["IDGeneral ServiceAncillary WHProgram Start Year","ID","General Service","Ancillary WH","Program Start Year","year",0,0,1]
["IDResidentialAncillary DLC WHSummer DR Event Hours","ID","Residential","Ancillary DLC WH","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["IDResidentialAncillary DLC WHWinter DR Event Hours","ID","Residential","Ancillary DLC WH","Winter DR Event Hours","hours/year",50,"Split 50 hrs summer, and 50 hrs winter",1]
["IDResidentialAncillary DLC WHAnnual O&M Cost","ID","Residential","Ancillary DLC WH","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["IDResidentialAncillary DLC WHAnnual Program Administration Cost","ID","Residential","Ancillary DLC WH","Annual Program Administration Cost","$/yr",81900,"Share of Cost as noted in table at right",1]
["IDResidentialAncillary DLC WHCost of Equip + Install","ID","Residential","Ancillary DLC WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["IDResidentialAncillary DLC WHCost of Equip + Install (per kW basis)","ID","Residential","Ancillary DLC WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
[{"$f":"B1218&C1218&D1218&E1218","v":"IDResidentialAncillary DLC WHDe-rate"},"ID","Residential","Ancillary DLC WH","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialAncillary DLC WHNet to Gross Ratio (free ridership)","ID","Residential","Ancillary DLC WH","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialAncillary DLC WHPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Ancillary DLC WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Same as DLC CAC",1]
["IDResidentialAncillary DLC WHPer Participant Annual Incentive","ID","Residential","Ancillary DLC WH","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["IDResidentialAncillary DLC WHPer kW Annual Incentive","ID","Residential","Ancillary DLC WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialAncillary DLC WHProgram Development Cost","ID","Residential","Ancillary DLC WH","Program Development Cost","$/program",68250,0,1]
["IDResidentialAncillary DLC WHProgram Life","ID","Residential","Ancillary DLC WH","Program Life","years",8,0,1]
["IDResidentialAncillary DLC WHProgram Start Year","ID","Residential","Ancillary DLC WH","Program Start Year","year",2022,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["IDGeneral ServiceAncillary DLC WHSummer DR Event Hours","ID","General Service","Ancillary DLC WH","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["IDGeneral ServiceAncillary DLC WHWinter DR Event Hours","ID","General Service","Ancillary DLC WH","Winter DR Event Hours","hours/year",0,"Split 50 hrs summer, and 50 hrs winter",1]
["IDGeneral ServiceAncillary DLC WHAnnual O&M Cost","ID","General Service","Ancillary DLC WH","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["IDGeneral ServiceAncillary DLC WHAnnual Program Administration Cost","ID","General Service","Ancillary DLC WH","Annual Program Administration Cost","$/yr",8100,"Share of Cost as noted in table at right",1]
["IDGeneral ServiceAncillary DLC WHCost of Equip + Install","ID","General Service","Ancillary DLC WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["IDGeneral ServiceAncillary DLC WHCost of Equip + Install (per kW basis)","ID","General Service","Ancillary DLC WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceAncillary DLC WHDe-rate","ID","General Service","Ancillary DLC WH","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceAncillary DLC WHNet to Gross Ratio (free ridership)","ID","General Service","Ancillary DLC WH","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceAncillary DLC WHPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Ancillary DLC WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Same as DLC CAC",1]
["IDGeneral ServiceAncillary DLC WHPer Participant Annual Incentive","ID","General Service","Ancillary DLC WH","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["IDGeneral ServiceAncillary DLC WHPer kW Annual Incentive","ID","General Service","Ancillary DLC WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceAncillary DLC WHProgram Development Cost","ID","General Service","Ancillary DLC WH","Program Development Cost","$/program",6750,"No startup costs; Framework already exists for current programs",1]
["IDGeneral ServiceAncillary DLC WHProgram Life","ID","General Service","Ancillary DLC WH","Program Life","years",8,0,1]
["IDGeneral ServiceAncillary DLC WHProgram Start Year","ID","General Service","Ancillary DLC WH","Program Start Year","year",2022,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["IDResidentialAncillary EVSummer DR Event Hours","ID","Residential","Ancillary EV","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["IDResidentialAncillary EVWinter DR Event Hours","ID","Residential","Ancillary EV","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["IDResidentialAncillary EVAnnual O&M Cost","ID","Residential","Ancillary EV","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["IDResidentialAncillary EVAnnual Program Administration Cost","ID","Residential","Ancillary EV","Annual Program Administration Cost","$/yr",31037.278871407852,"Share of Cost as noted in table at right",1]
["IDResidentialAncillary EVCost of Equip + Install","ID","Residential","Ancillary EV","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["IDResidentialAncillary EVCost of Equip + Install (per kW basis)","ID","Residential","Ancillary EV","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialAncillary EVDe-rate","ID","Residential","Ancillary EV","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialAncillary EVNet to Gross Ratio (free ridership)","ID","Residential","Ancillary EV","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialAncillary EVPer Customer Annual Marketing/Recruitment Cost","ID","Residential","Ancillary EV","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,"Assumption $50 for RAP C&I, MAP = RAPx1.2",1]
["IDResidentialAncillary EVPer Participant Annual Incentive","ID","Residential","Ancillary EV","Per Participant Annual Incentive","$/participant/year",20,"Avista would provide a rate based charger or give a rebate on it, with no further incentives",1]
["IDResidentialAncillary EVPer kW Annual Incentive","ID","Residential","Ancillary EV","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialAncillary EVProgram Development Cost","ID","Residential","Ancillary EV","Program Development Cost","$/program",25864.399059506544,"Share of Cost as noted in table at right",1]
["IDResidentialAncillary EVProgram Life","ID","Residential","Ancillary EV","Program Life","years",8,0,1]
["IDResidentialAncillary EVProgram Start Year","ID","Residential","Ancillary EV","Program Start Year","year",2024,"Technology won’t be available for mass market till 2024",1]
["IDGeneral ServiceAncillary Third PartySummer DR Event Hours","ID","General Service","Ancillary Third Party","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDGeneral ServiceAncillary Third PartyWinter DR Event Hours","ID","General Service","Ancillary Third Party","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDGeneral ServiceAncillary Third PartyAnnual O&M Cost","ID","General Service","Ancillary Third Party","Annual O&M Cost","$/participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["IDGeneral ServiceAncillary Third PartyAnnual Program Administration Cost","ID","General Service","Ancillary Third Party","Annual Program Administration Cost","$/yr",0,0,1]
["IDGeneral ServiceAncillary Third PartyCost of Equip + Install","ID","General Service","Ancillary Third Party","Cost of Equip + Install","$/tech",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["IDGeneral ServiceAncillary Third PartyCost of Equip + Install (per kW basis)","ID","General Service","Ancillary Third Party","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceAncillary Third PartyDe-rate","ID","General Service","Ancillary Third Party","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceAncillary Third PartyNet to Gross Ratio (free ridership)","ID","General Service","Ancillary Third Party","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceAncillary Third PartyPer Customer Annual Marketing/Recruitment Cost","ID","General Service","Ancillary Third Party","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["IDGeneral ServiceAncillary Third PartyPer Participant Annual Incentive","ID","General Service","Ancillary Third Party","Per Participant Annual Incentive","$/participant/year",0,0,1]
["IDGeneral ServiceAncillary Third PartyPer kW Annual Incentive","ID","General Service","Ancillary Third Party","Per kW Annual Incentive","$/kW @meter/year",0,"MPSC Demand Response Market Assessment",1]
["IDGeneral ServiceAncillary Third PartyAnnual O&M Cost per MW","ID","General Service","Ancillary Third Party","Annual O&M Cost per MW","$/MW @meter",40000,"Half for Ancillary",1]
["IDGeneral ServiceAncillary Third PartyProgram Development Cost","ID","General Service","Ancillary Third Party","Program Development Cost","$/program",0,0,1]
["IDGeneral ServiceAncillary Third PartyProgram Life","ID","General Service","Ancillary Third Party","Program Life","years",3,0,1]
["IDGeneral ServiceAncillary Third PartyProgram Start Year","ID","General Service","Ancillary Third Party","Program Start Year","year",2022,0,1]
["IDLarge General ServiceAncillary Third PartySummer DR Event Hours","ID","Large General Service","Ancillary Third Party","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDLarge General ServiceAncillary Third PartyWinter DR Event Hours","ID","Large General Service","Ancillary Third Party","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDLarge General ServiceAncillary Third PartyAnnual O&M Cost","ID","Large General Service","Ancillary Third Party","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceAncillary Third PartyAnnual Program Administration Cost","ID","Large General Service","Ancillary Third Party","Annual Program Administration Cost","$/yr",0,0,1]
["IDLarge General ServiceAncillary Third PartyCost of Equip + Install","ID","Large General Service","Ancillary Third Party","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceAncillary Third PartyCost of Equip + Install (per kW basis)","ID","Large General Service","Ancillary Third Party","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceAncillary Third PartyDe-rate","ID","Large General Service","Ancillary Third Party","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceAncillary Third PartyNet to Gross Ratio (free ridership)","ID","Large General Service","Ancillary Third Party","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceAncillary Third PartyPer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Ancillary Third Party","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDLarge General ServiceAncillary Third PartyPer Participant Annual Incentive","ID","Large General Service","Ancillary Third Party","Per Participant Annual Incentive","$/participant/year",0,"Not sure what to put for incentives here",1]
["IDLarge General ServiceAncillary Third PartyPer kW Annual Incentive","ID","Large General Service","Ancillary Third Party","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["IDLarge General ServiceAncillary Third PartyAnnual O&M Cost per MW","ID","Large General Service","Ancillary Third Party","Annual O&M Cost per MW","$/MW @meter",40000,"Half for Ancillary",1]
["IDLarge General ServiceAncillary Third PartyProgram Development Cost","ID","Large General Service","Ancillary Third Party","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
[{"$f":"B1282&C1282&D1282&E1282","v":"IDLarge General ServiceAncillary Third PartyProgram Life"},"ID","Large General Service","Ancillary Third Party","Program Life","years",3,0,1]
["IDLarge General ServiceAncillary Third PartyProgram Start Year","ID","Large General Service","Ancillary Third Party","Program Start Year","year",2022,0,1]
["IDExtra Large General ServiceAncillary Third PartySummer DR Event Hours","ID","Extra Large General Service","Ancillary Third Party","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDExtra Large General ServiceAncillary Third PartyWinter DR Event Hours","ID","Extra Large General Service","Ancillary Third Party","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["IDExtra Large General ServiceAncillary Third PartyAnnual O&M Cost","ID","Extra Large General Service","Ancillary Third Party","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceAncillary Third PartyAnnual Program Administration Cost","ID","Extra Large General Service","Ancillary Third Party","Annual Program Administration Cost","$/yr",0,0,1]
["IDExtra Large General ServiceAncillary Third PartyCost of Equip + Install","ID","Extra Large General Service","Ancillary Third Party","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceAncillary Third PartyCost of Equip + Install (per kW basis)","ID","Extra Large General Service","Ancillary Third Party","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceAncillary Third PartyDe-rate","ID","Extra Large General Service","Ancillary Third Party","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceAncillary Third PartyNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Ancillary Third Party","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceAncillary Third PartyPer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Ancillary Third Party","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["IDExtra Large General ServiceAncillary Third PartyPer Participant Annual Incentive","ID","Extra Large General Service","Ancillary Third Party","Per Participant Annual Incentive","$/participant/year",0,"Not sure what to put for incentives here",1]
["IDExtra Large General ServiceAncillary Third PartyPer kW Annual Incentive","ID","Extra Large General Service","Ancillary Third Party","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["IDExtra Large General ServiceAncillary Third PartyAnnual O&M Cost per MW","ID","Extra Large General Service","Ancillary Third Party","Annual O&M Cost per MW","$/MW @meter",40000,"Half for Ancillary",1]
["IDExtra Large General ServiceAncillary Third PartyProgram Development Cost","ID","Extra Large General Service","Ancillary Third Party","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
["IDExtra Large General ServiceAncillary Third PartyProgram Life","ID","Extra Large General Service","Ancillary Third Party","Program Life","years",3,0,1]
["IDExtra Large General ServiceAncillary Third PartyProgram Start Year","ID","Extra Large General Service","Ancillary Third Party","Program Start Year","year",2022,0,1]
["IDResidentialAncillary Battery StorageSummer DR Event Hours","ID","Residential","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDResidentialAncillary Battery StorageWinter DR Event Hours","ID","Residential","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDResidentialAncillary Battery StorageAnnual O&M Cost","ID","Residential","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDResidentialAncillary Battery StorageAnnual Program Administration Cost","ID","Residential","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",26847.881157877229,"half FTE @ $150,000",1]
["IDResidentialAncillary Battery StorageCost of Equip + Install","ID","Residential","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["IDResidentialAncillary Battery StorageCost of Equip + Install (per kW basis)","ID","Residential","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDResidentialAncillary Battery StorageDe-rate","ID","Residential","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["IDResidentialAncillary Battery StorageNet to Gross Ratio (free ridership)","ID","Residential","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDResidentialAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","ID","Residential","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDResidentialAncillary Battery StoragePer Participant Annual Incentive","ID","Residential","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0,1]
["IDResidentialAncillary Battery StoragePer kW Annual Incentive","ID","Residential","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDResidentialAncillary Battery StorageProgram Development Cost","ID","Residential","Ancillary Battery Storage","Program Development Cost","$/program",14915.489532154017,0,1]
["IDResidentialAncillary Battery StorageProgram Life","ID","Residential","Ancillary Battery Storage","Program Life","years",15,"NREL",1]
["IDResidentialAncillary Battery StorageProgram Start Year","ID","Residential","Ancillary Battery Storage","Program Start Year","year",2022,0,1]
["IDGeneral ServiceAncillary Battery StorageSummer DR Event Hours","ID","General Service","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDGeneral ServiceAncillary Battery StorageWinter DR Event Hours","ID","General Service","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDGeneral ServiceAncillary Battery StorageAnnual O&M Cost","ID","General Service","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDGeneral ServiceAncillary Battery StorageAnnual Program Administration Cost","ID","General Service","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",3855.3742177886193,"half FTE @ $150,000",1]
["IDGeneral ServiceAncillary Battery StorageCost of Equip + Install","ID","General Service","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["IDGeneral ServiceAncillary Battery StorageCost of Equip + Install (per kW basis)","ID","General Service","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDGeneral ServiceAncillary Battery StorageDe-rate","ID","General Service","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["IDGeneral ServiceAncillary Battery StorageNet to Gross Ratio (free ridership)","ID","General Service","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDGeneral ServiceAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","ID","General Service","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDGeneral ServiceAncillary Battery StoragePer Participant Annual Incentive","ID","General Service","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0,1]
["IDGeneral ServiceAncillary Battery StoragePer kW Annual Incentive","ID","General Service","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDGeneral ServiceAncillary Battery StorageProgram Development Cost","ID","General Service","Ancillary Battery Storage","Program Development Cost","$/program",2141.8745654381219,0,1]
["IDGeneral ServiceAncillary Battery StorageProgram Life","ID","General Service","Ancillary Battery Storage","Program Life","years",15,"NREL",1]
["IDGeneral ServiceAncillary Battery StorageProgram Start Year","ID","General Service","Ancillary Battery Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["IDLarge General ServiceAncillary Battery StorageSummer DR Event Hours","ID","Large General Service","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDLarge General ServiceAncillary Battery StorageWinter DR Event Hours","ID","Large General Service","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDLarge General ServiceAncillary Battery StorageAnnual O&M Cost","ID","Large General Service","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDLarge General ServiceAncillary Battery StorageAnnual Program Administration Cost","ID","Large General Service","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",1556.3617179130367,"half FTE @ $150,000",1]
["IDLarge General ServiceAncillary Battery StorageCost of Equip + Install","ID","Large General Service","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["IDLarge General ServiceAncillary Battery StorageCost of Equip + Install (per kW basis)","ID","Large General Service","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDLarge General ServiceAncillary Battery StorageDe-rate","ID","Large General Service","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["IDLarge General ServiceAncillary Battery StorageNet to Gross Ratio (free ridership)","ID","Large General Service","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDLarge General ServiceAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","ID","Large General Service","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDLarge General ServiceAncillary Battery StoragePer Participant Annual Incentive","ID","Large General Service","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0,1]
["IDLarge General ServiceAncillary Battery StoragePer kW Annual Incentive","ID","Large General Service","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDLarge General ServiceAncillary Battery StorageProgram Development Cost","ID","Large General Service","Ancillary Battery Storage","Program Development Cost","$/program",864.64539884057604,0,1]
["IDLarge General ServiceAncillary Battery StorageProgram Life","ID","Large General Service","Ancillary Battery Storage","Program Life","years",15,"NREL",1]
["IDLarge General ServiceAncillary Battery StorageProgram Start Year","ID","Large General Service","Ancillary Battery Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["IDExtra Large General ServiceAncillary Battery StorageSummer DR Event Hours","ID","Extra Large General Service","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["IDExtra Large General ServiceAncillary Battery StorageWinter DR Event Hours","ID","Extra Large General Service","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["IDExtra Large General ServiceAncillary Battery StorageAnnual O&M Cost","ID","Extra Large General Service","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["IDExtra Large General ServiceAncillary Battery StorageAnnual Program Administration Cost","ID","Extra Large General Service","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",15.36043391704847,"Calculated",1]
["IDExtra Large General ServiceAncillary Battery StorageCost of Equip + Install","ID","Extra Large General Service","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
[{"$f":"B1346&C1346&D1346&E1346","v":"IDExtra Large General ServiceAncillary Battery StorageCost of Equip + Install (per kW basis)"},"ID","Extra Large General Service","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["IDExtra Large General ServiceAncillary Battery StorageDe-rate","ID","Extra Large General Service","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["IDExtra Large General ServiceAncillary Battery StorageNet to Gross Ratio (free ridership)","ID","Extra Large General Service","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["IDExtra Large General ServiceAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","ID","Extra Large General Service","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["IDExtra Large General ServiceAncillary Battery StoragePer Participant Annual Incentive","ID","Extra Large General Service","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0,1]
["IDExtra Large General ServiceAncillary Battery StoragePer kW Annual Incentive","ID","Extra Large General Service","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["IDExtra Large General ServiceAncillary Battery StorageProgram Development Cost","ID","Extra Large General Service","Ancillary Battery Storage","Program Development Cost","$/program",8.5335743983602619,"Calculated",1]
["IDExtra Large General ServiceAncillary Battery StorageProgram Life","ID","Extra Large General Service","Ancillary Battery Storage","Program Life","years",15,"NREL",1]
["IDExtra Large General ServiceAncillary Battery StorageProgram Start Year","ID","Extra Large General Service","Ancillary Battery Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["WAResidentialAncillary CoolingSummer DR Event Hours","WA","Residential","Ancillary Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAResidentialAncillary CoolingWinter DR Event Hours","WA","Residential","Ancillary Cooling","Winter DR Event Hours","hours/year",0,0,1]
["WAResidentialAncillary CoolingAnnual O&M Cost","WA","Residential","Ancillary Cooling","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["WAResidentialAncillary CoolingAnnual Program Administration Cost","WA","Residential","Ancillary Cooling","Annual Program Administration Cost","$/yr",23726.507547512552,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAResidentialAncillary CoolingCost of Equip + Install","WA","Residential","Ancillary Cooling","Cost of Equip + Install","$/tech",0,"BYOT",1]
["WAResidentialAncillary CoolingCost of Equip + Install (per kW basis)","WA","Residential","Ancillary Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialAncillary CoolingDe-rate","WA","Residential","Ancillary Cooling","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialAncillary CoolingNet to Gross Ratio (free ridership)","WA","Residential","Ancillary Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialAncillary CoolingPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Ancillary Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["WAResidentialAncillary CoolingPer Participant Annual Incentive","WA","Residential","Ancillary Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC. Adding $20 to account for ancillary service option",1]
["WAResidentialAncillary CoolingPer kW Annual Incentive","WA","Residential","Ancillary Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialAncillary CoolingProgram Development Cost","WA","Residential","Ancillary Cooling","Program Development Cost","$/program",19772.089622927127,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAResidentialAncillary CoolingProgram Life","WA","Residential","Ancillary Cooling","Program Life","years",10,0,1]
["WAResidentialAncillary CoolingProgram Start Year","WA","Residential","Ancillary Cooling","Program Start Year","year",2022,0,1]
["WAGeneral ServiceAncillary CoolingSummer DR Event Hours","WA","General Service","Ancillary Cooling","Summer DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAGeneral ServiceAncillary CoolingWinter DR Event Hours","WA","General Service","Ancillary Cooling","Winter DR Event Hours","hours/year",0,0,1]
["WAGeneral ServiceAncillary CoolingAnnual O&M Cost","WA","General Service","Ancillary Cooling","Annual O&M Cost","$/participant/year",0,"Average subscription fees for EE and DR program management",1]
["WAGeneral ServiceAncillary CoolingAnnual Program Administration Cost","WA","General Service","Ancillary Cooling","Annual Program Administration Cost","$/yr",4909.476639008526,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAGeneral ServiceAncillary CoolingCost of Equip + Install","WA","General Service","Ancillary Cooling","Cost of Equip + Install","$/tech",0,"Bring Your Own Thermostat program",1]
["WAGeneral ServiceAncillary CoolingCost of Equip + Install (per kW basis)","WA","General Service","Ancillary Cooling","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceAncillary CoolingDe-rate","WA","General Service","Ancillary Cooling","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceAncillary CoolingNet to Gross Ratio (free ridership)","WA","General Service","Ancillary Cooling","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceAncillary CoolingPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Ancillary Cooling","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["WAGeneral ServiceAncillary CoolingPer Participant Annual Incentive","WA","General Service","Ancillary Cooling","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC. Adding $20 to account for ancillary service option",1]
["WAGeneral ServiceAncillary CoolingPer kW Annual Incentive","WA","General Service","Ancillary Cooling","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceAncillary CoolingProgram Development Cost","WA","General Service","Ancillary Cooling","Program Development Cost","$/program",4091.2305325071052,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAGeneral ServiceAncillary CoolingProgram Life","WA","General Service","Ancillary Cooling","Program Life","years",10,0,1]
["WAGeneral ServiceAncillary CoolingProgram Start Year","WA","General Service","Ancillary Cooling","Program Start Year","year",2022,0,1]
["WAResidentialAncillary HeatingSummer DR Event Hours","WA","Residential","Ancillary Heating","Summer DR Event Hours","hours/year",0,0,1]
["WAResidentialAncillary HeatingWinter DR Event Hours","WA","Residential","Ancillary Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAResidentialAncillary HeatingAnnual O&M Cost","WA","Residential","Ancillary Heating","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["WAResidentialAncillary HeatingAnnual Program Administration Cost","WA","Residential","Ancillary Heating","Annual Program Administration Cost","$/yr",24811.035477069418,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAResidentialAncillary HeatingCost of Equip + Install","WA","Residential","Ancillary Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["WAResidentialAncillary HeatingCost of Equip + Install (per kW basis)","WA","Residential","Ancillary Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialAncillary HeatingDe-rate","WA","Residential","Ancillary Heating","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialAncillary HeatingNet to Gross Ratio (free ridership)","WA","Residential","Ancillary Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialAncillary HeatingPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Ancillary Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Utah $50, All others $60 (20% higher)",1]
["WAResidentialAncillary HeatingPer Participant Annual Incentive","WA","Residential","Ancillary Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["WAResidentialAncillary HeatingPer kW Annual Incentive","WA","Residential","Ancillary Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialAncillary HeatingProgram Development Cost","WA","Residential","Ancillary Heating","Program Development Cost","$/program",20675.86289755785,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAResidentialAncillary HeatingProgram Life","WA","Residential","Ancillary Heating","Program Life","years",10,0,1]
["WAResidentialAncillary HeatingProgram Start Year","WA","Residential","Ancillary Heating","Program Start Year","year",2022,0,1]
["WAGeneral ServiceAncillary HeatingSummer DR Event Hours","WA","General Service","Ancillary Heating","Summer DR Event Hours","hours/year",0,0,1]
["WAGeneral ServiceAncillary HeatingWinter DR Event Hours","WA","General Service","Ancillary Heating","Winter DR Event Hours","hours/year",36,"2016 M&V Report Event Hours",1]
["WAGeneral ServiceAncillary HeatingAnnual O&M Cost","WA","General Service","Ancillary Heating","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["WAGeneral ServiceAncillary HeatingAnnual Program Administration Cost","WA","General Service","Ancillary Heating","Annual Program Administration Cost","$/yr",3944.7407126847475,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAGeneral ServiceAncillary HeatingCost of Equip + Install","WA","General Service","Ancillary Heating","Cost of Equip + Install","$/tech",0,"Bring your own thermostat program",1]
["WAGeneral ServiceAncillary HeatingCost of Equip + Install (per kW basis)","WA","General Service","Ancillary Heating","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceAncillary HeatingDe-rate","WA","General Service","Ancillary Heating","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceAncillary HeatingNet to Gross Ratio (free ridership)","WA","General Service","Ancillary Heating","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceAncillary HeatingPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Ancillary Heating","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Utah $50, All others $60 (20% higher)",1]
["WAGeneral ServiceAncillary HeatingPer Participant Annual Incentive","WA","General Service","Ancillary Heating","Per Participant Annual Incentive","$/participant/year",20,"Assume $20 per year per system, same as CAC DLC.",1]
["WAGeneral ServiceAncillary HeatingPer kW Annual Incentive","WA","General Service","Ancillary Heating","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceAncillary HeatingProgram Development Cost","WA","General Service","Ancillary Heating","Program Development Cost","$/program",3287.2839272372894,"Half for Ancillary- tied to participation reduction from parent program",1]
["WAGeneral ServiceAncillary HeatingProgram Life","WA","General Service","Ancillary Heating","Program Life","years",10,0,1]
[{"$f":"B1410&C1410&D1410&E1410","v":"WAGeneral ServiceAncillary HeatingProgram Start Year"},"WA","General Service","Ancillary Heating","Program Start Year","year",2022,0,1]
["WAResidentialAncillary WHSummer DR Event Hours","WA","Residential","Ancillary WH","Summer DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAResidentialAncillary WHWinter DR Event Hours","WA","Residential","Ancillary WH","Winter DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAResidentialAncillary WHAnnual O&M Cost","WA","Residential","Ancillary WH","Annual O&M Cost","$/participant/year",0,0,1]
["WAResidentialAncillary WHAnnual Program Administration Cost","WA","Residential","Ancillary WH","Annual Program Administration Cost","$/yr",81900,"Share of Cost as noted in table at right",1]
["WAResidentialAncillary WHCost of Equip + Install","WA","Residential","Ancillary WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["WAResidentialAncillary WHCost of Equip + Install (per kW basis)","WA","Residential","Ancillary WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialAncillary WHDe-rate","WA","Residential","Ancillary WH","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialAncillary WHNet to Gross Ratio (free ridership)","WA","Residential","Ancillary WH","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialAncillary WHPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Ancillary WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",60,"Same as Smart Thermostats",1]
["WAResidentialAncillary WHPer Participant Annual Incentive","WA","Residential","Ancillary WH","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["WAResidentialAncillary WHPer kW Annual Incentive","WA","Residential","Ancillary WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialAncillary WHProgram Development Cost","WA","Residential","Ancillary WH","Program Development Cost","$/program",68250,0,1]
["WAResidentialAncillary WHProgram Life","WA","Residential","Ancillary WH","Program Life","years",8,0,1]
["WAResidentialAncillary WHProgram Start Year","WA","Residential","Ancillary WH","Program Start Year","year",2022,0,1]
["WAGeneral ServiceAncillary WHSummer DR Event Hours","WA","General Service","Ancillary WH","Summer DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAGeneral ServiceAncillary WHWinter DR Event Hours","WA","General Service","Ancillary WH","Winter DR Event Hours","hours/year",75,"25 total events around 3 hrs ea.",1]
["WAGeneral ServiceAncillary WHAnnual O&M Cost","WA","General Service","Ancillary WH","Annual O&M Cost","$/participant/year",0,0,1]
["WAGeneral ServiceAncillary WHAnnual Program Administration Cost","WA","General Service","Ancillary WH","Annual Program Administration Cost","$/yr",8100,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceAncillary WHCost of Equip + Install","WA","General Service","Ancillary WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["WAGeneral ServiceAncillary WHCost of Equip + Install (per kW basis)","WA","General Service","Ancillary WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceAncillary WHDe-rate","WA","General Service","Ancillary WH","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceAncillary WHNet to Gross Ratio (free ridership)","WA","General Service","Ancillary WH","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceAncillary WHPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Ancillary WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",75,"Same as Smart Thermostats",1]
["WAGeneral ServiceAncillary WHPer Participant Annual Incentive","WA","General Service","Ancillary WH","Per Participant Annual Incentive","$/participant/year",24,"Assume $2/month year round",1]
["WAGeneral ServiceAncillary WHPer kW Annual Incentive","WA","General Service","Ancillary WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceAncillary WHProgram Development Cost","WA","General Service","Ancillary WH","Program Development Cost","$/program",6750,"No startup costs; Framework already exists for current programs",1]
["WAGeneral ServiceAncillary WHProgram Life","WA","General Service","Ancillary WH","Program Life","years",8,0,1]
["WAGeneral ServiceAncillary WHProgram Start Year","WA","General Service","Ancillary WH","Program Start Year","year",2022,0,1]
["WAResidentialAncillary DLC WHSummer DR Event Hours","WA","Residential","Ancillary DLC WH","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["WAResidentialAncillary DLC WHWinter DR Event Hours","WA","Residential","Ancillary DLC WH","Winter DR Event Hours","hours/year",0,"Split 50 hrs summer, and 50 hrs winter",1]
["WAResidentialAncillary DLC WHAnnual O&M Cost","WA","Residential","Ancillary DLC WH","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["WAResidentialAncillary DLC WHAnnual Program Administration Cost","WA","Residential","Ancillary DLC WH","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["WAResidentialAncillary DLC WHCost of Equip + Install","WA","Residential","Ancillary DLC WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["WAResidentialAncillary DLC WHCost of Equip + Install (per kW basis)","WA","Residential","Ancillary DLC WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialAncillary DLC WHDe-rate","WA","Residential","Ancillary DLC WH","De-rate","capacity equivalence factor",0,0,1]
["WAResidentialAncillary DLC WHNet to Gross Ratio (free ridership)","WA","Residential","Ancillary DLC WH","Net to Gross Ratio (free ridership)","ratio",0,0,1]
["WAResidentialAncillary DLC WHPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Ancillary DLC WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as DLC CAC",1]
["WAResidentialAncillary DLC WHPer Participant Annual Incentive","WA","Residential","Ancillary DLC WH","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["WAResidentialAncillary DLC WHPer kW Annual Incentive","WA","Residential","Ancillary DLC WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialAncillary DLC WHProgram Development Cost","WA","Residential","Ancillary DLC WH","Program Development Cost","$/program",0,0,1]
["WAResidentialAncillary DLC WHProgram Life","WA","Residential","Ancillary DLC WH","Program Life","years",0,0,1]
["WAResidentialAncillary DLC WHProgram Start Year","WA","Residential","Ancillary DLC WH","Program Start Year","year",0,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["WAGeneral ServiceAncillary DLC WHSummer DR Event Hours","WA","General Service","Ancillary DLC WH","Summer DR Event Hours","hours/year",0,"Current PC Cool Keeper CAC DLC program allows for max 100 hours of curtailment.  ",1]
["WAGeneral ServiceAncillary DLC WHWinter DR Event Hours","WA","General Service","Ancillary DLC WH","Winter DR Event Hours","hours/year",0,"Split 50 hrs summer, and 50 hrs winter",1]
["WAGeneral ServiceAncillary DLC WHAnnual O&M Cost","WA","General Service","Ancillary DLC WH","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["WAGeneral ServiceAncillary DLC WHAnnual Program Administration Cost","WA","General Service","Ancillary DLC WH","Annual Program Administration Cost","$/yr",0,"Share of Cost as noted in table at right",1]
["WAGeneral ServiceAncillary DLC WHCost of Equip + Install","WA","General Service","Ancillary DLC WH","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["WAGeneral ServiceAncillary DLC WHCost of Equip + Install (per kW basis)","WA","General Service","Ancillary DLC WH","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceAncillary DLC WHDe-rate","WA","General Service","Ancillary DLC WH","De-rate","capacity equivalence factor",0,0,1]
["WAGeneral ServiceAncillary DLC WHNet to Gross Ratio (free ridership)","WA","General Service","Ancillary DLC WH","Net to Gross Ratio (free ridership)","ratio",0,0,1]
["WAGeneral ServiceAncillary DLC WHPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Ancillary DLC WH","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Same as DLC CAC",1]
["WAGeneral ServiceAncillary DLC WHPer Participant Annual Incentive","WA","General Service","Ancillary DLC WH","Per Participant Annual Incentive","$/participant/year",0,"Assume $2/month year round",1]
["WAGeneral ServiceAncillary DLC WHPer kW Annual Incentive","WA","General Service","Ancillary DLC WH","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceAncillary DLC WHProgram Development Cost","WA","General Service","Ancillary DLC WH","Program Development Cost","$/program",0,"No startup costs; Framework already exists for current programs",1]
["WAGeneral ServiceAncillary DLC WHProgram Life","WA","General Service","Ancillary DLC WH","Program Life","years",0,0,1]
["WAGeneral ServiceAncillary DLC WHProgram Start Year","WA","General Service","Ancillary DLC WH","Program Start Year","year",0,"Existing programs in UT. Other states need 2 years to ramp up.",1]
["WAResidentialAncillary EVSummer DR Event Hours","WA","Residential","Ancillary EV","Summer DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each summer weekday",1]
["WAResidentialAncillary EVWinter DR Event Hours","WA","Residential","Ancillary EV","Winter DR Event Hours","hours/year",528,"Pacificorp: Six hours on-peak period each winter weekday",1]
["WAResidentialAncillary EVAnnual O&M Cost","WA","Residential","Ancillary EV","Annual O&M Cost","$/participant/year",0,"Zero for Ancillary",1]
["WAResidentialAncillary EVAnnual Program Administration Cost","WA","Residential","Ancillary EV","Annual Program Administration Cost","$/yr",58962.721128592144,"Share of Cost as noted in table at right",1]
["WAResidentialAncillary EVCost of Equip + Install","WA","Residential","Ancillary EV","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["WAResidentialAncillary EVCost of Equip + Install (per kW basis)","WA","Residential","Ancillary EV","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialAncillary EVDe-rate","WA","Residential","Ancillary EV","De-rate","capacity equivalence factor",1,0,1]
[{"$f":"B1474&C1474&D1474&E1474","v":"WAResidentialAncillary EVNet to Gross Ratio (free ridership)"},"WA","Residential","Ancillary EV","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialAncillary EVPer Customer Annual Marketing/Recruitment Cost","WA","Residential","Ancillary EV","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",50,"Assumption $50 for RAP C&I, MAP = RAPx1.2",1]
["WAResidentialAncillary EVPer Participant Annual Incentive","WA","Residential","Ancillary EV","Per Participant Annual Incentive","$/participant/year",20,"Avista would provide a rate based charger or give a rebate on it, with no further incentives",1]
["WAResidentialAncillary EVPer kW Annual Incentive","WA","Residential","Ancillary EV","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialAncillary EVProgram Development Cost","WA","Residential","Ancillary EV","Program Development Cost","$/program",49135.600940493452,"Share of Cost as noted in table at right",1]
["WAResidentialAncillary EVProgram Life","WA","Residential","Ancillary EV","Program Life","years",8,0,1]
["WAResidentialAncillary EVProgram Start Year","WA","Residential","Ancillary EV","Program Start Year","year",2024,"Technology won’t be available for mass market till 2024",1]
["WAGeneral ServiceAncillary Third PartySummer DR Event Hours","WA","General Service","Ancillary Third Party","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAGeneral ServiceAncillary Third PartyWinter DR Event Hours","WA","General Service","Ancillary Third Party","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAGeneral ServiceAncillary Third PartyAnnual O&M Cost","WA","General Service","Ancillary Third Party","Annual O&M Cost","$/participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["WAGeneral ServiceAncillary Third PartyAnnual Program Administration Cost","WA","General Service","Ancillary Third Party","Annual Program Administration Cost","$/yr",0,0,1]
["WAGeneral ServiceAncillary Third PartyCost of Equip + Install","WA","General Service","Ancillary Third Party","Cost of Equip + Install","$/tech",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["WAGeneral ServiceAncillary Third PartyCost of Equip + Install (per kW basis)","WA","General Service","Ancillary Third Party","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceAncillary Third PartyDe-rate","WA","General Service","Ancillary Third Party","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceAncillary Third PartyNet to Gross Ratio (free ridership)","WA","General Service","Ancillary Third Party","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceAncillary Third PartyPer Customer Annual Marketing/Recruitment Cost","WA","General Service","Ancillary Third Party","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"Pacificorp: included in 3rd Party Program Admin Cost",1]
["WAGeneral ServiceAncillary Third PartyPer Participant Annual Incentive","WA","General Service","Ancillary Third Party","Per Participant Annual Incentive","$/participant/year",0,0,1]
["WAGeneral ServiceAncillary Third PartyPer kW Annual Incentive","WA","General Service","Ancillary Third Party","Per kW Annual Incentive","$/kW @meter/year",0,"MPSC Demand Response Market Assessment",1]
["WAGeneral ServiceAncillary Third PartyAnnual O&M Cost per MW","WA","General Service","Ancillary Third Party","Annual O&M Cost per MW","$/MW @meter",40000,"Half for Ancillary",1]
["WAGeneral ServiceAncillary Third PartyProgram Development Cost","WA","General Service","Ancillary Third Party","Program Development Cost","$/program",0,0,1]
["WAGeneral ServiceAncillary Third PartyProgram Life","WA","General Service","Ancillary Third Party","Program Life","years",3,0,1]
["WAGeneral ServiceAncillary Third PartyProgram Start Year","WA","General Service","Ancillary Third Party","Program Start Year","year",2022,0,1]
["WALarge General ServiceAncillary Third PartySummer DR Event Hours","WA","Large General Service","Ancillary Third Party","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WALarge General ServiceAncillary Third PartyWinter DR Event Hours","WA","Large General Service","Ancillary Third Party","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WALarge General ServiceAncillary Third PartyAnnual O&M Cost","WA","Large General Service","Ancillary Third Party","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceAncillary Third PartyAnnual Program Administration Cost","WA","Large General Service","Ancillary Third Party","Annual Program Administration Cost","$/yr",0,0,1]
["WALarge General ServiceAncillary Third PartyCost of Equip + Install","WA","Large General Service","Ancillary Third Party","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceAncillary Third PartyCost of Equip + Install (per kW basis)","WA","Large General Service","Ancillary Third Party","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceAncillary Third PartyDe-rate","WA","Large General Service","Ancillary Third Party","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceAncillary Third PartyNet to Gross Ratio (free ridership)","WA","Large General Service","Ancillary Third Party","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceAncillary Third PartyPer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Ancillary Third Party","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WALarge General ServiceAncillary Third PartyPer Participant Annual Incentive","WA","Large General Service","Ancillary Third Party","Per Participant Annual Incentive","$/participant/year",0,"Not sure what to put for incentives here",1]
["WALarge General ServiceAncillary Third PartyPer kW Annual Incentive","WA","Large General Service","Ancillary Third Party","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["WALarge General ServiceAncillary Third PartyAnnual O&M Cost per MW","WA","Large General Service","Ancillary Third Party","Annual O&M Cost per MW","$/MW @meter",40000,"Half for Ancillary",1]
["WALarge General ServiceAncillary Third PartyProgram Development Cost","WA","Large General Service","Ancillary Third Party","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
["WALarge General ServiceAncillary Third PartyProgram Life","WA","Large General Service","Ancillary Third Party","Program Life","years",3,0,1]
["WALarge General ServiceAncillary Third PartyProgram Start Year","WA","Large General Service","Ancillary Third Party","Program Start Year","year",2022,0,1]
["WAExtra Large General ServiceAncillary Third PartySummer DR Event Hours","WA","Extra Large General Service","Ancillary Third Party","Summer DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAExtra Large General ServiceAncillary Third PartyWinter DR Event Hours","WA","Extra Large General Service","Ancillary Third Party","Winter DR Event Hours","hours/year",30,"30 hours is based on program experience as gathered during 2015 study.  Pretty low on the spectrum for these programs, which can often have up to 60-100 hrs of event.",1]
["WAExtra Large General ServiceAncillary Third PartyAnnual O&M Cost","WA","Extra Large General Service","Ancillary Third Party","Annual O&M Cost","$/participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceAncillary Third PartyAnnual Program Administration Cost","WA","Extra Large General Service","Ancillary Third Party","Annual Program Administration Cost","$/yr",0,0,1]
["WAExtra Large General ServiceAncillary Third PartyCost of Equip + Install","WA","Extra Large General Service","Ancillary Third Party","Cost of Equip + Install","$/tech",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceAncillary Third PartyCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Ancillary Third Party","Cost of Equip + Install (per kW basis)","$/kW @meter",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceAncillary Third PartyDe-rate","WA","Extra Large General Service","Ancillary Third Party","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceAncillary Third PartyNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Ancillary Third Party","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceAncillary Third PartyPer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Ancillary Third Party","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in 3rd Party Program Admin Cost",1]
["WAExtra Large General ServiceAncillary Third PartyPer Participant Annual Incentive","WA","Extra Large General Service","Ancillary Third Party","Per Participant Annual Incentive","$/participant/year",0,"Not sure what to put for incentives here",1]
["WAExtra Large General ServiceAncillary Third PartyPer kW Annual Incentive","WA","Extra Large General Service","Ancillary Third Party","Per kW Annual Incentive","$/kW @meter/year",0,"included in 3rd Party Program Admin Cost.  Capacity reserve incentive pmt given to customers typically in range of $10 to $70 per kW-year",1]
["WAExtra Large General ServiceAncillary Third PartyAnnual O&M Cost per MW","WA","Extra Large General Service","Ancillary Third Party","Annual O&M Cost per MW","$/MW @meter",40000,"Half for Ancillary",1]
["WAExtra Large General ServiceAncillary Third PartyProgram Development Cost","WA","Extra Large General Service","Ancillary Third Party","Program Development Cost","$/program",0,"No startup costs; Would be included in 3rd Party Costs",1]
["WAExtra Large General ServiceAncillary Third PartyProgram Life","WA","Extra Large General Service","Ancillary Third Party","Program Life","years",3,0,1]
["WAExtra Large General ServiceAncillary Third PartyProgram Start Year","WA","Extra Large General Service","Ancillary Third Party","Program Start Year","year",2022,0,1]
["WAResidentialAncillary Battery StorageSummer DR Event Hours","WA","Residential","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["WAResidentialAncillary Battery StorageWinter DR Event Hours","WA","Residential","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WAResidentialAncillary Battery StorageAnnual O&M Cost","WA","Residential","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WAResidentialAncillary Battery StorageAnnual Program Administration Cost","WA","Residential","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",49838.915828113793,"half FTE @ $150,000",1]
["WAResidentialAncillary Battery StorageCost of Equip + Install","WA","Residential","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Zero for Ancillary",1]
["WAResidentialAncillary Battery StorageCost of Equip + Install (per kW basis)","WA","Residential","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAResidentialAncillary Battery StorageDe-rate","WA","Residential","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["WAResidentialAncillary Battery StorageNet to Gross Ratio (free ridership)","WA","Residential","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAResidentialAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","WA","Residential","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["WAResidentialAncillary Battery StoragePer Participant Annual Incentive","WA","Residential","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0,1]
["WAResidentialAncillary Battery StoragePer kW Annual Incentive","WA","Residential","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAResidentialAncillary Battery StorageProgram Development Cost","WA","Residential","Ancillary Battery Storage","Program Development Cost","$/program",27688.286571174332,0,1]
[{"$f":"B1538&C1538&D1538&E1538","v":"WAResidentialAncillary Battery StorageProgram Life"},"WA","Residential","Ancillary Battery Storage","Program Life","years",15,"NREL",1]
["WAResidentialAncillary Battery StorageProgram Start Year","WA","Residential","Ancillary Battery Storage","Program Start Year","year",2022,0,1]
["WAGeneral ServiceAncillary Battery StorageSummer DR Event Hours","WA","General Service","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["WAGeneral ServiceAncillary Battery StorageWinter DR Event Hours","WA","General Service","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WAGeneral ServiceAncillary Battery StorageAnnual O&M Cost","WA","General Service","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WAGeneral ServiceAncillary Battery StorageAnnual Program Administration Cost","WA","General Service","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",5283.1160966009629,"half FTE @ $150,000",1]
["WAGeneral ServiceAncillary Battery StorageCost of Equip + Install","WA","General Service","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["WAGeneral ServiceAncillary Battery StorageCost of Equip + Install (per kW basis)","WA","General Service","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAGeneral ServiceAncillary Battery StorageDe-rate","WA","General Service","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["WAGeneral ServiceAncillary Battery StorageNet to Gross Ratio (free ridership)","WA","General Service","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAGeneral ServiceAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","WA","General Service","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["WAGeneral ServiceAncillary Battery StoragePer Participant Annual Incentive","WA","General Service","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0,1]
["WAGeneral ServiceAncillary Battery StoragePer kW Annual Incentive","WA","General Service","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WAGeneral ServiceAncillary Battery StorageProgram Development Cost","WA","General Service","Ancillary Battery Storage","Program Development Cost","$/program",2935.0644981116461,0,1]
["WAGeneral ServiceAncillary Battery StorageProgram Life","WA","General Service","Ancillary Battery Storage","Program Life","years",15,"NREL",1]
["WAGeneral ServiceAncillary Battery StorageProgram Start Year","WA","General Service","Ancillary Battery Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["WALarge General ServiceAncillary Battery StorageSummer DR Event Hours","WA","Large General Service","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["WALarge General ServiceAncillary Battery StorageWinter DR Event Hours","WA","Large General Service","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WALarge General ServiceAncillary Battery StorageAnnual O&M Cost","WA","Large General Service","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WALarge General ServiceAncillary Battery StorageAnnual Program Administration Cost","WA","Large General Service","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",2575.0982909510931,"half FTE @ $150,000",1]
["WALarge General ServiceAncillary Battery StorageCost of Equip + Install","WA","Large General Service","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["WALarge General ServiceAncillary Battery StorageCost of Equip + Install (per kW basis)","WA","Large General Service","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WALarge General ServiceAncillary Battery StorageDe-rate","WA","Large General Service","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["WALarge General ServiceAncillary Battery StorageNet to Gross Ratio (free ridership)","WA","Large General Service","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WALarge General ServiceAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","WA","Large General Service","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost",1]
["WALarge General ServiceAncillary Battery StoragePer Participant Annual Incentive","WA","Large General Service","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0,1]
["WALarge General ServiceAncillary Battery StoragePer kW Annual Incentive","WA","Large General Service","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0,1]
["WALarge General ServiceAncillary Battery StorageProgram Development Cost","WA","Large General Service","Ancillary Battery Storage","Program Development Cost","$/program",1430.610161639496,0,1]
["WALarge General ServiceAncillary Battery StorageProgram Life","WA","Large General Service","Ancillary Battery Storage","Program Life","years",15,"NREL",1]
["WALarge General ServiceAncillary Battery StorageProgram Start Year","WA","Large General Service","Ancillary Battery Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU",1]
["WAExtra Large General ServiceAncillary Battery StorageSummer DR Event Hours","WA","Extra Large General Service","Ancillary Battery Storage","Summer DR Event Hours","hours/year",36,0,1]
["WAExtra Large General ServiceAncillary Battery StorageWinter DR Event Hours","WA","Extra Large General Service","Ancillary Battery Storage","Winter DR Event Hours","hours/year",36,"Round trip efficiency assumption:",1]
["WAExtra Large General ServiceAncillary Battery StorageAnnual O&M Cost","WA","Extra Large General Service","Ancillary Battery Storage","Annual O&M Cost","$/participant/year",0,"included in listed Program Admin Cost",1]
["WAExtra Large General ServiceAncillary Battery StorageAnnual Program Administration Cost","WA","Extra Large General Service","Ancillary Battery Storage","Annual Program Administration Cost","$/yr",27.892256838212912,"Calculated",1]
["WAExtra Large General ServiceAncillary Battery StorageCost of Equip + Install","WA","Extra Large General Service","Ancillary Battery Storage","Cost of Equip + Install","$/tech",0,"Lazard's cost - avg. of hi/low case for Commercial Lithium-Ion Batteries - low=$1,286, hi=$1,440",1]
["WAExtra Large General ServiceAncillary Battery StorageCost of Equip + Install (per kW basis)","WA","Extra Large General Service","Ancillary Battery Storage","Cost of Equip + Install (per kW basis)","$/kW @meter",0,0,1]
["WAExtra Large General ServiceAncillary Battery StorageDe-rate","WA","Extra Large General Service","Ancillary Battery Storage","De-rate","capacity equivalence factor",1,0,1]
["WAExtra Large General ServiceAncillary Battery StorageNet to Gross Ratio (free ridership)","WA","Extra Large General Service","Ancillary Battery Storage","Net to Gross Ratio (free ridership)","ratio",1,0,1]
["WAExtra Large General ServiceAncillary Battery StoragePer Customer Annual Marketing/Recruitment Cost","WA","Extra Large General Service","Ancillary Battery Storage","Per Customer Annual Marketing/Recruitment Cost","$/new participant/year",0,"included in listed Program Admin Cost"]
["WAExtra Large General ServiceAncillary Battery StoragePer Participant Annual Incentive","WA","Extra Large General Service","Ancillary Battery Storage","Per Participant Annual Incentive","$/participant/year",20,0]
["WAExtra Large General ServiceAncillary Battery StoragePer kW Annual Incentive","WA","Extra Large General Service","Ancillary Battery Storage","Per kW Annual Incentive","$/kW @meter/year",0,0]
["WAExtra Large General ServiceAncillary Battery StorageProgram Development Cost","WA","Extra Large General Service","Ancillary Battery Storage","Program Development Cost","$/program",15.495698243451619,"Calculated"]
["WAExtra Large General ServiceAncillary Battery StorageProgram Life","WA","Extra Large General Service","Ancillary Battery Storage","Program Life","years",15,"NREL"]
["WAExtra Large General ServiceAncillary Battery StorageProgram Start Year","WA","Extra Large General Service","Ancillary Battery Storage","Program Start Year","year",2022,"Assumed rollout could piggyback on Utility's TOU"]

{"sheet":"DR","index":7,"n_rows":156,"n_cols":53,"rows_kept":156,"cut":false,"hidden":false,"merged":[[2,2,2,4],[1,2,1,4],[3,2,3,4],[4,2,4,4],[82,1,82,46]]}
[null,null,null,null,null,null,null,"Key"]
[null,"Customer Class","Residential",null,null,null,null,"Gray fill","Select Option for Analysis (automatically via runs or manual via drop-down menus"]
[null,"Option","DLC Water Heating",null,null,null,null,"Blue font","For Export to Results Tab"]
[null,"Potential","Market Potential"]
[null,"State","ID"]
[null,"Program Year",{"$f":"IF(C$7=$C$49,\"Year \"&C$7-$C$49+1,IF(C$7>$C$49,\"Year \"&C$7-$C$49+1,\"\"))","v":"Year 1"},{"$f":"IF(D$7=$C$49,\"Year \"&D$7-$C$49+1,IF(D$7>$C$49,\"Year \"&D$7-$C$49+1,\"\"))","v":"Year 2"},{"$f":"IF(E$7=$C$49,\"Year \"&E$7-$C$49+1,IF(E$7>$C$49,\"Year \"&E$7-$C$49+1,\"\"))","v":"Year 3"},{"$f":"IF(F$7=$C$49,\"Year \"&F$7-$C$49+1,IF(F$7>$C$49,\"Year \"&F$7-$C$49+1,\"\"))","v":"Year 4"},"Year 5",{"$f":"IF(H$7=$C$49,\"Year \"&H$7-$C$49+1,IF(H$7>$C$49,\"Year \"&H$7-$C$49+1,\"\"))","v":"Year 6"},"Year 7","Year 8","Year 9","Year 10","Year 11","Year 12","Year 13","Year 14","Year 15","Year 16","Year 17","Year 18","Year 19","Year 20","Year 21","Year 22","Year 23","Year 24","Year 25","Year 26","Year 27","Year 28","Year 29","Year 30","Year 31","Year 32","Year 33","Year 34","Year 35","Year 36","Year 37","Year 38","Year 39","Year 40","Year 41","Year 42","Year 43","Year 44","Year 45"]
[null,"Year",{"$f":"YearBase","v":2022},{"$f":"C$7+1","v":2023},{"$f":"D$7+1","v":2024},2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,{"$f":"Y$7+1","v":2045},2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,null,null,null,null,"Option","Relevant Equipment Saturation"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ControlPanel!B10","v":"DLC Central AC"},"Saturation Central AC"]
[null,"Impacts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ControlPanel!B8","v":"DLC Smart Thermostats - Cooling"},"Saturation Central AC"]
[null,"Customer Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ControlPanel!B9","v":"DLC Smart Thermostats - Heating"},"Saturation Elec Space Heat"]
[null,"Customer Population",{"$f":"INDEX(ClassValues,MATCH(State&Class&$B$11,KeyCV,0),MATCH(C$7,YearsCV,0))","v":120796.68660000582},{"$f":"INDEX(ClassValues,MATCH(State&Class&$B$11,KeyCV,0),MATCH(D$7,YearsCV,0))","v":122376.50927373911},{"$f":"INDEX(ClassValues,MATCH(State&Class&$B$11,KeyCV,0),MATCH(E$7,YearsCV,0))","v":123964.58984604779},125479.12305934337,127012.16003130926,128563.92683099561,130134.65228944356,131724.56803342985,133333.90851962357,134962.91106916027,136611.81590263854,138280.86617554407,139970.3080141065,141680.39055159441,143411.36596505373,145163.48951249503,146937.01957053496,148732.21767249788,150549.34854698274,152388.68015690125,154250.48373899297,156135.03384382327,158042.60837626981,159973.48863650372,161927.95936147158,163906.30876688403,165908.82858971745,167935.81413123498,169987.56430053301,172064.38165861974,174166.57246303238,176294.44671299928,178448.31819515399,180628.50452980766,182835.32721778695,185069.1116878441,187330.18734464614,189618.88761735064,191935.55000877465,194280.51614516453,0,0,0,0,0,null,null,null,null,{"$f":"ControlPanel!B11","v":"DLC Water Heating"},"Saturation Elec Water Heat"]
[null,"Eligible Customers",{"$f":"IF(C$11-IF(HierarchyStatus?=TRUE,SUMPRODUCT($A$86:$A$107,C$86:C$107),0)>0,C$11-IF(HierarchyStatus?=TRUE,SUMPRODUCT($A$86:$A$107,C$86:C$107),0),0)","v":120796.68660000582},122376.50927373911,123964.58984604779,125479.12305934337,127012.16003130926,128563.92683099561,130134.65228944356,131724.56803342985,133333.90851962357,134962.91106916027,136611.81590263854,138280.86617554407,139970.3080141065,141680.39055159441,143411.36596505373,145163.48951249503,146937.01957053496,148732.21767249788,150549.34854698274,152388.68015690125,154250.48373899297,156135.03384382327,158042.60837626981,159973.48863650372,161927.95936147158,163906.30876688403,165908.82858971745,167935.81413123498,169987.56430053301,172064.38165861974,174166.57246303238,176294.44671299928,178448.31819515399,180628.50452980766,182835.32721778695,185069.1116878441,187330.18734464614,189618.88761735064,191935.55000877465,194280.51614516453,0,0,0,0,0,null,null,null,null,{"$f":"ControlPanel!B12","v":"CTA-2045 WH"},"Saturation CTA-2045 Water Heat"]
[null,"Program Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ControlPanel!B13","v":"DLC Electric Vehicle Charging"},"Saturation Elec Vehicles"]
[null,"Participation Rate",{"$f":"IFERROR(INDEX(ParticipationRate,MATCH(State&Class&Option&Potential,KeyPR,0),MATCH(C$6,YearsPR,0)),)","v":1.4999999999999999E-2},4.5000000000000005E-2,0.105,0.13500000000000001,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0.15,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(INDEX(ParticipationRate,MATCH(State&Class&Option&Potential,KeyPR,0),MATCH(AP$6,YearsPR,0)),)","v":0},0,0,0,0,0,null,null,null,null,{"$f":"ControlPanel!B14","v":"Ancillary Cooling"},"Saturation Central AC"]
[null,"Program Dropout Rate (Attrition)",{"$f":"IFERROR(INDEX(ParticipationRate,MATCH(State&Class&Option&$B15,KeyPR,0),MATCH(C$6,YearsPR,0)),)","v":0.01},0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"Ancillary Heating","Saturation Elec Space Heat"]
[null,"Event Non-Performance Rate",{"$f":"IFERROR(INDEX(ImpactInput,MATCH(State&Class&Option&$B16,KeyImp,0),7),)","v":0},0,0,{"$f":"IFERROR(INDEX(ImpactInput,MATCH(State&Class&Option&$B16,KeyImp,0),7),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"Ancillary DLC WH","Saturation Elec Water Heat"]
[null,{"$f":"VLOOKUP(Option,$AZ$8:$BA$29,2,FALSE)","v":"Saturation Elec Water Heat"},{"$f":"IFERROR(INDEX(ClassValues,MATCH(State&Class&$B$17,KeyCV,0),MATCH(C$7,YearsCV,0)),100%)","v":0.50120862662826382},{"$f":"IFERROR(INDEX(ClassValues,MATCH(State&Class&$B$17,KeyCV,0),MATCH(D$7,YearsCV,0)),100%)","v":0.49441459619652989},0.48771266084667403,0.48110157220275923,0.47458009881095176,0.4681470259101369,0.46180115520564441,0.45554130464604092,0.44936630820294804,0.44327501565384531,0.43726629236781689,0.43133901909420302,0.42549209175411595,0.41972442123478221,0.41403493318667239,0.40842256782338127,0.40288627972422009,0.39742503763948522,0.39203782429836631,0.3867236362194581,0.38148148352384115,0.37631038975069608,0.37120939167541728,0.36617753913019213,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"Ancillary WH","Saturation CTA-2045 Water Heat"]
[null,"Participant Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ancillary EV","Saturation Elec Vehicles"]
[null,"Total # of Participants",{"$f":"C$12*C$14*(1-C$15)*(1-C$16)*C17","v":899.08346967170064},{"$f":"D$12*D$14*(1-D$15)*(1-D$16)*D17","v":2695.4858291558157},{"$f":"E$12*E$14*(1-E$15)*(1-E$16)*E17","v":6284.7234413183569},{"$f":"F$12*F$14*(1-F$15)*(1-F$16)*F17","v":8068.2103820675966},{"$f":"G$12*G$14*(1-G$15)*(1-G$16)*G17","v":8951.2003534908981},{"$f":"H$12*H$14*(1-H$15)*(1-H$16)*H17","v":8937.7427678109689},8924.305414793158,8910.8882640188931,8897.4912851153276,8884.1144477552753,8870.7577216571535,{"$f":"N$12*N$14*(1-N$15)*(1-N$16)*N17","v":8857.4210765849075},8844.1044823479242,{"$f":"P$12*P$14*(1-P$15)*(1-P$16)*P17","v":8830.8079088009999},{"$f":"Q$12*Q$14*(1-Q$15)*(1-Q$16)*Q17","v":8817.5313258442402},8804.2747034230106,8791.0380115278549,8777.8212201944425,8764.6242995034845,8751.4472195806829,8738.2899505966434,8725.1524627668277,8712.0347263514705,8698.9367116555241,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"Ancillary Third Party","Saturation AMI"]
[null,"Total # of New Participants",{"$f":"MAX(C19-IF(ISNUMBER(B19),B19,0),0)","v":899.08346967170064},1796.4023594841151,{"$f":"MAX(E19-IF(ISNUMBER(D19),D19,0),0)","v":3589.2376121625412},{"$f":"MAX(F19-IF(ISNUMBER(E19),E19,0),0)","v":1783.4869407492397},882.98997142330154,{"$f":"MAX(H19-IF(ISNUMBER(G19),G19,0),0)","v":0},0,0,0,{"$f":"MAX(L19-IF(ISNUMBER(K19),K19,0),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,"Ancillary Battery Storage","Saturation AMI"]
[null,{"$f":"\"Summer Peak Load\"","v":"Summer Peak Load"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ControlPanel!B21","v":"DLC Smart Appliances"},"Saturation Appliances"]
[null,"Per Customer Summer Peak (kW)",{"$f":"IFERROR(INDEX(ClassValues,MATCH(State&Class&$B22,KeyCV,0),MATCH(C$7,YearsCV,0)),)","v":1.961159299434293},1.9517625967282761,1.9448617061498685,1.9395650520645444,1.9331752270710694,1.9255592643527693,1.9179733055820232,1.9104172325548827,1.9028909275330765,1.8953942732421769,1.8879271528697712,1.8804894500636433,1.8730810489299601,1.8657018340314646,1.858351690385678,1.8510305034631089,1.8437381591854667,1.8364745439238856,1.8292395444971536,1.8220330481699487,1.8148549426510832,1.8077051160917521,1.8005834570837922,1.7934898546579454,1.7864241982821292,1.779386377859715,1.7723762837278123,1.7653938066555597,1.7584388378424234,1.751511268916502,1.7446109919328365,1.7377378993717303,1.730891884137072,1.7240728395546678,1.7172806593705794,1.7105152377494679,1.7037764692729434,1.6970642489379251,0,0,0,0,0,0,0,null,null,null,null,{"$f":"ControlPanel!B22","v":"Third Party Contracts"},"Saturation AMI"]
[null,"Per Customer Summer Peak Reduction (%)",{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},null,null,null,null,{"$f":"ControlPanel!B23","v":"Time-of-Use Opt-in"},"Saturation AMI"]
[null,"Per Customer Summer Peak Reduction (kW)",{"$f":"IF(C23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),C22*C23)","v":0.5},{"$f":"IF(D23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),D22*D23)","v":0.5},{"$f":"IF(E23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),E22*E23)","v":0.5},{"$f":"IF(F23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),F22*F23)","v":0.5},{"$f":"IF(G23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),G22*G23)","v":0.5},{"$f":"IF(H23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),H22*H23)","v":0.5},{"$f":"IF(I23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),I22*I23)","v":0.5},{"$f":"IF(J23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),J22*J23)","v":0.5},{"$f":"IF(K23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),K22*K23)","v":0.5},{"$f":"IF(L23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),L22*L23)","v":0.5},{"$f":"IF(M23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),M22*M23)","v":0.5},{"$f":"IF(N23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),N22*N23)","v":0.5},{"$f":"IF(O23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),O22*O23)","v":0.5},{"$f":"IF(P23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),P22*P23)","v":0.5},{"$f":"IF(Q23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),Q22*Q23)","v":0.5},{"$f":"IF(R23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),R22*R23)","v":0.5},{"$f":"IF(S23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),S22*S23)","v":0.5},{"$f":"IF(T23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),T22*T23)","v":0.5},{"$f":"IF(U23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),U22*U23)","v":0.5},{"$f":"IF(V23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),V22*V23)","v":0.5},{"$f":"IF(W23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),W22*W23)","v":0.5},{"$f":"IF(X23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),X22*X23)","v":0.5},{"$f":"IF(Y23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),Y22*Y23)","v":0.5},{"$f":"IF(Z23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),Z22*Z23)","v":0.5},{"$f":"IF(AA23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AA22*AA23)","v":0.5},{"$f":"IF(AB23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AB22*AB23)","v":0.5},{"$f":"IF(AC23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AC22*AC23)","v":0.5},{"$f":"IF(AD23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AD22*AD23)","v":0.5},{"$f":"IF(AE23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AE22*AE23)","v":0.5},{"$f":"IF(AF23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AF22*AF23)","v":0.5},{"$f":"IF(AG23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AG22*AG23)","v":0.5},{"$f":"IF(AH23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AH22*AH23)","v":0.5},{"$f":"IF(AI23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AI22*AI23)","v":0.5},{"$f":"IF(AJ23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AJ22*AJ23)","v":0.5},{"$f":"IF(AK23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AK22*AK23)","v":0.5},{"$f":"IF(AL23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AL22*AL23)","v":0.5},{"$f":"IF(AM23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AM22*AM23)","v":0.5},{"$f":"IF(AN23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AN22*AN23)","v":0.5},{"$f":"IF(AO23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AO22*AO23)","v":0.5},{"$f":"IF(AP23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AP22*AP23)","v":0.5},{"$f":"IF(AQ23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AQ22*AQ23)","v":0.5},{"$f":"IF(AR23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AR22*AR23)","v":0.5},{"$f":"IF(AS23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AS22*AS23)","v":0.5},{"$f":"IF(AT23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AT22*AT23)","v":0.5},{"$f":"IF(AU23=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B24,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AU22*AU23)","v":0.5},null,null,null,null,{"$f":"ControlPanel!B24","v":"Time-of-Use Opt-out"},"Saturation AMI"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ControlPanel!B25","v":"Variable Peak Pricing Rates"},"Saturation AMI"]
[null,"Summer Peak Reduction @Meter  (MW)",{"$f":"C24*C19/1000","v":0.4495417348358503},{"$f":"D24*D19/1000","v":1.3477429145779078},{"$f":"E24*E19/1000","v":3.1423617206591783},{"$f":"F24*F19/1000","v":4.0341051910337979},{"$f":"G24*G19/1000","v":4.4756001767454494},4.4688713839054843,4.4621527073965792,4.4554441320094469,4.4487456425576637,4.4420572238776375,4.4353788608285765,4.4287105382924539,4.4220522411739625,4.4154039544005004,4.4087656629221197,4.402137351711505,4.3955190057639273,4.3889106100972208,4.3823121497517423,4.3757236097903416,4.3691449752983216,4.3625762313834135,4.3560173631757353,4.3494683558277618,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,{"$f":"ControlPanel!B26","v":"Real Time Pricing"},"Saturation Central AC"]
[null,"Estimated Savings as % of Total Class Peak",{"$f":"C$26/INDEX(ClassValues,MATCH(State&Class&$B$21,KeyCV,0),MATCH(C$7,YearsCV,0))","v":1.8975888668443905E-3},{"$f":"D$26/INDEX(ClassValues,MATCH(State&Class&$B$21,KeyCV,0),MATCH(D$7,YearsCV,0))","v":5.642635609852782E-3},{"$f":"E$26/INDEX(ClassValues,MATCH(State&Class&$B$21,KeyCV,0),MATCH(E$7,YearsCV,0))","v":1.303376248673618E-2},1.6575681505618053E-2,1.8227821173821473E-2,1.8051855020682205E-2,1.7877587594272552E-2,1.7705002495572306E-2,1.7534083483872687E-2,1.7364814475248048E-2,1.7197179541042367E-2,1.7031162906370283E-2,1.6866748948632628E-2,1.6703922196046359E-2,1.6542667326188549E-2,1.6382969164554582E-2,1.622481268313012E-2,1.6068182998976978E-2,1.5913065372832578E-2,1.5759445207722964E-2,1.5607308047589153E-2,1.5456639575926832E-2,1.5307425614439091E-2,1.5159652121702241E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,null,{"$f":"ControlPanel!B27","v":"Behavioral"},"Saturation AMI"]
[null,"Estimated Savings as % of Total System Peak",{"$f":"C$26/INDEX(ClassValues,MATCH(State&\"All\"&$B$21,KeyCV,0),MATCH(C$7,YearsCV,0))","v":1.025846282941881E-3},3.0603177172035577E-3,7.0957934087626188E-3,9.0579272161278781E-3,9.9947917277939391E-3,9.9285374565969194E-3,9.8620678978253683E-3,9.795410117407876E-3,9.7285901878948981E-3,9.6616332130979362E-3,9.5945633528551049E-3,9.5274038478468572E-3,9.460177044392188E-3,9.3929044191622471E-3,9.3256066037539602E-3,9.2583034090722282E-3,9.191013849474277E-3,9.1237561666349786E-3,9.05654785309634E-3,8.989405675468895E-3,8.922345697256636E-3,8.8553833012809668E-3,8.7885332116825147E-3,8.7218095154829919E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,null,{"$f":"ControlPanel!B28","v":"Thermal Energy Storage"},"Saturation AMI"]
[null,"NPV MW @Meter",{"$f":"IF(C$71,NPV($C$50,OFFSET(C26,0,0,1,$C$51)),)","v":20.497386512376629},0,0,0,0,0,0,0,28.372447388693498,0,0,0,0,0,0,0,28.032987668258869,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"INDEX($C29:$AU29,MATCH(TRUE,INDEX($C29:$AU29<>0,0),0))","v":20.497386512376629},null,null,null,{"$f":"ControlPanel!B29","v":"Battery Energy Storage"},"Saturation AMI"]
[null,"Summer Peak Reduction @Generation (MW)",{"$f":"C$26/(100%-INDEX(EnergyCosts,MATCH(State&Class&\"Line Loss\",KeyEC,0),MATCH(C$7,YearsEC,0)))*$P$49*$P$50","v":0.47905129458210816},1.436213677086432,3.3486378097391074,4.2989185752704584,4.7693949027551676,4.7622244074014111,4.7550646924515974,4.7479157416980469,4.7407775389574418,4.7336500680707987,4.7265333129034275,4.7194272573448997,4.7123318853089966,4.7052471807336964,4.698173127581116,4.6911097098374945,4.6840569115131361,4.6770147166423923,4.6699831092836126,4.6629620735191191,4.6559515934551596,4.6489516532218813,4.6419622369732902,4.6349833288872144,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Estimated Savings as % of Total Class Peak",{"$f":"C$30/INDEX(ClassValues,MATCH(State&Class&$B$21,KeyCV,0),MATCH(C$7,YearsCV,0))","v":2.0221535239177222E-3},6.0130387999283693E-3,1.3889346213486978E-2,1.7663769720394344E-2,{"$f":"G$30/INDEX(ClassValues,MATCH(State&Class&$B$21,KeyCV,0),MATCH(G$7,YearsCV,0))","v":1.9424361864686136E-2},1.9236844651195871E-2,1.9051137675056E-2,1.8867223460754801E-2,1.8685084701484105E-2,1.8504704257510707E-2,1.8326065154563476E-2,1.8149150582236023E-2,1.797394389240476E-2,1.7800428597662361E-2,1.7628588369766142E-2,1.7458407038101642E-2,1.7289868588160826E-2,1.7122957160035143E-2,1.6957657046923036E-2,1.6793952693651922E-2,1.663182869521436E-2,1.6471269795318447E-2,1.6312260884952145E-2,1.6154787000961467E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,"Estimated Savings as % of Total System Peak",{"$f":"C$30/INDEX(ClassValues,MATCH(State&\"All\"&$B$21,KeyCV,0),MATCH(C$7,YearsCV,0))","v":1.0931865760250223E-3},3.2612081385374656E-3,7.561587178988298E-3,9.652522608831926E-3,1.0650886325441112E-2,1.0580282882136529E-2,1.0509450018995489E-2,1.0438416578652895E-2,1.036721034515654E-2,1.0295858070223717E-2,1.0224385499632463E-2,1.0152817399666302E-2,1.0081177583538136E-2,1.000948893772618E-2,9.9377734481606549E-3,9.8660522262065502E-3,9.7943455343928783E-3,9.7226728118446071E-3,9.6510526993780262E-3,9.5795030642251647E-3,9.5080410243570303E-3,9.4366829723795467E-3,9.3654445989796616E-3,9.2943409159025915E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,"NPV MW @Generation",{"$f":"IF(C$71,NPV($C$50,OFFSET(C30,0,0,1,$C$51)),)","v":21.84290975317203},0,0,0,0,0,0,0,30.234918359647807,0,0,0,0,0,0,0,29.873175264555492,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"INDEX($C33:$AU33,MATCH(TRUE,INDEX($C33:$AU33<>0,0),0))","v":21.84290975317203}]
[null,{"$f":"\"Winter Peak Load\"","v":"Winter Peak Load"}]
[null,"Per Customer Winter Peak (kW)",{"$f":"IFERROR(INDEX(ClassValues,MATCH(State&Class&$B35,KeyCV,0),MATCH(C$7,YearsCV,0)),)","v":1.871393579636597},1.8624269805852776,1.8558419559389212,1.8507877390521588,1.8446903876176064,1.837423020944287,1.8301842848849286,1.8229740666459844,1.815792253878272,1.8086387346752213,1.8015133975711299,1.7944161315394274,1.7873468259909455,1.780305370772195,1.7732916561636474,1.7663055728780275,1.7593470120586103,1.752415865277523,1.7455120245340576,1.7386353822529867,1.7317858312828873,1.7249632648944728,1.7181675767789273,1.7113986610462517,1.7046564122236114,1.6979407252536947,1.6912514954930755,1.6845886187105814,1.6779519910856706,1.6713415092068149,1.6647570700698868,1.6581985710765554,1.6516659100326876,1.645158985146755,1.63867769502825,1.632221938686103,1.6257916155271108,1.6193866253543681,0,0,0,0,0,0,0]
[null,"Per Customer Winter Peak Reduction (%)",{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"},{"$f":"IF(INDEX(ImpactInput,MATCH(State&Class&Option&$B36,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0))>0,INDEX(ImpactInput,MATCH(State&Class&Option&$B23,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),\"n/a\")","v":"n/a"}]
[null,"Per Customer Winter Peak Reduction (kW)",{"$f":"IFERROR(IF(C36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),C35*C36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(D36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),D35*D36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(E36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),E35*E36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(F36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),F35*F36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(G36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),G35*G36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(H36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),H35*H36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(I36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),I35*I36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(J36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),J35*J36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(K36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),K35*K36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(L36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),L35*L36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(M36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),M35*M36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(N36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),N35*N36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(O36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),O35*O36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(P36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),P35*P36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(Q36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),Q35*Q36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(R36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),R35*R36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(S36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),S35*S36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(T36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),T35*T36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(U36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),U35*U36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(V36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),V35*V36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(W36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),W35*W36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(X36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),X35*X36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(Y36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),Y35*Y36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(Z36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),Z35*Z36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AA36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AA35*AA36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AB36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AB35*AB36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AC36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AC35*AC36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AD36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AD35*AD36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AE36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AE35*AE36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AF36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AF35*AF36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AG36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AG35*AG36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AH36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AH35*AH36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AI36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AI35*AI36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AJ36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AJ35*AJ36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AK36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AK35*AK36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AL36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AL35*AL36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AM36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AM35*AM36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AN36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AN35*AN36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AO36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AO35*AO36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AP36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AP35*AP36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AQ36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AQ35*AQ36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AR36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AR35*AR36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AS36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AS35*AS36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AT36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AT35*AT36),\"n/a\")","v":0.5},{"$f":"IFERROR(IF(AU36=\"n/a\",INDEX(ImpactInput,MATCH(State&Class&Option&$B37,KeyImp,0),MATCH(Potential,ImpactInput!$A$1:$G$1,0)),AU35*AU36),\"n/a\")","v":0.5}]
[]
[null,"Winter Peak Reduction @Meter  (MW)",{"$f":"IFERROR(C37*C19/1000,\"0\")","v":0.4495417348358503},{"$f":"IFERROR(D37*D19/1000,\"0\")","v":1.3477429145779078},3.1423617206591783,4.0341051910337979,4.4756001767454494,4.4688713839054843,4.4621527073965792,4.4554441320094469,4.4487456425576637,4.4420572238776375,4.4353788608285765,4.4287105382924539,4.4220522411739625,4.4154039544005004,4.4087656629221197,4.402137351711505,4.3955190057639273,4.3889106100972208,4.3823121497517423,4.3757236097903416,4.3691449752983216,4.3625762313834135,4.3560173631757353,4.3494683558277618,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Estimated Savings as % of Total Class Peak",{"$f":"C$39/INDEX(ClassValues,MATCH(State&Class&$B$34,KeyCV,0),MATCH(C$7,YearsCV,0))","v":1.9886111041577505E-3},5.9132976729196571E-3,1.3658957039087522E-2,1.7370772392794283E-2,1.9102160760008098E-2,1.891775398349144E-2,1.873512741705952E-2,1.8554263875075208E-2,1.8375146337806583E-2,1.8197757949825314E-2,1.8022082018420562E-2,1.7848102012028126E-2,1.767580155867474E-2,1.7505164444437518E-2,1.7336174611918099E-2,1.716881615873166E-2,1.7003073336010407E-2,1.6838930546921628E-2,1.6676372345199926E-2,1.6515383433693742E-2,1.6355948662925807E-2,1.6198053029667571E-2,1.6041681675527338E-2,1.5886819885552066E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,"Estimated Savings as % of Total System Peak",{"$f":"C$39/INDEX(ClassValues,MATCH(State&\"All\"&$B$34,KeyCV,0),MATCH(C$7,YearsCV,0))","v":1.0439295074988202E-3},3.1146537173634644E-3,7.2228291929336066E-3,9.2214189597630038E-3,1.0176544629693612E-2,1.0110303326410445E-2,1.0043804806492198E-2,9.9770774402005939E-3,9.9101485809507776E-3,9.8430445893662542E-3,9.7757908575647028E-3,9.708411833590818E-3,9.6409310459193154E-3,9.5733711279580441E-3,9.5057538424872332E-3,9.4381001059771399E-3,9.3704300127317609E-3,9.3027628588117552E-3,9.2351171656944973E-3,9.1675107036339725E-3,9.0999605146874444E-3,9.0324829353799711E-3,8.9650936189814533E-3,8.8978075573745551E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,"NPV MW @Meter",{"$f":"IF(C$71,NPV($C$50,OFFSET(C39,0,0,1,$C$51)),)","v":20.497386512376629},0,0,0,0,0,0,0,28.372447388693498,0,0,0,0,0,0,0,28.032987668258869,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"INDEX($C42:$AU42,MATCH(TRUE,INDEX($C42:$AU42<>0,0),0))","v":20.497386512376629}]
[null,"Winter Peak Reduction @Generation (MW)",{"$f":"C$39/(100%-INDEX(EnergyCosts,MATCH(State&Class&\"Line Loss\",KeyEC,0),MATCH(G$7,YearsEC,0)))*$P$49*$P$50","v":0.47905129458210816},1.436213677086432,3.3486378097391074,4.2989185752704584,4.7693949027551676,4.7622244074014111,4.7550646924515974,4.7479157416980469,4.7407775389574418,4.7336500680707987,4.7265333129034275,4.7194272573448997,4.7123318853089966,4.7052471807336964,4.698173127581116,4.6911097098374945,4.6840569115131361,4.6770147166423923,4.6699831092836126,4.6629620735191191,4.6559515934551596,4.6489516532218813,4.6419622369732902,4.6349833288872144,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"Estimated Savings as % of Total Class Peak",{"$f":"C$43/INDEX(ClassValues,MATCH(State&Class&$B$34,KeyCV,0),MATCH(C$7,YearsCV,0))","v":2.1191507930069806E-3},6.3014681083969062E-3,1.4555580817441948E-2,1.8511053274503711E-2,2.0356096291568732E-2,2.0159584381384741E-2,1.9964969540771014E-2,1.9772233455962501E-2,1.9581357989989962E-2,1.939232518097327E-2,1.920511724043112E-2,1.9019716551607124E-2,1.8836105667811957E-2,1.865426731078167E-2,1.8474184369051679E-2,1.8295839896346609E-2,1.8119217109985514E-2,1.794429938930267E-2,1.7771070274083468E-2,1.7599513463015495E-2,1.7429612812154528E-2,1.7261352333405339E-2,1.7094716193017199E-2,1.6929688710093847E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"Estimated Savings as % of Total System Peak",{"$f":"C$43/INDEX(ClassValues,MATCH(State&\"All\"&$B$34,KeyCV,0),MATCH(C$7,YearsCV,0))","v":1.1124568494232951E-3},3.3191109520071017E-3,7.6969620555558472E-3,9.8267465470620249E-3,1.0844570150994898E-2,1.0773980526865351E-2,1.0703116801462274E-2,1.0632009207374888E-2,1.0560686893596309E-2,1.048917795115756E-2,1.0417509439007568E-2,1.0345707410049891E-2,1.0273796937254172E-2,1.0201802139767738E-2,1.0129746208959114E-2,1.0057651434331991E-2,9.9855392292537946E-3,9.9134301564490143E-3,9.8413439532123795E-3,9.769299556302187E-3,9.6973151264785219E-3,9.6254080726555519E-3,9.5535950756409343E-3,9.4818921114392107E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"NPV MW @Generation",{"$f":"IF(C$71,NPV($C$50,OFFSET(C43,0,0,1,$C$51)),)","v":21.84290975317203},0,0,0,0,0,0,0,30.234918359647807,0,0,0,0,0,0,0,29.873175264555492,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},0,0,0,0,{"$f":"INDEX($C46:$AU46,MATCH(TRUE,INDEX($C46:$AU46<>0,0),0))","v":21.84290975317203}]
[null,"Cost Effectiveness"]
[null,"Years Shifted",0,null,null,null,null,"Summer DR Event Hours",null,null,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&H48,KeyCE,0),MATCH(Potential,YearsCE,0))","v":0},null,"Line Loss Factor"]
[null,"Program Start Year",{"$f":"MIN(INDEX(CEInput,MATCH(State&Class&Option&B49,KeyCE,0),MATCH(Potential,YearsCE,0))+C48,YearEnd)","v":2022},{"$f":"NOT(AND(E49,F49))","v":false},{"$f":"IF(AvoidedCostSavings?,INDEX($C$80:$AU$80,1,MATCH($C$49,$C$7:$AU$7,0)),TRUE)","v":true},{"$f":"IF(SingleDataSet?,IFERROR(MATCH(TRUE,INDEX($C$110:$AU$131<>\"\",MATCH(Option,$B$112:$B$131,0)),0)=\"\",TRUE),TRUE)","v":true},null,"Winter DR Event Hours",null,null,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&H49,KeyCE,0),MATCH(Potential,YearsCE,0))","v":50},null,"De-Rate Factor (capacity equivalence)",null,null,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"De-rate\",KeyCE,0),MATCH(Potential,YearsCE,0))","v":1}]
[null,"Discount Rate",{"$f":"DiscountRate","v":5.21E-2},null,null,null,null,"Total Annual DR Event Hours",null,null,{"$f":"SUM(K48:K49)","v":50},null,"Net to Gross Factor (free ridership)",null,null,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Net to Gross Ratio (free ridership)\",KeyCE,0),MATCH(Potential,YearsCE,0))","v":1}]
[null,"Program Life",{"$f":"INDEX(CEInput,MATCH(State&Class&Option&B51,KeyCE,0),MATCH(Potential,YearsCE,0))","v":8},null,null,null,null,"Rebound Effect (% Energy Savings Shifted)",null,null,0]
["Inflation Applied",{"$f":"State","v":"ID"}]
[0,"Program Development Cost",{"$f":"IF(C$19=0,0,INDEX(CEInput,MATCH(State&Class&Option&\"Program Development Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))/(1/$C$50*(1-(1/(1+$C$50)^$C$51))))*(1+$A53)^(C$7-YearBase)","v":10649.586385869012},{"$f":"IF(D$19=0,0,INDEX(CEInput,MATCH(State&Class&Option&\"Program Development Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))/(1/$C$50*(1-(1/(1+$C$50)^$C$51))))*(1+$A53)^(D$7-YearBase)","v":10649.586385869012},10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,10649.586385869012,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Annual Marketing/Recruitment Cost (for new participants)",{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*C$20*(1+$A54)^(C$7-YearBase)","v":53945.008180302037},{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*D$20*(1+$A54)^(D$7-YearBase)","v":107784.1415690469},{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*E$20*(1+$A54)^(E$7-YearBase)","v":215354.25672975247},107009.21644495438,52979.398285398092,0,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*I$20*(1+$A54)^(I$7-YearBase)","v":0},0,0,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*L$20*(1+$A54)^(L$7-YearBase)","v":0},0,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*N$20*(1+$A54)^(N$7-YearBase)","v":0},{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*O$20*(1+$A54)^(O$7-YearBase)","v":0},{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Per Customer Annual Marketing/Recruitment Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*P$20*(1+$A54)^(P$7-YearBase)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"AMI Cost",{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B55,KeyCE,0),MATCH(Potential,YearsCE,0))*C$20*(1+$A55)^(C$7-YearBase),0)","v":0},0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B55,KeyCE,0),MATCH(Potential,YearsCE,0))*N$20*(1+$A55)^(N$7-YearBase),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Cost of Equip + Install",{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B56,KeyCE,0),MATCH(Potential,YearsCE,0))*C$20*IF(Option=\"Battery Storage\",(1+$A56),1)^(C$7-YearBase),0)","v":413578.39604898228},{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B56,KeyCE,0),MATCH(Potential,YearsCE,0))*D$20*(D$7-YearBase),0)","v":826345.08536269295},{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B56,KeyCE,0),MATCH(Potential,YearsCE,0))*E$20*IF(Option=\"Battery Energy Storage\",(1+$A56),1)^(E$7-YearBase),0)","v":1651049.3015947689},820403.99274465023,406175.38685471873,0,0,0,0,0,{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B56,KeyCE,0),MATCH(Potential,YearsCE,0))*M$20*IF(Option=\"Battery Energy Storage\",(1+$A56),1)^(M$7-YearBase),0)","v":0},{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B56,KeyCE,0),MATCH(Potential,YearsCE,0))*N$20*IF(Option=\"Battery Energy Storage\",(1+$A56),1)^(N$7-YearBase),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Cost of Equip + Install (per kW basis)",{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B57,KeyCE,0),MATCH(Potential,YearsCE,0))*MAX(C$26,C$39)*(1+$A57)^(C$7-YearBase),0)*1000*IFERROR(C20/C19,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Annual Program Administration Cost",{"$f":"IF(C$19=0,0,IFERROR(INDEX(CEInput,MATCH(State&Class&Option&$B58,KeyCE,0),MATCH(Potential,YearsCE,0))*(1+$A58)^(C$7-YearBase),0))","v":81900},81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,81900,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Annual Program Administration Cost (per MW basis)",{"$f":"IFERROR(MAX(C$26,C$39)*INDEX(CEInput,MATCH(State&Class&Option&$B59,KeyCE,0),MATCH(Potential,YearsCE,0))*(1+$A59)^(C$7-YearBase),0)","v":0},{"$f":"IFERROR(MAX(D$26,D$39)*INDEX(CEInput,MATCH(State&Class&Option&$B59,KeyCE,0),MATCH(Potential,YearsCE,0))*(1+$A59)^(D$7-YearBase),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Operation & Maintenance Costs",{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Annual O&M Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*C$19*(1+$A60)^(C$7-YearBase)","v":20678.919802449116},61996.174070583758,144548.63915032221,185568.83878755473,205877.60813029067,205568.08365965227,205259.02454024262,204950.43007243454,204642.29955765253,204334.63229837132,204027.42759811453,203720.68476145287,203414.40309400225,{"$f":"INDEX(CEInput,MATCH(State&Class&Option&\"Annual O&M Cost\",KeyCE,0),MATCH(Potential,YearsCE,0))*P$19*(1+$A60)^(P$7-YearBase)","v":203108.581902423},202803.22049441753,202498.31817872924,202193.87426514065,201889.88806447218,201586.35888858014,201283.2860503557,200980.66886372279,200678.50664363703,200376.79870608382,200075.54436807704,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Operation & Maintenance Costs (per MW basis)",{"$f":"IFERROR(MAX(C$26,C$39)*INDEX(CEInput,MATCH(State&Class&Option&\"Annual O&M Cost per MW\",KeyCE,0),MATCH(Potential,YearsCE,0))*(1+$A61)^(C$7-YearBase),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"Participant Incentives",{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&\"Per Participant Annual Incentive\",KeyCE,0),MATCH(Potential,YearsCE,0))*C$19,0)*(1+$A62)^(C$7-YearBase)","v":21578.003272120815},64691.659899739578,150833.36259164056,193637.0491696223,{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&\"Per Participant Annual Incentive\",KeyCE,0),MATCH(Potential,YearsCE,0))*G$19,0)*(1+$A62)^(G$7-YearBase)","v":214828.80848378155},214505.82642746327,214183.32995503579,213861.31833645343,213539.79084276786,213218.74674612662,212898.1853197717,212578.10583803779,212258.50757635018,211939.38981122401,211620.75182026176,211302.59288215224,210984.91227666853,210667.70928466663,210350.98318808363,210034.73326993641,209718.95881431946,209403.65910640388,209088.83343243529,208774.48107973259,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"kW Annual Incentive",{"$f":"IFERROR(INDEX(CEInput,MATCH(State&Class&Option&\"Per \"&$B63,KeyCE,0),MATCH(Potential,YearsCE,0))*MAX(C$26,C$39)*1000,0)*(1+$A63)^(C$7-YearBase)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,"kWh Annual Incentive",{"$f":"(IFERROR(INDEX(CEInput,MATCH(State&Class&Option&\"Per \"&$B64,KeyCE,0),MATCH(Potential,YearsCE,0))*C$26*1000*$K$48,0) + IFERROR(INDEX(CEInput,MATCH(State&Class&Option&\"Per \"&$B64,KeyCE,0),MATCH(Potential,YearsCE,0))*C$39*1000*$K$49,0) )*(1+$A64)^(C$7-YearBase)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Non-Incentive Costs",{"$f":"SUM(C53:C61)","v":580751.9104176024},{"$f":"SUM(D53:D61)","v":1088674.9873881927},2103501.7838607128,1205531.6343630282,757581.97965627653,298117.67004552128,297808.61092611164,297500.01645830355,297191.88594352151,296884.21868424036,296577.01398398355,296270.27114732191,295963.98947987123,295658.16828829201,295352.80688028655,295047.90456459823,294743.46065100969,294439.47445034119,294135.94527444919,293832.87243622472,293530.25524959178,293228.09302950604,292926.38509195286,292625.13075394602,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Incentive Costs",{"$f":"SUM(C62:C64)","v":21578.003272120815},{"$f":"SUM(D62:D64)","v":64691.659899739578},150833.36259164056,193637.0491696223,214828.80848378155,214505.82642746327,214183.32995503579,213861.31833645343,213539.79084276786,213218.74674612662,212898.1853197717,212578.10583803779,212258.50757635018,211939.38981122401,211620.75182026176,211302.59288215224,210984.91227666853,210667.70928466663,210350.98318808363,210034.73326993641,209718.95881431946,209403.65910640388,209088.83343243529,208774.48107973259,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"Avoided Capacity Costs",{"$f":"C$30*1000*INDEX(EnergyCosts,MATCH(State&\"All\"&$B68,KeyEC,0),MATCH(C$7,YearsEC,0))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Avoided Energy Costs",{"$f":"C$30*INDEX(EnergyCosts,MATCH(State&\"All\"&\"Avoided Summer Energy Costs\",KeyEC,0),MATCH(C$7,YearsEC,0))*$K$48 + C$43*INDEX(EnergyCosts,MATCH(State&\"All\"&\"Avoided Summer Energy Costs\",KeyEC,0),MATCH(C$7,YearsEC,0))*$K$49","v":0},{"$f":"D$30*INDEX(EnergyCosts,MATCH(State&\"All\"&\"Avoided Summer Energy Costs\",KeyEC,0),MATCH(D$7,YearsEC,0))*$K$48 + D$43*INDEX(EnergyCosts,MATCH(State&\"All\"&\"Avoided Summer Energy Costs\",KeyEC,0),MATCH(D$7,YearsEC,0))*$K$49","v":0},{"$f":"E$30*INDEX(EnergyCosts,MATCH(State&\"All\"&\"Avoided Summer Energy Costs\",KeyEC,0),MATCH(E$7,YearsEC,0))*$K$48 + E$43*INDEX(EnergyCosts,MATCH(State&\"All\"&\"Avoided Summer Energy Costs\",KeyEC,0),MATCH(E$7,YearsEC,0))*$K$49","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
[null,"Evaluate Program B/C Ratio?",{"$f":"IF(C7>=$C$49,IF(TRUNC((C7-$C$49)/$C$51)= (C7-$C$49)/$C$51,TRUE,FALSE),FALSE)","v":true},false,false,false,false,false,false,false,true,false,false,false,false,false,false,false,true,{"$f":"IF(T7>=$C$49,IF(TRUNC((T7-$C$49)/$C$51)= (T7-$C$49)/$C$51,TRUE,FALSE),FALSE)","v":false},false,false,false,false,false,false,true,false,false,false,false,false,false,false,true,false,false,false,false,false,false,false,true,false,false,false,false]
[null,"Program Annual Benefits",{"$f":"SUM(C68:C69)","v":0},{"$f":"SUM(D68:D69)","v":0},{"$f":"SUM(E68:E69)","v":0},{"$f":"SUM(F68:F69)","v":0},{"$f":"SUM(G68:G69)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"Program Annual Costs",{"$f":"SUM(C65:C66)","v":602329.91368972324},{"$f":"SUM(D65:D66)","v":1153366.6472879322},{"$f":"SUM(E65:E66)","v":2254335.1464523533},1399168.6835326506,972410.78814005805,512623.49647298455,511991.9408811474,511361.33479475696,510731.67678628938,510102.96543036698,509475.19930375525,{"$f":"SUM(N65:N66)","v":508848.3769853597},{"$f":"SUM(O65:O66)","v":508222.49705622141},507597.55809951603,506973.55870054831,506350.49744675047,505728.37292767823,505107.18373500783,504486.92846253281,503867.60570616112,503249.21406391123,502631.75213590992,502015.21852438815,501399.61183367862,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Annual B/C Ratio",{"$f":"IFERROR(C72/C73,)","v":0},0,{"$f":"IFERROR(E72/E73,)","v":0},0,0,0,{"$f":"IFERROR(I72/I73,)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(Z72/Z73,)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(AU72/AU73,)","v":0}]
[null,"NPV Program Benefits",{"$f":"IF(C$71,NPV($C$50,OFFSET(C72,0,0,1,$C$51)),)","v":0},{"$f":"IF(D$71,NPV($C$50,OFFSET(D72,0,0,1,$C$51)),)","v":0},{"$f":"IF(E$71,NPV($C$50,OFFSET(E72,0,0,1,$C$51)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},0,0,0,0,{"$f":"INDEX($C75:$AU75,MATCH(TRUE,INDEX($C75:$AU75<>0,0),0))","v":{"$error":"#N/A"}}]
[null,"NPV Program Cost",{"$f":"IF(C$71,NPV($C$50,OFFSET(C73,0,0,1,$C$51)),)","v":6523882.0770330578},{"$f":"IF(D$71,NPV($C$50,OFFSET(D73,0,0,1,$C$51)),)","v":0},{"$f":"IF(E$71,NPV($C$50,OFFSET(E73,0,0,1,$C$51)),)","v":0},0,0,0,0,0,3260132.5516904076,0,0,0,0,0,0,0,3228223.3379695532,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"INDEX($C76:$AU76,MATCH(TRUE,INDEX($C76:$AU76<>0,0),0))","v":6523882.0770330578}]
[null,"Net Benefits",{"$f":"C75-C76","v":-6523882.0770330578},0,0,0,0,0,0,0,-3260132.5516904076,0,0,0,0,0,0,0,-3228223.3379695532,0,0,0,0,0,0,{"$f":"Z75-Z76","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},0,0,0,{"$f":"AU75-AU76","v":0},{"$f":"INDEX($C77:$AU77,MATCH(TRUE,INDEX($C77:$AU77<>0,0),0))","v":-6523882.0770330578}]
[]
[null,"Program B/C Ratio",{"$f":"IF(C76=0,IF(ISNUMBER(B79),B79,),C75/C76)","v":0},{"$f":"IF(D76=0,IF(ISNUMBER(C79),C79,),D75/D76)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(Z76=0,IF(ISNUMBER(Y79),Y79,),Z75/Z76)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Cost Effective Test",{"$f":"OR(C74>=BCmin,C79>=BCmin)","v":false},{"$f":"OR(D74>=BCmin,D79>=BCmin)","v":false},false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false,false]
[]
[]
["Options to Subtract if Hierarchy On","Data from Results"]
[null,"Participants"]
[null,"Total"]
[{"$f":"INDEX($C$135:$X$156,MATCH(Option,$B$135:$B$156,0),MATCH(B86,$C$134:$X$134,0))","v":0},{"$f":"ControlPanel!B8","v":"DLC Smart Thermostats - Cooling"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B86&$B$84&Potential&IFERROR(INDEX($C110:$AU110,MATCH(TRUE,INDEX($C110:$AU110<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":785.40997072114271},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B86&$B$84&Potential&IFERROR(INDEX($C110:$AU110,MATCH(TRUE,INDEX($C110:$AU110<>\"\",0),0)),YearMax),KeyR,0),MATCH(D$7,YearR,0)),)","v":2524.1579217239628},6308.8283794785284,8682.0609109653215,10325.473218605584,11051.967781997324,11829.578099550015,12661.900647349104,13552.784947540795,14506.351372512398,15527.010201764948,16619.482019616764,17788.81954807814,19040.431015874936,20380.105171703759,21814.03805740584,23348.861664886565,24991.674609319987,26750.074960502949,28632.195384205072,30541.595780320611,30914.736701077007,31292.436458501423,31674.750750027739,32061.735953571373,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B9","v":"DLC Smart Thermostats - Heating"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B87&$B$84&Potential&IFERROR(INDEX($C111:$AU111,MATCH(TRUE,INDEX($C111:$AU111<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":243.96098825737178},741.45479438773054,1752.5121995715467,2280.7587323758494,2565.1375839923221,2596.4770662787878,2628.1994376376019,2660.3093760031493,2692.8116164623175,2725.7109519527608,2759.0122339696882,2792.7203732812877,2826.8403406528946,2861.3771675800003,2896.3359470302253,2931.7218341943494,2967.540047246524,3003.795868113767,3040.4946432548631,3077.6417844487773,3115.2427695927022,3153.3031435098546,3191.8285187671449,3230.8245765028291,3270.29706726428,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B10","v":"DLC Central AC"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B88&$B$84&Potential&IFERROR(INDEX($C112:$AU112,MATCH(TRUE,INDEX($C112:$AU112<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":390.1516503334658},1236.047113526191,2993.8791709442066,4040.6690095947142,4743.0311371579992,5050.9439833623837,5377.1193532282996,5722.3936573029023,6087.6030207586919,6473.5754669227654,6881.1215229585368,7311.0230011660051,7764.0196741537593,8240.7935220901381,8741.9501847112406,9267.9971990127797,9819.3185447453943,10396.144953022243,10998.519357460609,11626.256781100434,12247.179907908565,12396.809417131881,12548.267019859069,12701.575050761123,12856.756117382121,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B11","v":"DLC Water Heating"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B89&$B$84&Potential&IFERROR(INDEX($C113:$AU113,MATCH(TRUE,INDEX($C113:$AU113<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":899.08346967170064},2695.4858291558157,6284.7234413183569,8068.2103820675966,8951.2003534908981,8937.7427678109689,8924.305414793158,8910.8882640188931,8897.4912851153276,8884.1144477552753,8870.7577216571535,8857.4210765849075,8844.1044823479242,8830.8079088009999,8817.5313258442402,8804.2747034230106,8791.0380115278549,8777.8212201944425,8764.6242995034845,8751.4472195806829,8738.2899505966434,8725.1524627668277,8712.0347263514705,8698.9367116555241,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B12","v":"CTA-2045 WH"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B90&$B$84&Potential&IFERROR(INDEX($C114:$AU114,MATCH(TRUE,INDEX($C114:$AU114<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B13","v":"DLC Electric Vehicle Charging"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B91&$B$84&Potential&IFERROR(INDEX($C115:$AU115,MATCH(TRUE,INDEX($C115:$AU115<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,56.147534921456717,199.76696382635797,552.80527007123476,842.92389335515327,1110.7532058030197,1317.31396456414,1562.2877090695806,1852.8178942652046,2197.3764047301052,2606.010595541818,3090.6362739934693,3665.3851655343205,4347.0169960696712,5155.4082069746028,6114.1315537923183,7251.1434897638228,8599.5993783502836,10198.820306413674,12095.439690409152,14344.763110721977,17012.38102703229,20176.081401623207,20422.581998566762,20672.094208275154,20924.654825026195,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B14","v":"Ancillary Cooling"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B92&$B$84&Potential&IFERROR(INDEX($C116:$AU116,MATCH(TRUE,INDEX($C116:$AU116<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":392.70498536057136},1262.0789608619814,3154.4141897392642,4341.0304554826607,5162.7366093027922,5525.983890998662,5914.7890497750077,6330.9503236745522,6776.3924737703974,7253.1756862561988,7763.5051008824739,8309.7410098083819,8894.4097740390698,9520.2155079374679,10190.052585851879,10907.01902870292,11674.430832443282,12495.837304659994,13375.037480251474,14316.097692102536,15270.797890160306,15457.368350538503,15646.218229250711,15837.375375013869,16030.867976785687,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B15","v":"Ancillary Heating"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B93&$B$84&Potential&IFERROR(INDEX($C117:$AU117,MATCH(TRUE,INDEX($C117:$AU117<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":121.98049412868589},370.72739719386527,876.25609978577336,1140.3793661879247,1282.5687919961611,1298.2385331393939,1314.099718818801,1330.1546880015746,1346.4058082311587,1362.8554759763804,1379.5061169848441,1396.3601866406439,1413.4201703264473,1430.6885837900002,1448.1679735151126,1465.8609170971747,1483.770023623262,1501.8979340568835,1520.2473216274316,1538.8208922243887,1557.6213847963511,1576.6515717549273,1595.9142593835725,1615.4122882514146,1635.14853363214,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B16","v":"Ancillary DLC WH"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B94&$B$84&Potential&IFERROR(INDEX($C118:$AU118,MATCH(TRUE,INDEX($C118:$AU118<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":899.08346967170064},2695.4858291558157,6284.7234413183569,8068.2103820675966,8951.2003534908981,8937.7427678109689,8924.305414793158,8910.8882640188931,8897.4912851153276,8884.1144477552753,8870.7577216571535,8857.4210765849075,8844.1044823479242,8830.8079088009999,8817.5313258442402,8804.2747034230106,8791.0380115278549,8777.8212201944425,8764.6242995034845,8751.4472195806829,8738.2899505966434,8725.1524627668277,8712.0347263514705,8698.9367116555241,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B17","v":"Ancillary WH"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B95&$B$84&Potential&IFERROR(INDEX($C119:$AU119,MATCH(TRUE,INDEX($C119:$AU119<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B18","v":"Ancillary EV"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B96&$B$84&Potential&IFERROR(INDEX($C120:$AU120,MATCH(TRUE,INDEX($C120:$AU120<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,56.147534921456717,199.76696382635797,552.80527007123476,842.92389335515327,1110.7532058030197,1317.31396456414,1562.2877090695806,1852.8178942652046,2197.3764047301052,2606.010595541818,3090.6362739934693,3665.3851655343205,4347.0169960696712,5155.4082069746028,6114.1315537923183,7251.1434897638228,8599.5993783502836,10198.820306413674,12095.439690409152,14344.763110721977,17012.38102703229,20176.081401623207,20422.581998566762,20672.094208275154,20924.654825026195,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B19","v":"Ancillary Third Party"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B97&$B$84&Potential&IFERROR(INDEX($C121:$AU121,MATCH(TRUE,INDEX($C121:$AU121<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B20","v":"Ancillary Battery Storage"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B98&$B$84&Potential&IFERROR(INDEX($C122:$AU122,MATCH(TRUE,INDEX($C122:$AU122<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":3.9862906578001924},24.230548836200345,61.982294923023893,100.3832984474747,139.71337603444019,179.98949756339388,221.22890889205408,276.62159287020273,333.3347712990589,391.39244210056478,464.480174068971,539.2953780846218,615.86935526206855,708.40195275797191,717.05682982526866,725.81744756247519,734.68509785267486,743.66108836248941,752.74674273491371,761.94340078450625,771.25241869496494,780.67516921911636,790.21304188134911,799.86744318251863,809.63979680735792,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B21","v":"DLC Smart Appliances"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B99&$B$84&Potential&IFERROR(INDEX($C123:$AU123,MATCH(TRUE,INDEX($C123:$AU123<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":597.9435986700289},1817.2911627150261,4295.373038165556,5590.0949322937486,6287.101921549809,6363.9143781342837,6441.6652883274564,6520.3661176547776,6600.0284717213672,6680.6640979234335,6762.2848871806082,6844.9028756894313,6928.5302466982721,7013.1793323039228,7098.8626152701599,7185.5927308685041,7273.3824687414808,7362.2447747886454,7452.1927530756457,7543.239667766612,7635.3989450801528,7728.6841752692517,7823.1091146253557,7918.6876875069347,8015.4339883928433,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B22","v":"Third Party Contracts"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B100&$B$84&Potential&IFERROR(INDEX($C124:$AU124,MATCH(TRUE,INDEX($C124:$AU124<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B23","v":"Time-of-Use Opt-in"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B101&$B$84&Potential&IFERROR(INDEX($C125:$AU125,MATCH(TRUE,INDEX($C125:$AU125<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":503.18825578083323},2935.0696512542081,8233.5552146786467,11861.851924739289,12924.995792888638,12989.278546299989,13047.020412970978,13097.680092622872,13140.684111522367,13175.425541423198,13201.262760408492,13217.51827602,13223.477634794055,13218.388446623861,13201.459557312863,13171.860408365679,13128.720629583955,13071.129917511767,12998.13826134177,12908.756587699781,12819.572165044932,12991.625633758762,13165.757960714165,13341.994579170523,14638.231207732766,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B24","v":"Time-of-Use Opt-out"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B102&$B$84&Potential&IFERROR(INDEX($C126:$AU126,MATCH(TRUE,INDEX($C126:$AU126<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B25","v":"Variable Peak Pricing Rates"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B103&$B$84&Potential&IFERROR(INDEX($C127:$AU127,MATCH(TRUE,INDEX($C127:$AU127<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":953.82700396447592},5444.9707001786601,16874.072181969688,19965.298647961932,21438.068876567584,21544.691587885307,21640.46524495956,21724.492019052566,21795.820716864899,21853.444655705502,21896.299608160531,21923.261850074403,21933.146351849533,21924.705160202993,21896.626025720594,21847.531340972873,21775.977464773441,21680.454520562238,21559.386771105172,21411.133687967293,21263.207775554733,21548.584588966842,21837.409504558753,22129.724707254565,24279.730058802656,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B26","v":"Real Time Pricing"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B104&$B$84&Potential&IFERROR(INDEX($C128:$AU128,MATCH(TRUE,INDEX($C128:$AU128<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B27","v":"Behavioral"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B105&$B$84&Potential&IFERROR(INDEX($C129:$AU129,MATCH(TRUE,INDEX($C129:$AU129<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":1915.7905620249282},7449.8012386146693,17763.666132678878,20071.855108770618,19683.754276660242,19781.651865383046,19869.588196909961,19946.738913396137,20012.230659350302,20065.139130683347,20104.487187568491,20129.243062159443,20138.318697899263,20130.568263700672,20104.7868938098,20059.709712817974,19994.011215217211,19906.305080282102,19795.144516107124,19659.023241562994,19523.202364792593,19785.226295390188,20050.416163946978,20318.810703321076,22292.877363757751,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B28","v":"Thermal Energy Storage"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B106&$B$84&Potential&IFERROR(INDEX($C130:$AU130,MATCH(TRUE,INDEX($C130:$AU130<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[0,{"$f":"ControlPanel!B29","v":"Battery Energy Storage"},{"$f":"IFERROR(INDEX(Results,MATCH(State&Class&$B107&$B$84&Potential&IFERROR(INDEX($C131:$AU131,MATCH(TRUE,INDEX($C131:$AU131<>\"\",0),0)),YearMax),KeyR,0),MATCH(C$7,YearR,0)),)","v":3.9862906578001924},24.230548836200345,61.982294923023893,100.3832984474747,139.71337603444019,179.98949756339388,221.22890889205408,276.62159287020273,333.3347712990589,391.39244210056478,464.480174068971,539.2953780846218,615.86935526206855,708.40195275797191,717.05682982526866,725.81744756247519,734.68509785267486,743.66108836248941,752.74674273491371,761.94340078450625,771.25241869496494,780.67516921911636,790.21304188134911,799.86744318251863,809.63979680735792,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"Shift Year CE Check"]
[null,{"$f":"ControlPanel!B8","v":"DLC Smart Thermostats - Cooling"},{"$f":"IF(ISNUMBER(INDEX(Results,MATCH(State&Class&$B110&$B$84&Potential&C$7-$F$7,KeyR,0),MATCH(C$7,YearR,0))),C$7-$F$7,\"\")","v":""},"","",0,"","","","","","","","","","","","",{"$f":"IF(ISNUMBER(INDEX(Results,MATCH(State&Class&$B110&$B$84&Potential&S$7-$F$7,KeyR,0),MATCH(S$7,YearR,0))),S$7-$F$7,\"\")","v":""},"","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B9","v":"DLC Smart Thermostats - Heating"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B10","v":"DLC Central AC"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B11","v":"DLC Water Heating"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B12","v":"CTA-2045 WH"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B13","v":"DLC Electric Vehicle Charging"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B14","v":"Ancillary Cooling"},"","","",0,"","","","","","","","","","","","","","","",{"$f":"IF(ISNUMBER(INDEX(Results,MATCH(State&Class&$B116&$B$84&Potential&V$7-$F$7,KeyR,0),MATCH(V$7,YearR,0))),V$7-$F$7,\"\")","v":""},"","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B15","v":"Ancillary Heating"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B16","v":"Ancillary DLC WH"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B17","v":"Ancillary WH"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B18","v":"Ancillary EV"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B19","v":"Ancillary Third Party"},"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B20","v":"Ancillary Battery Storage"},"","","",0,"","","","","","","","","","","","","","","","","","",{"$f":"IF(ISNUMBER(INDEX(Results,MATCH(State&Class&$B122&$B$84&Potential&Y$7-$F$7,KeyR,0),MATCH(Y$7,YearR,0))),Y$7-$F$7,\"\")","v":""},"","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B21","v":"DLC Smart Appliances"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B22","v":"Third Party Contracts"},"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B23","v":"Time-of-Use Opt-in"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B24","v":"Time-of-Use Opt-out"},"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B25","v":"Variable Peak Pricing Rates"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B26","v":"Real Time Pricing"},"","","","","","","","","","","","","","","","","","","","","","","","","",{"$f":"IF(ISNUMBER(INDEX(Results,MATCH(State&Class&$B128&$B$84&Potential&AB$7-$F$7,KeyR,0),MATCH(AB$7,YearR,0))),AB$7-$F$7,\"\")","v":""},"","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B27","v":"Behavioral"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B28","v":"Thermal Energy Storage"},"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[null,{"$f":"ControlPanel!B29","v":"Battery Energy Storage"},"","","",0,"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[]
[null,"Hierarchy Matrix","Options prior to X whose participants will no longer be available for X"]
[null,"Option X; currently under consideration","DLC Smart Thermostats - Cooling","DLC Smart Thermostats - Heating","DLC Central AC","DLC Water Heating","CTA-2045 WH","DLC Electric Vehicle Charging","Ancillary Cooling","Ancillary Heating","Ancillary DLC WH","Ancillary WH","Ancillary EV","Ancillary Third Party","Ancillary Battery Storage","DLC Smart Appliances","Third Party Contracts","Time-of-Use Opt-in","Time-of-Use Opt-out","Variable Peak Pricing Rates","Real Time Pricing","Behavioral","Thermal Energy Storage","Battery Energy Storage"]
[{"$f":"B135","v":"DLC Smart Thermostats - Cooling"},{"$f":"ControlPanel!B8","v":"DLC Smart Thermostats - Cooling"}]
[{"$f":"B136","v":"DLC Smart Thermostats - Heating"},{"$f":"ControlPanel!B9","v":"DLC Smart Thermostats - Heating"}]
["DLC Central AC",{"$f":"ControlPanel!B10","v":"DLC Central AC"},1]
["DLC Water Heating",{"$f":"ControlPanel!B11","v":"DLC Water Heating"}]
["CTA-2045 WH",{"$f":"ControlPanel!B12","v":"CTA-2045 WH"}]
["DLC Electric Vehicle Charging",{"$f":"ControlPanel!B13","v":"DLC Electric Vehicle Charging"}]
["Ancillary Cooling",{"$f":"ControlPanel!B14","v":"Ancillary Cooling"}]
["Ancillary Heating",{"$f":"ControlPanel!B15","v":"Ancillary Heating"}]
["Ancillary DLC WH",{"$f":"ControlPanel!B16","v":"Ancillary DLC WH"}]
["Ancillary WH",{"$f":"ControlPanel!B17","v":"Ancillary WH"}]
["Ancillary EV",{"$f":"ControlPanel!B18","v":"Ancillary EV"}]
["Ancillary Third Party",{"$f":"ControlPanel!B19","v":"Ancillary Third Party"}]
["Ancillary Battery Storage",{"$f":"ControlPanel!B20","v":"Ancillary Battery Storage"}]
["DLC Smart Appliances",{"$f":"ControlPanel!B21","v":"DLC Smart Appliances"}]
["Third Party Contracts",{"$f":"ControlPanel!B22","v":"Third Party Contracts"}]
["Time-of-Use Opt-in",{"$f":"ControlPanel!B23","v":"Time-of-Use Opt-in"},1,1,1,1,1,null,null,null,null,null,null,null,null,null,1]
["Time-of-Use Opt-out",{"$f":"ControlPanel!B24","v":"Time-of-Use Opt-out"},1,1,1,1,1,null,null,null,null,null,null,null,null,null,1]
["Variable Peak Pricing Rates",{"$f":"ControlPanel!B25","v":"Variable Peak Pricing Rates"},1,1,1,1,1,null,null,null,null,null,null,null,null,null,1,1,1]
["Real Time Pricing",{"$f":"ControlPanel!B26","v":"Real Time Pricing"},1,1,1,1,1,null,null,null,null,null,null,null,null,null,1,1,1,1]
["Behavioral",{"$f":"ControlPanel!B27","v":"Behavioral"},1,1,1,1,1]
["Thermal Energy Storage",{"$f":"ControlPanel!B28","v":"Thermal Energy Storage"},1,1,1,1,1]
["Battery Energy Storage",{"$f":"ControlPanel!B29","v":"Battery Energy Storage"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]

{"sheet":"Results","index":8,"n_rows":1161,"n_cols":53,"rows_kept":1161,"cut":false,"hidden":false,"merged":[]}
["Key","State","Customer Class","Option","Type","Potential","Years Shifted",{"$f":"YearBase","v":2022},{"$f":"H1+1","v":2023},{"$f":"I1+1","v":2024},2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,"NPV"]
[{"$f":"B2&C2&D2&E2&F2&G2","v":"WAResidentialAncillary ServicesParticipantsMarket Potential0"},"WA","Residential","Ancillary Services","Participants","Market Potential",0]
["WAResidentialAncillary ServicesNew ParticipantsMarket Potential0","WA","Residential","Ancillary Services","New Participants","Market Potential",0]
["WAResidentialAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WAResidentialAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
[{"$f":"B6&C6&D6&E6&F6&G6","v":"WAResidentialAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0"},"WA","Residential","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WAResidentialAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WAResidentialAncillary ServicesNon-Incentive CostsMarket Potential0","WA","Residential","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["WAResidentialAncillary ServicesIncentive CostsMarket Potential0","WA","Residential","Ancillary Services","Incentive Costs","Market Potential",0]
["WAResidentialAncillary ServicesProgram Annual BenefitsMarket Potential0","WA","Residential","Ancillary Services","Program Annual Benefits","Market Potential",0]
["WAResidentialAncillary ServicesProgram Annual CostsMarket Potential0","WA","Residential","Ancillary Services","Program Annual Costs","Market Potential",0]
["WAGeneral ServiceAncillary ServicesParticipantsMarket Potential0","WA","General Service","Ancillary Services","Participants","Market Potential",0]
["WAGeneral ServiceAncillary ServicesNew ParticipantsMarket Potential0","WA","General Service","Ancillary Services","New Participants","Market Potential",0]
["WAGeneral ServiceAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WAGeneral ServiceAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WAGeneral ServiceAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WAGeneral ServiceAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WAGeneral ServiceAncillary ServicesNon-Incentive CostsMarket Potential0","WA","General Service","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["WAGeneral ServiceAncillary ServicesIncentive CostsMarket Potential0","WA","General Service","Ancillary Services","Incentive Costs","Market Potential",0]
["WAGeneral ServiceAncillary ServicesProgram Annual BenefitsMarket Potential0","WA","General Service","Ancillary Services","Program Annual Benefits","Market Potential",0]
["WAGeneral ServiceAncillary ServicesProgram Annual CostsMarket Potential0","WA","General Service","Ancillary Services","Program Annual Costs","Market Potential",0]
["WALarge General ServiceAncillary ServicesParticipantsMarket Potential0","WA","Large General Service","Ancillary Services","Participants","Market Potential",0]
["WALarge General ServiceAncillary ServicesNew ParticipantsMarket Potential0","WA","Large General Service","Ancillary Services","New Participants","Market Potential",0]
["WALarge General ServiceAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WALarge General ServiceAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WALarge General ServiceAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WALarge General ServiceAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WALarge General ServiceAncillary ServicesNon-Incentive CostsMarket Potential0","WA","Large General Service","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["WALarge General ServiceAncillary ServicesIncentive CostsMarket Potential0","WA","Large General Service","Ancillary Services","Incentive Costs","Market Potential",0]
["WALarge General ServiceAncillary ServicesProgram Annual BenefitsMarket Potential0","WA","Large General Service","Ancillary Services","Program Annual Benefits","Market Potential",0]
["WALarge General ServiceAncillary ServicesProgram Annual CostsMarket Potential0","WA","Large General Service","Ancillary Services","Program Annual Costs","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesParticipantsMarket Potential0","WA","Extra Large General Service","Ancillary Services","Participants","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesNew ParticipantsMarket Potential0","WA","Extra Large General Service","Ancillary Services","New Participants","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesIncentive CostsMarket Potential0","WA","Extra Large General Service","Ancillary Services","Incentive Costs","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Ancillary Services","Program Annual Benefits","Market Potential",0]
["WAExtra Large General ServiceAncillary ServicesProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Ancillary Services","Program Annual Costs","Market Potential",0]
["WAResidentialDLC Central ACParticipantsMarket Potential0","WA","Residential","DLC Central AC","Participants","Market Potential",0,758.84063791856556,2394.837918380932,5782.0874932011657,7779.9046579885598,9104.3214161772667,9665.732362383309,10258.467756702032,10883.815216915176,11543.044257423364,12237.391660479048,12968.044143859022,13736.11792250779,14542.63470629816,15388.493613310549,16274.438406966698,17201.01938487991,18168.549156176534,19177.05144091597,20226.201908524716,21315.259940096435,22385.016967391239,22589.252645666395,22795.351722675674,23003.331199634893,23213.208232874993,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Central ACNew ParticipantsMarket Potential0","WA","Residential","DLC Central AC","New Participants","Market Potential",0,758.84063791856556,1635.9972804623665,3387.2495748202336,1997.8171647873942,1324.4167581887068,561.41094620604235,592.73539431872268,625.34746021314459,659.22904050818761,694.34740305568448,730.652483379974,768.07377864876798,806.51678379037003,845.85890701238895,885.94479365614825,926.58097791321234,967.52977129662395,1008.5022847394357,1049.1504676087461,1089.0580315717198,1069.7570272948033,204.23567827515581,206.09907700927943,207.97947695921903,209.87703324009999,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Central ACSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Central AC","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.3794203189592828,1.197418959190466,2.8910437466005829,3.8899523289942799,4.5521607080886337,4.8328661811916547,5.1292338783510161,5.4419076084575879,5.7715221287116822,6.118695830239524,6.4840220719295107,6.8680589612538956,7.2713173531490805,7.6942468066552747,8.1372192034833493,8.6005096924399549,9.0842745780882677,9.5885257204579855,10.113100954262357,10.657629970048218,11.192508483695619,11.294626322833198,11.397675861337836,11.501665599817446,11.606604116437497,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Central ACSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Central AC","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.40432685311091515,1.2760219087707438,3.0808224068633661,4.1453029933869141,4.8509811467270181,5.1501131513125049,5.4659355054891474,5.7991342801125194,6.1503859001616394,6.5203493502126211,6.9096569393963243,7.3189034113958815,7.7486331555297108,8.199325241533753,8.6713759627912932,9.1650785298805992,9.6805995077666953,10.217951535014903,10.776961801217345,11.35723568845718,11.927225579385784,12.036046806088233,12.145860892303746,12.256676896651157,12.368503960398014,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Central ACWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Central AC","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Central ACWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Central AC","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Central ACNon-Incentive CostsMarket Potential0","WA","Residential","DLC Central AC","Non-Incentive Costs","Market Potential",0,306317.34000000003,608275.43000000005,1212710.4099999999,794063.66,595792.94999999995,358929.43,376658.81,395224.19,414636.27,434900.67,456016.77,477976.55,500763.03,524348.67000000004,548693.43999999994,573742.56999999995,599424.06999999995,625645.81000000006,652292.18000000005,679220.35,686950.87,412639.11,415914.68,419220.14,422555.76,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Central ACIncentive CostsMarket Potential0","WA","Residential","DLC Central AC","Incentive Costs","Market Potential",0,15176.81,47896.76,115641.75,155598.09,182086.43,193314.65,205169.36,217676.3,230860.89,244747.83,259360.88,274722.36,290852.69,307769.87,325488.77,344020.39,363370.98,383541.03,404524.04,426305.2,447700.34,451785.05,455907.03,460066.62,464264.16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B50&C50&D50&E50&F50&G50","v":"WAResidentialDLC Central ACProgram Annual BenefitsMarket Potential0"},"WA","Residential","DLC Central AC","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Central ACProgram Annual CostsMarket Potential0","WA","Residential","DLC Central AC","Program Annual Costs","Market Potential",0,321494.15000000002,656172.18999999994,1328352.1599999999,949661.75,777879.38,552244.07999999996,581828.17000000004,612900.5,645497.16,679648.5,715377.66,752698.91,791615.72,832118.55,874182.21,917762.96,962795.05,1009186.83,1056816.22,1105525.55,1134651.21,864424.16,871821.72,879286.77,886819.93,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACParticipantsMarket Potential0","WA","General Service","DLC Central AC","Participants","Market Potential",0,75.34674423495477,237.93939337849065,574.74965265827882,773.79093597292388,906.05062700593771,962.48813176016756,1022.1133484584773,1085.060306047895,1151.4615454872555,1221.446655229513,1295.1405314840561,1372.661321896717,1454.1180055507946,1539.6075556910378,1629.2116242034044,1722.9926785325099,1820.989512257265,1923.2120398276952,2029.635273827832,2140.1923693849963,2248.9422573893944,2270.8143054496295,2292.9000259367103,2315.2015062594037,2337.7208542187905,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACNew ParticipantsMarket Potential0","WA","General Service","DLC Central AC","New Participants","Market Potential",0,75.34674423495477,162.59264914353588,336.81025927978817,199.04128331464506,132.25969103301384,56.437504754229849,59.625216698309714,62.946957589417707,66.401239439360552,69.985109742257464,73.693876254543056,77.520790412660972,81.456683654077551,85.489550140243182,89.604068512366666,93.781054329105473,97.996833724755106,102.2225275704302,106.42323400013674,110.5570955571643,108.74988800439814,21.872048060235102,22.085720487080835,22.301480322693351,22.519347959386778,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Central AC","Summer Peak Reduction @Meter  (MW)","Market Potential",0,9.4183430293693457E-2,0.29742424172311333,0.71843706582284861,0.96723866996615482,1.1325632837574222,1.2031101647002094,1.2776416855730965,1.3563253825598687,1.4393269318590693,1.5268083190368911,1.61892566435507,1.7158266523708963,1.8176475069384932,1.9245094446137974,2.0365145302542556,2.1537408481656377,2.2762368903215813,2.4040150497846189,2.5370440922847903,2.6752404617312453,2.8111778217367429,2.8385178818120367,2.8661250324208876,2.8940018828242544,2.9221510677734881,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Central AC","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.10036597431126754,0.31694825418064082,0.7655978962306571,1.0307317454882297,1.2069088701592308,1.2820867057760117,1.3615107476269144,1.4453595295821278,1.5338096034303808,1.6270335880614781,1.7251978520407822,1.8284597744787896,1.9369645214604574,2.0508412666387441,2.1701987747807499,2.2951202559309865,2.4256573852531771,2.561823369335698,2.7035849235771421,2.85085300695998,2.9957137912795639,3.024848552655623,3.054267937362412,3.0839747259423,3.11397172610133,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Central AC","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Central AC","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Central ACNon-Incentive CostsMarket Potential0","WA","General Service","DLC Central AC","Non-Incentive Costs","Market Potential",0,37316.39,68657.48,131398.91,87833.84,67181.38,42514.64,44357.65,46288.74,48309.14,50419.55,52620,54909.79,57287.25,59749.62,62292.84,64911.29,67597.53,70342.03,73132.77,75954.86,76763.19,47943.45,48302.14,48664.34,49030.080000000002,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACIncentive CostsMarket Potential0","WA","General Service","DLC Central AC","Incentive Costs","Market Potential",0,2863.18,9041.7000000000007,21840.49,29404.06,34429.919999999998,36574.550000000003,38840.31,41232.29,43755.54,46414.97,49215.34,52161.13,55256.480000000003,58505.09,61910.04,65473.72,69197.600000000006,73082.06,77126.14,81327.31,85459.81,86290.94,87130.2,87977.66,88833.39,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Central ACProgram Annual BenefitsMarket Potential0","WA","General Service","DLC Central AC","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Central ACProgram Annual CostsMarket Potential0","WA","General Service","DLC Central AC","Program Annual Costs","Market Potential",0,40179.57,77699.17,153239.4,117237.89,101611.31,79089.19,83197.960000000006,87521.03,92064.68,96834.52,101835.34,107070.92,112543.73,118254.71,124202.88,130385.01,136795.13,143424.09,150258.91,157282.17000000001,162222.99,134234.39000000001,135432.35,136642,137863.47,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingParticipantsMarket Potential0","WA","Residential","DLC Water Heating","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingNew ParticipantsMarket Potential0","WA","Residential","DLC Water Heating","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Water Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Water Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Water Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Water Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Water HeatingIncentive CostsMarket Potential0","WA","Residential","DLC Water Heating","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingNon-Incentive CostsMarket Potential0","WA","Residential","DLC Water Heating","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Water HeatingProgram Annual BenefitsMarket Potential0","WA","Residential","DLC Water Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Water HeatingProgram Annual CostsMarket Potential0","WA","Residential","DLC Water Heating","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingParticipantsMarket Potential0","WA","General Service","DLC Water Heating","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingNew ParticipantsMarket Potential0","WA","General Service","DLC Water Heating","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Water Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Water Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Water Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Water Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Water HeatingIncentive CostsMarket Potential0","WA","General Service","DLC Water Heating","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingNon-Incentive CostsMarket Potential0","WA","General Service","DLC Water Heating","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Water HeatingProgram Annual BenefitsMarket Potential0","WA","General Service","DLC Water Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Water HeatingProgram Annual CostsMarket Potential0","WA","General Service","DLC Water Heating","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B82&C82&D82&E82&F82&G82","v":"WAResidentialCTA-2045 WHParticipantsMarket Potential0"},"WA","Residential","CTA-2045 WH","Participants","Market Potential",0,81.223478302358103,491.81281650640284,1241.5057254489357,2505.665868742532,4214.2116336938188,6769.4297929861241,10787.475694178424,15766.426960499786,21731.586539070602,26098.830033606551,29379.222083309924,32717.300650097168,36113.845300565023,39569.645024472273,43085.498341795646,46662.213410954857,50300.608138219097,54001.510288307625,57765.757596197072,61594.197880148349,64186.730065662581,66821.442276759699,69498.888384410369,72219.628855167524,74984.230825413499,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialCTA-2045 WHNew ParticipantsMarket Potential0","WA","Residential","CTA-2045 WH","New Participants","Market Potential",0,81.223478302358103,410.58933820404474,749.69290894253277,1264.1601432935963,1708.5457649512869,2555.2181592923052,4018.0459011922994,4978.9512663213627,5965.1595785708159,4367.2434945359491,3280.3920497033723,3338.0785667872442,3396.5446504678548,3455.7997239072502,3515.8533173233736,3576.7150691592105,3638.3947272642399,3700.9021500885283,3764.2473078894473,3828.4402839512768,2592.532185514232,2634.7122110971177,2677.4461076506705,2720.740470757155,2764.6019702459744,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialCTA-2045 WHSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","CTA-2045 WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.0611739151179049E-2,0.24590640825320143,0.62075286272446784,1.2528329343712661,2.1071058168469095,3.3847148964930622,5.3937378470892119,7.8832134802498928,10.865793269535301,13.049415016803275,14.689611041654961,16.358650325048583,18.056922650282512,19.784822512236136,21.542749170897824,23.331106705477428,25.150304069109549,27.000755144153814,28.882878798098535,30.797098940074175,32.093365032831294,33.410721138379849,34.749444192205182,36.109814427583764,37.492115412706752,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialCTA-2045 WHSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","CTA-2045 WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.3277641891708275E-2,0.2620486021453553,0.66150134561430929,1.3350734594749212,2.2454239309962802,3.606899932324235,5.7478024798478389,8.4006963770778906,11.579063586461318,13.906026232740063,15.653890709350982,17.432491821236766,19.242244938493727,21.083570452084544,22.956893830880034,24.862645679323773,26.801261795726287,28.773183231195453,30.77885634920986,32.818732885842046,34.200090614696606,35.603922781734703,37.030524501497425,38.480194402795995,39.95323466827233,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialCTA-2045 WHWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","CTA-2045 WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.0611739151179049E-2,0.24590640825320143,0.62075286272446784,1.2528329343712661,2.1071058168469095,3.3847148964930622,5.3937378470892119,7.8832134802498928,10.865793269535301,13.049415016803275,14.689611041654961,16.358650325048583,18.056922650282512,19.784822512236136,21.542749170897824,23.331106705477428,25.150304069109549,27.000755144153814,28.882878798098535,30.797098940074175,32.093365032831294,33.410721138379849,34.749444192205182,36.109814427583764,37.492115412706752,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialCTA-2045 WHWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","CTA-2045 WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,4.3277641891708275E-2,0.2620486021453553,0.66150134561430929,1.3350734594749212,2.2454239309962802,3.606899932324235,5.7478024798478389,8.4006963770778906,11.579063586461318,13.906026232740063,15.653890709350982,17.432491821236766,19.242244938493727,21.083570452084544,22.956893830880034,24.862645679323773,26.801261795726287,28.773183231195453,30.77885634920986,32.818732885842046,34.200090614696606,35.603922781734703,37.030524501497425,38.480194402795995,39.95323466827233,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialCTA-2045 WHIncentive CostsMarket Potential0","WA","Residential","CTA-2045 WH","Incentive Costs","Market Potential",0,1949.36,11803.51,29796.14,60135.98,101141.08,162466.32,258899.42,378394.25,521558.08,626371.92000000004,705101.33,785215.22,866732.29,949671.48,1034051.96,1119893.1200000001,1207214.6000000001,1296036.25,1386378.18,1478260.75,1540481.52,1603714.61,1667973.32,1733271.09,1799621.54,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialCTA-2045 WHNon-Incentive CostsMarket Potential0","WA","Residential","CTA-2045 WH","Non-Incentive Costs","Market Potential",0,111230.99,186985.13,264978.96000000002,383306.42,485515.11,680249.76,1016700.14,1237708.3799999999,1464536.29,1097015.5900000001,847039.76,860307.66,873754.86,887383.52,901195.85,915194.05,929380.37,943757.08,958326.47,973090.85,688831.99,698533.39,708362.19,718319.89,728408.04,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialCTA-2045 WHProgram Annual BenefitsMarket Potential0","WA","Residential","CTA-2045 WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialCTA-2045 WHProgram Annual CostsMarket Potential0","WA","Residential","CTA-2045 WH","Program Annual Costs","Market Potential",0,113180.35,198788.64,294775.09000000003,443442.4,586656.18999999994,842716.08,1275599.56,1616102.62,1986094.37,1723387.51,1552141.09,1645522.87,1740487.14,1837055,1935247.81,2035087.17,2136594.9700000002,2239793.33,2344704.65,2451351.6,2229313.5099999998,2302248.0099999998,2376335.5099999998,2451590.9900000002,2528029.58,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHParticipantsMarket Potential0","WA","General Service","CTA-2045 WH","Participants","Market Potential",0,8.0648351441846877,48.864118242463242,123.4078497279866,249.21404863475183,419.39304628012889,671.27643049437745,1067.4563437341569,1558.101959656949,2145.8566905152543,2575.8316978759526,2898.8180517589435,3227.8417375788331,3562.9900303907057,3904.3513342781184,4252.0151960832236,4606.0723192973946,4966.6145781142013,5333.7350316465581,5707.5279383099378,6088.088770373507,6487.3010789993705,6893.7052237882954,7307.4037671981741,7728.5005892240351,8157.100903352336,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHNew ParticipantsMarket Potential0","WA","General Service","CTA-2045 WH","New Participants","Market Potential",0,8.0648351441846877,40.799283098278551,74.543731485523352,125.80619890676523,170.17899764537705,251.88338421424857,396.17991323977947,490.6456159227921,587.75473085830527,429.97500736069833,322.9863538829909,329.02368581988958,335.14829281187258,341.36130388741276,347.66386180510517,354.05712321417104,360.54225881680668,367.12045353235681,373.79290666337965,380.56083206356925,399.21230862586344,406.4041447889249,413.69854340987877,421.096822025861,428.60031412830085,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","CTA-2045 WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.0161692281672708E-2,6.1568788985503685E-2,0.1554938906572631,0.31400970127978728,0.52843523831296235,0.8458083024229156,1.3449949931050378,1.9632084691677558,2.7037794300492206,3.2455479393237003,3.6525107452162686,4.06708058934933,4.4893674382922892,4.9194826811904298,5.3575391470648617,5.8036511223147169,6.2579343684238937,6.7205061398746633,7.1914852022705213,7.6709918506706192,8.1739993595392075,8.6860685819732524,9.2073287466697007,9.7379107424222831,10.277947138223942,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","CTA-2045 WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.082874284065719E-2,6.5610388944483886E-2,0.1657010770004935,0.33462244381904016,0.56312365549122156,0.90133024554871655,1.4332853720215661,2.092080636368026,2.8812653772903034,3.4585975482989135,3.8922748776814458,4.3340585990508629,4.784065897583428,5.2424154744143543,5.7092275650733821,6.1846239581358873,6.6687280140919585,7.161664684435916,7.663560530978816,8.1745437453864227,8.7105705024927609,9.2562538171070461,9.8117314009694159,10.377142734891606,10.952629090178966,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","CTA-2045 WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.0161692281672708E-2,6.1568788985503685E-2,0.1554938906572631,0.31400970127978728,0.52843523831296235,0.8458083024229156,1.3449949931050378,1.9632084691677558,2.7037794300492206,3.2455479393237003,3.6525107452162686,4.06708058934933,4.4893674382922892,4.9194826811904298,5.3575391470648617,5.8036511223147169,6.2579343684238937,6.7205061398746633,7.1914852022705213,7.6709918506706192,8.1739993595392075,8.6860685819732524,9.2073287466697007,9.7379107424222831,10.277947138223942,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","CTA-2045 WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.082874284065719E-2,6.5610388944483886E-2,0.1657010770004935,0.33462244381904016,0.56312365549122156,0.90133024554871655,1.4332853720215661,2.092080636368026,2.8812653772903034,3.4585975482989135,3.8922748776814458,4.3340585990508629,4.784065897583428,5.2424154744143543,5.7092275650733821,6.1846239581358873,6.6687280140919585,7.161664684435916,7.663560530978816,8.1745437453864227,8.7105705024927609,9.2562538171070461,9.8117314009694159,10.377142734891606,10.952629090178966,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceCTA-2045 WHIncentive CostsMarket Potential0","WA","General Service","CTA-2045 WH","Incentive Costs","Market Potential",0,193.56,1172.74,2961.79,5981.14,10065.43,16110.63,25618.95,37394.449999999997,51500.56,61819.96,69571.63,77468.2,85511.76,93704.43,102048.36,110545.74,119198.75,128009.64,136980.67000000001,146114.13,155695.23000000001,165448.93,175377.69,185484.01,195770.42,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHNon-Incentive CostsMarket Potential0","WA","General Service","CTA-2045 WH","Non-Incentive Costs","Market Potential",0,11129.14,19149.080000000002,27416.47,39975.769999999997,50847.11,70864.679999999993,106217.33,129361.43,153153.16,114497.13,88284.91,89764.06,91264.59,92786.78,94330.9,95897.25,97486.11,99097.77,100732.52,102390.66,106960.27,108722.27,110509.4,112321.98,114160.33,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceCTA-2045 WHProgram Annual BenefitsMarket Potential0","WA","General Service","CTA-2045 WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceCTA-2045 WHProgram Annual CostsMarket Potential0","WA","General Service","CTA-2045 WH","Program Annual Costs","Market Potential",0,11322.7,20321.82,30378.26,45956.91,60912.54,86975.32,131836.29,166755.88,204653.73,176317.09,157856.54999999999,167232.26,176776.35,186491.21,196379.27,206442.99,216684.86,227107.41,237713.19,248504.79,262655.5,274171.2,285887.09000000003,297805.99,309930.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B102&C102&D102&E102&F102&G102","v":"WAResidentialDLC Smart Thermostats - CoolingParticipantsMarket Potential0"},"WA","Residential","DLC Smart Thermostats - Cooling","Participants","Market Potential",0,1527.6136925224514,4890.5491034893848,12184.258477682957,16716.441253111807,19819.905085557548,21149.583723428306,22568.467898478873,24082.542235592948,25698.192856423731,27422.23431502633,29261.938340548979,31225.06450821523,33319.892967962231,35555.259368779341,37940.592126052252,40485.9521891002,43202.075476639613,46100.418159159679,49193.204979204107,52493.480813365866,55822.984956087887,56332.300862010954,56846.26364757026,57364.915709812696,57888.299832605961,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - CoolingNew ParticipantsMarket Potential0","WA","Residential","DLC Smart Thermostats - Cooling","New Participants","Market Potential",0,1527.6136925224514,3362.9354109669334,7293.7093741935723,4532.1827754288497,3103.463832445741,1329.6786378707584,1418.8841750505671,1514.0743371140743,1615.6506208307837,1724.0414586025981,1839.7040255226493,1963.1261676662507,2094.828459747001,2235.3664008171108,2385.3327572729104,2545.3600630479486,2716.1232875394126,2898.3426825200659,3092.7868200444282,3300.2758341617591,3329.5041427220203,509.31590592306748,513.96278555930621,518.65206224243593,523.3841227932644,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.76380684626122575,2.4452745517446925,6.0921292388414789,8.3582206265559034,9.9099525427787736,10.574791861714154,11.284233949239436,12.041271117796473,12.849096428211865,13.711117157513165,14.63096917027449,15.612532254107615,16.659946483981116,17.77762968438967,18.970296063026126,20.242976094550102,21.601037738319807,23.05020907957984,24.596602489602052,26.246740406682932,27.911492478043943,28.166150431005477,28.42313182378513,28.68245785490635,28.94414991630298,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - CoolingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.81394591460062415,2.6057912955506102,6.4920388308199906,8.906884725656333,10.560477986763399,11.268959784435372,12.02497223917246,12.831704089723436,13.692558001078288,14.611164916361002,15.591399371562755,16.637395837710585,17.753566159400165,18.944618163245597,20.215575514733722,21.571798907235827,23.019008672548814,24.563308908333163,26.211213224213608,27.969672215135265,29.743704686747595,30.015079316928258,30.288929905994383,30.565279044017849,30.844149527177088,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - CoolingWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Smart Thermostats - CoolingNon-Incentive CostsMarket Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Non-Incentive Costs","Market Potential",0,211498.35,469586.81,1026356.46,1060080.9099999999,1110910.18,1062988.93,1130772.1599999999,1203102.8400000001,1280286.05,1362647.32,1450534.05,1544316.93,1644391.52,1751179.92,1865132.54,1986730.02,2116485.2400000002,2254945.48,2402694.75,2560356.23,2708608.11,2561806.7200000002,2584699.89,2607801.94,2631114.7599999998,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - CoolingIncentive CostsMarket Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Incentive Costs","Market Potential",0,30552.27,97810.98,243685.17,334328.83,396398.1,422991.67,451369.36,481650.84,513963.86,548444.68999999994,585238.77,624501.29,666397.86,711105.19,758811.84,809719.04,864041.51,922008.36,983864.1,1049869.6200000001,1116459.7,1126646.02,1136925.27,1147298.31,1157766,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - CoolingProgram Annual BenefitsMarket Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Smart Thermostats - CoolingProgram Annual CostsMarket Potential0","WA","Residential","DLC Smart Thermostats - Cooling","Program Annual Costs","Market Potential",0,242050.62,567397.79,1270041.6299999999,1394409.73,1507308.28,1485980.6,1582141.52,1684753.69,1794249.9,1911092.01,2035772.82,2168818.2200000002,2310789.38,2462285.11,2623944.39,2796449.07,2980526.75,3176953.85,3386558.85,3610225.85,3825067.81,3688452.73,3721625.16,3755100.25,3788880.76,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingParticipantsMarket Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Participants","Market Potential",0,151.67969719704959,485.90106162954532,1211.1366934833288,1662.6207250624643,1972.4520487665013,2106.0197574566887,2248.6333086363197,2400.9053928030767,2563.4902026523459,2737.0862445451621,2922.4393404443281,3120.3458332230016,3331.6560091243909,3557.2777520847085,3798.1804456283858,4055.3991391088653,4330.0389962047611,4623.2800447946456,4936.3822486294039,5270.6909226045791,5608.3348064573438,5662.8785672060594,5717.9551768995279,5773.5698410458963,5829.7278160069591,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingNew ParticipantsMarket Potential0","WA","General Service","DLC Smart Thermostats - Cooling","New Participants","Market Potential",0,151.67969719704959,334.22136443249576,725.2356318537835,451.48403157913549,309.831323704037,133.56770869018737,142.61355117963103,152.27208416675694,162.58480984926928,173.59604189281617,185.35309589916596,197.90649277867351,211.31017590138936,225.62174296031753,240.90269354367729,257.21869348047949,274.63985709589588,293.24104858988449,313.10220383475826,334.30867397517522,337.6438838527647,54.543760748715613,55.076609693468527,55.614664146368341,56.157974961062791,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.18959962149631199,0.60737632703693167,1.5139208668541611,2.0782759063280807,2.4655650609581268,2.6325246968208607,2.8107916357953995,3.0011317410038458,3.2043627533154324,3.4213578056814526,3.6530491755554104,3.9004322915287521,4.1645700114054893,4.4465971901058854,4.7477255570354817,5.0692489238860814,5.4125487452559522,5.7791000559933074,6.1704778107867551,6.5883636532557235,7.0104185080716794,7.0785982090075743,7.1474439711244102,7.2169623013073707,7.2871597700086985,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.20204563245557544,0.64724672531642335,1.613300156494204,2.21470151995746,2.6274137478240909,2.8053332233811386,2.9953022546839296,3.1981369789043539,3.4147088164060446,3.6459482157730738,3.892848652552654,4.1564708989010573,4.4379475824866681,4.7384880542475338,5.0593835859286891,5.4020129197422007,5.7678481940067687,6.1584612702400978,6.5755304889031914,7.0208478828385799,7.4706079583031535,7.5432632235801087,7.6166282727242223,7.6907100397563628,7.7655155264372322,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Smart Thermostats - CoolingNon-Incentive CostsMarket Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Non-Incentive Costs","Market Potential",0,28939.34,57335.7,118572.14,117906.07,120914.69,113571.9,120525.34,127949.7,135876.88,144340.95000000001,153378.26999999999,163027.66,173330.58,184331.3,196077.09,208618.42,222009.16,236306.85,251572.94,267873,282979.48,264146.89,266610.23,269097.63,271609.33,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingIncentive CostsMarket Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Incentive Costs","Market Potential",0,3033.59,9718.02,24222.73,33252.410000000003,39449.040000000001,42120.4,44972.67,48018.11,51269.8,54741.72,58448.79,62406.92,66633.119999999995,71145.56,75963.61,81107.98,86600.78,92465.600000000006,98727.65,105413.82,112166.7,113257.57,114359.1,115471.4,116594.56,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - CoolingProgram Annual BenefitsMarket Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Smart Thermostats - CoolingProgram Annual CostsMarket Potential0","WA","General Service","DLC Smart Thermostats - Cooling","Program Annual Costs","Market Potential",0,31972.93,67053.72,142794.87,151158.48000000001,160363.73000000001,155692.29999999999,165498,175967.8,187146.69,199082.68,211827.05,225434.57,239963.7,255476.86,272040.7,289726.40000000002,308609.94,328772.45,350300.58,373286.82,395146.17,377404.46,380969.33,384569.02,388203.88,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B122&C122&D122&E122&F122&G122","v":"WAResidentialDLC Smart Thermostats - HeatingParticipantsMarket Potential0"},"WA","Residential","DLC Smart Thermostats - Heating","Participants","Market Potential",0,474.50141963576914,1436.5666461527235,3384.6318746488732,4391.3731720229944,4923.8211527694102,4968.7449495351793,5014.0786205537379,5059.8259054222499,5105.9905778570956,5152.5764460051651,5199.5873527579897,5247.027176068751,5294.8998292721681,5343.209261407319,5391.9594575433894,5441.1544391084099,5490.7982642209827,5540.8950280250392,5591.4488630276483,5642.463939439911,5693.9444655209645,5745.8946879251171,5798.3188920521661,5851.2214024008945,5904.6065829258077,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - HeatingNew ParticipantsMarket Potential0","WA","Residential","DLC Smart Thermostats - Heating","New Participants","Market Potential",0,474.50141963576914,962.06522651695434,1948.0652284961498,1006.7412973741211,532.44798074641585,44.923796765769112,45.333671018558562,45.747284868511997,46.16467243484567,46.585868148069494,47.010906752824667,47.439823310761312,47.87265320341703,48.309432135150928,48.750196136070372,49.194981565020498,49.643825112572813,50.096763804056536,50.553835002609048,51.015076412262715,51.48052608105354,51.950222404152555,52.424204127049052,52.902510348728356,53.385180524913267,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - HeatingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.51720654740298833,1.5658576443064687,3.6892487433672723,4.7865967575050643,5.3669650565186577,5.415931994993346,5.4653456964035749,5.5152102369102529,5.5655297298642346,5.6163083261456306,5.6675502145062095,5.7192596219149392,5.771440813906664,5.8240980949339782,5.8772358087222951,5.930858338628167,5.9849701080008719,6.0395755805472939,6.0946792607001372,6.1502856939895034,6.2063994674178522,6.2630252098383776,6.320167592336861,6.377831328616975,6.436021175389131,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - HeatingWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Smart Thermostats - Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.55115787233907532,1.6686462535235174,3.9314244920793611,5.1008064338289261,5.7192722256166428,5.7714535326016048,5.8241109296713285,5.8772487605607981,5.930871408636226,5.9849832972566395,6.0395888901387567,6.0946926917252124,6.1502992475561209,6.2064131446440518,6.2630390118524026,6.3201815202772451,6.3778453836326428,6.4360353586394865,6.4947562454178787,6.5540128878831023,6.613810174145196,6.6741530369121671,6.7350464538969108,6.7964954482278079,6.8585050888630974,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Smart Thermostats - HeatingNon-Incentive CostsMarket Potential0","WA","Residential","DLC Smart Thermostats - Heating","Non-Incentive Costs","Market Potential",0,104380.21,175964.9,320839.77,308656.96000000002,303627.07,276352.26,278371.53999999998,280409.24,282465.52,284540.57,286634.56,288747.64,290880.01,293031.83,295203.28999999998,297394.55,299605.81,301837.25,304089.03999999998,306361.38,308654.45,310968.44,313303.53999999998,315659.95,318037.86,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - HeatingIncentive CostsMarket Potential0","WA","Residential","DLC Smart Thermostats - Heating","Incentive Costs","Market Potential",0,9490.0300000000007,28731.33,67692.639999999999,87827.46,98476.42,99374.9,100281.57,101196.52,102119.81,103051.53,103991.75,104940.54,105898,106864.19,107839.19,108823.09,109815.97,110817.9,111828.98,112849.28,113878.89,114917.89,115966.38,117024.43,118092.13,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart Thermostats - HeatingProgram Annual BenefitsMarket Potential0","WA","Residential","DLC Smart Thermostats - Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Smart Thermostats - HeatingProgram Annual CostsMarket Potential0","WA","Residential","DLC Smart Thermostats - Heating","Program Annual Costs","Market Potential",0,113870.23,204696.24,388532.41,396484.42,402103.49,375727.16,378653.11,381605.75,384585.34,387592.1,390626.3,393688.19,396778.01,399896.02,403042.48,406217.64,409421.78,412655.15,415918.02,419210.66,422533.34,425886.33,429269.92,432684.38,436129.99,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingParticipantsMarket Potential0","WA","General Service","DLC Smart Thermostats - Heating","Participants","Market Potential",0,9.8385445917029699,29.80543294858154,70.25624434686064,91.207203366326695,102.3261384394816,103.32056052748511,104.32469732447058,105.33864373537725,106.36249559228976,107.39634966349558,108.44030366263101,109.49445625791637,110.55890708148168,111.63375673878316,112.71910681811192,113.81505990019545,114.92171956789292,116.03919041598519,117.16757806106054,118.30698915149685,119.45753137754139,120.61931348148903,121.79244526795993,122.97703761427755,124.17320248094819,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingNew ParticipantsMarket Potential0","WA","General Service","DLC Smart Thermostats - Heating","New Participants","Market Potential",0,9.8385445917029699,19.96688835687857,40.4508113982791,20.950959019466055,11.118935073154901,0.9944220880035175,1.0041367969854633,1.0139464109066694,1.0238518569125148,1.0338540712058233,1.0439539991354252,1.054152595285359,1.0644508235653092,1.0748496573014847,1.0853500793287623,1.0959530820835255,1.1066596676974711,1.1174708480922675,1.1283876450753496,1.1394110904363117,1.1505422260445357,1.1617821039476439,1.1731317864709041,1.1845923463176149,1.1961648666706424,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.328203519879901E-2,4.0237334480585085E-2,9.4845929868261875E-2,0.12312972454454105,0.13814028689330016,0.13948275671210489,0.14083834138803528,0.14220716904275929,0.14358936904959119,0.14498507204571906,0.14639440994455188,0.14781751594818709,0.14925452456000027,0.15070557159735729,0.15217079420445112,0.15365033086526386,0.15514432141665546,0.15665290706158,0.15817623038243173,0.15971443535452076,0.16126766735968087,0.1628360732000102,0.16441980111174592,0.1660190007792747,0.16763382334928006,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Smart Thermostats - Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.4153916452258108E-2,4.2878659932422299E-2,0.10107196277521513,0.13121240893493291,0.14720831936626189,0.1486389138023283,0.15008348400259514,0.1515421664991041,0.15301509915770586,0.15450242119109023,0.1560042731719436,0.15752079704623517,0.15905213614663286,0.16059843520604997,0.16215984037132472,0.16373649921703309,0.16532856075943678,0.16693617547056691,0.16855949529244643,0.17019867365145008,0.17185386547280571,0.17352522719523678,0.17521291678574799,0.1769170937545553,0.17863791917016206,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Smart Thermostats - HeatingNon-Incentive CostsMarket Potential0","WA","General Service","DLC Smart Thermostats - Heating","Non-Incentive Costs","Market Potential",0,9920.41,11558.58,14874.71,14334.06,14085.89,13370.31,13415.22,13460.57,13506.36,13552.6,13599.29,13646.44,13694.05,13742.12,13790.66,13839.68,13889.18,13939.16,13989.63,14040.59,14092.04,14144.01,14196.48,14249.46,14302.96,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingIncentive CostsMarket Potential0","WA","General Service","DLC Smart Thermostats - Heating","Incentive Costs","Market Potential",0,196.77,596.11,1405.12,1824.14,2046.52,2066.41,2086.4899999999998,2106.77,2127.25,2147.9299999999998,2168.81,2189.89,2211.1799999999998,2232.6799999999998,2254.38,2276.3000000000002,2298.4299999999998,2320.7800000000002,2343.35,2366.14,2389.15,2412.39,2435.85,2459.54,2483.46,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart Thermostats - HeatingProgram Annual BenefitsMarket Potential0","WA","General Service","DLC Smart Thermostats - Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Smart Thermostats - HeatingProgram Annual CostsMarket Potential0","WA","General Service","DLC Smart Thermostats - Heating","Program Annual Costs","Market Potential",0,10117.18,12154.69,16279.83,16158.21,16132.42,15436.72,15501.71,15567.34,15633.61,15700.53,15768.1,15836.33,15905.23,15974.8,16045.05,16115.98,16187.61,16259.94,16332.98,16406.73,16481.2,16556.39,16632.32,16709,16786.419999999998,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesParticipantsMarket Potential0","WA","Residential","DLC Smart Appliances","Participants","Market Potential",0,1162.9936755778656,3520.9966817468717,8295.6663594335132,10763.169539272047,12068.189099925026,12178.296444939166,12289.408383710143,12401.53408191728,12514.682788865432,12628.863838247955,12744.086648916642,12860.360725658704,12977.695659980805,13096.101130900292,13215.586905743603,13336.162840951985,13457.838882894566,13580.625068688822,13704.53152702855,13829.56847901939,13955.746239021972,14083.075215502739,14211.565911892565,14341.228927453174,14472.07495815149,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesNew ParticipantsMarket Potential0","WA","Residential","DLC Smart Appliances","New Participants","Market Potential",0,1162.9936755778656,2358.0030061690059,4774.6696776866411,2467.5031798385335,1305.0195606529796,110.10734501413936,111.11193877097685,112.12569820713725,113.14870694815181,114.18104938252327,115.22281066868709,116.27407674206188,117.33493432210162,118.40547091948611,119.48577484331145,120.57593520838236,121.67604194258092,122.78618579425529,123.90645833972849,125.03695199083995,126.17776000258164,127.32897648076687,128.49069638982655,129.66301556060898,130.8460306983161,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Smart Appliances","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.16281911458090118,0.49293953544456209,1.1613932903206918,1.5068437354980868,1.6895464739895036,1.7049615022914835,1.72051717371942,1.7362147714684193,1.7520555904411605,1.7680409373547139,1.78417213084833,1.8004505015922185,1.8168773923973129,1.8334541583260409,1.8501821668041045,1.8670627977332781,1.8840974436052396,1.9012875096164352,1.9186344137839972,1.9361395870627147,1.9538044734630762,1.9716305301703836,1.9896192276649591,2.0077720498434446,2.0260904941412088,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Smart Appliances","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.17350715535049144,0.52529788517110199,1.2376313835471993,1.605758456413136,1.8004544692982776,1.8168813963037973,1.8334581987632352,1.8501862441053061,1.8670669122348258,1.8841015956465408,1.9012916995399936,1.9186386419354418,1.936143853790828,1.9538087791198218,1.9716348751109383,1.9896236122477389,2.0077764744301358,2.026094959096798,2.0445805773486758,2.0632348540736518,2.0820593280723316,2.1010555521849783,2.1202250934196067,2.1395695330812496,2.1590904669023963,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Smart Appliances","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.16281911458090118,0.49293953544456209,1.1613932903206918,1.5068437354980868,1.6895464739895036,1.7049615022914835,1.72051717371942,1.7362147714684193,1.7520555904411605,1.7680409373547139,1.78417213084833,1.8004505015922185,1.8168773923973129,1.8334541583260409,1.8501821668041045,1.8670627977332781,1.8840974436052396,1.9012875096164352,1.9186344137839972,1.9361395870627147,1.9538044734630762,1.9716305301703836,1.9896192276649591,2.0077720498434446,2.0260904941412088,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Smart Appliances","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.17350715535049144,0.52529788517110199,1.2376313835471993,1.605758456413136,1.8004544692982776,1.8168813963037973,1.8334581987632352,1.8501862441053061,1.8670669122348258,1.8841015956465408,1.9012916995399936,1.9186386419354418,1.936143853790828,1.9538087791198218,1.9716348751109383,1.9896236122477389,2.0077764744301358,2.026094959096798,2.0445805773486758,2.0632348540736518,2.0820593280723316,2.1010555521849783,2.1202250934196067,2.1395695330812496,2.1590904669023963,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Smart AppliancesNon-Incentive CostsMarket Potential0","WA","Residential","DLC Smart Appliances","Non-Incentive Costs","Market Potential",0,466106.83,884360.1,1730193.43,922685.16,515815.89,97596.61,97948.22,98303.039999999994,98661.09,99022.41,99387.03,99754.97,100126.27,100500.96,100879.06,101260.62,101645.66,102034.21,102426.3,102821.98,103221.26,103624.19,104030.79,104441.1,104855.15,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesIncentive CostsMarket Potential0","WA","Residential","DLC Smart Appliances","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Smart AppliancesProgram Annual BenefitsMarket Potential0","WA","Residential","DLC Smart Appliances","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Smart AppliancesProgram Annual CostsMarket Potential0","WA","Residential","DLC Smart Appliances","Program Annual Costs","Market Potential",0,466106.83,884360.1,1730193.43,922685.16,515815.89,97596.61,97948.22,98303.039999999994,98661.09,99022.41,99387.03,99754.97,100126.27,100500.96,100879.06,101260.62,101645.66,102034.21,102426.3,102821.98,103221.26,103624.19,104030.79,104441.1,104855.15,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesParticipantsMarket Potential0","WA","General Service","DLC Smart Appliances","Participants","Market Potential",0,115.47587548947151,349.82902521809325,824.60380688803571,1070.5070817643982,1201.0110145479064,1212.6826352991211,1224.4682784562276,1236.369057926963,1248.3860985010538,1260.5205359565211,1272.7735171670311,1285.1462002102862,1297.6397544774848,1310.2553607838404,1322.9942114801872,1335.8575105656746,1348.8464738015603,1361.9623288261173,1375.2063152706637,1388.5796848767238,1402.083701614336,1415.7196418015149,1429.488794224882,1443.3924602614741,1457.4319540017398,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesNew ParticipantsMarket Potential0","WA","General Service","DLC Smart Appliances","New Participants","Market Potential",0,115.47587548947151,234.35314972862176,474.77478166994246,245.9032748763625,130.50393278350816,11.671620751214732,11.785643157106506,11.900779470735415,12.017040574090743,12.134437455467378,12.252981210509915,12.372683043255165,12.493554267198533,12.61560630635563,12.738850696346844,12.86329908548737,12.988963235885649,13.11585502455705,13.243986444546408,13.373369606060123,13.504016737612119,13.635940187178903,13.769152423367132,13.903666036592085,14.039493740265698,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Smart Appliances","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.6166622568526013E-2,4.8976063530533062E-2,0.11544453296432501,0.14987099144701577,0.16814154203670692,0.16977556894187698,0.17142555898387191,0.17309166810977483,0.17477405379014754,0.17647287503391296,0.17818829240338438,0.17992046802944009,0.18166956562684788,0.18343575050973765,0.18521918960722625,0.18702005147919445,0.18883850633221846,0.19067472603565644,0.19252888413789293,0.19440115588274137,0.19629171822600705,0.19820074985221212,0.20012843119148349,0.2020749444366064,0.20404047356024357,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Smart Appliances","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.7227858662112121E-2,5.2191031042767545E-2,0.12302273333794225,0.15970907016945413,0.1791789663647772,0.18092025675818094,0.18267855816695641,0.18445403677512237,0.18624686039018279,0.18805719845898652,0.18988522208374295,0.19173110403819277,0.19359501878393851,0.19547714248693271,0.19737765303412858,0.19929673005029247,0.20123455491498132,0.20319131077968502,0.20516718258513739,0.20716235707879516,0.20917702283248832,0.21121137026024309,0.21326559163627823,0.21533988111317817,0.21743443474024252,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","DLC Smart Appliances","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.6166622568526013E-2,4.8976063530533062E-2,0.11544453296432501,0.14987099144701577,0.16814154203670692,0.16977556894187698,0.17142555898387191,0.17309166810977483,0.17477405379014754,0.17647287503391296,0.17818829240338438,0.17992046802944009,0.18166956562684788,0.18343575050973765,0.18521918960722625,0.18702005147919445,0.18883850633221846,0.19067472603565644,0.19252888413789293,0.19440115588274137,0.19629171822600705,0.19820074985221212,0.20012843119148349,0.2020749444366064,0.20404047356024357,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","DLC Smart Appliances","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.7227858662112121E-2,5.2191031042767545E-2,0.12302273333794225,0.15970907016945413,0.1791789663647772,0.18092025675818094,0.18267855816695641,0.18445403677512237,0.18624686039018279,0.18805719845898652,0.18988522208374295,0.19173110403819277,0.19359501878393851,0.19547714248693271,0.19737765303412858,0.19929673005029247,0.20123455491498132,0.20319131077968502,0.20516718258513739,0.20716235707879516,0.20917702283248832,0.21121137026024309,0.21326559163627823,0.21533988111317817,0.21743443474024252,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[{"$f":"B158&C158&D158&E158&F158&G158","v":"WAGeneral ServiceDLC Smart AppliancesNon-Incentive CostsMarket Potential0"},"WA","General Service","DLC Smart Appliances","Non-Incentive Costs","Market Potential",0,46677.04,88284.09,172431.66,92326.63,51936.86,10345.549999999999,10385.459999999999,10425.76,10466.450000000001,10507.54,10549.03,10590.92,10633.23,10675.95,10719.08,10762.64,10806.62,10851.03,10895.88,10941.16,10986.89,11033.06,11079.69,11126.77,11174.31,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesIncentive CostsMarket Potential0","WA","General Service","DLC Smart Appliances","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceDLC Smart AppliancesProgram Annual BenefitsMarket Potential0","WA","General Service","DLC Smart Appliances","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceDLC Smart AppliancesProgram Annual CostsMarket Potential0","WA","General Service","DLC Smart Appliances","Program Annual Costs","Market Potential",0,46677.04,88284.09,172431.66,92326.63,51936.86,10345.549999999999,10385.459999999999,10425.76,10466.450000000001,10507.54,10549.03,10590.92,10633.23,10675.95,10719.08,10762.64,10806.62,10851.03,10895.88,10941.16,10986.89,11033.06,11079.69,11126.77,11174.31,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsParticipantsMarket Potential0","WA","General Service","Third Party Contracts","Participants","Market Potential",0,857.32089378547005,1731.4769935036936,2973.5713036265533,3532.3129297276428,3566.6387704756003,3601.2999472519355,3636.299736021524,3671.6414447527995,3707.3284137304013,3743.3640158708808,3779.751657041485,3816.4947763820624,3853.596846630106,3891.0613744489797,3928.8919007593431,3967.0920010738209,4005.6652858349362,4044.6154007563482,4083.9460271674257,4123.6608823611796,4163.7637199456021,4204.2583301984369,4245.1485404254072,4286.4382153219522,4328.1312573384994,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsNew ParticipantsMarket Potential0","WA","General Service","Third Party Contracts","New Participants","Market Potential",0,857.32089378547005,874.15609971822357,1242.0943101228597,558.74162610108942,34.3258407479575,34.661176776335196,34.999788769588577,35.341708731275503,35.686968977601737,36.035602140479568,36.387641170604184,36.743119340577323,37.102070248043674,37.464527818873648,37.830526310363439,38.200100314477822,38.573284761115247,38.950114921412023,39.330626411077446,39.71485519375392,40.102837584422559,40.494610252834718,40.890210226970339,41.289674896544966,41.693042016547224,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Third Party Contracts","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.30338317074624171,0.61314560194558998,1.05323010304581,1.2512312237654748,1.2634877031992238,1.2758648547410021,1.2883638675593585,1.3009859425434545,1.3137322924185866,1.3266041418628516,1.3396027276249527,1.3527292986431787,1.3659851161655454,1.3793714538711284,1.3928895979925855,1.4065408474398959,1.4203265139253065,1.4342479220895208,1.4483064096291269,1.4625033274252817,1.4768400396736614,1.4913179240156995,1.5059383716711101,1.5207027875717229,1.5356125904966356,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Third Party Contracts","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.32329834904757215,0.65339471648080771,1.1223679699976663,1.333366606740702,1.3464276462054814,1.3596172791357652,1.3729367727614648,1.3863874068024877,1.3999704735918441,1.4136872781999696,1.4275391385602649,1.4415273855958852,1.455653363347768,1.4699184291039304,1.4843239535300357,1.4988713208012532,1.5135619287354076,1.5283971889274519,1.5433785268852589,1.5585073821667537,1.5737852085183945,1.589213474015025,1.6047936612010978,1.6205272672332938,1.6364158040245478,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Third Party Contracts","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.30178674596080152,0.60991918423223457,1.0476879279899614,1.2446471521011746,1.2568391370295029,1.2691511590802618,1.2815844011645079,1.2941400578522335,1.3068193354872861,1.3196234523034132,1.3325536385414565,1.3456111365676975,1.3587972009933715,1.3721130987953603,1.3855601094380701,1.3991395249965188,1.4128526502806258,1.4267008029607378,1.4406853136943829,1.4548075262542819,1.4690687976576113,1.4834704982965541,1.498014012070122,1.5127007365172884,1.5275320829514318,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Third Party Contracts","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.3215971291142386,0.6499565049363113,1.1164619863490637,1.3263503325886346,1.3393426438933322,1.3524628719951639,1.3657122774557842,1.3790921332611183,1.3926037249438257,1.4062483507069621,1.4200273215488666,1.433941961389277,1.4479936071966875,1.4621836091169653,1.476513330603229,1.490984148547015,1.5055974534107266,1.5203546493614,1.5352571544057789,1.5503064005267284,1.5655038338209839,1.5808509146382717,1.5963491177217839,1.6119999323500516,1.6278048624802128,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceThird Party ContractsNon-Incentive CostsMarket Potential0","WA","General Service","Third Party Contracts","Non-Incentive Costs","Market Potential",0,24270.65,49051.65,84258.41,100098.5,101079.02,102069.19,103069.11,104078.88,105098.58,106128.33,107168.22,108218.34,109278.81,110349.72,111431.17,112523.27,113626.12,114739.83,115864.51,117000.27,118147.2,119305.43,120475.07,121656.22,122849.01,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsIncentive CostsMarket Potential0","WA","General Service","Third Party Contracts","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThird Party ContractsProgram Annual BenefitsMarket Potential0","WA","General Service","Third Party Contracts","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceThird Party ContractsProgram Annual CostsMarket Potential0","WA","General Service","Third Party Contracts","Program Annual Costs","Market Potential",0,24270.65,49051.65,84258.41,100098.5,101079.02,102069.19,103069.11,104078.88,105098.58,106128.33,107168.22,108218.34,109278.81,110349.72,111431.17,112523.27,113626.12,114739.83,115864.51,117000.27,118147.2,119305.43,120475.07,121656.22,122849.01,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsParticipantsMarket Potential0","WA","Large General Service","Third Party Contracts","Participants","Market Potential",0,101.02428298943731,201.79866483287421,342.6367774079489,402.60963190455857,402.13426696530439,401.67540291446733,401.23246701063357,400.80490639209006,400.39218738680592,399.9937948463633,399.60923150300766,399.23801734901514,398.87968903760139,398.53379930462444,398.19991641036103,397.8776236006579,397.56651858678669,397.2662130433531,396.97633212363297,396.69651399173171,396.42640937098139,396.16568110801393,395.91400375196395,395.67106314827845,395.43655604662496,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsNew ParticipantsMarket Potential0","WA","Large General Service","Third Party Contracts","New Participants","Market Potential",0,101.02428298943731,100.7743818434369,140.83811257507469,59.972854496609671,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Third Party Contracts","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.1368921317594523,4.2674992140977173,7.2435336205967937,8.5089955402056319,8.4965951031674045,8.484589935320006,8.4729674383358518,8.4617154154310743,8.450822058567196,8.4402759360607522,8.430065980587786,8.4201814775707167,8.4106120539353384,8.401347667226128,8.392378595068541,8.3836954249671312,8.375289044428829,8.3671506314010511,8.3592716450145428,8.3516438166212961,8.3442591411180835,8.3371098685465714,8.3301884959611314,8.3234877595558636,8.3170006270425532,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Third Party Contracts","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.2771655283029117,4.5476334336079685,7.7190255973964126,9.0675570547800852,9.0543426078084028,9.0415493769394786,9.0291639368455368,9.0171732901013151,9.0055648535456054,8.9943264450775278,8.9834462708735998,8.9729129130122729,8.9627153174929006,8.9528427826365391,8.9432849478565011,8.9340317827867981,8.9250735767570646,8.9164009286029948,8.9080047368015158,8.8998761899203913,8.8920067573722115,8.8843881804630982,8.8770124637266949,8.8698718665343819,8.8629588949728824,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Third Party Contracts","Winter Peak Reduction @Meter  (MW)","Market Potential",0,2.1256476465938379,4.2450433161635139,7.2054176085001203,8.4642205734658074,8.4518853884486145,8.4399433926863967,8.4283820541449117,8.4171892402206652,8.4063532050099692,8.3958625769837187,8.3857063470550344,8.3758738570272513,8.3663547884100335,8.3571391515920208,8.3482172753585182,8.3395797967433278,8.3312176512039997,8.3231220631102492,8.3152845365355077,8.3076968463420009,8.3003510295499581,8.2932393769818997,8.2863544251732524,8.2796889485408069,8.2732359518007641,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Third Party Contracts","Winter Peak Reduction @Generation (MW)","Market Potential",0,2.2651829141025552,4.5237034485970948,7.6784075111893868,9.0198428958501786,9.0066979842802795,8.9939720723427072,8.9816518053547654,8.9697242542845963,8.9581769021845368,8.9469976310568189,8.93617470913793,8.9256967785882892,8.9155528435742042,8.905732258729774,8.8962247179864864,8.8870202437588741,8.878109176474851,8.8694821644397361,8.8611301540233463,8.8530443801598473,8.8452163571504236,8.8376378697590567,8.8303009645921264,8.8231979417527775,8.8163213467612582,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceThird Party ContractsNon-Incentive CostsMarket Potential0","WA","Large General Service","Third Party Contracts","Non-Incentive Costs","Market Potential",0,170951.37,341399.94,579482.68999999994,680719.64,679727.61,678767.19,677837.4,676937.23,676065.76,675222.07,674405.28,673614.52,672848.96,672107.81,671390.29,670695.63,670023.12,669372.05000000005,668741.73,668131.51,667540.73,666968.79,666415.07999999996,665879.02,665360.05000000005,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsIncentive CostsMarket Potential0","WA","Large General Service","Third Party Contracts","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThird Party ContractsProgram Annual BenefitsMarket Potential0","WA","Large General Service","Third Party Contracts","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceThird Party ContractsProgram Annual CostsMarket Potential0","WA","Large General Service","Third Party Contracts","Program Annual Costs","Market Potential",0,170951.37,341399.94,579482.68999999994,680719.64,679727.61,678767.19,677837.4,676937.23,676065.76,675222.07,674405.28,673614.52,672848.96,672107.81,671390.29,670695.63,670023.12,669372.05000000005,668741.73,668131.51,667540.73,666968.79,666415.07999999996,665879.02,665360.05000000005,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsParticipantsMarket Potential0","WA","Extra Large General Service","Third Party Contracts","Participants","Market Potential",0,1.1380049999999999,2.2760099999999999,3.8692169999999995,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,4.5520199999999997,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsNew ParticipantsMarket Potential0","WA","Extra Large General Service","Third Party Contracts","New Participants","Market Potential",0,1.1380049999999999,1.1380049999999999,1.5932069999999996,0.68280300000000027,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Third Party Contracts","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.80545943505763085,1.6134994647614569,2.7448538121885515,3.230317174650629,3.2313954897634924,3.2324747250593835,3.2335548812142432,3.2346359589045175,3.2357179588071592,3.2368008815996241,3.2378847279598753,3.2389694985663833,3.2400551940981228,3.241141815234581,3.242229362655745,3.2433178370421154,3.2444072390746967,3.2454975694350097,3.2465888288050762,3.2476810178674289,3.2487741373051149,3.2498681878016864,3.2509631700412083,3.2520590847082573,3.2531559324879189,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Third Party Contracts","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.85833273130608567,1.7194154569069233,2.9250360317439807,3.4423669806592381,3.4435160803106268,3.444666160549215,3.4458172220953145,3.4469692656697757,3.4481222919939887,3.4492763017898809,3.4504312957799184,3.451587274687109,3.4527442392349985,3.4539021901476779,3.455061128149771,3.4562210539664484,3.4573819683234195,3.458543871946941,3.4597067655638067,3.4608706499013522,3.4620355256874626,3.4632013936505608,3.4643682545196168,3.4655361090241446,3.4667049578942017,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Third Party Contracts","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.90102712972794563,1.8049410414412386,3.0705304876614958,3.613594037517343,3.6148002946282509,3.6160075811018246,3.6172158976942081,3.6184252451621051,3.6196356242627901,3.6208470357540978,3.6220594803944333,3.6232729589427666,3.6244874721586338,3.6257030208021406,3.6269196056339563,3.6281372274153236,3.6293558869080473,3.63057558487451,3.6317963220776557,3.6330180992810006,3.6342409172486327,3.6354647767452115,3.6366896785359617,3.6379156233866885,3.6391426120637607,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Third Party Contracts","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.96017383815850987,1.9234239572050709,3.2720913125122504,3.8508035352912864,3.8520889755203016,3.8533755126831037,3.8546631475854731,3.8559518810337861,3.8572417138350277,3.8585326467967795,3.8598246807272307,3.8611178164351734,3.8624120547300018,3.8637073964217183,3.8650038423209252,3.8663013932388357,3.8676000499872627,3.8688998133786336,3.870200684225976,3.8715026633429246,3.8728057515437264,3.8741099496432345,3.8754152584569073,3.876721678800819,3.8780292114916461,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceThird Party ContractsNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Third Party Contracts","Non-Incentive Costs","Market Potential",0,72082.17,144395.28,245642.44,289087.52,289184.02,289280.61,289377.27,289474.02,289570.84999999998,289667.76,289764.76,289861.84000000003,289959,290056.24,290153.57,290250.98,290348.46999999997,290446.05,290543.71000000002,290641.45,290739.27,290837.18,290935.17,291033.25,291131.40999999997,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsIncentive CostsMarket Potential0","WA","Extra Large General Service","Third Party Contracts","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThird Party ContractsProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Third Party Contracts","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceThird Party ContractsProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Third Party Contracts","Program Annual Costs","Market Potential",0,72082.17,144395.28,245642.44,289087.52,289184.02,289280.61,289377.27,289474.02,289570.84999999998,289667.76,289764.76,289861.84000000003,289959,290056.24,290153.57,290250.98,290348.46999999997,290446.05,290543.71000000002,290641.45,290739.27,290837.18,290935.17,291033.25,291131.40999999997,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingParticipantsMarket Potential0","WA","Residential","DLC Electric Vehicle Charging","Participants","Market Potential",0,0,0,108.4378964235363,384.6313391902396,1061.1182414250179,1613.0602085207281,2119.0948533702572,2505.4902950762039,2962.3410243940675,3502.4938480319229,4141.1380575302674,4896.2325575994128,5789.0108769746712,6844.5782628760726,8092.6176495834243,9568.224353216794,11312.892964639643,13375.684192267749,15814.604466823066,18698.2371030141,22107.670886995493,26138.780322179318,30904.921654729886,36540.120491948037,36873.504036119564,37209.929294057438,37549.424017649246,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingNew ParticipantsMarket Potential0","WA","Residential","DLC Electric Vehicle Charging","New Participants","Market Potential",0,0,0,108.4378964235363,276.1934427667033,676.48690223477831,551.9419670957102,506.03464484952906,386.39544170594672,456.85072931786362,540.15282363785536,638.64420949834448,755.0945000691454,892.77831937525843,1055.5673859014014,1248.0393867073517,1475.6067036333698,1744.6686114228487,2062.7912276281058,2438.9202745553175,2883.6326361910342,3409.4337839813925,4031.1094351838256,4766.1413325505673,5635.1988372181513,333.38354417152732,336.42525793787354,339.494723591808,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Electric Vehicle Charging","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,5.4218948211768148E-2,0.19231566959511981,0.53055912071250899,0.80653010426036409,1.0595474266851286,1.252745147538102,1.4811705121970338,1.7512469240159614,2.0705690287651337,2.4481162787997062,2.8945054384873354,3.4222891314380361,4.0463088247917121,4.7841121766083967,5.6564464823198213,6.687842096133874,7.9073022334115333,9.3491185515070505,11.053835443497746,13.069390161089659,15.452460827364943,18.270060245974019,18.436752018059781,18.604964647028719,18.774712008824622,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Electric Vehicle Charging","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,5.7778077804527012E-2,0.20493997186180712,0.56538695728101984,0.85947368314190542,1.1290999858110917,1.3349799099937147,1.5783999490590725,1.8662051619948437,2.206488734830705,2.6088195639383058,3.0845113368364614,3.6469406771505075,4.3119233000764199,5.0981587559765522,6.0277562684567574,7.1268564536805989,8.4263664038912331,9.962828805953805,11.779449534844145,13.92731261838199,16.466816738453691,19.469373663655176,19.647007691879562,19.826262411582181,20.007152609574405,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","DLC Electric Vehicle Charging","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,5.4218948211768148E-2,0.19231566959511981,0.53055912071250899,0.80653010426036409,1.0595474266851286,1.252745147538102,1.4811705121970338,1.7512469240159614,2.0705690287651337,2.4481162787997062,2.8945054384873354,3.4222891314380361,4.0463088247917121,4.7841121766083967,5.6564464823198213,6.687842096133874,7.9073022334115333,9.3491185515070505,11.053835443497746,13.069390161089659,15.452460827364943,18.270060245974019,18.436752018059781,18.604964647028719,18.774712008824622,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","DLC Electric Vehicle Charging","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,5.7778077804527012E-2,0.20493997186180712,0.56538695728101984,0.85947368314190542,1.1290999858110917,1.3349799099937147,1.5783999490590725,1.8662051619948437,2.206488734830705,2.6088195639383058,3.0845113368364614,3.6469406771505075,4.3119233000764199,5.0981587559765522,6.0277562684567574,7.1268564536805989,8.4263664038912331,9.962828805953805,11.779449534844145,13.92731261838199,16.466816738453691,19.469373663655176,19.647007691879562,19.826262411582181,20.007152609574405,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Electric Vehicle ChargingNon-Incentive CostsMarket Potential0","WA","Residential","DLC Electric Vehicle Charging","Non-Incentive Costs","Market Potential",0,0,0,148500.35,275697.98,579300.5,488651.51,456751.19,368953.77,424079.49,489256.82,566318.57999999996,657431.77,765158.53,892528.17,1043122.37,1221175.8899999999,1431695.66,1680601.58,1974892.97,2322845.4,2734243.43,3220655.71,3795760.34,4475729.47,501034.92,504998.33,508997.9,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingIncentive CostsMarket Potential0","WA","Residential","DLC Electric Vehicle Charging","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialDLC Electric Vehicle ChargingProgram Annual BenefitsMarket Potential0","WA","Residential","DLC Electric Vehicle Charging","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialDLC Electric Vehicle ChargingProgram Annual CostsMarket Potential0","WA","Residential","DLC Electric Vehicle Charging","Program Annual Costs","Market Potential",0,0,0,148500.35,275697.98,579300.5,488651.51,456751.19,368953.77,424079.49,489256.82,566318.57999999996,657431.77,765158.53,892528.17,1043122.37,1221175.8899999999,1431695.66,1680601.58,1974892.97,2322845.4,2734243.43,3220655.71,3795760.34,4475729.47,501034.92,504998.33,508997.9,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageParticipantsMarket Potential0","WA","General Service","Thermal Energy Storage","Participants","Market Potential",0,11.426347287469042,33.791175162603686,75.601238413453558,94.679917548862349,103.27000324535499,102.24489437273046,100.45631573976333,98.147344596591992,95.301113725582013,93.175336906447214,91.51440249132078,89.754420443694116,87.890326834618975,85.916827604360421,83.828395602989744,81.619269032214575,79.283451589742626,76.814714664521574,74.206601984866623,71.452437182675212,68.611393574026494,67.57927800102037,66.52062491674144,65.435013604136486,64.322017658681744,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageNew ParticipantsMarket Potential0","WA","General Service","Thermal Energy Storage","New Participants","Market Potential",0,11.426347287469042,22.364827875134644,41.810063250849872,19.078679135408791,8.5900856964926362,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Thermal Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.9196263442947992E-2,5.6769174273174197E-2,0.12701008053460197,0.15906226148208874,0.17349360545219636,0.17177142254618716,0.16876661044280236,0.16488753892227453,0.16010587105897778,0.15653456600283133,0.1537441961854189,0.15078742634540612,0.14765574908215987,0.14434027037532551,0.14083170461302277,0.13712037197412047,0.13319619867076762,0.12904872063639625,0.12466709133457593,0.12004009446689434,0.1152671412043645,0.11353318704171421,0.11175464986012561,0.1099308228549493,0.10806098966658532,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Thermal Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.0456376217975268E-2,6.0495710009776424E-2,0.13534748565068411,0.16950368870640317,0.1848823587512749,0.1830471254754765,0.17984506654177573,0.17571135861282453,0.1706158046238041,0.16681006607292342,0.16383652619929551,0.16068566319842936,0.15734841121287282,0.15381529238632302,0.15007641156545479,0.14612145351035855,0.14193968315299194,0.13751994952727647,0.13285069409055406,0.12791996426565894,0.12283369693559729,0.12098591969492137,0.11909063284327111,0.11714708317876098,0.11515450731733304,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Thermal Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Thermal Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceThermal Energy StorageNon-Incentive CostsMarket Potential0","WA","General Service","Thermal Energy Storage","Non-Incentive Costs","Market Potential",0,63391.87,97237.13,157575.93,92748.35,62818.05,37628.269999999997,37478.03,37284.080000000002,37045,36866.43,36726.910000000003,36579.07,36422.49,36256.720000000001,36081.29,35895.72,35699.51,35492.14,35273.06,35041.71,34803.06,34716.36,34627.43,34536.239999999998,34442.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageIncentive CostsMarket Potential0","WA","General Service","Thermal Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceThermal Energy StorageProgram Annual BenefitsMarket Potential0","WA","General Service","Thermal Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceThermal Energy StorageProgram Annual CostsMarket Potential0","WA","General Service","Thermal Energy Storage","Program Annual Costs","Market Potential",0,63391.87,97237.13,157575.93,92748.35,62818.05,37628.269999999997,37478.03,37284.080000000002,37045,36866.43,36726.910000000003,36579.07,36422.49,36256.720000000001,36081.29,35895.72,35699.51,35492.14,35273.06,35041.71,34803.06,34716.36,34627.43,34536.239999999998,34442.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B212&C212&D212&E212&F212&G212","v":"WALarge General ServiceThermal Energy StorageParticipantsMarket Potential0"},"WA","Large General Service","Thermal Energy Storage","Participants","Market Potential",0,2.7427407146453571,8.2180451741894487,19.15190930414407,24.593801043943621,27.294181015744641,27.263036396909545,27.232972874024902,27.203952922540047,27.175940320371442,27.148900102694338,27.122798518303686,27.097602987489719,27.073282061375657,27.049805382666815,27.027143647762056,27.005268570180398,26.984152845257015,26.963770116064687,26.944094940518074,26.925102759619797,26.906769866808691,26.889073378371982,26.871991204884431,26.85550202363881,26.839585252033366,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThermal Energy StorageNew ParticipantsMarket Potential0","WA","Large General Service","Thermal Energy Storage","New Participants","Market Potential",0,2.7427407146453571,5.4753044595440912,10.933864129954621,5.4418917397995514,2.70037997180102,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThermal Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Thermal Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.3039022003020999E-2,6.9031579463191384E-2,0.16087603815481019,0.20658792876912643,0.22927112053225499,0.22900950573404016,0.22875697214180921,0.22851320454933638,0.22827789869112014,0.22805076086263246,0.22783150755375098,0.22761986509491364,0.22741556931555554,0.22721836521440125,0.22702800664120126,0.22684425598951535,0.22666688390015893,0.22649566897494339,0.22633039750035183,0.22617086318080629,0.22601686688119302,0.22586821637832466,0.22572472612102923,0.22558621699856601,0.22545251611708028,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThermal Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Thermal Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.4551387471249998E-2,7.3563064219087149E-2,0.17143652829796482,0.22014911420409891,0.24432131344016941,0.24404252529202916,0.24377341447336873,0.24351364508667558,0.24326289289335054,0.24302084490902862,0.24278719901294862,0.24256166357087983,0.24234395707113762,0.24213380777323237,0.24193095336871404,0.24173514065378873,0.2415461252132981,0.24136367111566856,0.24118755061844824,0.24101754388406466,0.24085343870544865,0.24069503024118144,0.24054212075983505,0.24039451939318629,0.2402520418979969,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThermal Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Thermal Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThermal Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Thermal Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceThermal Energy StorageNon-Incentive CostsMarket Potential0","WA","Large General Service","Thermal Energy Storage","Non-Incentive Costs","Market Potential",0,223263.09,418645.67,808939.72,423162.55,230581.49,39759.56,39746.93,39734.74,39722.980000000003,39711.620000000003,39700.660000000003,39690.080000000002,39679.86,39670,39660.480000000003,39651.300000000003,39642.43,39633.870000000003,39625.599999999999,39617.629999999997,39609.93,39602.49,39595.32,39588.39,39581.71,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThermal Energy StorageIncentive CostsMarket Potential0","WA","Large General Service","Thermal Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceThermal Energy StorageProgram Annual BenefitsMarket Potential0","WA","Large General Service","Thermal Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceThermal Energy StorageProgram Annual CostsMarket Potential0","WA","Large General Service","Thermal Energy Storage","Program Annual Costs","Market Potential",0,223263.09,418645.67,808939.72,423162.55,230581.49,39759.56,39746.93,39734.74,39722.980000000003,39711.620000000003,39700.660000000003,39690.080000000002,39679.86,39670,39660.480000000003,39651.300000000003,39642.43,39633.870000000003,39625.599999999999,39617.629999999997,39609.93,39602.49,39595.32,39588.39,39581.71,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageParticipantsMarket Potential0","WA","Extra Large General Service","Thermal Energy Storage","Participants","Market Potential",0,3.2670000000000005E-2,9.801E-2,0.22868999999999998,0.29403000000000001,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0.32669999999999993,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageNew ParticipantsMarket Potential0","WA","Extra Large General Service","Thermal Energy Storage","New Participants","Market Potential",0,3.2670000000000005E-2,6.5339999999999995E-2,0.13067999999999996,6.5340000000000037E-2,3.2669999999999921E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Thermal Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.7442800000000006E-4,8.2328399999999997E-4,1.9209959999999999E-3,2.4698520000000002E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,2.7442799999999995E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Thermal Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.9244245524296682E-4,8.7732736572890019E-4,2.0470971867007672E-3,2.6319820971867011E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,2.9244245524296668E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Thermal Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Thermal Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceThermal Energy StorageNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Thermal Energy Storage","Non-Incentive Costs","Market Potential",0,2628.81,4964.72,9636.5300000000007,5047.05,2752.31,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageIncentive CostsMarket Potential0","WA","Extra Large General Service","Thermal Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceThermal Energy StorageProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Thermal Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceThermal Energy StorageProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Thermal Energy Storage","Program Annual Costs","Market Potential",0,2628.81,4964.72,9636.5300000000007,5047.05,2752.31,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,443.84,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B232&C232&D232&E232&F232&G232","v":"WAResidentialBattery Energy StorageParticipantsMarket Potential0"},"WA","Residential","Battery Energy Storage","Participants","Market Potential",0,23.494821728845764,71.131246095896373,119.70658527321089,193.27801641790427,268.18197999833387,344.43666712959265,422.06048994560086,526.12568832376337,632.05468630633493,739.8728309276579,875.35140618821379,1013.2405420215947,1153.5729475538492,1322.8384980707363,1334.9077682569293,1347.0871556517156,1359.3776649388451,1371.7803099685677,1384.2961138412677,1396.9261089918577,1409.6713372749466,1422.5328500507817,1435.5117082719762,1448.6089825710276,1461.8257533486353,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBattery Energy StorageNew ParticipantsMarket Potential0","WA","Residential","Battery Energy Storage","New Participants","Market Potential",0,23.494821728845764,47.636424367050608,48.575339177314518,73.571431144693378,74.903963580429604,76.254687131258777,77.623822816008214,104.06519837816251,105.92899798257156,107.81814462132297,135.47857526055589,137.88913583338092,140.33240553225448,169.26555051688706,12.06927018619308,12.179387394786318,12.290509287129453,12.402645029722635,12.515803872699962,12.629995150590048,12.745228283088863,12.861512775835081,12.978858221194514,13.097274299051378,13.216770777607735,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.6989643457691528E-2,0.14226249219179274,0.23941317054642178,0.38655603283580853,0.53636395999666775,0.68887333425918529,0.84412097989120172,1.0522513766475268,1.2641093726126698,1.4797456618553158,1.7507028123764277,2.0264810840431893,2.3071458951076984,2.6456769961414723,2.6698155365138585,2.6941743113034313,2.7187553298776903,2.7435606199371354,2.7685922276825354,2.7938522179837153,2.8193426745498931,2.8450657001015633,2.8710234165439523,2.8972179651420551,2.9236515066972708,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.0074215108366932E-2,0.15160112126150121,0.25512912462321163,0.4119309812828309,0.57157284739627845,0.73409349345607977,0.89953216100937949,1.1213249964274581,1.3470901242675508,1.5768815663419817,1.8656253328819561,2.159506696550713,2.4585953698931142,2.8193488876187898,2.8450719698570528,2.8710297435032301,2.8972243498270358,2.9236579496346287,2.9503327234468619,2.9772508716791508,3.0044146148229891,3.0318261936291169,3.0594878692923619,3.0874019236381662,3.115570659310817,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.6989643457691528E-2,0.14226249219179274,0.23941317054642178,0.38655603283580853,0.53636395999666775,0.68887333425918529,0.84412097989120172,1.0522513766475268,1.2641093726126698,1.4797456618553158,1.7507028123764277,2.0264810840431893,2.3071458951076984,2.6456769961414723,2.6698155365138585,2.6941743113034313,2.7187553298776903,2.7435606199371354,2.7685922276825354,2.7938522179837153,2.8193426745498931,2.8450657001015633,2.8710234165439523,2.8972179651420551,2.9236515066972708,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,5.0074215108366932E-2,0.15160112126150121,0.25512912462321163,0.4119309812828309,0.57157284739627845,0.73409349345607977,0.89953216100937949,1.1213249964274581,1.3470901242675508,1.5768815663419817,1.8656253328819561,2.159506696550713,2.4585953698931142,2.8193488876187898,2.8450719698570528,2.8710297435032301,2.8972243498270358,2.9236579496346287,2.9503327234468619,2.9772508716791508,3.0044146148229891,3.0318261936291169,3.0594878692923619,3.0874019236381662,3.115570659310817,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialBattery Energy StorageNon-Incentive CostsMarket Potential0","WA","Residential","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,214940.68,381807.43,388297.21,561070.19999999995,570280.66,579616.86,589080.32999999996,771843.12,784725.7,797783.48,988972.38,1005634.17,1022522.05,1222507.95,135967.26,136728.39000000001,137496.47,138271.54999999999,139053.70000000001,139842.99,140639.49,141443.24,142254.34,143072.82999999999,143898.79,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBattery Energy StorageIncentive CostsMarket Potential0","WA","Residential","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBattery Energy StorageProgram Annual BenefitsMarket Potential0","WA","Residential","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialBattery Energy StorageProgram Annual CostsMarket Potential0","WA","Residential","Battery Energy Storage","Program Annual Costs","Market Potential",0,214940.68,381807.43,388297.21,561070.19999999995,570280.66,579616.86,589080.32999999996,771843.12,784725.7,797783.48,988972.38,1005634.17,1022522.05,1222507.95,135967.26,136728.39000000001,137496.47,138271.54999999999,139053.70000000001,139842.99,140639.49,141443.24,142254.34,143072.82999999999,143898.79,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageParticipantsMarket Potential0","WA","General Service","Battery Energy Storage","Participants","Market Potential",0,2.3317033347555256,7.0571156821601706,11.861244213232464,19.147727792369853,26.575536653050253,34.154951883610899,41.881670190021936,52.245911215672869,62.811550170284718,73.57846938709072,87.111678473305361,100.90390080714063,114.95903851548186,131.91944220378022,133.21663695937769,134.52700573217979,135.85070130786545,137.18787883335591,138.53869580529422,139.90331204405874,141.28155935681025,142.66408763034991,144.0602043728791,145.47004314020901,146.89373880077122,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageNew ParticipantsMarket Potential0","WA","General Service","Battery Energy Storage","New Participants","Market Potential",0,2.3317033347555256,4.725412347404645,4.8041285310722932,7.2864835791373892,7.4278088606804005,7.5794152305606453,7.726718306411037,10.364241025650934,10.565638954611849,10.766919216806002,13.53320908621464,13.792222333835269,14.055137708341235,16.960403688298356,1.2971947555974737,1.310368772802093,1.3236955756856617,1.3371775254904605,1.3508169719383147,1.364616238764512,1.3782473127515118,1.3825282735396627,1.3961167425291876,1.4098387673299158,1.4236956605622026,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.6634066695110509E-3,1.4114231364320341E-2,2.3722488426464929E-2,3.8295455584739707E-2,5.3151073306100506E-2,6.8309903767221791E-2,8.3763340380043877E-2,0.10449182243134574,0.12562310034056945,0.14715693877418143,0.17422335694661073,0.20180780161428127,0.22991807703096373,0.26383888440756043,0.26643327391875538,0.26905401146435959,0.27170140261573089,0.27437575766671179,0.27707739161058847,0.27980662408811746,0.2825631187136205,0.28532817526069981,0.28812040874575817,0.29094008628041801,0.29378747760154245,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.9695296989674459E-3,1.5040741010571549E-2,2.527971912453637E-2,4.0809309020396103E-2,5.6640103693627993E-2,7.2794015097209924E-2,8.9261871675238566E-2,0.11135104692172393,0.1338694590159521,0.15681685717623767,0.18566001379647348,0.21505520206125456,0.2450107385240449,0.28115823146585722,0.28392292617088166,0.2867156984914318,0.28953687405768425,0.29238678353230158,0.29526576258587861,0.29817415184155738,0.30111159283207639,0.30405815777994438,0.30703368365916256,0.31003845511553496,0.31307275959243652,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.6634066695110509E-3,1.4114231364320341E-2,2.3722488426464929E-2,3.8295455584739707E-2,5.3151073306100506E-2,6.8309903767221791E-2,8.3763340380043877E-2,0.10449182243134574,0.12562310034056945,0.14715693877418143,0.17422335694661073,0.20180780161428127,0.22991807703096373,0.26383888440756043,0.26643327391875538,0.26905401146435959,0.27170140261573089,0.27437575766671179,0.27707739161058847,0.27980662408811746,0.2825631187136205,0.28532817526069981,0.28812040874575817,0.29094008628041801,0.29378747760154245,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,4.9695296989674459E-3,1.5040741010571549E-2,2.527971912453637E-2,4.0809309020396103E-2,5.6640103693627993E-2,7.2794015097209924E-2,8.9261871675238566E-2,0.11135104692172393,0.1338694590159521,0.15681685717623767,0.18566001379647348,0.21505520206125456,0.2450107385240449,0.28115823146585722,0.28392292617088166,0.2867156984914318,0.28953687405768425,0.29238678353230158,0.29526576258587861,0.29817415184155738,0.30111159283207639,0.30405815777994438,0.30703368365916256,0.31003845511553496,0.31307275959243652,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceBattery Energy StorageNon-Incentive CostsMarket Potential0","WA","General Service","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,20824.849999999999,36485.449999999997,37000.449999999997,53241.01,54165.61,55157.48,56121.2,73376.929999999993,74694.55,76011.41,94109.58,95804.15,97524.25,116531.66,14056.68,14142.87,14230.06,14318.27,14407.5,14497.78,14586.96,14614.97,14703.87,14793.64,14884.3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageIncentive CostsMarket Potential0","WA","General Service","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceBattery Energy StorageProgram Annual BenefitsMarket Potential0","WA","General Service","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceBattery Energy StorageProgram Annual CostsMarket Potential0","WA","General Service","Battery Energy Storage","Program Annual Costs","Market Potential",0,20824.849999999999,36485.449999999997,37000.449999999997,53241.01,54165.61,55157.48,56121.2,73376.929999999993,74694.55,76011.41,94109.58,95804.15,97524.25,116531.66,14056.68,14142.87,14230.06,14318.27,14407.5,14497.78,14586.96,14614.97,14703.87,14793.64,14884.3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageParticipantsMarket Potential0","WA","Large General Service","Battery Energy Storage","Participants","Market Potential",0,0.18442207034909824,0.55093830188137594,0.91163180408501665,1.4524567088958513,1.9917675872341358,2.5320843386519614,3.0712833323661668,3.7898953444743904,4.5071342772077321,5.2230735969623598,6.1177161525281738,7.0108615470834632,7.9025907623005116,8.972429553109162,8.9649126480110404,8.95765667741186,8.9506525843451001,8.9438916262091332,8.9373653638556849,8.9310656510570521,8.9249846243389168,8.9191146931660477,8.9134485304686528,8.9079790634975673,8.9026994649968589,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageNew ParticipantsMarket Potential0","WA","Large General Service","Battery Energy Storage","New Participants","Market Potential",0,0.18442207034909824,0.36651623153227769,0.36069350220364071,0.54082490481083467,0.53931087833828451,0.54031675141782554,0.53919899371420543,0.71861201210822356,0.71723893273334172,0.71593931975462777,0.89464255556581396,0.89314539455528941,0.8917292152170484,1.0698387908086504,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.7663310552364737E-3,8.2640745282206388E-3,1.367447706127525E-2,2.1786850633437767E-2,2.9876513808512035E-2,3.7981265079779419E-2,4.6069249985492507E-2,5.6848430167115854E-2,6.7607014158115986E-2,7.8346103954435392E-2,9.17657422879226E-2,0.10516292320625195,0.11853886143450768,0.13458644329663744,0.1344736897201656,0.13436485016117791,0.1342597887651765,0.13415837439313699,0.13406048045783528,0.13396598476585578,0.13387476936508375,0.1337867203974907,0.13370172795702978,0.13361968595246349,0.13354049197495288,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.9479231193909566E-3,8.8065585339094608E-3,1.4572119630514972E-2,2.3217019004089692E-2,3.1837717187246414E-2,4.0474493904283267E-2,4.9093403650354334E-2,6.0580168549782452E-2,7.2044985249484217E-2,8.3489028084436687E-2,9.7789580443225277E-2,0.11206620120018324,0.12632018481938159,0.14342118850877816,0.14330103337613556,0.14318504919136607,0.14307309118198688,0.14296501960052962,0.14286069955012284,0.14276000081612936,0.14266279770362716,0.14256896888053144,0.14247839722616132,0.1423909696850634,0.14230657712590886,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,2.7663310552364737E-3,8.2640745282206388E-3,1.367447706127525E-2,2.1786850633437767E-2,2.9876513808512035E-2,3.7981265079779419E-2,4.6069249985492507E-2,5.6848430167115854E-2,6.7607014158115986E-2,7.8346103954435392E-2,9.17657422879226E-2,0.10516292320625195,0.11853886143450768,0.13458644329663744,0.1344736897201656,0.13436485016117791,0.1342597887651765,0.13415837439313699,0.13406048045783528,0.13396598476585578,0.13387476936508375,0.1337867203974907,0.13370172795702978,0.13361968595246349,0.13354049197495288,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,2.9479231193909566E-3,8.8065585339094608E-3,1.4572119630514972E-2,2.3217019004089692E-2,3.1837717187246414E-2,4.0474493904283267E-2,4.9093403650354334E-2,6.0580168549782452E-2,7.2044985249484217E-2,8.3489028084436687E-2,9.7789580443225277E-2,0.11206620120018324,0.12632018481938159,0.14342118850877816,0.14330103337613556,0.14318504919136607,0.14307309118198688,0.14296501960052962,0.14286069955012284,0.14276000081612936,0.14266279770362716,0.14256896888053144,0.14247839722616132,0.1423909696850634,0.14230657712590886,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceBattery Energy StorageNon-Incentive CostsMarket Potential0","WA","Large General Service","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,11764.11,20699.11,20413.400000000001,29252.09,29177.8,29227.15,29172.31,37975.74,37908.370000000003,37844.6,46613.21,46539.75,46470.26,55209.74,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageIncentive CostsMarket Potential0","WA","Large General Service","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceBattery Energy StorageProgram Annual BenefitsMarket Potential0","WA","Large General Service","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceBattery Energy StorageProgram Annual CostsMarket Potential0","WA","Large General Service","Battery Energy Storage","Program Annual Costs","Market Potential",0,11764.11,20699.11,20413.400000000001,29252.09,29177.8,29227.15,29172.31,37975.74,37908.370000000003,37844.6,46613.21,46539.75,46470.26,55209.74,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageParticipantsMarket Potential0","WA","Extra Large General Service","Battery Energy Storage","Participants","Market Potential",0,2.1967330000000002E-3,6.5705970000000001E-3,1.0885654999999999E-2,1.7364776000000002E-2,2.3840630000000002E-2,3.0342620000000008E-2,3.6844610000000007E-2,4.5513930000000008E-2,5.4183250000000002E-2,6.2852569999999996E-2,7.368922E-2,8.4525870000000003E-2,9.5362519999999992E-2,0.10836649999999999,0.1083665,0.1083665,0.1083665,0.1083665,0.1083665,0.1083665,0.1083665,0.1083665,0.1083665,0.1083665,0.1083665,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageNew ParticipantsMarket Potential0","WA","Extra Large General Service","Battery Energy Storage","New Participants","Market Potential",0,2.1967330000000002E-3,4.3738639999999999E-3,4.3150579999999992E-3,6.4791210000000026E-3,6.4758539999999996E-3,6.5019900000000061E-3,6.5019899999999992E-3,8.6693200000000012E-3,8.6693199999999943E-3,8.6693199999999943E-3,1.0836650000000003E-2,1.0836650000000003E-2,1.0836649999999989E-2,1.3003979999999998E-2,1.3877787807814457E-17,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,3.2950995000000003E-5,9.8558955000000006E-5,1.6328482499999999E-4,2.6047164000000001E-4,3.5760944999999999E-4,4.5513930000000012E-4,5.5266915000000004E-4,6.8270895000000008E-4,8.1274875E-4,9.4278854999999993E-4,1.1053383000000001E-3,1.26788805E-3,1.4304378E-3,1.6254974999999998E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,3.511401854219949E-5,1.0502872442455243E-4,1.7400343670076726E-4,2.7756994884910489E-4,3.8108423913043476E-4,4.8501630434782619E-4,5.8894836956521746E-4,7.2752445652173915E-4,8.6610054347826084E-4,1.0046766304347824E-3,1.1778967391304349E-3,1.351116847826087E-3,1.524336956521739E-3,1.7322010869565215E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,3.2950995000000003E-5,9.8558955000000006E-5,1.6328482499999999E-4,2.6047164000000001E-4,3.5760944999999999E-4,4.5513930000000012E-4,5.5266915000000004E-4,6.8270895000000008E-4,8.1274875E-4,9.4278854999999993E-4,1.1053383000000001E-3,1.26788805E-3,1.4304378E-3,1.6254974999999998E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,1.6254975E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,3.511401854219949E-5,1.0502872442455243E-4,1.7400343670076726E-4,2.7756994884910489E-4,3.8108423913043476E-4,4.8501630434782619E-4,5.8894836956521746E-4,7.2752445652173915E-4,8.6610054347826084E-4,1.0046766304347824E-3,1.1778967391304349E-3,1.351116847826087E-3,1.524336956521739E-3,1.7322010869565215E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,1.7322010869565217E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceBattery Energy StorageNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,137.19999999999999,244.02,241.14,347.32,347.16,348.45,348.45,454.79,454.79,454.79,561.14,561.14,561.14,667.49,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageIncentive CostsMarket Potential0","WA","Extra Large General Service","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceBattery Energy StorageProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceBattery Energy StorageProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Battery Energy Storage","Program Annual Costs","Market Potential",0,137.19999999999999,244.02,241.14,347.32,347.16,348.45,348.45,454.79,454.79,454.79,561.14,561.14,561.14,667.49,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B272&C272&D272&E272&F272&G272","v":"WAResidentialTime-of-Use Opt-inParticipantsMarket Potential0"},"WA","Residential","Time-of-Use Opt-in","Participants","Market Potential",0,2987.2047098332096,8798.8478485741816,16742.893448243463,24347.945023132692,26478.678889413972,26186.936487235387,25693.975138518559,25063.479665002964,24291.231859549407,23708.796102471111,23249.333767018019,22764.424716651021,22252.795906062736,21713.117584953085,21144.002706558891,20544.006702600778,19911.627701288395,19245.307276849187,18543.43183252131,17804.334734298805,17225.927561742043,17119.375356514105,17009.444896289289,16896.083405983292,16779.237428713208,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialTime-of-Use Opt-inNew ParticipantsMarket Potential0","WA","Residential","Time-of-Use Opt-in","New Participants","Market Potential",0,2987.2047098332096,5811.6431387409721,7944.0455996692817,7605.0515748892285,2130.7338662812799,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.36883717464904631,1.0828676904650669,2.0536793480161304,2.9778495756550862,3.2273561490825484,3.1755312056132543,3.0998744072278055,3.0083978784620031,2.9008452171367525,2.8168623675085089,2.7481962796942869,2.6771642922151475,2.603658602211965,2.527567406583942,2.448774966767687,2.367161715624591,2.2826044137061876,2.1949763631884673,2.104147688920694,2.0099856973389141,1.9347771156835669,1.9130104777067063,1.8910398639202879,1.8688639952074111,1.846481585499425,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.39304899259276033,1.1539510767956809,2.1884903538108804,3.1733264872709785,3.4392115825687855,3.3839846607131867,3.3033614740279256,3.2058800921376847,3.0912672816887814,3.0017714913773541,2.928597911012667,2.8529031246964487,2.7745722529965526,2.6934861536487018,2.6095214905879018,2.5225508478522922,2.432442896106338,2.3390626206185714,2.2422716207594777,2.1419284924753987,2.0617829451018403,2.0385874655868568,2.0151746205459165,1.9915430468962181,1.9676913741468722,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.34257360040328888,1.005760560431544,1.907444196733123,2.7658075723040643,2.9975476762257021,2.9494130013739435,2.879143452642718,2.7941806398744169,2.6942864183708366,2.6162836866867241,2.5525070650636219,2.4865330110174586,2.418261397944621,2.3475883838427047,2.2744064714769103,2.1986046076563479,2.1200683283723034,2.0386799574990584,1.954318867830221,1.8668618144352964,1.7970085665260744,1.7767918528840634,1.7563856878193704,1.7357888832964281,1.7150002448229278,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.36506138150393103,1.0717823534010487,2.0326557936201226,2.9473652731287983,3.1943176430367668,3.1430232324956773,3.0681409341887447,2.9776008523810922,2.8711492096875921,2.7880260940821868,2.7200629423099123,2.6497581106324155,2.5770048997704826,2.5016926511537774,2.4237068110367757,2.3429290362919306,2.2592373490753448,2.1725063485710341,2.0826074891626396,1.989409435672737,1.9149707656927477,1.8934269532012611,1.8716812530044442,1.8497323990797401,1.8275791185240067,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","WA","Residential","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,202501.04,343722.96,450343.08,433393.38,159677.5,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialTime-of-Use Opt-inIncentive CostsMarket Potential0","WA","Residential","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","WA","Residential","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialTime-of-Use Opt-inProgram Annual CostsMarket Potential0","WA","Residential","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,202501.04,343722.96,450343.08,433393.38,159677.5,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,53140.800000000003,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inParticipantsMarket Potential0","WA","General Service","Time-of-Use Opt-in","Participants","Market Potential",0,286.05130957117603,811.71822750851811,1455.2084228623512,2052.530049620068,2225.9936746190197,2194.879950479668,2143.8724332078759,2079.2907055717064,2000.6957900180294,1940.7878107250451,1892.9204265131013,1842.4320538156755,1789.1905835387988,1733.0579188217869,1673.889898050006,1611.536254299378,1545.8406190463518,1476.6405792002186,1403.7677979100847,1327.0482111896717,1248.0198421676898,1215.9731809299908,1183.1856306825275,1149.6457553956138,1115.3419663062605,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inNew ParticipantsMarket Potential0","WA","General Service","Time-of-Use Opt-in","New Participants","Market Potential",0,286.05130957117603,525.66691793734208,643.49019535383309,597.32162675771679,173.46362499895167,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.0245197317104967E-3,5.7488660038018122E-3,1.0308609820758013E-2,1.4541122130985988E-2,1.5771239064422245E-2,1.555199639135626E-2,1.5191749746260424E-2,1.4735251353456593E-2,1.4179367853779453E-2,1.3755847079092014E-2,1.3417608333129214E-2,1.3060737488122212E-2,1.2684293683885394E-2,1.2287293317066258E-2,1.1868709478762202E-2,1.142747165021033E-2,1.0962465712242325E-2,1.0472534332905601E-2,9.9564778075887737E-3,9.4130554373198939E-3,8.8531712997611083E-3,8.6265041651600385E-3,8.3945455622438415E-3,8.1572131318766589E-3,7.9144234050904476E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.1574165938943912E-3,6.126242544545836E-3,1.0985304583075462E-2,1.5495654444784727E-2,1.6806520742137943E-2,1.6572886180047167E-2,1.6188991630712302E-2,1.5702527017749993E-2,1.5110153296866425E-2,1.4658831073201208E-2,1.4298389101800101E-2,1.3918091952389399E-2,1.351693700328793E-2,1.3093876083830199E-2,1.2647814875066285E-2,1.2177612585475629E-2,1.1682081961042546E-2,1.1159989698322251E-2,1.0610057339715233E-2,1.0030962742242001E-2,9.4343257670088543E-3,9.1927793746377218E-3,8.9455941626639408E-3,8.6926823655974622E-3,8.4339550352626243E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,2.0138665584630631E-3,5.7186150437565668E-3,1.0254365149964932E-2,1.4464605665946349E-2,1.5688249632682782E-2,1.5470160630851913E-2,1.5111809630368426E-2,1.4657713366024767E-2,1.4104754966624347E-2,1.3683462789720354E-2,1.3347003881169507E-2,1.299201091706397E-2,1.2617547988094327E-2,1.2222636666702003E-2,1.1806255447655335E-2,1.1367339445340699E-2,1.0904780403167615E-2,1.0417427079150221E-2,9.9040860816119389E-3,9.3635232402309865E-3,8.8065852546026953E-3,8.5811108593049686E-3,8.3503728397915367E-3,8.1142892703064372E-3,7.8727771211015343E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,2.1460641074840824E-3,6.094005801104611E-3,1.092749909416553E-2,1.5414115159789374E-2,1.6718083581290264E-2,1.6485678421623948E-2,1.6103803953930549E-2,1.5619899153905336E-2,1.5030642547553652E-2,1.4581695214962014E-2,1.4223149915994786E-2,1.3844853918439865E-2,1.3445809876485856E-2,1.3024975135019184E-2,1.2581261133477552E-2,1.211353308327014E-2,1.1620609977800102E-2,1.1101265003357013E-2,1.0554226429680241E-2,9.9781790710048879E-3,9.3846816438647642E-3,9.144406286556871E-3,8.8985217815340332E-3,8.6469408251347371E-3,8.3895749372352238E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","WA","General Service","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,17485.740000000002,31862.68,38932.080000000002,36161.96,10730.48,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inIncentive CostsMarket Potential0","WA","General Service","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","WA","General Service","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceTime-of-Use Opt-inProgram Annual CostsMarket Potential0","WA","General Service","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,17485.740000000002,31862.68,38932.080000000002,36161.96,10730.48,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,322.67,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inParticipantsMarket Potential0","WA","Large General Service","Time-of-Use Opt-in","Participants","Market Potential",0,22.470237004852368,63.431611727111274,115.81291430791416,166.51200205067303,184.79488864468556,184.58402441812413,184.38047973728061,184.18400054268511,183.99434159320393,183.81126615995734,183.63454573086153,183.46395972542598,183.29929521944976,183.14034667927393,182.9869157052577,182.8388107841588,182.69584705010803,182.55784605388109,182.42463554017843,182.29604923263571,182.17192662629671,182.05211278728916,181.93645815945396,181.82481837768623,181.71705408775523,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inNew ParticipantsMarket Potential0","WA","Large General Service","Time-of-Use Opt-in","New Participants","Market Potential",0,22.470237004852368,40.96137472225891,52.381302580802881,50.699087742758877,18.282886594012524,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,5.8846214379771458E-2,0.16607909172581337,0.3031290420261461,0.43570619131529004,0.4834124693954639,0.4827294372203218,0.48206817704498911,0.48142799493532662,0.48080821907480464,0.48020819905955331,0.47962730521588115,0.4790649279395478,0.47852047705609368,0.47799338120155976,0.47748308722294353,0.47698905959776711,0.47651077987214108,0.47604774611674283,0.47559947240013195,0.47516548827885374,0.47474533830379362,0.47433858154226594,0.47394479111533516,0.47356355374988385,0.47319446934495724,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,6.2709094607599589E-2,0.17698112929008245,0.32302753839103376,0.46430753550222725,0.51514542774452676,0.51441755884518525,0.51371289113916141,0.51303068513994732,0.51237022493052498,0.51173081741214121,0.51111179157702591,0.5105124978042922,0.50993230717827542,0.50937061082860158,0.50882681929128681,0.50830036189020367,0.50779068613825773,0.50729725715765428,0.50681955711864013,0.50635708469613572,0.50590935454368458,0.50547589678417082,0.50505625651676811,0.50464999333960336,0.50425668088763553,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,5.8536561227508201E-2,0.16520517120569242,0.30153395448491244,0.43341347296418775,0.48086871706458956,0.48018927905550152,0.47953149848034221,0.4788946850565054,0.47827817050261007,0.47768130783725971,0.47710347070015258,0.47654405269483113,0.47600246675237784,0.47547814451539289,0.47497053574160641,0.47447910772649926,0.47400334474432493,0.47354274750695036,0.47309683263994257,0.47266513217535489,0.47224719306068014,0.47184257668345309,0.47145085841100692,0.47107162714489814,0.47070448488953265,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,6.2379114692570549E-2,0.17604984143829117,0.3213277434834958,0.46186431475297074,0.51243469422910226,0.51171065542998884,0.51100969573779009,0.51033107955723078,0.50967409473850178,0.50903805182998685,0.50842228335480877,0.50782614311043384,0.5072490054905987,0.50669026482885005,0.50614933476300772,0.50562564761988416,0.50511865381961307,0.50462782129896666,0.50415263495305052,0.50369259609479422,0.50324722193167104,0.50281604505909328,0.50239861296995625,0.50199448757981469,0.50160324476719165,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","WA","Large General Service","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,9255.57,10365.040000000001,11050.23,10949.3,9004.33,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inIncentive CostsMarket Potential0","WA","Large General Service","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","WA","Large General Service","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceTime-of-Use Opt-inProgram Annual CostsMarket Potential0","WA","Large General Service","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,9255.57,10365.040000000001,11050.23,10949.3,9004.33,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,7907.35,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inParticipantsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Participants","Market Potential",0,0.26849387564999999,0.76154325390000011,1.4000590632600001,2.0209995234000004,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,2.2455550260000003,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inNew ParticipantsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","New Participants","Market Potential",0,0.26849387564999999,0.49304937825000011,0.63851580935999996,0.62094046014000037,0.2245555025999999,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.8052804552168326E-2,7.9695102622929323E-2,0.14661718891817707,0.21171401831064898,0.2353163230661976,0.23539491501891793,0.23547357403032776,0.23555230014968709,0.23563109342629288,0.23570995390947871,0.23578888164861528,0.23586787669310991,0.23594693909240697,0.2360260688959879,0.23610526615337069,0.23618453091411074,0.23626386322779999,0.23634326314406803,0.23642273071258105,0.2365022659830425,0.23658186900519287,0.23666153982880997,0.23674127850370857,0.23682108507974087,0.23690095960679614,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.9894293001031889E-2,8.492657994770815E-2,0.15624167617026541,0.22561169896701724,0.25076334512595649,0.25084709614121686,0.25093091861714384,0.25101481260623093,0.25109877816101117,0.25118281533405662,0.25126692417797875,0.25135110474542827,0.2514353570890952,0.2515196812617092,0.25160407731603868,0.2516885453048921,0.2517730852811168,0.25185769729760021,0.25194238140726882,0.25202713766308876,0.25211196611806574,0.25219686682524506,0.25228183983771163,0.25236688520859002,0.25245200299104448,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,3.1381267468362013E-2,8.9150919890303645E-2,0.16401330613288156,0.23683386889367658,0.26323658513640652,0.26332450201775048,0.26341249391429189,0.26350056088113527,0.26358870297342685,0.26367692024635359,0.26376521275514392,0.26385358055506758,0.26394202370143527,0.26403054224959949,0.26411913625495348,0.26420780577293235,0.26429655085901238,0.2643853715687115,0.26447426795758877,0.26456324008124493,0.26465228799532237,0.26474141175550481,0.26483061141751768,0.26491988703712804,0.26500923867014453,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,3.3441248367819705E-2,9.5003111562557169E-2,0.17477973799326679,0.2523805081987176,0.280516395072897,0.28061008313912028,0.28070385114481233,0.28079769914869485,0.28089162720953414,0.2809856353861398,0.28107972373736562,0.28117389232210954,0.28126814119931293,0.28136247042796192,0.28145688006708597,0.2815513701757591,0.28164594081309929,0.28174059203826884,0.28183532391047394,0.2819301364889652,0.28202502983303745,0.28212000400202986,0.28221505905532573,0.282310195052353,0.28240541205258368,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,4202.6400000000003,4216.12,4224.84,4223.79,4200.01,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inIncentive CostsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceTime-of-Use Opt-inProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,4202.6400000000003,4216.12,4224.84,4223.79,4200.01,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,4186.53,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B312&C312&D312&E312&F312&G312","v":"WAResidentialTime-of-Use Opt-outParticipantsMarket Potential0"},"WA","Residential","Time-of-Use Opt-out","Participants","Market Potential",0]
["WAResidentialTime-of-Use Opt-outNew ParticipantsMarket Potential0","WA","Residential","Time-of-Use Opt-out","New Participants","Market Potential",0]
["WAResidentialTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WAResidentialTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WAResidentialTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WAResidentialTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WAResidentialTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","WA","Residential","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["WAResidentialTime-of-Use Opt-outIncentive CostsMarket Potential0","WA","Residential","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["WAResidentialTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","WA","Residential","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["WAResidentialTime-of-Use Opt-outProgram Annual CostsMarket Potential0","WA","Residential","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outParticipantsMarket Potential0","WA","General Service","Time-of-Use Opt-out","Participants","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outNew ParticipantsMarket Potential0","WA","General Service","Time-of-Use Opt-out","New Participants","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","WA","General Service","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outIncentive CostsMarket Potential0","WA","General Service","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","WA","General Service","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["WAGeneral ServiceTime-of-Use Opt-outProgram Annual CostsMarket Potential0","WA","General Service","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outParticipantsMarket Potential0","WA","Large General Service","Time-of-Use Opt-out","Participants","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outNew ParticipantsMarket Potential0","WA","Large General Service","Time-of-Use Opt-out","New Participants","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","WA","Large General Service","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outIncentive CostsMarket Potential0","WA","Large General Service","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","WA","Large General Service","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["WALarge General ServiceTime-of-Use Opt-outProgram Annual CostsMarket Potential0","WA","Large General Service","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outParticipantsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Participants","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outNew ParticipantsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","New Participants","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outIncentive CostsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["WAExtra Large General ServiceTime-of-Use Opt-outProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
["WAResidentialVariable Peak Pricing RatesParticipantsMarket Potential0","WA","Residential","Variable Peak Pricing Rates","Participants","Market Potential",0,5613.4114170810099,16103.228140011501,34313.341589914176,40981.290015697683,43918.911146113969,43435.012055364459,42617.36077588849,41571.588258497934,40290.697965891392,39324.63978865854,38562.551711302927,37758.256391813666,36909.642291168238,36014.503816500059,35070.540340054911,34075.355825906248,33026.459191549977,31921.265551111734,30757.09850925078,29531.19370030042,28571.817542453227,28395.084524413611,28212.748157292379,28024.720905595525,27830.91410296243,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialVariable Peak Pricing RatesNew ParticipantsMarket Potential0","WA","Residential","Variable Peak Pricing Rates","New Participants","Market Potential",0,5613.4114170810099,10489.816722930491,18210.113449902674,6667.9484257835065,2937.6211304162862,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.2159668050514827,3.4768637984347075,7.3839760682110969,8.7932862843032833,9.3913340709446445,9.2405278584148203,9.0203729590003778,8.7541839790409632,8.4412148098305178,8.196831803848065,7.9970192823228237,7.7903221924062391,7.5764268368746128,7.3550078781385286,7.125728526744477,6.8882408524081313,6.6421862387333439,6.3871960057429531,6.1228922277071289,5.8488887775513829,5.6300381510012061,5.5666990711478359,5.5027664389000375,5.4382365321355692,5.3731056085031677,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.2957873029107871,3.7050978244189126,7.8686871997134453,9.3705096806300965,10.007815506121744,9.847109823545205,9.6125031532399596,9.3288405573752797,8.9953269499472697,8.7349017517562491,8.5219728072493854,8.301707366161807,8.073771139039442,7.8378174319464282,7.5934873473406617,7.3404101155244366,7.0782035792128557,6.8064748569298308,6.5248212145216637,6.2328311781238099,5.999614397912624,5.9321175097483332,5.8639881062447117,5.7952222209458322,5.7258158658388405,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.1293821637521528,3.2292887794592926,6.8581895775167023,8.1671478604533974,8.7226108060685998,8.5825429638325712,8.3780645063381733,8.1308298903070089,7.840146134761854,7.613164767397115,7.4275801799170367,7.2356012495042243,7.036936616190804,6.8312841085119267,6.6183309185848893,6.3977538909948217,6.1692199451347909,5.932386653408412,5.6869030008235608,5.432410355031843,5.2291432978021959,5.1703143669813079,5.1109341485062387,5.0509991852937413,4.9905060014719815,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.2035189298296598,3.4412710778551712,7.3083861652991287,8.7032692460074568,9.2951948061259593,9.1459323996510768,8.9280312301131435,8.6645672317849627,8.3548019338894441,8.1129206813694754,7.9151536444128689,7.7105725165219781,7.4988668117975319,7.2797145231371765,7.0527823088074264,6.8177258002928616,6.5741900523601782,6.3218101592161249,6.0602120639637267,5.789013592318673,5.5724033437789808,5.5097126672861334,5.4464345146059658,5.3825652017196735,5.3181010245865101,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","WA","Residential","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,332320.68,576140.94999999995,962155.78,385047.53,198531.17,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialVariable Peak Pricing RatesIncentive CostsMarket Potential0","WA","Residential","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B360&C360&D360&E360&F360&G360","v":"WAResidentialVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0"},"WA","Residential","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","WA","Residential","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,332320.68,576140.94999999995,962155.78,385047.53,198531.17,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,51650.11,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesParticipantsMarket Potential0","WA","General Service","Variable Peak Pricing Rates","Participants","Market Potential",0,543.01890234037512,1500.7265129700277,3012.7758330584752,3489.9721037934146,3729.8236321068312,3677.6901939479508,3592.2231751038894,3484.0115226242842,3352.3196958513631,3251.9392682398689,3171.7337838862791,3087.1366317107654,2997.9264527641449,2903.8718551335055,2804.7312849441737,2700.252958405862,2590.1748680290125,2474.2248781868275,2352.1209275366473,2223.5713584799255,2091.1532470782845,2037.4566010467322,1982.5185384878578,1926.3198974542279,1868.8412600820095,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesNew ParticipantsMarket Potential0","WA","General Service","Variable Peak Pricing Rates","New Participants","Market Potential",0,543.01890234037512,957.70761062965255,1512.0493200884475,477.19627073493939,239.85152831341657,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,7.6864006260130124E-2,0.21257316489980863,0.42684649226149712,0.4944932290213031,0.52851848449350403,0.52117132522264265,0.5090989059198735,0.49380094247179734,0.47517243119223218,0.46097959846203357,0.44964469771751858,0.4376854066692647,0.42507019564497472,0.41176610258307039,0.39773871418636558,0.38295215572416397,0.36736909134910534,0.35095073708694802,0.33365688899046531,0.31544596932833951,0.29668339051853276,0.28908742611938237,0.28131413647627146,0.27336076160785133,0.26522450434058875,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,8.1909640089652735E-2,0.22652724307311234,0.45486625347559367,0.52695356886328126,0.56321236625479965,0.55538291264134976,0.54251801568613967,0.52621583809867578,0.50636448336768136,0.49123998131077745,0.47916101632301639,0.46641667377372625,0.45297335426787588,0.43879593199389427,0.42384773464020203,0.40809053252788147,0.39148453894832197,0.37398842400569909,0.35555934461899541,0.33615299374290231,0.31615877079980048,0.30806417958160953,0.29978062284342655,0.29130515942865659,0.28263480854708944,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,7.6459542148293994E-2,0.21145458911219722,0.42460039430508006,0.49189116890999168,0.52573738095986589,0.51842888298697187,0.50641998965153889,0.4912025252237453,0.47267203855460738,0.45855388956474402,0.44727863391011496,0.43538227353991676,0.42283344469333017,0.40959935875759446,0.39564578352084984,0.38093703302789816,0.36543596789538252,0.34910400823321491,0.33190116165032618,0.31378606920051,0.29512222047443559,0.28756622660432379,0.27983384058886018,0.27192231696992308,0.26382887329291416,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,8.1478625477721653E-2,0.22533523988938323,0.45247271345383638,0.52418070003196049,0.56024870093762347,0.5524604464908055,0.53966324557921874,0.52344685126145063,0.50369995583398053,0.48865504003063087,0.47663963545408672,0.46396235458217899,0.45058977482238938,0.43648695519777753,0.42161741636919209,0.40594312982512593,0.38942451821758578,0.37202046913172943,0.3536883649300151,0.33438413171409848,0.31449511985766793,0.30644312297988469,0.29820315493271543,0.2897722900361499,0.28114756318511741,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","WA","General Service","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,30762.639999999999,51497.07,79214.16,27471.5,15604.27,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesIncentive CostsMarket Potential0","WA","General Service","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0","WA","General Service","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","WA","General Service","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,30762.639999999999,51497.07,79214.16,27471.5,15604.27,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,3611.69,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesParticipantsMarket Potential0","WA","Large General Service","Variable Peak Pricing Rates","Participants","Market Potential",0,42.655855874230618,117.27407153524523,239.77207931262791,283.12484010219919,309.63805091560482,309.28473168367606,308.94367691363965,308.61446090931065,308.29667275030494,307.98991577917462,307.6938071063455,307.40797713223776,307.13206908597419,306.86573858009876,306.60865318075201,306.36049199276454,306.12094525915217,305.88971397451263,305.6665095118413,305.45105326229907,305.24307628748522,305.04231898377884,304.84853075833115,304.66146971630388,304.4809023589637,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesNew ParticipantsMarket Potential0","WA","Large General Service","Variable Peak Pricing Rates","New Participants","Market Potential",0,42.655855874230618,74.618215661014602,122.49800777738268,43.352760789571278,26.513210813405635,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.17186054319734853,0.47238691714283948,0.96550785098925529,1.1397584117610653,1.2461458123794902,1.2443850847635101,1.2426804812405301,1.2410302129797341,1.2394325481653174,1.2378858101792567,1.2363883758420038,1.2349386737092543,1.2335351824230012,1.2321764291151449,1.2308609878619847,1.2295874781879719,1.2283545636171496,1.2271609502707632,1.2260053855095712,1.2248866566194241,1.2238035895387438,1.2227550476265567,1.2217399304697971,1.2207571727286208,1.2198057430185245,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.18314209633136033,0.50339611801240358,1.0288873092383368,1.214576312618356,1.3279473703958762,1.3260710621947038,1.3242545622767796,1.322495964385906,1.3207934230235694,1.319145151512422,1.3175494201214875,1.3160045542511234,1.3145089326758324,1.3130609858430786,1.3116591942263265,1.3103020867305752,1.30898823914871,1.3077162726670537,1.3064848524185542,1.3052926860820802,1.304138522526368,1.3030211504971831,1.3019393973463311,1.3008921278011731,1.2998782427733637,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.17095620025003011,0.46990118208710241,0.96042727694137686,1.1337609183158164,1.2395885005277421,1.2378370379912973,1.2361414042187051,1.2344998197921102,1.2329105620086513,1.231371963072794,1.2298824083462809,1.228440334653865,1.2270442286430379,1.2256926251960409,1.2243841058924905,1.2231172975210025,1.2218908706382556,1.2207035381739817,1.2195540540804202,1.2184412120248129,1.2173638441235819,1.2163208197168422,1.2153110441819832,1.2143334577850584,1.2133870345687865,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.18217838901324607,0.50074721023774771,1.0234732277721408,1.2081851218199238,1.3209596126680967,1.3190931777400867,1.3172862363796942,1.3155368923615838,1.3138433098983924,1.312203711714401,1.3106163771806063,1.3090796405092338,1.3075918890057947,1.3061515613768553,1.3047571460917418,1.3034071797964648,1.3021002457781923,1.3008349724786676,1.2996100320550086,1.2984241389863735,1.2972760487250445,1.2961645563904969,1.2950884955050972,1.2940467367700963,1.2930381868806335,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","WA","Large General Service","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,15339.57,21732.04,31308,15478.95,12111.04,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesIncentive CostsMarket Potential0","WA","Large General Service","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0","WA","Large General Service","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","WA","Large General Service","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,15339.57,21732.04,31308,15478.95,12111.04,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,6808.4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesParticipantsMarket Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Participants","Market Potential",0,0.50454077754657489,1.3937398358383501,2.8693191551509094,3.4016491950903007,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,3.7245941186299998,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesNew ParticipantsMarket Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","New Participants","Market Potential",0,0.50454077754657489,0.88919905829177526,1.4755793193125593,0.53233003993939132,0.32294492353969906,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,6.8019975583202441E-2,0.18819889519624247,0.38771775228998834,0.45980239090240371,0.50362305446982569,0.50379125665304025,0.50395960235499426,0.50412809168111361,0.50429672473690346,0.50446550162794734,0.50463442245990853,0.50480348733852798,0.50497269636962649,0.50514204965910403,0.50531154731293881,0.505481189437189,0.50565097613799148,0.50582090752156283,0.50599098369419859,0.50616120476227378,0.50633157083224312,0.5065020820106404,0.50667273840407945,0.50684354011925359,0.50701448726293563,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,7.2485054969312068E-2,0.20055295737024986,0.41316896024082306,0.48998549755158111,0.53668270936682194,0.53686195295507277,0.53704134948315674,0.5372208990634203,0.53740060180829441,0.5375804578302934,0.53776046724201676,0.53794063015614657,0.53812094668545019,0.53830141694277922,0.53848204104106867,0.53866281909333869,0.53884375121269334,0.53902483751232189,0.53920607810549726,0.53938747310557733,0.53956902262600503,0.53975072678030733,0.53993258568209657,0.5401145994450699,0.54029676818300898,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,7.609054000281551E-2,0.21052867838652592,0.43372043120386694,0.51435790616469312,0.56337788780300257,0.56356604716120173,0.56375436706662652,0.56394284763721192,0.56413148899098131,0.56432029124604588,0.56450925452060496,0.56469837893294672,0.56488766460144701,0.56507711164457086,0.5652667201808711,0.56545649032898926,0.56564642220765549,0.56583651593568929,0.56602677163199766,0.56621718941557742,0.56640776940551374,0.5665985117209813,0.5667894164812427,0.56698048380565103,0.5671717138136475,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,8.1085400685012271E-2,0.22434854900524928,0.46219142285152059,0.54812223589587927,0.60036006799126451,0.60056057881628488,0.60076126072743663,0.60096211385039633,0.60116313831093493,0.60136433423491675,0.60156570174830026,0.60176724097713841,0.60196895204757783,0.60217083508585978,0.60237289021831952,0.60257511757138671,0.60277751727158513,0.60298008944553416,0.60318283421994634,0.60338575172162978,0.60358884207748698,0.60379210541451545,0.60399554185980675,0.60419915154054882,0.60440293458402339,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,3194.57,3348.43,3582.98,3205.68,3121.93,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesIncentive CostsMarket Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,3194.57,3348.43,3582.98,3205.68,3121.93,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,2992.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B392&C392&D392&E392&F392&G392","v":"WALarge General ServiceReal Time PricingParticipantsMarket Potential0"},"WA","Large General Service","Real Time Pricing","Participants","Market Potential",0]
["WALarge General ServiceReal Time PricingNew ParticipantsMarket Potential0","WA","Large General Service","Real Time Pricing","New Participants","Market Potential",0]
["WALarge General ServiceReal Time PricingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Real Time Pricing","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WALarge General ServiceReal Time PricingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Real Time Pricing","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WALarge General ServiceReal Time PricingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Real Time Pricing","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
[{"$f":"B397&C397&D397&E397&F397&G397","v":"WALarge General ServiceReal Time PricingWinter Peak Reduction @Generation (MW)Market Potential0"},"WA","Large General Service","Real Time Pricing","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WALarge General ServiceReal Time PricingNon-Incentive CostsMarket Potential0","WA","Large General Service","Real Time Pricing","Non-Incentive Costs","Market Potential",0]
["WALarge General ServiceReal Time PricingIncentive CostsMarket Potential0","WA","Large General Service","Real Time Pricing","Incentive Costs","Market Potential",0]
["WALarge General ServiceReal Time PricingProgram Annual BenefitsMarket Potential0","WA","Large General Service","Real Time Pricing","Program Annual Benefits","Market Potential",0]
["WALarge General ServiceReal Time PricingProgram Annual CostsMarket Potential0","WA","Large General Service","Real Time Pricing","Program Annual Costs","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingParticipantsMarket Potential0","WA","Extra Large General Service","Real Time Pricing","Participants","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingNew ParticipantsMarket Potential0","WA","Extra Large General Service","Real Time Pricing","New Participants","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Real Time Pricing","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Real Time Pricing","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Real Time Pricing","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
[{"$f":"B407&C407&D407&E407&F407&G407","v":"WAExtra Large General ServiceReal Time PricingWinter Peak Reduction @Generation (MW)Market Potential0"},"WA","Extra Large General Service","Real Time Pricing","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Real Time Pricing","Non-Incentive Costs","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingIncentive CostsMarket Potential0","WA","Extra Large General Service","Real Time Pricing","Incentive Costs","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Real Time Pricing","Program Annual Benefits","Market Potential",0]
["WAExtra Large General ServiceReal Time PricingProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Real Time Pricing","Program Annual Costs","Market Potential",0]
[{"$f":"B412&C412&D412&E412&F412&G412","v":"WAResidentialBehavioralParticipantsMarket Potential0"},"WA","Residential","Behavioral","Participants","Market Potential",0,11373.195864943846,22333.257942508935,36122.326450108274,41200.010571820836,40324.949979216311,39880.649195789709,39129.90774786043,38169.712621138933,36993.639817184798,36106.635867011173,35406.91078737787,34668.432357914528,33889.261830522897,33067.374099850851,32200.656802529469,31286.909974434751,30323.846382692504,29309.092667151828,28240.191446574801,27114.604568162908,26233.735836064025,26071.465189407652,25904.049725506608,25731.409072049144,25553.461818397733,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBehavioralNew ParticipantsMarket Potential0","WA","Residential","Behavioral","New Participants","Market Potential",0,11373.195864943846,10960.06207756509,13789.068507599339,5077.684121712562,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBehavioralSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Behavioral","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.49272813309350644,0.96439912999156285,1.554651232884342,1.7680433570323018,1.7245649619547145,1.6968718665745108,1.6564440186388851,1.6075627644285024,1.5500910932777259,1.5052141496794333,1.4685218468629078,1.4305653056180399,1.3912869205783753,1.3506269488146039,1.3085235444498062,1.2649128157756235,1.2197289087539709,1.1729041213346409,1.1243690536361077,1.0740527997339855,1.0338644601861506,1.02223327371015,1.0104930910409804,0.99864322867174438,0.98668299938081827,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBehavioralSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Behavioral","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.52507260559836577,1.0277058077488948,1.6567042123660933,1.8841041741605944,1.8377716985877179,1.8082607273811921,1.7651790479954019,1.7130890499024962,1.6518447285568263,1.6040218986353723,1.5649209791804217,1.524472832073785,1.4826160705225653,1.4392870298535847,1.3944198044009017,1.3479463083712953,1.2997963648273347,1.2498978275092081,1.1981767408739425,1.1445575444735565,1.1017310956800412,1.0893363956843032,1.076825544587575,1.0641978140150727,1.0514524716334381,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBehavioralWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Behavioral","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.45764272740253159,0.8957277218636327,1.4439500864503709,1.6421473216846727,1.6017648674061471,1.5760436981673493,1.5384945724940982,1.4930939773317131,1.4397146580533648,1.3980332408855027,1.3639536655419784,1.3286998736608238,1.2922183617474221,1.2544536409524942,1.2153482692225206,1.1748429043488713,1.1328763815236615,1.0893858195172108,1.044306760165006,0.99757334649959273,0.96024667467961822,0.94944370333640438,0.93853949702857609,0.92753342091931434,0.91642483672158503,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBehavioralWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Behavioral","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.48768406585947527,0.95452655782569551,1.5387362387578547,1.7499438636878439,1.7069105577644363,1.6795009571263313,1.6394869698359955,1.5911061139511009,1.5342227813867912,1.4898052439103822,1.4534885608929864,1.4159205814799911,1.3770442900121718,1.3368005551497169,1.2951281641331209,1.2519638793146539,1.207242520805266,1.1608970796219211,1.1128588663309953,1.0630577008733937,1.0232807701189452,1.0117686523192715,1.0001486541225235,0.98842009901887717,0.97658230682180847,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialBehavioralNon-Incentive CostsMarket Potential0","WA","Residential","Behavioral","Non-Incentive Costs","Market Potential",0,146093.48000000001,181713.68,226528.16,243030.63,240186.68,238742.7,236302.79,233182.16,229359.92,226477.16,224203.05,221803,219270.7,216599.56,213782.73,210813.05,207683.1,204385.15,200911.22,197253.06,194390.24,193862.86,193318.76,192757.67,192179.35,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBehavioralIncentive CostsMarket Potential0","WA","Residential","Behavioral","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialBehavioralProgram Annual BenefitsMarket Potential0","WA","Residential","Behavioral","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialBehavioralProgram Annual CostsMarket Potential0","WA","Residential","Behavioral","Program Annual Costs","Market Potential",0,146093.48000000001,181713.68,226528.16,243030.63,240186.68,238742.7,236302.79,233182.16,229359.92,226477.16,224203.05,221803,219270.7,216599.56,213782.73,210813.05,207683.1,204385.15,200911.22,197253.06,194390.24,193862.86,193318.76,192757.67,192179.35,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary ServicesParticipantsMarket Potential0","ID","Residential","Ancillary Services","Participants","Market Potential",0]
["IDResidentialAncillary ServicesNew ParticipantsMarket Potential0","ID","Residential","Ancillary Services","New Participants","Market Potential",0]
["IDResidentialAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDResidentialAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDResidentialAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDResidentialAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDResidentialAncillary ServicesNon-Incentive CostsMarket Potential0","ID","Residential","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["IDResidentialAncillary ServicesIncentive CostsMarket Potential0","ID","Residential","Ancillary Services","Incentive Costs","Market Potential",0]
["IDResidentialAncillary ServicesProgram Annual BenefitsMarket Potential0","ID","Residential","Ancillary Services","Program Annual Benefits","Market Potential",0]
["IDResidentialAncillary ServicesProgram Annual CostsMarket Potential0","ID","Residential","Ancillary Services","Program Annual Costs","Market Potential",0]
["IDGeneral ServiceAncillary ServicesParticipantsMarket Potential0","ID","General Service","Ancillary Services","Participants","Market Potential",0]
["IDGeneral ServiceAncillary ServicesNew ParticipantsMarket Potential0","ID","General Service","Ancillary Services","New Participants","Market Potential",0]
["IDGeneral ServiceAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDGeneral ServiceAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDGeneral ServiceAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDGeneral ServiceAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDGeneral ServiceAncillary ServicesNon-Incentive CostsMarket Potential0","ID","General Service","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["IDGeneral ServiceAncillary ServicesIncentive CostsMarket Potential0","ID","General Service","Ancillary Services","Incentive Costs","Market Potential",0]
["IDGeneral ServiceAncillary ServicesProgram Annual BenefitsMarket Potential0","ID","General Service","Ancillary Services","Program Annual Benefits","Market Potential",0]
["IDGeneral ServiceAncillary ServicesProgram Annual CostsMarket Potential0","ID","General Service","Ancillary Services","Program Annual Costs","Market Potential",0]
["IDLarge General ServiceAncillary ServicesParticipantsMarket Potential0","ID","Large General Service","Ancillary Services","Participants","Market Potential",0]
["IDLarge General ServiceAncillary ServicesNew ParticipantsMarket Potential0","ID","Large General Service","Ancillary Services","New Participants","Market Potential",0]
["IDLarge General ServiceAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDLarge General ServiceAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDLarge General ServiceAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDLarge General ServiceAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDLarge General ServiceAncillary ServicesNon-Incentive CostsMarket Potential0","ID","Large General Service","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["IDLarge General ServiceAncillary ServicesIncentive CostsMarket Potential0","ID","Large General Service","Ancillary Services","Incentive Costs","Market Potential",0]
["IDLarge General ServiceAncillary ServicesProgram Annual BenefitsMarket Potential0","ID","Large General Service","Ancillary Services","Program Annual Benefits","Market Potential",0]
["IDLarge General ServiceAncillary ServicesProgram Annual CostsMarket Potential0","ID","Large General Service","Ancillary Services","Program Annual Costs","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesParticipantsMarket Potential0","ID","Extra Large General Service","Ancillary Services","Participants","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesNew ParticipantsMarket Potential0","ID","Extra Large General Service","Ancillary Services","New Participants","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Ancillary Services","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Ancillary Services","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Ancillary Services","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Ancillary Services","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Ancillary Services","Non-Incentive Costs","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesIncentive CostsMarket Potential0","ID","Extra Large General Service","Ancillary Services","Incentive Costs","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Ancillary Services","Program Annual Benefits","Market Potential",0]
["IDExtra Large General ServiceAncillary ServicesProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Ancillary Services","Program Annual Costs","Market Potential",0]
["IDResidentialDLC Central ACParticipantsMarket Potential0","ID","Residential","DLC Central AC","Participants","Market Potential",0,390.1516503334658,1236.047113526191,2993.8791709442066,4040.6690095947142,4743.0311371579992,5050.9439833623837,5377.1193532282996,5722.3936573029023,6087.6030207586919,6473.5754669227654,6881.1215229585368,7311.0230011660051,7764.0196741537593,8240.7935220901381,8741.9501847112406,9267.9971990127797,9819.3185447453943,10396.144953022243,10998.519357460609,11626.256781100434,12247.179907908565,12396.809417131881,12548.267019859069,12701.575050761123,12856.756117382121,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Central ACNew ParticipantsMarket Potential0","ID","Residential","DLC Central AC","New Participants","Market Potential",0,390.1516503334658,845.89546319272517,1757.8320574180157,1046.7898386505076,702.36212756328496,307.91284620438455,326.17536986591585,345.2743040746027,365.20936345578957,385.97244616407352,407.54605603577147,429.90147820746824,452.99667298775421,476.77384793637884,501.15666262110244,526.04701430153909,551.32134573261465,576.82640827684918,602.37440443836567,627.73742363982456,620.9231268081312,149.62950922331584,151.45760272718871,153.30803090205336,155.18106662099854,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Central ACSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Central AC","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.19507582516673289,0.61802355676309551,1.4969395854721033,2.0203345047973573,2.3715155685789995,2.5254719916811919,2.6885596766141497,2.8611968286514511,3.0438015103793461,3.2367877334613828,3.4405607614792686,3.6555115005830023,3.8820098370768799,4.1203967610450691,4.3709750923556205,4.6339985995063895,4.9096592723726973,5.1980724765111219,5.4992596787303043,5.8131283905502169,6.1235899539542826,6.1984047085659402,6.274133509929535,6.3507875253805617,6.4283780586910604,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Central ACSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Central AC","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.20788131411629676,0.6585928780510395,1.5952041618415422,2.1529566334157688,2.5271905036008091,2.6912531880660611,2.8650465437064683,3.0490162283156979,3.2436077476335741,3.4492622905598709,3.6664117236565095,3.8954726135794995,4.136839127319778,4.3908746387948305,4.6579018460737647,4.9381911759445751,5.2319472211985261,5.539292920408271,5.8602511495420977,6.1947233488386795,6.5255647420655185,6.6052906101512576,6.6859905263528718,6.7676763910705047,6.8503602500970375,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Central ACWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Central AC","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Central ACWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Central AC","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Central ACNon-Incentive CostsMarket Potential0","ID","Residential","DLC Central AC","Non-Incentive Costs","Market Potential",0,158807.06,315641.71999999997,630313.25,416388.01,315301.84999999998,193080.94,203165.23,213765.45,224892.4,236554.22,248755.88,261498.33,274777.75,288584.51,302902.03999999998,317705.57,332960.53000000003,348620.89,364627.12,380903.87,386795.3,237926.53,240480.46,243065.61,245682.33,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Central ACIncentive CostsMarket Potential0","ID","Residential","DLC Central AC","Incentive Costs","Market Potential",0,7803.03,24720.94,59877.58,80813.38,94860.62,101018.88,107542.39,114447.87,121752.06,129471.51,137622.43,146220.46,155280.39000000001,164815.87,174839,185359.94,196386.37,207922.9,219970.39,232525.14,244943.6,247936.19,250965.34,254031.5,257135.12,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Central ACProgram Annual BenefitsMarket Potential0","ID","Residential","DLC Central AC","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Central ACProgram Annual CostsMarket Potential0","ID","Residential","DLC Central AC","Program Annual Costs","Market Potential",0,166610.09,340362.66,690190.83,497201.39,410162.47,294099.82,310707.62,328213.33,346644.46,366025.73,386378.31,407718.79,430058.14,453400.38,477741.05,503065.51,529346.9,556543.79,584597.51,613429.01,631738.9,485862.71,491445.8,497097.11,502817.45,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Central ACParticipantsMarket Potential0","ID","General Service","DLC Central AC","Participants","Market Potential",0,54.574646537132622,172.69458884808466,417.81635031123909,563.68799632753905,661.41941941163202,704.0930560979358,749.28112874030421,797.09760325632817,847.65626411665733,901.0696282456995,957.44764167803487,1016.8961251858478,1079.5149302839368,1145.3957615520178,1214.6196150007702,1287.253775148263,1363.3483054536568,1442.9319576469316,1526.0074151513311,1612.5457740544266,1698.0824301412449,1718.2403738070518,1738.6407291871635,1759.2863865301115,1780.1802707409511,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Central ACNew ParticipantsMarket Potential0","ID","General Service","DLC Central AC","New Participants","Market Potential",0,54.574646537132622,118.11994231095204,245.12176146315443,145.87164601629996,97.731423084092967,42.67363668630378,45.188072642368411,47.816474516023959,50.558660860329155,53.413364129042179,56.378013432335365,59.448483507812966,62.618805098088956,65.88083126808101,69.223853448752379,72.634160147492821,76.094530305393846,79.583652193274702,83.075457504399537,86.538358903095514,85.536656086818311,20.157943665806897,20.400355380111705,20.64565734294797,20.893884210839587,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Central ACSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Central AC","Summer Peak Reduction @Meter  (MW)","Market Potential",0,6.8218308171415776E-2,0.21586823606010583,0.52227043788904881,0.70460999540942382,0.82677427426454009,0.8801163201224198,0.9366014109253803,0.99637200407041016,1.0595703301458215,1.1263370353071243,1.1968095520975435,1.2711201564823098,1.3493936628549208,1.4317447019400222,1.5182745187509628,1.6090672189353288,1.7041853818170711,1.8036649470586645,1.9075092689391637,2.0156822175680333,2.1226030376765563,2.1478004672588149,2.1733009114839543,2.1991079831626394,2.2252253384261889,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Central ACSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Central AC","Summer Peak Reduction @Generation (MW)","Market Potential",0,7.2696406832284496E-2,0.23003861472730799,0.5565541750735814,0.75086316646358031,0.88104675433135127,0.93789036671187109,0.99808334497589546,1.0617774979437449,1.1291243927385139,1.2002739080425451,1.2753724979726593,1.3545611215710889,1.4379727865035388,1.5257296482736811,1.6179395979869595,1.7146922622925498,1.8160543284495643,1.9220640953310577,2.0327251374032009,2.1479989530776145,2.2619384459468845,2.2887899267463925,2.3159643131755692,2.3434654552031535,2.3712972489622643,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B476&C476&D476&E476&F476&G476","v":"IDGeneral ServiceDLC Central ACWinter Peak Reduction @Meter  (MW)Market Potential0"},"ID","General Service","DLC Central AC","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Central ACWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Central AC","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Central ACNon-Incentive CostsMarket Potential0","ID","General Service","DLC Central AC","Non-Incentive Costs","Market Potential",0,27089.13,49912.36,95644.55,64292.09,49435.63,31546.03,32975.81,34477.94,36053.83,37704.53,39430.6,41232.04,43108.14,45057.37,47077.2,49163.89,51312.35,53515.79,55765.52,58050.59,58827,37187.19,37533.599999999999,37884.17,38238.94,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Central ACIncentive CostsMarket Potential0","ID","General Service","DLC Central AC","Incentive Costs","Market Potential",0,2073.84,6562.39,15877.02,21420.14,25133.94,26755.54,28472.68,30289.71,32210.94,34240.65,36383.01,38642.050000000003,41021.57,43525.04,46155.55,48915.64,51807.24,54831.41,57988.28,61276.74,64527.13,65293.13,66068.350000000006,66852.88,67646.850000000006,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Central ACProgram Annual BenefitsMarket Potential0","ID","General Service","DLC Central AC","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Central ACProgram Annual CostsMarket Potential0","ID","General Service","DLC Central AC","Program Annual Costs","Market Potential",0,29162.959999999999,56474.75,111521.57,85712.24,74569.570000000007,58301.56,61448.49,64767.65,68264.77,71945.179999999993,75813.61,79874.09,84129.71,88582.41,93232.74,98079.54,103119.58,108347.2,113753.81,119327.33,123354.13,102480.32000000001,103601.95,104737.05,105885.79,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingParticipantsMarket Potential0","ID","Residential","DLC Water Heating","Participants","Market Potential",0,899.08346967170064,2695.4858291558157,6284.7234413183569,8068.2103820675966,8951.2003534908981,8937.7427678109689,8924.305414793158,8910.8882640188931,8897.4912851153276,8884.1144477552753,8870.7577216571535,8857.4210765849075,8844.1044823479242,8830.8079088009999,8817.5313258442402,8804.2747034230106,8791.0380115278549,8777.8212201944425,8764.6242995034845,8751.4472195806829,8738.2899505966434,8725.1524627668277,8712.0347263514705,8698.9367116555241,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingNew ParticipantsMarket Potential0","ID","Residential","DLC Water Heating","New Participants","Market Potential",0,899.08346967170064,1796.4023594841151,3589.2376121625412,1783.4869407492397,882.98997142330154,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Water Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.4495417348358503,1.3477429145779078,3.1423617206591783,4.0341051910337979,4.4756001767454494,4.4688713839054843,4.4621527073965792,4.4554441320094469,4.4487456425576637,4.4420572238776375,4.4353788608285765,4.4287105382924539,4.4220522411739625,4.4154039544005004,4.4087656629221197,4.402137351711505,4.3955190057639273,4.3889106100972208,4.3823121497517423,4.3757236097903416,4.3691449752983216,4.3625762313834135,4.3560173631757353,4.3494683558277618,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Water Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.47905129458210816,1.436213677086432,3.3486378097391074,4.2989185752704584,4.7693949027551676,4.7622244074014111,4.7550646924515974,4.7479157416980469,4.7407775389574418,4.7336500680707987,4.7265333129034275,4.7194272573448997,4.7123318853089966,4.7052471807336964,4.698173127581116,4.6911097098374945,4.6840569115131361,4.6770147166423923,4.6699831092836126,4.6629620735191191,4.6559515934551596,4.6489516532218813,4.6419622369732902,4.6349833288872144,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Water Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.4495417348358503,1.3477429145779078,3.1423617206591783,4.0341051910337979,4.4756001767454494,4.4688713839054843,4.4621527073965792,4.4554441320094469,4.4487456425576637,4.4420572238776375,4.4353788608285765,4.4287105382924539,4.4220522411739625,4.4154039544005004,4.4087656629221197,4.402137351711505,4.3955190057639273,4.3889106100972208,4.3823121497517423,4.3757236097903416,4.3691449752983216,4.3625762313834135,4.3560173631757353,4.3494683558277618,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Water Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.47905129458210816,1.436213677086432,3.3486378097391074,4.2989185752704584,4.7693949027551676,4.7622244074014111,4.7550646924515974,4.7479157416980469,4.7407775389574418,4.7336500680707987,4.7265333129034275,4.7194272573448997,4.7123318853089966,4.7052471807336964,4.698173127581116,4.6911097098374945,4.6840569115131361,4.6770147166423923,4.6699831092836126,4.6629620735191191,4.6559515934551596,4.6489516532218813,4.6419622369732902,4.6349833288872144,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Water HeatingIncentive CostsMarket Potential0","ID","Residential","DLC Water Heating","Incentive Costs","Market Potential",0,21578,64691.66,150833.35999999999,193637.05,214828.81,214505.83,214183.33,213861.32,213539.79,213218.75,212898.19,212578.11,212258.51,211939.39,211620.75,211302.59,210984.91,210667.71,210350.98,210034.73,209718.96,209403.66,209088.83,208774.48,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingNon-Incentive CostsMarket Potential0","ID","Residential","DLC Water Heating","Non-Incentive Costs","Market Potential",0,580751.91,1088674.99,2103501.7799999998,1205531.6299999999,757581.98,298117.67,297808.61,297500.02,297191.89,296884.21999999997,296577.01,296270.27,295963.99,295658.17,295352.81,295047.90000000002,294743.46000000002,294439.46999999997,294135.95,293832.87,293530.26,293228.09000000003,292926.39,292625.13,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Water HeatingProgram Annual BenefitsMarket Potential0","ID","Residential","DLC Water Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Water HeatingProgram Annual CostsMarket Potential0","ID","Residential","DLC Water Heating","Program Annual Costs","Market Potential",0,602329.91,1153366.6499999999,2254335.15,1399168.68,972410.79,512623.5,511991.94,511361.33,510731.68,510102.97,509475.2,508848.38,508222.5,507597.56,506973.56,506350.5,505728.37,505107.18,504486.93,503867.61,503249.21,502631.75,502015.22,501399.61,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingParticipantsMarket Potential0","ID","General Service","DLC Water Heating","Participants","Market Potential",0,50.259424863317136,152.56960785769235,360.20676037751235,468.60239450699208,526.83094568232082,533.06681519963627,539.37781985627009,545.76485433700429,552.22882406374367,558.77064532370673,565.39124539915269,572.09156269866321,578.87254688999485,585.73515903452517,592.68037172330799,599.70916921475873,606.82254757398914,614.021514813811,621.30709103742845,628.68030858283942,636.14221216896692,643.69385904353987,651.33631913274655,659.07067519267753,666.8980229625854,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingNew ParticipantsMarket Potential0","ID","General Service","DLC Water Heating","New Participants","Market Potential",0,50.259424863317136,102.31018299437521,207.63715251982001,108.39563412947973,58.228551175328732,6.2358695173154501,6.3110046566338269,6.3870344807342008,6.4639697267393785,6.5418212599630579,6.6206000754459637,6.700317299510516,6.7809841913316404,6.862612144530317,6.9452126887828172,7.0287974914507458,7.1133783592304098,7.1989672398218545,7.2855762236174542,7.3732175454109665,7.4619035861275052,7.5516468745729526,7.6424600892066792,7.734356059930974,7.827347769907874,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Water Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,6.3326875327779586E-2,0.19223770590069236,0.45386051807566558,0.59043901707881008,0.66380699155972422,0.67166418715154164,0.67961605301890027,0.68766371646462543,0.69580831832031709,0.70405101310787055,0.71239296920293238,0.72083536900031564,0.72937940908139354,0.7380263003835017,0.74677726837136815,0.755633553210596,0.76459640994322642,0.77366710866540189,0.78284693470715994,0.79213718881437767,0.80153918733289831,0.81105426239486034,0.82068376210726068,0.83042905074277373,0.84029150893285764,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Water Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,6.7483882489108679E-2,0.20485689034600635,0.48365357851200508,0.62919758853240626,0.70738170456066096,0.71575467514017654,0.72422853049754932,0.73280447193587539,0.74148371517510347,0.75026749052415875,0.75915704305512832,0.76815363277953497,0.77725853482671947,0.78647303962436244,0.79579845308116814,0.80523609677173491,0.81478730812364275,0.8244534406067795,0.83423586392493598,0.84413596420969483,0.85415514421664351,0.86429482352393472,0.87455643873322753,0.88494144367303251,0.89545130960449448,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Water Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,6.3326875327779586E-2,0.19223770590069236,0.45386051807566558,0.59043901707881008,0.66380699155972422,0.67166418715154164,0.67961605301890027,0.68766371646462543,0.69580831832031709,0.70405101310787055,0.71239296920293238,0.72083536900031564,0.72937940908139354,0.7380263003835017,0.74677726837136815,0.755633553210596,0.76459640994322642,0.77366710866540189,0.78284693470715994,0.79213718881437767,0.80153918733289831,0.81105426239486034,0.82068376210726068,0.83042905074277373,0.84029150893285764,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Water Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,6.7483882489108679E-2,0.20485689034600635,0.48365357851200508,0.62919758853240626,0.70738170456066096,0.71575467514017654,0.72422853049754932,0.73280447193587539,0.74148371517510347,0.75026749052415875,0.75915704305512832,0.76815363277953497,0.77725853482671947,0.78647303962436244,0.79579845308116814,0.80523609677173491,0.81478730812364275,0.8244534406067795,0.83423586392493598,0.84413596420969483,0.85415514421664351,0.86429482352393472,0.87455643873322753,0.88494144367303251,0.89545130960449448,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Water HeatingIncentive CostsMarket Potential0","ID","General Service","DLC Water Heating","Incentive Costs","Market Potential",0,1206.23,3661.67,8644.9599999999991,11246.46,12643.94,12793.6,12945.07,13098.36,13253.49,13410.5,13569.39,13730.2,13892.94,14057.64,14224.33,14393.02,14563.74,14736.52,14911.37,15088.33,15267.41,15448.65,15632.07,15817.7,16005.55,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingNon-Incentive CostsMarket Potential0","ID","General Service","DLC Water Heating","Non-Incentive Costs","Market Potential",0,38517.32,70146.77,134165.07999999999,81218.42,54536.89,25572.21,25767.33,25964.79,26164.63,26366.86,26571.53,26778.65,26988.27,27200.400000000001,27415.07,27632.33,27852.19,28074.7,28299.88,28527.759999999998,28758.37,28991.75,29227.94,29466.959999999999,29708.85,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Water HeatingProgram Annual BenefitsMarket Potential0","ID","General Service","DLC Water Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Water HeatingProgram Annual CostsMarket Potential0","ID","General Service","DLC Water Heating","Program Annual Costs","Market Potential",0,39723.550000000003,73808.44,142810.04,92464.88,67180.84,38365.82,38712.400000000001,39063.15,39418.120000000003,39777.360000000001,40140.92,40508.85,40881.21,41258.04,41639.4,42025.35,42415.94,42811.22,43211.25,43616.08,44025.78,44440.41,44860.01,45284.66,45714.400000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B502&C502&D502&E502&F502&G502","v":"IDResidentialCTA-2045 WHParticipantsMarket Potential0"},"ID","Residential","CTA-2045 WH","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialCTA-2045 WHNew ParticipantsMarket Potential0","ID","Residential","CTA-2045 WH","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialCTA-2045 WHSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","CTA-2045 WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialCTA-2045 WHSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","CTA-2045 WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialCTA-2045 WHWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","CTA-2045 WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialCTA-2045 WHWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","CTA-2045 WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialCTA-2045 WHIncentive CostsMarket Potential0","ID","Residential","CTA-2045 WH","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialCTA-2045 WHNon-Incentive CostsMarket Potential0","ID","Residential","CTA-2045 WH","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialCTA-2045 WHProgram Annual BenefitsMarket Potential0","ID","Residential","CTA-2045 WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialCTA-2045 WHProgram Annual CostsMarket Potential0","ID","Residential","CTA-2045 WH","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHParticipantsMarket Potential0","ID","General Service","CTA-2045 WH","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHNew ParticipantsMarket Potential0","ID","General Service","CTA-2045 WH","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","CTA-2045 WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","CTA-2045 WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","CTA-2045 WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","CTA-2045 WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceCTA-2045 WHIncentive CostsMarket Potential0","ID","General Service","CTA-2045 WH","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHNon-Incentive CostsMarket Potential0","ID","General Service","CTA-2045 WH","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceCTA-2045 WHProgram Annual BenefitsMarket Potential0","ID","General Service","CTA-2045 WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceCTA-2045 WHProgram Annual CostsMarket Potential0","ID","General Service","CTA-2045 WH","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingParticipantsMarket Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Participants","Market Potential",0,785.40997072114271,2524.1579217239628,6308.8283794785284,8682.0609109653215,10325.473218605584,11051.967781997324,11829.578099550015,12661.900647349104,13552.784947540795,14506.351372512398,15527.010201764948,16619.482019616764,17788.81954807814,19040.431015874936,20380.105171703759,21814.03805740584,23348.861664886565,24991.674609319987,26750.074960502949,28632.195384205072,30541.595780320611,30914.736701077007,31292.436458501423,31674.750750027739,32061.735953571373,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingNew ParticipantsMarket Potential0","ID","Residential","DLC Smart Thermostats - Cooling","New Participants","Market Potential",0,785.40997072114271,1738.7479510028202,3784.6704577545656,2373.2325314867931,1643.412307640263,726.49456339173958,777.61031755269141,832.32254779908908,890.88430019169027,953.56642497160283,1020.6588292525503,1092.471817851816,1169.3375284613758,1251.6114677967962,1339.6741558288231,1433.932885702081,1534.8236074807246,1642.8129444334227,1758.4003511829615,1882.1204237021229,1909.4003961155395,373.14092075639564,377.69975742441602,382.31429152631608,386.98520354363427,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.39270498536057136,1.2620789608619813,3.1544141897392644,4.3410304554826604,5.162736609302792,5.5259838909986616,5.914789049775008,6.3309503236745526,6.7763924737703976,7.2531756862561991,7.7635051008824743,8.3097410098083824,8.8944097740390706,9.5202155079374684,10.190052585851879,10.907019028702919,11.674430832443282,12.495837304659993,13.375037480251475,14.316097692102536,15.270797890160306,15.457368350538504,15.646218229250712,15.837375375013869,16.030867976785686,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.4184835734873949,1.3449264288810543,3.3614814468662235,4.6259915339755544,5.5016374779441515,5.8887296366140891,6.3030573846707245,6.7465370030632483,7.2212196012046013,7.7293006034273217,8.2731299029011875,8.8552227299748321,9.4782712852078763,10.145157190896706,10.858964818682734,11.622995554883758,12.440783069526088,13.31610965969735,14.253023742808477,15.255858580671926,16.273228783205781,16.472046409354757,16.673293083174244,16.87699848147258,17.08319264363351,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Smart Thermostats - CoolingNon-Incentive CostsMarket Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Non-Incentive Costs","Market Potential",0,110032.18,243737.37,533018.22,552754.18000000005,581275.11,558225.80000000005,595507.6,635412.53,678125.14,723842.99,772777.53,825155.06,881217.86,941225.2,1005454.62,1074203.19,1147788.8799999999,1226552.01,1310856.8700000001,1401093.37,1486743.78,1410986.42,1427878.74,1444977.44,1462285.04,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingIncentive CostsMarket Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Incentive Costs","Market Potential",0,15708.2,50483.16,126176.57,173641.22,206509.46,221039.35999999999,236591.56,253238.01,271055.7,290127.03000000003,310540.2,332389.64,355776.39,380808.62,407602.1,436280.76,466977.23,499833.49,535001.5,572643.91,610831.92000000004,618294.73,625848.73,633495.02,641234.72,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - CoolingProgram Annual BenefitsMarket Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Smart Thermostats - CoolingProgram Annual CostsMarket Potential0","ID","Residential","DLC Smart Thermostats - Cooling","Program Annual Costs","Market Potential",0,125740.38,294220.53000000003,659194.79,726395.4,787784.57,779265.16,832099.16,888650.54,949180.84,1013970.02,1083317.73,1157544.7,1236994.25,1322033.82,1413056.73,1510483.96,1614766.11,1726385.5,1845858.37,1973737.28,2097575.7000000002,2029281.15,2053727.47,2078472.45,2103519.7599999998,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - CoolingParticipantsMarket Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Participants","Market Potential",0,109.86361714018201,352.66326801750915,880.44022411978949,1211.1790169585222,1439.8953546597725,1540.6256329816285,1648.4067116030947,1763.7323230622833,1887.1307833041228,2019.1674145485313,2160.4471379251086,2311.6172477707705,2473.3703803204453,2646.4476904131056,2831.6422507900265,3029.802689583747,3241.8370826893615,3468.7171188795219,3711.4825567762932,3971.2459941324678,4234.6195265367714,4284.8887127357893,4335.7624169255951,4387.2478467085066,4439.3522961120971,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - CoolingNew ParticipantsMarket Potential0","ID","General Service","DLC Smart Thermostats - Cooling","New Participants","Market Potential",0,109.86361714018201,242.79965087732714,527.77695610228034,330.73879283873271,228.71633770125027,100.73027832185608,107.78107862146612,115.32561145918862,123.39846024183953,132.03663124440845,141.27972337657729,151.17010984566195,161.75313254967477,173.07731009266035,185.19456037692089,198.16043879372046,212.03439310561453,226.88003619016035,242.76543789677135,259.76343735617456,263.37353240430366,50.269186199017895,50.873704189805721,51.485429782911524,52.104449403590479,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.1373295214252275,0.44082908502188645,1.1005502801497369,1.5139737711981527,1.7998691933247155,1.9257820412270357,2.0605083895038683,2.2046654038278537,2.3589134791301536,2.523959268185664,2.7005589224063855,2.8895215597134629,3.0917129754005566,3.3080596130163822,3.5395528134875329,3.7872533619796838,4.0522963533617018,4.3358963985994023,4.6393531959703669,4.9640574926655843,5.293274408170964,5.3561108909197364,5.4197030211569936,5.4840598083856333,5.5491903701401215,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - CoolingSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.14634433229457322,0.46976671464395403,1.1727944161868467,1.6133565336723708,1.9180191744722033,2.0521974011370796,2.1957676784994336,2.3493876852385482,2.5137611670184925,2.6896411638807161,2.8778334637749206,3.0792002980748752,3.2946642960363985,3.5252127163431184,3.7719019751572174,4.0358624914532006,4.3183038718688209,4.620520458865518,4.9438972676581061,5.2899163391576982,5.6407442542316328,5.707705552983521,5.775472102682218,5.844053504247265,5.9134594737213568,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - CoolingWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Smart Thermostats - CoolingNon-Incentive CostsMarket Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Non-Incentive Costs","Market Potential",0,21020.39,41673.78,86269.26,86043.91,88455.74,83288.92,88560.1,94200.26,100235.26,106692.73,113602.27,120995.54,128906.4,137371.12,146428.47,156119.97,166490.03,177586.18,189459.26,202163.7,214022.89,200251.91,202535.69,204846.93,207185.95,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - CoolingIncentive CostsMarket Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Incentive Costs","Market Potential",0,2197.27,7053.27,17608.8,24223.58,28797.91,30812.51,32968.129999999997,35274.65,37742.620000000003,40383.35,43208.94,46232.35,49467.41,52928.95,56632.85,60596.05,64836.74,69374.34,74229.649999999994,79424.92,84692.39,85697.77,86715.25,87744.960000000006,88787.05,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B540&C540&D540&E540&F540&G540","v":"IDGeneral ServiceDLC Smart Thermostats - CoolingProgram Annual BenefitsMarket Potential0"},"ID","General Service","DLC Smart Thermostats - Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Smart Thermostats - CoolingProgram Annual CostsMarket Potential0","ID","General Service","DLC Smart Thermostats - Cooling","Program Annual Costs","Market Potential",0,23217.66,48727.040000000001,103878.07,110267.49,117253.65,114101.43,121528.23,129474.91,137977.87,147076.07999999999,156811.22,167227.88,178373.81,190300.07,203061.32,216716.03,231326.77,246960.52,263688.90999999997,281588.62,298715.28000000003,285949.69,289250.94,292591.89,295973,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingParticipantsMarket Potential0","ID","Residential","DLC Smart Thermostats - Heating","Participants","Market Potential",0,243.96098825737178,741.45479438773054,1752.5121995715467,2280.7587323758494,2565.1375839923221,2596.4770662787878,2628.1994376376019,2660.3093760031493,2692.8116164623175,2725.7109519527608,2759.0122339696882,2792.7203732812877,2826.8403406528946,2861.3771675800003,2896.3359470302253,2931.7218341943494,2967.540047246524,3003.795868113767,3040.4946432548631,3077.6417844487773,3115.2427695927022,3153.3031435098546,3191.8285187671449,3230.8245765028291,3270.29706726428,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingNew ParticipantsMarket Potential0","ID","Residential","DLC Smart Thermostats - Heating","New Participants","Market Potential",0,243.96098825737178,497.49380613035873,1011.0574051838162,528.24653280430266,284.37885161647273,31.339482286465682,31.722371358814144,32.10993836554735,32.502240459168206,32.899335490443264,33.301282016927416,33.708139311599552,34.11996737160689,34.536826927105722,34.958779450224938,35.385887164124142,35.818213052174542,36.255820867243074,36.698775141096121,37.147141193914194,37.600985143924845,38.060373917152447,38.525375257290307,38.99605773568419,39.472490761450899,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.26591747720053527,0.80818572588262638,1.9102382975329861,2.486027018289676,2.7959999665516313,2.8301600022438786,2.8647373870249861,2.8997372198434328,2.9351646619439262,2.9710249376285098,3.0073233350269604,3.0440652068766041,3.0812559713116552,3.1189011126622002,3.157006182262946,3.1955767992718411,3.2346186514987112,3.2741374962440064,3.3141391611478013,3.3546295450491677,3.3956146188560457,3.4371004264257419,3.4790930854561886,3.5215987883880837,3.5646238033180655,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Smart Thermostats - Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.28337327067405721,0.86123798580842537,2.0356333093915029,2.6492189026957331,2.9795396062996922,3.015942031376682,3.0527892018595333,3.0900865514103075,3.1278395800766479,3.1660538551028452,3.2047350117508104,3.2438887541310786,3.2835208560439635,3.3236371618309892,3.3642435872367287,3.4053461202811608,3.4469508221427017,3.4890638280520103,3.5316913481967189,3.5748396686372206,3.6185151522336376,3.662724239584124,3.7074734499746254,3.7527693823402428,3.7986187162383476,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Smart Thermostats - HeatingNon-Incentive CostsMarket Potential0","ID","Residential","DLC Smart Thermostats - Heating","Non-Incentive Costs","Market Potential",0,55017.33,92119.03,167419.37,161693.57,159574.18,145770.75,147189.51,148625.60000000001,150079.24,151550.63,153040.01,154547.57999999999,156073.56,157618.20000000001,159181.70000000001,160764.31,162366.25,163987.76,165629.07999999999,167290.46,168972.13,170674.35,172397.37,174141.44,175906.81,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingIncentive CostsMarket Potential0","ID","Residential","DLC Smart Thermostats - Heating","Incentive Costs","Market Potential",0,4879.22,14829.1,35050.239999999998,45615.17,51302.75,51929.54,52563.99,53206.19,53856.23,54514.22,55180.24,55854.41,56536.81,57227.54,57926.720000000001,58634.44,59350.8,60075.92,60809.89,61552.84,62304.86,63066.06,63836.57,64616.49,65405.94,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart Thermostats - HeatingProgram Annual BenefitsMarket Potential0","ID","Residential","DLC Smart Thermostats - Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Smart Thermostats - HeatingProgram Annual CostsMarket Potential0","ID","Residential","DLC Smart Thermostats - Heating","Program Annual Costs","Market Potential",0,59896.55,106948.13,202469.62,207308.74,210876.93,197700.29,199753.5,201831.79,203935.47,206064.85,208220.25,210401.98,212610.37,214845.74,217108.42,219398.74,221717.05,224063.68,226438.98,228843.29,231276.99,233740.42,236233.94,238757.93,241312.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingParticipantsMarket Potential0","ID","General Service","DLC Smart Thermostats - Heating","Participants","Market Potential",0,7.1261883839025,21.632554893114005,51.073032343409984,66.442243409791089,74.698359076167492,75.582531170031984,76.477356532581737,77.382962019472458,78.299476008756258,79.227028419057319,80.165750727965829,81.115775990652082,82.077238858703396,83.050275599186932,84.035024113940821,85.03162395909618,86.040216364833199,87.060944255373727,88.093952269213375,89.139386779595981,90.197395915233201,91.268129581272305,92.35173948051515,93.448379134891184,94.558203907187661,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingNew ParticipantsMarket Potential0","ID","General Service","DLC Smart Thermostats - Heating","New Participants","Market Potential",0,7.1261883839025,14.506366509211505,29.44047745029598,15.369211066381105,8.2561156663764024,0.88417209386449258,0.89482536254975287,0.90560548689072107,0.9165139892837999,0.92755241030106106,0.93872230890850972,0.95002526268625331,0.96146286805131354,0.97303674048353628,0.98474851475388903,0.99659984515535882,1.0085924057370192,1.0207278905405275,1.0330080138396482,1.0454345103826057,1.0580091356372208,1.0707336660391036,1.0836098992428447,1.0966396543760339,1.1098247722964771,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,9.6203543182683763E-3,2.9203949105703911E-2,6.8948593663603494E-2,8.9697028603217974E-2,0.10084278475282613,0.10203641707954318,0.10324443131898535,0.10446699872628783,0.10570429261182096,0.10695648836572738,0.10822376348275388,0.10950629758738031,0.11080427245924959,0.11211787205890236,0.11344728255382011,0.11479269234477985,0.11615429209252483,0.11753227474475454,0.11892683556343805,0.12033817215245457,0.12176648448556483,0.12321197493471761,0.12467484829869546,0.1261553118321031,0.12765357527470336,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Smart Thermostats - Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.0251869478120606E-2,3.1121002883316186E-2,7.3474630928818729E-2,9.5585068844008927E-2,0.10746247309550951,0.10873445980343477,0.1100217725053126,0.11132459369809018,0.11264310806886292,0.11397750252102236,0.11532796620071811,0.1166946905236363,0.11807786920209888,0.1194776982724876,0.12089437612299671,0.12232810352171765,0.12377908364506056,0.12524752210651591,0.12673362698576093,0.12823760885811442,0.12975968082434444,0.1313000585408329,0.13285896025010172,0.13443660681170408,0.13603322173348611,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Smart Thermostats - HeatingNon-Incentive CostsMarket Potential0","ID","General Service","DLC Smart Thermostats - Heating","Non-Incentive Costs","Market Potential",0,7233.09,8424.8799999999992,10840.32,10461.219999999999,10291.01,9777.02,9817.19,9857.84,9898.99,9940.6299999999992,9982.77,10025.42,10068.58,10112.26,10156.469999999999,10201.209999999999,10246.48,10292.31,10338.68,10385.61,10433.11,10481.17,10529.82,10579.05,10628.87,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingIncentive CostsMarket Potential0","ID","General Service","DLC Smart Thermostats - Heating","Incentive Costs","Market Potential",0,142.52000000000001,432.65,1021.46,1328.84,1493.97,1511.65,1529.55,1547.66,1565.99,1584.54,1603.32,1622.32,1641.54,1661.01,1680.7,1700.63,1720.8,1741.22,1761.88,1782.79,1803.95,1825.36,1847.03,1868.97,1891.16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart Thermostats - HeatingProgram Annual BenefitsMarket Potential0","ID","General Service","DLC Smart Thermostats - Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Smart Thermostats - HeatingProgram Annual CostsMarket Potential0","ID","General Service","DLC Smart Thermostats - Heating","Program Annual Costs","Market Potential",0,7375.61,8857.5300000000007,11861.78,11790.07,11784.97,11288.67,11346.73,11405.5,11464.98,11525.17,11586.08,11647.73,11710.12,11773.27,11837.17,11901.84,11967.29,12033.53,12100.56,12168.4,12237.05,12306.54,12376.85,12448.02,12520.03,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesParticipantsMarket Potential0","ID","Residential","DLC Smart Appliances","Participants","Market Potential",0,597.9435986700289,1817.2911627150261,4295.373038165556,5590.0949322937486,6287.101921549809,6363.9143781342837,6441.6652883274564,6520.3661176547776,6600.0284717213672,6680.6640979234335,6762.2848871806082,6844.9028756894313,6928.5302466982721,7013.1793323039228,7098.8626152701599,7185.5927308685041,7273.3824687414808,7362.2447747886454,7452.1927530756457,7543.239667766612,7635.3989450801528,7728.6841752692517,7823.1091146253557,7918.6876875069347,8015.4339883928433,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesNew ParticipantsMarket Potential0","ID","Residential","DLC Smart Appliances","New Participants","Market Potential",0,597.9435986700289,1219.3475640449972,2478.0818754505299,1294.7218941281926,697.00698925606048,76.812456584474603,77.750910193172786,78.700829327321117,79.662354066589614,80.635626202066305,81.620789257174692,82.617988508823146,83.627371008840782,84.649085605650725,85.68328296623713,86.730115598344128,87.78973787297673,88.862306047164566,89.947978287000296,91.046914690966332,92.15927731354077,93.285230189098911,94.424939356104005,95.578572881579021,96.746300885908568,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Smart Appliances","Summer Peak Reduction @Meter  (MW)","Market Potential",0,8.3712103813804048E-2,0.25442076278010367,0.60135222534317789,0.78261329052112494,0.88019426901697329,0.89094801293879977,0.90183314036584394,0.91285125647166898,0.92400398604099143,0.93529297370928077,0.94671988420528519,0.95828640259652043,0.96999423453775824,0.9818451065225493,0.99384076613782246,1.0059829823215907,1.0182735456238075,1.0307142684704105,1.0433069854305905,1.0560535534873259,1.0689558523112215,1.0820157845376952,1.0952352760475499,1.108616276250971,1.122160758374998,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Smart Appliances","Summer Peak Reduction @Generation (MW)","Market Potential",0,8.9207271753840633E-2,0.27112186997027243,0.640827179606967,0.83398688248201713,0.93797343245628018,0.94943309136700738,0.96103275827562229,0.97277414372513749,0.98465897915706668,0.99668901716675273,1.0088660317618128,1.021191818623743,1.0336681953727176,1.0462970018356237,1.0590801003173727,1.0720193758755228,1.0851167365982604,1.0983741138857741,1.111793462735071,1.1253767620282671,1.1391260148244049,1.153043248654833,1.1671305158221972,1.1813898937030809,1.1958234850543457,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Smart Appliances","Winter Peak Reduction @Meter  (MW)","Market Potential",0,8.3712103813804048E-2,0.25442076278010367,0.60135222534317789,0.78261329052112494,0.88019426901697329,0.89094801293879977,0.90183314036584394,0.91285125647166898,0.92400398604099143,0.93529297370928077,0.94671988420528519,0.95828640259652043,0.96999423453775824,0.9818451065225493,0.99384076613782246,1.0059829823215907,1.0182735456238075,1.0307142684704105,1.0433069854305905,1.0560535534873259,1.0689558523112215,1.0820157845376952,1.0952352760475499,1.108616276250971,1.122160758374998,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Smart Appliances","Winter Peak Reduction @Generation (MW)","Market Potential",0,8.9207271753840633E-2,0.27112186997027243,0.640827179606967,0.83398688248201713,0.93797343245628018,0.94943309136700738,0.96103275827562229,0.97277414372513749,0.98465897915706668,0.99668901716675273,1.0088660317618128,1.021191818623743,1.0336681953727176,1.0462970018356237,1.0590801003173727,1.0720193758755228,1.0851167365982604,1.0983741138857741,1.111793462735071,1.1253767620282671,1.1391260148244049,1.153043248654833,1.1671305158221972,1.1813898937030809,1.1958234850543457,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Smart AppliancesNon-Incentive CostsMarket Potential0","ID","Residential","DLC Smart Appliances","Non-Incentive Costs","Market Potential",0,241094.96,458586.35,899143.36,484967.36,275767.15000000002,58699.06,59027.519999999997,59359.99,59696.52,60037.17,60381.98,60731,61084.28,61441.88,61803.85,62170.239999999998,62541.11,62916.51,63296.49,63681.120000000003,64070.45,64464.53,64863.43,65267.199999999997,65675.91,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesIncentive CostsMarket Potential0","ID","Residential","DLC Smart Appliances","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Smart AppliancesProgram Annual BenefitsMarket Potential0","ID","Residential","DLC Smart Appliances","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Smart AppliancesProgram Annual CostsMarket Potential0","ID","Residential","DLC Smart Appliances","Program Annual Costs","Market Potential",0,241094.96,458586.35,899143.36,484967.36,275767.15000000002,58699.06,59027.519999999997,59359.99,59696.52,60037.17,60381.98,60731,61084.28,61441.88,61803.85,62170.239999999998,62541.11,62916.51,63296.49,63681.120000000003,64070.45,64464.53,64863.43,65267.199999999997,65675.91,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesParticipantsMarket Potential0","ID","General Service","DLC Smart Appliances","Participants","Market Potential",0,83.640708731250015,253.90322644500009,599.44873642499988,779.83853767360449,876.74130371088609,887.11891044638514,897.62155554673404,908.25072792808078,919.00793437507355,929.89469975419399,940.91256722964602,952.06309848183218,963.34787392844373,974.76849294820363,986.32657410728689,998.02375538845308,1009.8616944229251,1021.8420687250438,1033.9665759297345,1046.2369340328169,1058.6548816341929,1071.2221781839473,1083.9406042313988,1096.8119616771266,1109.8380740280243,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesNew ParticipantsMarket Potential0","ID","General Service","DLC Smart Appliances","New Participants","Market Potential",0,83.640708731250015,170.26251771375007,345.54550997999979,180.38980124860461,96.902766037281594,10.377606735499057,10.5026451003489,10.629172381346734,10.757206446992768,10.886765379120448,11.017867475452022,11.15053125218617,11.284775446611548,11.420619019759897,11.558081159083258,11.697181281166195,11.837939034472015,11.980374302118662,12.124507204690758,12.270358103082344,12.417947601376,12.567296549754474,12.71842604745143,12.871357445727881,13.02611235089762,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Smart Appliances","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.1709699222375003E-2,3.5546451702300016E-2,8.3922823099499999E-2,0.10917739527430464,0.12274378251952406,0.12419664746249393,0.12566701777654277,0.12715510190993132,0.1286611108125103,0.13018525796558716,0.13172775941215045,0.13328883378745651,0.13486870234998213,0.13646758901274852,0.13808572037502018,0.13972332575438343,0.14138063721920952,0.14305788962150615,0.14475532063016286,0.14647317076459437,0.14821168342878702,0.14997110494575264,0.15175168459239582,0.15355367463479774,0.15537733036392343,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Smart Appliances","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.2478366605258953E-2,3.7879850492647076E-2,8.943182342231458E-2,0.11634419786264348,0.13080113226718248,0.13234936856616999,0.13391625935266704,0.13550202675823883,0.13710689558025393,0.13873109331371181,0.14037485018345103,0.14203839917674393,0.14372197607628104,0.14542581949355129,0.14715017090262167,0.14889527467432165,0.15066137811083707,0.15244873148071839,0.15425758805430825,0.15608820413959332,0.15794083911848575,0.1598157554835386,0.16171321887510212,0.16363349811892342,0.16557686526419801,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","DLC Smart Appliances","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.1709699222375003E-2,3.5546451702300016E-2,8.3922823099499999E-2,0.10917739527430464,0.12274378251952406,0.12419664746249393,0.12566701777654277,0.12715510190993132,0.1286611108125103,0.13018525796558716,0.13172775941215045,0.13328883378745651,0.13486870234998213,0.13646758901274852,0.13808572037502018,0.13972332575438343,0.14138063721920952,0.14305788962150615,0.14475532063016286,0.14647317076459437,0.14821168342878702,0.14997110494575264,0.15175168459239582,0.15355367463479774,0.15537733036392343,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","DLC Smart Appliances","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.2478366605258953E-2,3.7879850492647076E-2,8.943182342231458E-2,0.11634419786264348,0.13080113226718248,0.13234936856616999,0.13391625935266704,0.13550202675823883,0.13710689558025393,0.13873109331371181,0.14037485018345103,0.14203839917674393,0.14372197607628104,0.14542581949355129,0.14715017090262167,0.14889527467432165,0.15066137811083707,0.15244873148071839,0.15425758805430825,0.15608820413959332,0.15794083911848575,0.1598157554835386,0.16171321887510212,0.16363349811892342,0.16557686526419801,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Smart AppliancesNon-Incentive CostsMarket Potential0","ID","General Service","DLC Smart Appliances","Non-Incentive Costs","Market Potential",0,33842.86,64160.49,125509.54,67705.039999999994,38484.58,8200.7800000000007,8244.5400000000009,8288.82,8333.64,8378.98,8424.8700000000008,8471.2999999999993,8518.2800000000007,8565.83,8613.94,8662.6299999999992,8711.89,8761.74,8812.19,8863.24,8914.89,8967.17,9020.06,9073.59,9127.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesIncentive CostsMarket Potential0","ID","General Service","DLC Smart Appliances","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceDLC Smart AppliancesProgram Annual BenefitsMarket Potential0","ID","General Service","DLC Smart Appliances","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceDLC Smart AppliancesProgram Annual CostsMarket Potential0","ID","General Service","DLC Smart Appliances","Program Annual Costs","Market Potential",0,33842.86,64160.49,125509.54,67705.039999999994,38484.58,8200.7800000000007,8244.5400000000009,8288.82,8333.64,8378.98,8424.8700000000008,8471.2999999999993,8518.2800000000007,8565.83,8613.94,8662.6299999999992,8711.89,8761.74,8812.19,8863.24,8914.89,8967.17,9020.06,9073.59,9127.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsParticipantsMarket Potential0","ID","General Service","Third Party Contracts","Participants","Market Potential",0,204.91973639156251,829.41720638699996,2161.6484737749997,2573.204602424687,2603.655992838389,2634.474340113507,2665.6640134418162,2697.2294344530878,2729.1750778411269,2761.5054719973027,2794.2251996516757,2827.3388985218044,2860.8512619693174,2894.7670396643621,2929.0910382580032,2963.8281220626786,2998.9832137408075,3034.5612950016448,3070.5674073064843,3107.0066525823049,3143.8841939439658,3181.2052564250562,3218.9751277174864,3257.1991589199515,3295.8827652953451,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsNew ParticipantsMarket Potential0","ID","General Service","Third Party Contracts","New Participants","Market Potential",0,204.91973639156251,624.49746999543743,1332.2312673879997,411.55612864968725,30.451390413702029,30.818347275117958,31.189673328309254,31.56542101127161,31.945643388039116,32.330394156175771,32.719727654372946,33.113698870128701,33.512363447513053,33.915777695044653,34.323998593641136,34.737083804675422,35.155091678128883,35.57808126083728,36.006112304839462,36.439245275820667,36.87754136166086,37.321062481090394,37.769871292430253,38.224031202465085,38.683606375393538,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Third Party Contracts","Summer Peak Reduction @Meter  (MW)","Market Potential",0,7.769207745394259E-2,0.31450629987776008,0.81968618358880885,0.97575884798432222,0.98731749140454961,0.99901424975298014,1.0108507754873255,1.0228287408396208,1.0349498380528621,1.0472157796204775,1.0596282985286609,1.07218914850161,1.0849001042496951,1.0977629617206011,1.1107795383534727,1.1239516733360997,1.1372812278651854,1.1507700854097231,1.1644201519775292,1.1782333563849627,1.1922116505298757,1.2063570096678271,1.2206714326916033,1.2351569424140842,1.2498155858544935,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Third Party Contracts","Summer Peak Reduction @Generation (MW)","Market Potential",0,8.2792068898063287E-2,0.3351516409609549,0.87349337552089601,1.0398112190796271,1.0521286140287187,1.0645931902738492,1.0772067087460844,1.0899709514488714,1.1028877217102111,1.115958844437849,1.1291861663775158,1.1425715563742647,1.15611690563693,1.1698241280057555,1.1836951602232231,1.1977319622081199,1.2119365173328915,1.2263108327043086,1.2408569394474949,1.2555768929933533,1.2704727733694328,1.2855466854942743,1.3008007594752806,1.3162371509101494,1.3318580411919154,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Third Party Contracts","Winter Peak Reduction @Meter  (MW)","Market Potential",0,7.852309430102887E-2,0.31787034988489404,0.82845378319753316,0.98619584578308994,0.99787812378391383,1.0096999940300095,1.0216631266542537,1.0337692117753565,1.0460199597370328,1.0584171013500339,1.0709623881370731,1.0836575925806882,1.0965045083740619,1.109504950674854,1.1226607563620614,1.1359737842959572,1.1494459155811398,1.1630790538327305,1.1768751254457539,1.1908360798677449,1.2049638898746176,1.2192605518498327,1.2337280860669109,1.2483685369753212,1.2631839734897943,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Third Party Contracts","Winter Peak Reduction @Generation (MW)","Market Potential",0,8.3677636723176546E-2,0.33873651948518119,0.88283651235883753,1.0509333394960463,1.0633824848507181,1.0759803857949803,1.0887288220953257,1.1016295948160235,1.1146845265739906,1.1278954617967112,1.1412642669832407,1.1547928309683377,1.1684830651897504,1.1823369039587106,1.1963563047336545,1.2105432483972263,1.2248997395365939,1.2394278067271212,1.2541295028194308,1.2690069052299071,1.2840621162346735,1.2992972632670852,1.3147144992187882,1.3303160027443748,1.3461039785696869,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceThird Party ContractsNon-Incentive CostsMarket Potential0","ID","General Service","Third Party Contracts","Non-Incentive Costs","Market Potential",0,6281.85,25429.63,66276.3,78895.67,79830.25,80776,81733.05,82701.539999999994,83681.600000000006,84673.37,85676.99,86692.61,87720.36,88760.4,89812.86,90877.9,91955.67,93046.32,94150.01,95266.89,96397.11,97540.84,98698.25,99869.48,101054.72,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsIncentive CostsMarket Potential0","ID","General Service","Third Party Contracts","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThird Party ContractsProgram Annual BenefitsMarket Potential0","ID","General Service","Third Party Contracts","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceThird Party ContractsProgram Annual CostsMarket Potential0","ID","General Service","Third Party Contracts","Program Annual Costs","Market Potential",0,6281.85,25429.63,66276.3,78895.67,79830.25,80776,81733.05,82701.539999999994,83681.600000000006,84673.37,85676.99,86692.61,87720.36,88760.4,89812.86,90877.9,91955.67,93046.32,94150.01,95266.89,96397.11,97540.84,98698.25,99869.48,101054.72,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsParticipantsMarket Potential0","ID","Large General Service","Third Party Contracts","Participants","Market Potential",0,18.269401102137607,72.952603903939504,187.57640720164054,220.30022929285562,219.93440844695951,219.58027851356323,219.23746670306673,218.90561211306215,218.58436534928538,218.27338815865414,217.97235307400786,217.68094307017523,217.39885123100942,217.12578042704004,216.86144300340416,216.60556047772812,216.35786324764331,216.11809030762811,215.8859889748791,215.66131462392337,215.44383042969361,215.23330711879498,215.02952272870465,214.83226237464831,214.64131802391157,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsNew ParticipantsMarket Potential0","ID","Large General Service","Third Party Contracts","New Participants","Market Potential",0,18.269401102137607,54.683202801801897,114.62380329770103,32.723822091215084,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Third Party Contracts","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.33950094331310943,1.3531967651476922,3.4733009999114013,4.0723304913981035,4.058863856758304,4.0458225635654035,4.0331930551346931,4.0209622068706787,4.0091173124951966,3.997646070714469,3.9865365723111381,3.97577728764769,3.9653570545682015,3.955265066685671,3.9454908620426772,3.9360243121334553,3.9268556112758586,3.9179752663220806,3.9093740866973099,3.9010431747558911,3.8929739164448596,3.8851579722650578,3.8775872685203305,3.8702539888456537,3.8631505660052761,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Third Party Contracts","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.36178702399095208,1.4420255383074299,3.7013011508007261,4.3396531238257712,4.3253024901516453,4.3114051188889633,4.2979465634427676,4.284912837671226,4.2722904012097151,4.2600661452626483,4.2482273788481866,4.2367618154813407,4.2256575602815447,4.2149030974911241,4.2044872783915999,4.1943993096051315,4.1846287417688179,4.1751654585699924,4.1659996661309782,4.1571218827321941,4.1485229288628087,4.1401939175885101,4.132126245226269,4.1243115823163405,4.116741864882008,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Third Party Contracts","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.34313234322852726,1.3676709476655562,3.5104524282232417,4.1158893117586635,4.1022786341144046,4.0890978474917201,4.0763332501996956,4.0639715772583829,4.0519999864796059,4.0404060449914017,4.0291777161919944,4.0183033471195442,4.0077716562244925,3.9975717215316062,3.9876929691793572,3.9781251623245599,3.9688583904006682,3.9598830587184315,3.9511898783980013,3.9427698566219402,3.9346142871988929,3.9267147414280115,3.9190630592545648,3.9116513407074351,3.9044719376095363,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Third Party Contracts","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.36565680224693869,1.4574498589786404,3.7408913344237442,4.3860713040906472,4.3715671719036706,4.3575211503534952,4.3439186383202211,4.330745500062215,4.317988050383212,4.3056330402721672,4.2936676430008465,4.282079440664476,4.2708564111514198,4.25998691552814,4.2494596858262543,4.23926381321884,4.2293887365736023,4.2198242313708771,4.2105603989748523,4.2015876562467396,4.1928967254890166,4.1844786247101569,4.1763246581996638,4.1684264074034898,4.1607757220902988,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceThird Party ContractsNon-Incentive CostsMarket Potential0","ID","Large General Service","Third Party Contracts","Non-Incentive Costs","Market Potential",0,27450.59,109413.68,280836.19,329271.14,328182.28999999998,327127.83,326106.65999999997,325117.73,324160,323232.48,322334.21999999997,321464.27,320621.73,319805.74,319015.44,318250.01,317508.67,316790.64,316095.19,315421.59000000003,314769.14,314137.18,313525.03999999998,312932.11,312357.76000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsIncentive CostsMarket Potential0","ID","Large General Service","Third Party Contracts","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThird Party ContractsProgram Annual BenefitsMarket Potential0","ID","Large General Service","Third Party Contracts","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceThird Party ContractsProgram Annual CostsMarket Potential0","ID","Large General Service","Third Party Contracts","Program Annual Costs","Market Potential",0,27450.59,109413.68,280836.19,329271.14,328182.28999999998,327127.83,326106.65999999997,325117.73,324160,323232.48,322334.21999999997,321464.27,320621.73,319805.74,319015.44,318250.01,317508.67,316790.64,316095.19,315421.59000000003,314769.14,314137.18,313525.03999999998,312932.11,312357.76000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThird Party ContractsParticipantsMarket Potential0","ID","Extra Large General Service","Third Party Contracts","Participants","Market Potential",0,0.56900249999999997,1.1380049999999999,1.9346084999999997,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,2.2760099999999999,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThird Party ContractsNew ParticipantsMarket Potential0","ID","Extra Large General Service","Third Party Contracts","New Participants","Market Potential",0,0.56900249999999997,0.56900249999999997,0.7966034999999998,0.34140150000000014,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B604&C604&D604&E604&F604&G604","v":"IDExtra Large General ServiceThird Party ContractsSummer Peak Reduction @Meter  (MW)Market Potential0"},"ID","Extra Large General Service","Third Party Contracts","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.51800028741200932,1.0311291245278289,1.7439079004906772,2.0413816814835712,2.0314239882459852,2.0217733498544455,2.0124201530689763,2.0033550856327329,1.9945691268484533,1.986053538449946,1.9777998557593961,1.9697998791215179,1.9620456656059071,1.9545295209691773,1.9472439918687672,1.9401818583205117,1.9333361263923781,1.9267000211269398,1.9202669796854555,1.9140306447065916,1.9079848578730847,1.9021236536798252,1.8964412533970521,1.8909320592225669,1.8855906486170235,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThird Party ContractsSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Third Party Contracts","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.55200371633845835,1.0988162026085133,1.8583843781869962,2.1753854235758432,2.1647740710208709,2.15448992951241,2.144522754762336,2.1348626232232872,2.1254999220465187,2.1164253393541625,2.1076298548160657,2.0991047305216517,2.0908415021375824,2.0828319703422604,2.0750681925285241,2.0675424747661038,2.0602473640157482,2.0531756405871056,2.046320310832753,2.0396746000709629,2.0332319457300563,2.0269859907074013,2.0209305769363302,2.0150597391544829,2.009367698867246,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThird Party ContractsWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Third Party Contracts","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.5354813757820357,1.0659269031870555,1.8027600070599097,2.1102727119292433,2.0999789738675942,2.090002652910524,2.0803338113975851,2.0709628228088182,2.0618803620231771,2.0530773958819646,2.0445451740477147,2.0362752201492769,2.0282593232041375,2.0204895293093106,2.0129581335923725,2.0056576724145034,1.9985809158176551,1.9917208602081786,1.9850707212695313,1.9786239270968797,1.97237411154665,1.9663151077943031,1.9604409420938056,1.9547458277324934,1.9492241591751982,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThird Party ContractsWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Third Party Contracts","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.57063232713345657,1.1358982344278086,1.9210997517688722,2.248798712627071,2.2378292560396358,2.2271980529737041,2.2168945134245366,2.2069083789522783,2.1972297123009135,2.187848887342247,2.1787565793347343,2.169943755487294,2.1614016658185609,2.1531218343023344,2.1450960502902521,2.137316360203009,2.1297750594817297,2.122464684791324,2.1153780064679575,2.1085080212029834,2.1018479449559355,2.0953912060894107,2.0891314387188893,2.083062476270773,2.0771783452421122,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceThird Party ContractsNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Third Party Contracts","Non-Incentive Costs","Market Potential",0,42838.51,85274.15,144220.79999999999,168821.82,167998.32,167200.21,166426.70000000001,165677.03,164950.43,164246.19,163563.60999999999,162902.01999999999,162260.75,161639.16,161036.65,160452.60999999999,159886.47,159337.67000000001,158805.66,158289.91,157789.93,157305.21,156835.28,156379.67000000001,155937.93,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThird Party ContractsIncentive CostsMarket Potential0","ID","Extra Large General Service","Third Party Contracts","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThird Party ContractsProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Third Party Contracts","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceThird Party ContractsProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Third Party Contracts","Program Annual Costs","Market Potential",0,42838.51,85274.15,144220.79999999999,168821.82,167998.32,167200.21,166426.70000000001,165677.03,164950.43,164246.19,163563.60999999999,162902.01999999999,162260.75,161639.16,161036.65,160452.60999999999,159886.47,159337.67000000001,158805.66,158289.91,157789.93,157305.21,156835.28,156379.67000000001,155937.93,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingParticipantsMarket Potential0","ID","Residential","DLC Electric Vehicle Charging","Participants","Market Potential",0,0,0,56.147534921456717,199.76696382635797,552.80527007123476,842.92389335515327,1110.7532058030197,1317.31396456414,1562.2877090695806,1852.8178942652046,2197.3764047301052,2606.010595541818,3090.6362739934693,3665.3851655343205,4347.0169960696712,5155.4082069746028,6114.1315537923183,7251.1434897638228,8599.5993783502836,10198.820306413674,12095.439690409152,14344.763110721977,17012.38102703229,20176.081401623207,20422.581998566762,20672.094208275154,20924.654825026195,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingNew ParticipantsMarket Potential0","ID","Residential","DLC Electric Vehicle Charging","New Participants","Market Potential",0,0,0,56.147534921456717,143.61942890490124,353.03830624487682,290.11862328391851,267.82931244786641,206.56075876112027,244.97374450544066,290.53018519562397,344.55851046490056,408.63419081171287,484.62567845165131,574.74889154085122,681.63183053535067,808.39121090493154,958.72334681771554,1137.0119359715045,1348.4558885864608,1599.2209280633906,1896.6193839954776,2249.323420312825,2667.6179163103134,3163.7003745909169,246.50059694355514,249.51220970839131,252.56061675104138,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Electric Vehicle Charging","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,2.8073767460728358E-2,9.9883481913178987E-2,0.27640263503561741,0.42146194667757664,0.55537660290150981,0.65865698228206992,0.78114385453479029,0.92640894713260225,1.0986882023650526,1.303005297770909,1.5453181369967346,1.8326925827671603,2.1735084980348356,2.5777041034873012,3.0570657768961591,3.6255717448819116,4.299799689175142,5.0994101532068372,6.0477198452045755,7.172381555360988,8.5061905135161453,10.088040700811604,10.211290999283381,10.336047104137577,10.462327412513098,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Electric Vehicle Charging","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,2.9916631991398504E-2,0.1064401981171984,0.29454671252729903,0.44912824667260937,0.59183354955403855,0.70189362988285375,0.83242098735591463,0.98722181066986603,1.1708101048220936,1.3885393198752227,1.6467584580101604,1.9529972109624469,2.3161855264650848,2.7469140062737649,3.257742729002727,3.8635675030710908,4.582054229726281,5.4341540422067744,6.4447142425453698,7.6432028509814449,9.0645678959038207,10.750256501291137,10.881597399065837,11.014542949848229,11.149112758432542,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","DLC Electric Vehicle Charging","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,2.8073767460728358E-2,9.9883481913178987E-2,0.27640263503561741,0.42146194667757664,0.55537660290150981,0.65865698228206992,0.78114385453479029,0.92640894713260225,1.0986882023650526,1.303005297770909,1.5453181369967346,1.8326925827671603,2.1735084980348356,2.5777041034873012,3.0570657768961591,3.6255717448819116,4.299799689175142,5.0994101532068372,6.0477198452045755,7.172381555360988,8.5061905135161453,10.088040700811604,10.211290999283381,10.336047104137577,10.462327412513098,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","DLC Electric Vehicle Charging","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,2.9916631991398504E-2,0.1064401981171984,0.29454671252729903,0.44912824667260937,0.59183354955403855,0.70189362988285375,0.83242098735591463,0.98722181066986603,1.1708101048220936,1.3885393198752227,1.6467584580101604,1.9529972109624469,2.3161855264650848,2.7469140062737649,3.257742729002727,3.8635675030710908,4.582054229726281,5.4341540422067744,6.4447142425453698,7.6432028509814449,9.0645678959038207,10.750256501291137,10.881597399065837,11.014542949848229,11.149112758432542,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Electric Vehicle ChargingNon-Incentive CostsMarket Potential0","ID","Residential","DLC Electric Vehicle Charging","Non-Incentive Costs","Market Potential",0,0,0,77464.490000000005,143786.51,302615.86,256876.69,241498.86,196580.24,226614.85,262234.83,304478.87,354578.8,413995.55,484461.7,568032.06000000006,667143.55000000005,784686.27,924087.77,1089413.02,1285482.8999999999,1518014.84,1793789.49,2120848.4500000002,2508728.79,322061.46000000002,325567.73,329116.84000000003,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingIncentive CostsMarket Potential0","ID","Residential","DLC Electric Vehicle Charging","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialDLC Electric Vehicle ChargingProgram Annual BenefitsMarket Potential0","ID","Residential","DLC Electric Vehicle Charging","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialDLC Electric Vehicle ChargingProgram Annual CostsMarket Potential0","ID","Residential","DLC Electric Vehicle Charging","Program Annual Costs","Market Potential",0,0,0,77464.490000000005,143786.51,302615.86,256876.69,241498.86,196580.24,226614.85,262234.83,304478.87,354578.8,413995.55,484461.7,568032.06000000006,667143.55000000005,784686.27,924087.77,1089413.02,1285482.8999999999,1518014.84,1793789.49,2120848.4500000002,2508728.79,322061.46000000002,325567.73,329116.84000000003,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageParticipantsMarket Potential0","ID","General Service","Thermal Energy Storage","Participants","Market Potential",0,2.7239084578356274,16.071974170143967,54.021330130318482,67.693197361251762,74.295052180880646,74.587719269164808,74.845117621848772,75.064382966566384,75.242482467415613,75.37620812856126,75.462170433099814,75.49679232553585,75.476303665896623,75.396736306156129,75.253919965669851,75.043479112211273,74.760831089487397,74.401185771305961,73.959547067563847,73.430716658712512,72.903232417846297,73.768666996314863,74.644508959746062,75.530882394260047,76.427912873874462,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageNew ParticipantsMarket Potential0","ID","General Service","Thermal Energy Storage","New Participants","Market Potential",0,2.7239084578356274,13.34806571230834,37.949355960174515,13.67186723093328,6.6018548196288833,0.29266708828416199,0.25739835268396405,0.21926534471761272,0.17809950084922832,0.13372566114564677,8.596230453855469E-2,3.4621892436035751E-2,0,0,0,0,0,0,0,0,0,0.86543457846856597,0.87584196343119913,0.88637343451398465,0.89703047961441484,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Thermal Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.5761662091638542E-3,2.7000916605841866E-2,9.0755834618935036E-2,0.11372457156690295,0.12481568766387949,0.12530736837219689,0.12573979760470594,0.12610816338383152,0.12640737054525822,0.12663202965598291,0.12677644632760768,0.12683461110690022,0.12680019015870633,0.12666651699434228,0.12642658554232533,0.12607304490851493,0.12559819623033883,0.12499399209579401,0.12425203907350726,0.12336360398663701,0.12247743046198177,0.12393136055380898,0.12540277505237338,0.12689188242235688,0.12839889362810908,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Thermal Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.8765624564832202E-3,2.8773355291817845E-2,9.6713378749930773E-2,0.12118986739866043,0.133009044825106,0.13353300124914416,0.13399381671430727,0.13438636336725437,0.13470521157849341,0.13494461813297412,0.13509851484186666,0.13516049776950151,0.13512381730467427,0.13498136934605956,0.13472568791807898,0.134348939587079,0.13384292010905671,0.13319905381052216,0.13240839628464116,0.13146164107697891,0.13051729588872737,0.1320666672568297,0.1336346707719239,0.13522152858307426,0.13682746550310004,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Thermal Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Thermal Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceThermal Energy StorageNon-Incentive CostsMarket Potential0","ID","General Service","Thermal Energy Storage","Non-Incentive Costs","Market Potential",0,29380.99,61550.27,136632.82,66832.73,46725.88,28312.49,28231.040000000001,28138.02,28032.68,27914.23,27781.87,27634.74,27531.84,27525.16,27513.16,27495.49,27471.74,27441.53,27404.44,27360.01,27315.7,29917.55,30021.53,30126.77,30233.26,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageIncentive CostsMarket Potential0","ID","General Service","Thermal Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceThermal Energy StorageProgram Annual BenefitsMarket Potential0","ID","General Service","Thermal Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceThermal Energy StorageProgram Annual CostsMarket Potential0","ID","General Service","Thermal Energy Storage","Program Annual Costs","Market Potential",0,29380.99,61550.27,136632.82,66832.73,46725.88,28312.49,28231.040000000001,28138.02,28032.68,27914.23,27781.87,27634.74,27531.84,27525.16,27513.16,27495.49,27471.74,27441.53,27404.44,27360.01,27315.7,29917.55,30021.53,30126.77,30233.26,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageParticipantsMarket Potential0","ID","Large General Service","Thermal Energy Storage","Participants","Market Potential",0,0.49600183987703911,2.9709205209749117,10.484707349572666,13.457253825581679,14.927674781467839,14.903638813137773,14.880371043194573,14.857846975999694,14.836042897010319,14.814935847872453,14.794503602308223,14.774724642772075,14.755578137851318,14.737043920387332,14.719102466294398,14.701734874053944,14.684922844862667,14.668648663413672,14.652895179290436,14.637645788954075,14.622884418304993,14.608595505800565,14.594763986111174,14.581375274297395,14.568415250491734,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageNew ParticipantsMarket Potential0","ID","Large General Service","Thermal Energy Storage","New Participants","Market Potential",0,0.49600183987703911,2.4749186810978725,7.5137868285977545,2.972546476009013,1.4704209558861603,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Thermal Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.1664154549671288E-3,2.4955732376189262E-2,8.8071541736410394E-2,0.1130409321348861,0.12539246816432986,0.1251905660303573,0.12499511676283442,0.12480591459839743,0.12462276033488669,0.12444546112212862,0.12427383025938908,0.12410768699928544,0.12394685635795108,0.1237911689312536,0.12364046071687296,0.12349457294205314,0.1233533518968464,0.12321664877267484,0.12308431950603967,0.12295622462721423,0.12283222911376196,0.12271220224872476,0.12259601748333386,0.12248355230409813,0.12237468810413057,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Thermal Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.4399141676972811E-3,2.6593917706936553E-2,9.3852879088246369E-2,0.12046135137988714,0.1336236873021418,0.13340853157540206,0.13320025230481078,0.13299863021994612,0.13280345304229185,0.1326145152622854,0.13243161792347516,0.13225456841356079,0.1320831802620962,0.13191727294464364,0.13175667169317237,0.13160120731250335,0.13145071600260699,0.13130503918656738,0.13116402334403204,0.13102751984997255,0.13089538481858692,0.13076747895217897,0.13064366739485705,0.1305238195908974,0.13040780914762423,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Thermal Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Thermal Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceThermal Energy StorageNon-Incentive CostsMarket Potential0","ID","Large General Service","Thermal Energy Storage","Non-Incentive Costs","Market Potential",0,52365.52,193235.25,552437.46,232801.89,127279.27,23369.23,23359.46,23350,23340.84,23331.98,23323.4,23315.09,23307.05,23299.26,23291.73,23284.43,23277.37,23270.54,23263.919999999998,23257.52,23251.32,23245.32,23239.51,23233.88,23228.44,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageIncentive CostsMarket Potential0","ID","Large General Service","Thermal Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceThermal Energy StorageProgram Annual BenefitsMarket Potential0","ID","Large General Service","Thermal Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceThermal Energy StorageProgram Annual CostsMarket Potential0","ID","Large General Service","Thermal Energy Storage","Program Annual Costs","Market Potential",0,52365.52,193235.25,552437.46,232801.89,127279.27,23369.23,23359.46,23350,23340.84,23331.98,23323.4,23315.09,23307.05,23299.26,23291.73,23284.43,23277.37,23270.54,23263.919999999998,23257.52,23251.32,23245.32,23239.51,23233.88,23228.44,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageParticipantsMarket Potential0","ID","Extra Large General Service","Thermal Energy Storage","Participants","Market Potential",0,1.6335000000000002E-2,4.9005E-2,0.11434499999999999,0.14701500000000001,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0.16334999999999997,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageNew ParticipantsMarket Potential0","ID","Extra Large General Service","Thermal Energy Storage","New Participants","Market Potential",0,1.6335000000000002E-2,3.2669999999999998E-2,6.5339999999999981E-2,3.2670000000000018E-2,1.6334999999999961E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Thermal Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.3721400000000003E-4,4.1164199999999999E-4,9.6049799999999995E-4,1.2349260000000001E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,1.3721399999999998E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Thermal Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.4622122762148341E-4,4.386636828644501E-4,1.0235485933503836E-3,1.3159910485933506E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,1.4622122762148334E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Thermal Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Thermal Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceThermal Energy StorageNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Thermal Energy Storage","Non-Incentive Costs","Market Potential",0,1329.96,2497.91,4833.8100000000004,2539.0700000000002,1391.7,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageIncentive CostsMarket Potential0","ID","Extra Large General Service","Thermal Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceThermal Energy StorageProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Thermal Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceThermal Energy StorageProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Thermal Energy Storage","Program Annual Costs","Market Potential",0,1329.96,2497.91,4833.8100000000004,2539.0700000000002,1391.7,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,237.47,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageParticipantsMarket Potential0","ID","Residential","Battery Energy Storage","Participants","Market Potential",0,3.9862906578001924,24.230548836200345,61.982294923023893,100.3832984474747,139.71337603444019,179.98949756339388,221.22890889205408,276.62159287020273,333.3347712990589,391.39244210056478,464.480174068971,539.2953780846218,615.86935526206855,708.40195275797191,717.05682982526866,725.81744756247519,734.68509785267486,743.66108836248941,752.74674273491371,761.94340078450625,771.25241869496494,780.67516921911636,790.21304188134911,799.86744318251863,809.63979680735792,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageNew ParticipantsMarket Potential0","ID","Residential","Battery Energy Storage","New Participants","Market Potential",0,3.9862906578001924,20.244258178400152,37.751746086823545,38.401003524450807,39.330077586965487,40.276121528953695,41.239411328660196,55.392683978148654,56.713178428856168,58.057670801505878,73.087731968406217,74.815204015650806,76.57397717744675,92.53259749590336,8.6548770672967521,8.7606177372065304,8.8676502901996628,8.9759905098145509,9.0856543724243011,9.1966580495925427,9.3090179104586923,9.4227505241514109,9.5378726622327576,9.6544013011695142,9.7723536248392975,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,7.9725813156003855E-3,4.8461097672400692E-2,0.12396458984604779,0.20076659689494941,0.2794267520688804,0.35997899512678777,0.44245781778410814,0.55324318574040543,0.66666954259811784,0.78278488420112957,0.92896034813794204,1.0785907561692436,1.2317387105241371,1.4168039055159438,1.4341136596505373,1.4516348951249505,1.4693701957053498,1.4873221767249789,1.5054934854698274,1.5238868015690126,1.5425048373899299,1.5613503384382328,1.5804260837626982,1.5997348863650374,1.6192795936147157,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,8.4959306432229164E-3,5.1642260946718553E-2,0.1321020778410569,0.21394564886503561,0.29776934363691432,0.38360932984525553,0.47150236336754919,0.58956008710614394,0.71043216389398745,0.83416974019728218,0.98994069494665604,1.1493933889271564,1.3125945338066252,1.5098080834568881,1.5282541130120815,1.5469255063138858,1.5658250167363061,1.5849554312926033,1.6043195710462781,1.6239202915270807,1.6437604831520993,1.6638430716519956,1.684171018502449,1.7047473213608668,1.7255750145084354,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,7.9725813156003855E-3,4.8461097672400692E-2,0.12396458984604779,0.20076659689494941,0.2794267520688804,0.35997899512678777,0.44245781778410814,0.55324318574040543,0.66666954259811784,0.78278488420112957,0.92896034813794204,1.0785907561692436,1.2317387105241371,1.4168039055159438,1.4341136596505373,1.4516348951249505,1.4693701957053498,1.4873221767249789,1.5054934854698274,1.5238868015690126,1.5425048373899299,1.5613503384382328,1.5804260837626982,1.5997348863650374,1.6192795936147157,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,8.4959306432229164E-3,5.1642260946718553E-2,0.1321020778410569,0.21394564886503561,0.29776934363691432,0.38360932984525553,0.47150236336754919,0.58956008710614394,0.71043216389398745,0.83416974019728218,0.98994069494665604,1.1493933889271564,1.3125945338066252,1.5098080834568881,1.5282541130120815,1.5469255063138858,1.5658250167363061,1.5849554312926033,1.6043195710462781,1.6239202915270807,1.6437604831520993,1.6638430716519956,1.684171018502449,1.7047473213608668,1.7255750145084354,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialBattery Energy StorageNon-Incentive CostsMarket Potential0","ID","Residential","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,55858.58,168233.66,289245.40999999997,293733.08,300154.84000000003,306693.90000000002,313352.15000000002,411179.57,420306.83,429599.96,533487.75,545428.03,557584.67000000004,667890.66,88127.85,88858.73,89598.54,90347.39,91105.39,91872.639999999999,92649.27,93435.39,94231.12,95036.56,95851.85,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageIncentive CostsMarket Potential0","ID","Residential","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBattery Energy StorageProgram Annual BenefitsMarket Potential0","ID","Residential","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialBattery Energy StorageProgram Annual CostsMarket Potential0","ID","Residential","Battery Energy Storage","Program Annual Costs","Market Potential",0,55858.58,168233.66,289245.40999999997,293733.08,300154.84000000003,306693.90000000002,313352.15000000002,411179.57,420306.83,429599.96,533487.75,545428.03,557584.67000000004,667890.66,88127.85,88858.73,89598.54,90347.39,91105.39,91872.639999999999,92649.27,93435.39,94231.12,95036.56,95851.85,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageParticipantsMarket Potential0","ID","General Service","Battery Energy Storage","Participants","Market Potential",0,0.55751483589589146,3.3821941017143113,8.6230432516015068,13.949680013129706,19.401415525065165,24.985809003628003,30.700170258213525,38.374213859385755,46.226435933986686,54.2600883759658,64.371766571654661,74.716594511529308,85.298826390842819,98.084480252631181,99.252677279695561,100.43526294670694,101.63242760444399,102.84436464943072,104.07127054039294,105.31334480385965,106.5703203666171,107.83541708763939,109.11572737756477,110.41143262612229,111.72271639805733,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageNew ParticipantsMarket Potential0","ID","General Service","Battery Energy Storage","New Participants","Market Potential",0,0.55751483589589146,2.8246792658184199,5.240849149887195,5.3266367615281993,5.4517355119354587,5.5843934785628377,5.7143612545855227,7.6740436011722295,7.852222074600931,8.0336524419791147,10.11167819568886,10.344827939874648,10.582231879313511,12.785653861788361,1.1681970270643802,1.1825856670113808,1.1971646577370478,1.2119370449867262,1.2269058909622288,1.242074263466705,1.2569755627574466,1.2650967210222888,1.2803102899253815,1.2957052485575247,1.3112837719350381,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.1150296717917828E-3,6.7643882034286226E-3,1.7246086503203015E-2,2.7899360026259413E-2,3.8802831050130326E-2,4.9971618007256004E-2,6.1400340516427052E-2,7.6748427718771509E-2,9.2452871867973366E-2,0.1085201767519316,0.12874353314330933,0.1494331890230586,0.17059765278168565,0.19616896050526236,0.19850535455939111,0.20087052589341389,0.20326485520888798,0.20568872929886142,0.20814254108078589,0.2106266896077193,0.21314064073323419,0.21567083417527877,0.21823145475512953,0.22082286525224459,0.22344543279611465,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.1882242879281573E-3,7.2084273267568437E-3,1.8378182548170304E-2,2.9730775816559477E-2,4.1349990462628224E-2,5.3251937347885768E-2,6.5430882903268386E-2,8.1786474551120536E-2,9.8521815716084149E-2,0.11564383711842668,0.13719472841358624,0.15924252879695078,0.18179630518082443,0.20904620684704003,0.21153597033183197,0.21405640014217167,0.21660790197025573,0.21919088799963921,0.22180577694030892,0.22445299404062158,0.22713197009082928,0.22982825466248802,0.23255696372030002,0.23531848385789064,0.23811320630447,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.1150296717917828E-3,6.7643882034286226E-3,1.7246086503203015E-2,2.7899360026259413E-2,3.8802831050130326E-2,4.9971618007256004E-2,6.1400340516427052E-2,7.6748427718771509E-2,9.2452871867973366E-2,0.1085201767519316,0.12874353314330933,0.1494331890230586,0.17059765278168565,0.19616896050526236,0.19850535455939111,0.20087052589341389,0.20326485520888798,0.20568872929886142,0.20814254108078589,0.2106266896077193,0.21314064073323419,0.21567083417527877,0.21823145475512953,0.22082286525224459,0.22344543279611465,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.1882242879281573E-3,7.2084273267568437E-3,1.8378182548170304E-2,2.9730775816559477E-2,4.1349990462628224E-2,5.3251937347885768E-2,6.5430882903268386E-2,8.1786474551120536E-2,9.8521815716084149E-2,0.11564383711842668,0.13719472841358624,0.15924252879695078,0.18179630518082443,0.20904620684704003,0.21153597033183197,0.21405640014217167,0.21660790197025573,0.21919088799963921,0.22180577694030892,0.22445299404062158,0.22713197009082928,0.22982825466248802,0.23255696372030002,0.23531848385789064,0.23811320630447,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[{"$f":"B668&C668&D668&E668&F668&G668","v":"IDGeneral ServiceBattery Energy StorageNon-Incentive CostsMarket Potential0"},"ID","General Service","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,7712.15,22544.85,38352.400000000001,38913.660000000003,39732.1,40600,41450.300000000003,54271.33,55437.04,56624.03,70219.31,71744.67,73297.86,87713.53,11707.48,11801.62,11897,11993.64,12091.58,12190.81,12288.3,12341.44,12440.97,12541.69,12643.61,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageIncentive CostsMarket Potential0","ID","General Service","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceBattery Energy StorageProgram Annual BenefitsMarket Potential0","ID","General Service","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceBattery Energy StorageProgram Annual CostsMarket Potential0","ID","General Service","Battery Energy Storage","Program Annual Costs","Market Potential",0,7712.15,22544.85,38352.400000000001,38913.660000000003,39732.1,40600,41450.300000000003,54271.33,55437.04,56624.03,70219.31,71744.67,73297.86,87713.53,11707.48,11801.62,11897,11993.64,12091.58,12190.81,12288.3,12341.44,12440.97,12541.69,12643.61,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageParticipantsMarket Potential0","ID","Large General Service","Battery Energy Storage","Participants","Market Potential",0,3.3384429237401168E-2,0.19947374568128548,0.49907257415458683,0.79475631145246717,1.0893332452565216,1.3841917634658421,1.6781801889862176,2.0699081947240954,2.4605602121194812,2.8501891411812448,3.3369924418159878,3.8226092881565621,4.3070986081494,4.8882824303601273,4.8823312439966084,4.8765704078027756,4.8709938520594136,4.8655957005932589,4.8603702646053781,4.8553120366963327,4.8504156850818738,4.8456760479930736,4.8410881282550244,4.8366470880384105,4.8323482437784291,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageNew ParticipantsMarket Potential0","ID","Large General Service","Battery Energy Storage","New Participants","Market Potential",0,3.3384429237401168E-2,0.16608931644388431,0.29959882847330133,0.29568373729788033,0.29457693380405447,0.29485851820932041,0.29398842552037552,0.3917280057378778,0.3906520173953858,0.38962892906176361,0.48680330063474297,0.48561684634057434,0.48448931999283795,0.58118382221072729,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,5.0076643856101751E-4,2.9921061852192822E-3,7.4860886123188026E-3,1.1921344671787008E-2,1.6339998678847823E-2,2.0762876451987631E-2,2.5172702834793264E-2,3.104862292086143E-2,3.690840318179222E-2,4.275283711771867E-2,5.0054886627239815E-2,5.733913932234843E-2,6.4606479122241003E-2,7.3324236455401912E-2,7.3234968659949135E-2,7.314855611704163E-2,7.3064907780891197E-2,7.2983935508898881E-2,7.2905553969080675E-2,7.2829680550444989E-2,7.2756235276228112E-2,7.268514071989611E-2,7.2616321923825361E-2,7.2549706320576168E-2,7.2485223656676437E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.3363857476664272E-4,3.1885189527059701E-3,7.97750278380094E-3,1.270390523421463E-2,1.7412615812923936E-2,2.2125827421129188E-2,2.6825130898117288E-2,3.3086767818479787E-2,3.9331205436692475E-2,4.5559289341132424E-2,5.334067202391285E-2,6.1103089644446322E-2,6.8847484145610621E-2,7.8137506879158047E-2,7.8042379219894639E-2,7.7950294242371723E-2,7.7861154924223352E-2,7.7774867336848769E-2,7.7691340546761162E-2,7.7610486520082039E-2,7.7532220030081103E-2,7.7456458567664227E-2,7.7383122254715858E-2,7.7312133760204779E-2,7.724341821896466E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,5.0076643856101751E-4,2.9921061852192822E-3,7.4860886123188026E-3,1.1921344671787008E-2,1.6339998678847823E-2,2.0762876451987631E-2,2.5172702834793264E-2,3.104862292086143E-2,3.690840318179222E-2,4.275283711771867E-2,5.0054886627239815E-2,5.733913932234843E-2,6.4606479122241003E-2,7.3324236455401912E-2,7.3234968659949135E-2,7.314855611704163E-2,7.3064907780891197E-2,7.2983935508898881E-2,7.2905553969080675E-2,7.2829680550444989E-2,7.2756235276228112E-2,7.268514071989611E-2,7.2616321923825361E-2,7.2549706320576168E-2,7.2485223656676437E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,5.3363857476664272E-4,3.1885189527059701E-3,7.97750278380094E-3,1.270390523421463E-2,1.7412615812923936E-2,2.2125827421129188E-2,2.6825130898117288E-2,3.3086767818479787E-2,3.9331205436692475E-2,4.5559289341132424E-2,5.334067202391285E-2,6.1103089644446322E-2,6.8847484145610621E-2,7.8137506879158047E-2,7.8042379219894639E-2,7.7950294242371723E-2,7.7861154924223352E-2,7.7774867336848769E-2,7.7691340546761162E-2,7.7610486520082039E-2,7.7532220030081103E-2,7.7456458567664227E-2,7.7383122254715858E-2,7.7312133760204779E-2,7.724341821896466E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceBattery Energy StorageNon-Incentive CostsMarket Potential0","ID","Large General Service","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,3278.96,9790.52,16341.57,16149.46,16095.15,16108.97,16066.27,20862.16,20809.36,20759.16,25527.31,25469.1,25413.77,30158.38,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageIncentive CostsMarket Potential0","ID","Large General Service","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceBattery Energy StorageProgram Annual BenefitsMarket Potential0","ID","Large General Service","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceBattery Energy StorageProgram Annual CostsMarket Potential0","ID","Large General Service","Battery Energy Storage","Program Annual Costs","Market Potential",0,3278.96,9790.52,16341.57,16149.46,16095.15,16108.97,16066.27,20862.16,20809.36,20759.16,25527.31,25469.1,25413.77,30158.38,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageParticipantsMarket Potential0","ID","Extra Large General Service","Battery Energy Storage","Participants","Market Potential",0,1.0983665000000001E-3,3.2852985E-3,5.4428274999999996E-3,8.682388000000001E-3,1.1920315000000001E-2,1.5171310000000004E-2,1.8422305000000003E-2,2.2756965000000004E-2,2.7091625000000001E-2,3.1426284999999998E-2,3.684461E-2,4.2262935000000001E-2,4.7681259999999996E-2,5.4183249999999995E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,5.4183250000000002E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageNew ParticipantsMarket Potential0","ID","Extra Large General Service","Battery Energy Storage","New Participants","Market Potential",0,1.0983665000000001E-3,2.1869319999999999E-3,2.1575289999999996E-3,3.2395605000000013E-3,3.2379269999999998E-3,3.250995000000003E-3,3.2509949999999996E-3,4.3346600000000006E-3,4.3346599999999971E-3,4.3346599999999971E-3,5.4183250000000016E-3,5.4183250000000016E-3,5.4183249999999947E-3,6.5019899999999992E-3,6.9388939039072284E-18,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Battery Energy Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.6475497500000002E-5,4.9279477500000003E-5,8.1642412499999994E-5,1.3023582000000001E-4,1.7880472499999999E-4,2.2756965000000006E-4,2.7633457500000002E-4,3.4135447500000004E-4,4.06374375E-4,4.7139427499999997E-4,5.5266915000000004E-4,6.3394402500000001E-4,7.1521889999999998E-4,8.1274874999999989E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Battery Energy Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.7557009271099745E-5,5.2514362212276217E-5,8.7001718350383629E-5,1.3878497442455244E-4,1.9054211956521738E-4,2.4250815217391309E-4,2.9447418478260873E-4,3.6376222826086957E-4,4.3305027173913042E-4,5.0233831521739121E-4,5.8894836956521746E-4,6.7555842391304349E-4,7.6216847826086952E-4,8.6610054347826073E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Battery Energy Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.6475497500000002E-5,4.9279477500000003E-5,8.1642412499999994E-5,1.3023582000000001E-4,1.7880472499999999E-4,2.2756965000000006E-4,2.7633457500000002E-4,3.4135447500000004E-4,4.06374375E-4,4.7139427499999997E-4,5.5266915000000004E-4,6.3394402500000001E-4,7.1521889999999998E-4,8.1274874999999989E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,8.1274875E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Battery Energy Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.7557009271099745E-5,5.2514362212276217E-5,8.7001718350383629E-5,1.3878497442455244E-4,1.9054211956521738E-4,2.4250815217391309E-4,2.9447418478260873E-4,3.6376222826086957E-4,4.3305027173913042E-4,5.0233831521739121E-4,5.8894836956521746E-4,6.7555842391304349E-4,7.6216847826086952E-4,8.6610054347826073E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,8.6610054347826084E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceBattery Energy StorageNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Battery Energy Storage","Non-Incentive Costs","Market Potential",0,70.09,123.5,122.06,175.15,175.07,175.71,175.71,228.89,228.89,228.89,282.06,282.06,282.06,335.23,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageIncentive CostsMarket Potential0","ID","Extra Large General Service","Battery Energy Storage","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceBattery Energy StorageProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Battery Energy Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceBattery Energy StorageProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Battery Energy Storage","Program Annual Costs","Market Potential",0,70.09,123.5,122.06,175.15,175.07,175.71,175.71,228.89,228.89,228.89,282.06,282.06,282.06,335.23,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inParticipantsMarket Potential0","ID","Residential","Time-of-Use Opt-in","Participants","Market Potential",0,503.18825578083323,2935.0696512542081,8233.5552146786467,11861.851924739289,12924.995792888638,12989.278546299989,13047.020412970978,13097.680092622872,13140.684111522367,13175.425541423198,13201.262760408492,13217.51827602,13223.477634794055,13218.388446623861,13201.459557312863,13171.860408365679,13128.720629583955,13071.129917511767,12998.13826134177,12908.756587699781,12819.572165044932,12991.625633758762,13165.757960714165,13341.994579170523,14638.231207732766,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inNew ParticipantsMarket Potential0","ID","Residential","Time-of-Use Opt-in","New Participants","Market Potential",0,503.18825578083323,2431.8813954733751,5298.4855634244386,3628.296710060642,1063.1438681493491,64.282753411351223,57.741866670989111,50.659679651893384,43.00401889949535,34.741429900830553,25.837218985294385,16.255515611508599,5.9593587740546354,0,0,0,0,0,0,0,0,172.05346871382972,174.13232695540319,176.23661845635797,1296.2366285622429,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,5.6249442649870057E-2,0.32652787235428532,0.91274819582244637,1.3113895064213659,1.4242180555781763,1.4256626615989372,1.4263587015593386,1.4262559240599528,1.4253014489114557,1.4234396887683076,1.4206122777999932,1.4167580094225034,1.4118127854448692,1.4057095793649683,1.3983784169817597,1.3897463779848462,1.3797376227448148,1.3682734491684401,1.3552723852118072,1.3406503234735208,1.3261428426650304,1.3386466030961848,1.3512446210897768,1.3639377193626874,1.4905551556239198,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.9941861306340639E-2,0.34796235331871839,0.97266431779885587,1.3974738985734929,1.5177089253816882,1.5192483606126781,1.5199900911757658,1.5198805669863096,1.5188634366064107,1.5168794637343432,1.5138664511935136,1.5097591745764103,1.5044893280529297,1.4979854852567864,1.4901730786250635,1.4809744010921209,1.4703086346385494,1.4580919108785593,1.4442374096460009,1.428655502422763,1.4131956976396316,1.4265202505287562,1.4399452483906403,1.4534715679483028,1.5884006347228472,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,5.3674806459356982E-2,0.3115821157783929,0.87097010119459839,1.2513648959713044,1.3590290834509615,1.3604075673064726,1.3610717482903643,1.3609736750983816,1.3600628879607251,1.3582863438626931,1.355588348480766,1.351910496764227,1.3471916244093505,1.3413677728352227,1.3343721706833902,1.3261352353346618,1.3165845984732139,1.3056451603394241,1.2932391780085113,1.279286393823172,1.2654429459963983,1.2773743872612289,1.2893957717536333,1.3015078845332908,1.4223298174367862,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,5.7198216602042821E-2,0.33203550274764804,0.92814375660123438,1.3335090536778607,1.4482407112648781,1.4497096838304269,1.4504174640775407,1.4503129530033905,1.449342378474771,1.4474492155399543,1.4445741138968096,1.4406548345739845,1.435626198219683,1.4294200477783703,1.4219652287759912,1.4131875909363403,1.4030100154232883,1.3913524726549702,1.3781321163773563,1.3632634205276768,1.3485112382740816,1.3612259028785474,1.3740364149122264,1.3869436109689799,1.5156967363989622,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","ID","Residential","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,57498.99,173220.58,345216.83,245005.5,91096.320000000007,31164.66,30772.2,30347.27,29887.93,29392.18,28857.93,28283.02,27665.25,27307.69,27307.69,27307.69,27307.69,27307.69,27307.69,27307.69,27307.69,37630.9,37755.629999999997,37881.89,105081.89,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inIncentive CostsMarket Potential0","ID","Residential","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","ID","Residential","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialTime-of-Use Opt-inProgram Annual CostsMarket Potential0","ID","Residential","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,57498.99,173220.58,345216.83,245005.5,91096.320000000007,31164.66,30772.2,30347.27,29887.93,29392.18,28857.93,28283.02,27665.25,27307.69,27307.69,27307.69,27307.69,27307.69,27307.69,27307.69,27307.69,37630.9,37755.629999999997,37881.89,105081.89,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inParticipantsMarket Potential0","ID","General Service","Time-of-Use Opt-in","Participants","Market Potential",0,69.951305291297714,396.73562152026579,1036.9814334736207,1461.9688422936943,1596.5808304245961,1600.2238534256767,1602.9020996381062,1604.5405289166135,1605.059711634653,1604.3756570965402,1602.3996480654243,1599.0380842241759,1594.1923378978611,1587.7586259552561,1579.6279024836113,1569.6857776080265,1557.8124687182303,1543.8827913872433,1527.7661984363151,1509.3268769391825,1490.8661471034152,1508.5642254022816,1526.4751340161574,1544.6014104977635,1562.9456228272252,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inNew ParticipantsMarket Potential0","ID","General Service","Time-of-Use Opt-in","New Participants","Market Potential",0,69.951305291297714,326.78431622896807,640.24581195335486,424.9874088200736,134.61198813090186,3.6430230010805644,2.6782462124294852,1.638429278507374,0.51918271803947391,0,0,0,0,0,0,0,0,0,0,0,0,17.698078298866449,17.91090861387579,18.126276481606055,18.344212329461698,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,5.30418623837314E-4,3.0087596783185786E-3,7.8643624434646953E-3,1.1087567867718518E-2,1.2108605627281494E-2,1.2136359865232144E-2,1.2156782117168408E-2,1.2169303418199542E-2,1.2173321543999225E-2,1.2168199712711705E-2,1.2153265333475299E-2,1.2127808822934728E-2,1.2091082514991677E-2,1.2042299693506021E-2,1.1980633782789634E-2,1.190521773662493E-2,1.1815143673296228E-2,1.1709462811864784E-2,1.1587185773784132E-2,1.1447283324096315E-2,1.1307210318885928E-2,1.1441368168071436E-2,1.1577129458150601E-2,1.1714513373947397E-2,1.1853539329864365E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.6523723767829708E-4,3.2062656418569676E-3,8.3806078894551311E-3,1.1815396278472419E-2,1.2903458682098778E-2,1.293303480949717E-2,1.2954797652566505E-2,1.2968140897484593E-2,1.2972422787722959E-2,1.2966964740741374E-2,1.2951050014359868E-2,1.2923922445582617E-2,1.288478528878056E-2,1.2832800184895589E-2,1.2767086298795433E-2,1.2686719668185135E-2,1.2590732814680549E-2,1.2478114675900239E-2,1.2347810926879936E-2,1.2198724769923609E-2,1.2049456861557895E-2,1.2192421321474248E-2,1.2337094477995098E-2,1.2483496775306262E-2,1.2631648902242503E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,5.3609213427572948E-4,3.0409422387990717E-3,7.9484819302423036E-3,1.1206163688466766E-2,1.223812276211368E-2,1.2266173867390715E-2,1.2286814561618273E-2,1.2299469794093193E-2,1.2303530898924237E-2,1.2298354283053431E-2,1.2283260161393436E-2,1.2257531360680939E-2,1.2220412217565597E-2,1.217110760096477E-2,1.2108782093898594E-2,1.2032559375973305E-2,1.1941521854508783E-2,1.1834710600131979E-2,1.1711125651618413E-2,1.1569726765016445E-2,1.1428155498580892E-2,1.1563748338778296E-2,1.170096177073518E-2,1.1839815184481928E-2,1.1980328202083116E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,5.7128317804319001E-4,3.240560783033964E-3,8.4702492862769648E-3,1.1941777161622726E-2,1.3041477794238789E-2,1.3071370276418068E-2,1.3093365901127741E-2,1.3106851869238269E-2,1.3111179559808436E-2,1.3105663131983622E-2,1.3089578177102979E-2,1.3062160444033395E-2,1.3022604664924976E-2,1.2970063513389567E-2,1.2903646732628509E-2,1.2822420477379907E-2,1.2725406920832037E-2,1.2611584185988895E-2,1.2479886670522605E-2,1.2329205845072938E-2,1.2178341324148436E-2,1.2322834973122651E-2,1.2469055595412596E-2,1.2617023853880997E-2,1.2766760658656347E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","ID","General Service","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,5288.58,23780.55,46349.78,30851.18,9944.15,514.38,444.92,370.05,289.45999999999998,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,1526.34,1541.67,1557.18,1572.87,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inIncentive CostsMarket Potential0","ID","General Service","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","ID","General Service","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceTime-of-Use Opt-inProgram Annual CostsMarket Potential0","ID","General Service","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,5288.58,23780.55,46349.78,30851.18,9944.15,514.38,444.92,370.05,289.45999999999998,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,252.08,1526.34,1541.67,1557.18,1572.87,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inParticipantsMarket Potential0","ID","Large General Service","Time-of-Use Opt-in","Participants","Market Potential",0,4.2210906388467837,23.888955824206707,63.40174728985771,91.112157596049755,101.06762307226425,100.90488786916514,100.74735374300163,100.59485484637959,100.44723062030307,100.30432562554248,100.16598937937979,100.03207619755977,99.902445041280529,99.776959369063505,99.655486993346685,99.537899941650579,99.424074322171421,99.313890193660086,99.207231439450169,99.103985645503059,99.004043982341713,98.907301090749328,98.81365497111257,98.723006876293525,98.635261207917623,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inNew ParticipantsMarket Potential0","ID","Large General Service","Time-of-Use Opt-in","New Participants","Market Potential",0,4.2210906388467837,19.667865185359922,39.512791465651006,27.710410306192045,9.9554654762144992,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,9.7117032926775475E-3,5.4861966887602712E-2,0.14535149002108919,0.20852515432641913,0.2309284338151037,0.23018645144805647,0.22946789751161381,0.22877202528393703,0.22809811184328768,0.22744545730945126,0.2268133841093411,0.22620123626600719,0.2256083787103077,0.22503419661451915,0.22447809474718589,0.22393949684853273,0.22341784502578471,0.22291259916775991,0.22242323637812025,0.22194925042668712,0.22149015121824397,0.22104546427827124,0.22061473025506989,0.2201975044377561,0.21979335628961771,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.034921493252083E-2,5.8463306572466657E-2,0.1548928921793363,0.22221350631545089,0.24608741881404911,0.24529673001711047,0.24453100757844609,0.24378945575867117,0.24307130418082659,0.24237580702200687,0.24170224223075565,0.24104991076940238,0.24041813588054955,0.23980626237693856,0.23921365595394914,0.23863970252401187,0.23808380757223435,0.23754539553256596,0.23702390918384511,0.23651880906509709,0.23602957290946716,0.23555569509619698,0.23509668612006596,0.23465207207774519,0.23422139417052185,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,9.8155824694816807E-3,5.5448786293673002E-2,0.14690621144076321,0.2107555994627234,0.23339851088422786,0.23264859205998364,0.23192235226358854,0.23121903678605202,0.23053791497305617,0.22987827945826628,0.22923944542107849,0.22862074986802447,0.22802155093707996,0.22744122722414667,0.22687917713100209,0.22633481823403029,0.22580758667307435,0.22529693655976771,0.22480233940472233,0.22432328356297557,0.22385927369711148,0.22340983025749417,0.22297448897906644,0.2225528003941889,0.22214432936100445,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.0459913117520973E-2,5.908864694551684E-2,0.15654967118580904,0.22459036600886978,0.24871964075471853,0.24792049452257423,0.24714658169606621,0.24639709802435211,0.24567126489029856,0.24496832849346364,0.24428755905912031,0.24362825007248984,0.24298971753738274,0.24237129925846831,0.24177235414642165,0.24119226154521556,0.24063042058085501,0.24008624953086924,0.23955918521389846,0.23904868239873781,0.23855421323221598,0.23807526668530921,0.23761134801690798,0.237161978254677,0.23672669369245999,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","ID","Large General Service","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,4408.3999999999996,5520.57,6949.4,6099.63,4821.28,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inIncentive CostsMarket Potential0","ID","Large General Service","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","ID","Large General Service","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceTime-of-Use Opt-inProgram Annual CostsMarket Potential0","ID","Large General Service","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,4408.3999999999996,5520.57,6949.4,6099.63,4821.28,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,4104.4799999999996,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inParticipantsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Participants","Market Potential",0,0.134246937825,0.38077162695000005,0.70002953163000003,1.0104997617000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,1.1227775130000002,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inNew ParticipantsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","New Participants","Market Potential",0,0.134246937825,0.24652468912500006,0.31925790467999998,0.31047023007000019,0.11227775129999995,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.8041083372120899E-2,5.0930256372217431E-2,9.3151363095099249E-2,0.13379154285039493,0.1479321318039912,0.14722935408806861,0.14654823663171163,0.14588810129878774,0.14524829118508381,0.14462816995355091,0.1440271211903624,0.14344454778113272,0.14287987130666707,0.1423325314576292,0.14180198546753564,0.14128770756350245,0.14078918843418869,0.14030593471439798,0.13983746848581713,0.13938332679338608,0.13894306117680968,0.1385162372167382,0.13810243409515546,0.13770124416953219,0.13731227256031106,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.9225365912319797E-2,5.4273504232968277E-2,9.9266158455988115E-2,0.1425741078968403,0.15764293670502047,0.15689402609555478,0.15616819760412576,0.15546472857927082,0.15478291899518734,0.15412209074334068,0.1534815869462515,0.15286077129276718,0.15225902739414648,0.1516757581603039,0.15111038519558359,0.15056234821345105,0.15003110446951054,0.14951612821227406,0.14901691015112653,0.14853295694094851,0.14806379068287476,0.14760894844068434,0.14716798177233106,0.14674045627614257,0.14632595115122662,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.8649920433379538E-2,5.2649012778317031E-2,9.6294966003486526E-2,0.1383066403137862,0.15292443534450084,0.15219794080900287,0.1514938375073977,0.15081142441831916,0.15015002246883929,0.14950897384727985,0.14888764133753876,0.14828540767425852,0.14770167491818362,0.14713586385107505,0.14658741338956988,0.14605578001739192,0.14554043723533999,0.14504087502849611,0.14455659935011531,0.14408713162167455,0.14363200824857436,0.14319078015100373,0.14276301230949331,0.14234828332469687,0.1419461849909556,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.9874169259782117E-2,5.61050860809005E-2,0.1026161189295466,0.14738559283225297,0.16296295326566584,0.16218876897805079,0.16143844576662159,0.16071123659241171,0.16000641780566846,0.15932328841355481,0.15866116937077873,0.15801940289243235,0.15739735178834571,0.15679439881828117,0.15620994606731659,0.15564341434078421,0.1550942425781543,0.15456188728526865,0.15404582198435135,0.15354553668123885,0.15306053734929068,0.15259034542945837,0.15213449734600737,0.15169254403740076,0.15126405050187083,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceTime-of-Use Opt-inNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Non-Incentive Costs","Market Potential",0,2600.19,2608.2800000000002,2613.5100000000002,2612.88,2598.61,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inIncentive CostsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceTime-of-Use Opt-inProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceTime-of-Use Opt-inProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-in","Program Annual Costs","Market Potential",0,2600.19,2608.2800000000002,2613.5100000000002,2612.88,2598.61,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,2590.5300000000002,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B732&C732&D732&E732&F732&G732","v":"IDResidentialTime-of-Use Opt-outParticipantsMarket Potential0"},"ID","Residential","Time-of-Use Opt-out","Participants","Market Potential",0]
["IDResidentialTime-of-Use Opt-outNew ParticipantsMarket Potential0","ID","Residential","Time-of-Use Opt-out","New Participants","Market Potential",0]
["IDResidentialTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDResidentialTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDResidentialTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDResidentialTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDResidentialTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","ID","Residential","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["IDResidentialTime-of-Use Opt-outIncentive CostsMarket Potential0","ID","Residential","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["IDResidentialTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","ID","Residential","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["IDResidentialTime-of-Use Opt-outProgram Annual CostsMarket Potential0","ID","Residential","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outParticipantsMarket Potential0","ID","General Service","Time-of-Use Opt-out","Participants","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outNew ParticipantsMarket Potential0","ID","General Service","Time-of-Use Opt-out","New Participants","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","ID","General Service","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outIncentive CostsMarket Potential0","ID","General Service","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","ID","General Service","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["IDGeneral ServiceTime-of-Use Opt-outProgram Annual CostsMarket Potential0","ID","General Service","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outParticipantsMarket Potential0","ID","Large General Service","Time-of-Use Opt-out","Participants","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outNew ParticipantsMarket Potential0","ID","Large General Service","Time-of-Use Opt-out","New Participants","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","ID","Large General Service","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outIncentive CostsMarket Potential0","ID","Large General Service","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","ID","Large General Service","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["IDLarge General ServiceTime-of-Use Opt-outProgram Annual CostsMarket Potential0","ID","Large General Service","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outParticipantsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Participants","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outNew ParticipantsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","New Participants","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Non-Incentive Costs","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outIncentive CostsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Incentive Costs","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Program Annual Benefits","Market Potential",0]
["IDExtra Large General ServiceTime-of-Use Opt-outProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Time-of-Use Opt-out","Program Annual Costs","Market Potential",0]
[{"$f":"B772&C772&D772&E772&F772&G772","v":"IDResidentialVariable Peak Pricing RatesParticipantsMarket Potential0"},"ID","Residential","Variable Peak Pricing Rates","Participants","Market Potential",0,953.82700396447592,5444.9707001786601,16874.072181969688,19965.298647961932,21438.068876567584,21544.691587885307,21640.46524495956,21724.492019052566,21795.820716864899,21853.444655705502,21896.299608160531,21923.261850074403,21933.146351849533,21924.705160202993,21896.626025720594,21847.531340972873,21775.977464773441,21680.454520562238,21559.386771105172,21411.133687967293,21263.207775554733,21548.584588966842,21837.409504558753,22129.724707254565,24279.730058802656,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialVariable Peak Pricing RatesNew ParticipantsMarket Potential0","ID","Residential","Variable Peak Pricing Rates","New Participants","Market Potential",0,953.82700396447592,4491.1436962141843,11429.101481791029,3091.2264659922439,1472.7702286056519,106.62271131772286,95.773657074252696,84.026774093006679,71.328697812332393,57.623938840602932,42.854952455028979,26.962241913872276,9.8845017751300475,0,0,0,0,0,0,0,0,285.37681341210919,288.82491559191112,292.31520269581233,2150.0053515480904,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.18706066988764822,1.0627290152890081,3.2817736813521603,3.872399551161847,4.1443543668423759,4.1485580484675726,4.1505834660207972,4.1502843921699037,4.1475069500259698,4.1420893851039065,4.1338618577617998,4.1226462620047668,4.1082560775056658,4.0904962627989843,4.0691631988640902,4.0440446937507071,4.0149200605365589,3.9815602827712087,3.9437282836814389,3.9011793178261325,3.8589637728082451,3.8953486606011252,3.932007829947286,3.9689436748834335,4.3373897304803046,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.19934001479928412,1.1324904254997954,3.4972012802132997,4.1265979871716185,4.4164049092523188,4.4208845358776347,4.4230429092293235,4.4227242030796079,4.4197644394991151,4.4139912458481527,4.4052236335910058,4.3932718052054209,4.3779369964894137,4.3590113627440159,4.3362779186531224,4.3095105432126033,4.2784740628053699,4.2429244275055504,4.2026089979554975,4.1572669627303203,4.1122802353029035,4.1510535598903724,4.190119170873067,4.2294796194409994,4.6221118184998984,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.17849857313031314,1.0140860340509048,3.1315611122841167,3.6951529944162584,3.9546599585688407,3.9586712302725191,3.9606039408923466,3.960318556179049,3.9576682424602856,3.9524986490390179,3.944647710133268,3.9339454719736424,3.9202139515973151,3.9032670349306247,3.8829104229546099,3.8589416361187752,3.831150088730479,3.7993172468261065,3.7632168850544572,3.7226154604048816,3.6823321953329806,3.7170516826438966,3.7520328971576826,3.7872781233317618,4.1388597531796316,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.1902158707697284,1.0806543414864713,3.337128210021437,3.9377163197104204,4.2142582678696083,4.2185328540840992,4.2205924348810173,4.2202883164738374,4.2174640264922054,4.2119550820961402,4.2035887789143951,4.1921840067920311,4.177551099315127,4.1594917252031376,4.1377988309405476,4.1122566454803655,4.0826407595167078,4.0487182937192099,4.0102481724791739,3.96698152217059,3.9240539165952479,3.9610525177364626,3.9983300268091249,4.0358888782307778,4.4105496091002045,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","ID","Residential","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,74233.009999999995,251098.85,597996.74,181102.99,100180.18,31872.799999999999,31330.35,30743,30108.1,29422.86,28684.41,27889.78,27035.89,26541.66,26541.66,26541.66,26541.66,26541.66,26541.66,26541.66,26541.66,40810.5,40982.910000000003,41157.42,134041.93,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialVariable Peak Pricing RatesIncentive CostsMarket Potential0","ID","Residential","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0","ID","Residential","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","ID","Residential","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,74233.009999999995,251098.85,597996.74,181102.99,100180.18,31872.799999999999,31330.35,30743,30108.1,29422.86,28684.41,27889.78,27035.89,26541.66,26541.66,26541.66,26541.66,26541.66,26541.66,26541.66,26541.66,40810.5,40982.910000000003,41157.42,134041.93,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesParticipantsMarket Potential0","ID","General Service","Variable Peak Pricing Rates","Participants","Market Potential",0,133.9504136588366,743.51108917560282,2146.9038750851005,2485.8249832515685,2675.1939952864432,2681.2981605572922,2685.7857681051578,2688.5310823943182,2689.4010129755252,2688.2548269773374,2684.9438718450083,2679.3113130471615,2671.191892327704,2660.4117130669511,2646.7880604499433,2630.129265442064,2610.2346230657577,2586.8943771840482,2559.8897859568488,2528.9932843790571,2498.0609114830877,2527.7154030634765,2557.7265082082263,2588.0984787821176,2618.8356176333873,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesNew ParticipantsMarket Potential0","ID","General Service","Variable Peak Pricing Rates","New Participants","Market Potential",0,133.9504136588366,609.5606755167662,1403.3927859094977,338.921108166468,189.36901203487469,6.1041652708490801,4.4876075478655366,2.745314289160433,0.86993058120697242,0,0,0,0,0,0,0,0,0,0,0,0,29.654491580388822,30.011105144749763,30.371970573891304,30.737138851269719,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.0314072419231322E-2,0.11277264072845607,0.32563804249399014,0.37704980313848779,0.40577800319424479,0.40670809040679867,0.40739247148803215,0.40781207954912541,0.40794673312640478,0.40777509268021955,0.40727461865603964,0.40642153182396251,0.40519077674277865,0.40355598934429976,0.40148946980556183,0.39896216207389618,0.39594364163626933,0.39240211338376096,0.38830442171915819,0.38361607539558151,0.37892201349405036,0.38341784941694768,0.38796741911102367,0.39257136548924476,0.39723033915810851,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.1647562254082823E-2,0.12017544834660707,0.34701411177961439,0.40180072798219074,0.43241475191202555,0.43340589344288005,0.43413519979543069,0.43458235246070481,0.43472584519011592,0.43454293763876761,0.434009610673529,0.43310052410908195,0.43178897777363451,0.43004687696536631,0.42784470354386384,0.42515149411114256,0.42193482697812162,0.41816081988891834,0.41379414079194182,0.40879803430901696,0.40379583705674588,0.40858679605386583,0.4134350161029664,0.41834118232016704,0.42330598802014974,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,2.0531357591240262E-2,0.11397888938864041,0.3291211608277112,0.38108283647814079,0.41011832163960182,0.41105835733298185,0.41175005875146159,0.41217415506128469,0.41231024893202645,0.41213677257017139,0.41163094533161926,0.41076873363697297,0.40952481404480401,0.40787254048925398,0.40578391686207094,0.40322957631867457,0.4001787689166732,0.39659935945749974,0.39245783770212012,0.38771934347533954,0.38297507253513591,0.38751899721452038,0.3921172304169831,0.39677042193227319,0.40147922932596231,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,2.1879110817604713E-2,0.12146087957016241,0.35072587470983718,0.40609850434584482,0.43703998469693289,0.43804172776319461,0.4387788349866385,0.43923077052566567,0.43937579809465732,0.43919093411143584,0.43865190252730102,0.43773309211101125,0.43640751709804348,0.4346467822775511,0.4324210537745854,0.42969903699773504,0.42644796346619052,0.42263358850969707,0.41822020215485944,0.41317065587738655,0.40811495368194362,0.41295715815699102,0.41785723616473047,0.42281588014948124,0.42783379084181833,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","ID","General Service","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,9519.16,33299.67,72991.28,19767.689999999999,12290.09,3126.84,3046.02,2958.9,2865.13,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,4304.3599999999997,4322.1899999999996,4340.2299999999996,4358.49,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesIncentive CostsMarket Potential0","ID","General Service","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0","ID","General Service","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","ID","General Service","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,9519.16,33299.67,72991.28,19767.689999999999,12290.09,3126.84,3046.02,2958.9,2865.13,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,2821.64,4304.3599999999997,4322.1899999999996,4340.2299999999996,4358.49,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesParticipantsMarket Potential0","ID","Large General Service","Variable Peak Pricing Rates","Participants","Market Potential",0,8.083006239989496,44.76962138177074,131.26315722722572,154.92045458019101,169.3465768901228,169.07390153923765,168.80994099284101,168.55441736086641,168.30706161436552,168.06761330295222,167.83582028125696,167.6114384441035,167.39423147013022,167.18397057358661,166.98043426404413,166.78340811376953,166.59268453251531,166.40806254949237,166.2293476022941,166.05635133255154,165.88889138810447,165.72679123148055,165.56987995448148,165.41799209868182,165.27096748165118,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesNew ParticipantsMarket Potential0","ID","Large General Service","Variable Peak Pricing Rates","New Participants","Market Potential",0,8.083006239989496,36.686615141781246,86.493535845454971,23.657297352965287,14.426122309931799,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.8610818691192957E-2,0.1581773412135879,0.46296456397022911,0.54547836006150907,0.59528977628136071,0.59337708623281538,0.59152479024221638,0.58973096340205433,0.58799374215697209,0.58631132234829852,0.58468195732091399,0.58310395609044974,0.5815756815689086,0.5800955488468359,0.57866202353024576,0.57727362013055206,0.57592890050581713,0.57462647235168407,0.57336498774040301,0.57214314170642744,0.57095967087708865,0.56981335214691642,0.56870300139420815,0.56762747223851162,0.56658565483770396,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,3.0488937224203917E-2,0.16856067904261285,0.49335524719760138,0.58128554993766945,0.63436676926828717,0.63232852326600109,0.63035463580798845,0.62844305562878766,0.62659179684246813,0.62479893685880061,0.62306261436585042,0.62138102737686463,0.61975243133941671,0.61817513730481233,0.61664751015584585,0.61516796689104014,0.61373497496357321,0.6123470506731501,0.61100275760912515,0.6097007051432517,0.60843954697046954,0.6072179796962025,0.60603474146867875,0.60488861065485044,0.60377840455850806,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,2.891684825199866E-2,0.15986925163333099,0.46791656634770823,0.55131295377797696,0.60165716725866203,0.59972401852622403,0.5978519098439784,0.59603889571505064,0.59428309265095813,0.59258267719522895,0.59093588401001695,0.58934100402369749,0.58779638263750811,0.58630041798934629,0.58485155927290555,0.58344830511038637,0.58208920197707015,0.58077284267611118,0.57949786486193655,0.5782629496107119,0.57706682003637055,0.57590823995075346,0.57478601256645145,0.57369897924099644,0.57264601826107453,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,3.0815055682010508E-2,0.17036365263568945,0.49863231707982547,0.58750314767474099,0.64115213902244461,0.63909209135360612,0.63709709062657549,0.6351650636349645,0.63329400325123419,0.6314819663205764,0.62972707162192765,0.62802749789396572,0.62638148192402821,0.6247873166979393,0.62324334960880812,0.62174798072291815,0.62029966110088464,0.61889689117232649,0.61753821916233642,0.61622223956810729,0.61494759168411184,0.61371295817428972,0.61251706368973935,0.61135867353047357,0.61023659234982364,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","ID","Large General Service","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,5150.6499999999996,10871.37,20832.75,8265.51,6419.27,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesIncentive CostsMarket Potential0","ID","Large General Service","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0","ID","Large General Service","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","ID","Large General Service","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,5150.6499999999996,10871.37,20832.75,8265.51,6419.27,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,3534.05,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesParticipantsMarket Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Participants","Market Potential",0,0.25227038877328745,0.69686991791917507,1.4346595775754547,1.7008245975451504,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,1.8622970593149999,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesNew ParticipantsMarket Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","New Participants","Market Potential",0,0.25227038877328745,0.44459952914588763,0.73778965965627963,0.26616501996969566,0.16147246176984953,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.3744433758275726E-2,0.12027110406850737,0.24633153444331835,0.29056966456924832,0.31660375745545072,0.31509967539563249,0.3136419505367975,0.3122291315347045,0.31085981248558098,0.30953263150341709,0.30824626934180382,0.30699944805891893,0.30579092972431271,0.30461951516618202,0.30348404275786783,0.3023833872423442,0.3013164585935143,0.30028220091315599,0.29927959136240473,0.29830763912669056,0.29736538441308163,0.29645189747902118,0.29556627769147248,0.29470765261552284,0.29387517713152128,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.6615978003277631E-2,0.12816613818042133,0.26250163516977659,0.30964371757166276,0.33738678330717253,0.33578396781290759,0.33423055257544487,0.33272499097901159,0.3312657848311818,0.32985148284677868,0.32848067917924534,0.32715201199799543,0.32586416211030766,0.32461585162636619,0.32340584266609956,0.32223293610650489,0.32109597036819509,0.31999382023993606,0.31892539573998796,0.31788964101309736,0.31688553326202218,0.31591208171251189,0.31496832661069102,0.31405333825183596,0.31316621603955808,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.5220688368182826E-2,0.12432992382145848,0.25464454782684715,0.30037559346044951,0.32728826554715967,0.32573342484484163,0.32422650577184164,0.32276600800503252,0.32135047819524687,0.31997850849655912,0.31864873514161346,0.31735983706155801,0.31611053454918686,0.31489958796393919,0.31372579647744342,0.31258799685833644,0.31148506229513168,0.31041590125593915,0.30937945638388936,0.30837470342713919,0.307400650202379,0.30645633559079166,0.30554082856544673,0.30465322724914706,0.30379265800177258,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Winter Peak Reduction @Generation (MW)","Market Potential",0,4.8189139352283486E-2,0.13249139367163093,0.27136034508402296,0.32009334341480128,0.3487726614952682,0.34711575537600342,0.34550991663665986,0.34395354646742599,0.342445096115992,0.34098306532028894,0.33956600079029564,0.33819249473738067,0.33686118344968763,0.33557074591212616,0.33431990246956883,0.33310741353190154,0.33193207831962029,0.33079273364869899,0.32968825275350527,0.32861754414656774,0.32757955051404414,0.32657324764577117,0.32559764339881364,0.32465177669346446,0.32373471654067837,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceVariable Peak Pricing RatesNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Non-Incentive Costs","Market Potential",0,1952.75,2029.68,2146.96,1958.31,1916.43,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesIncentive CostsMarket Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceVariable Peak Pricing RatesProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceVariable Peak Pricing RatesProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Variable Peak Pricing Rates","Program Annual Costs","Market Potential",0,1952.75,2029.68,2146.96,1958.31,1916.43,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,1851.84,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceReal Time PricingParticipantsMarket Potential0","ID","Large General Service","Real Time Pricing","Participants","Market Potential",0]
["IDLarge General ServiceReal Time PricingNew ParticipantsMarket Potential0","ID","Large General Service","Real Time Pricing","New Participants","Market Potential",0]
["IDLarge General ServiceReal Time PricingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Real Time Pricing","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDLarge General ServiceReal Time PricingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Real Time Pricing","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDLarge General ServiceReal Time PricingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Real Time Pricing","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDLarge General ServiceReal Time PricingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Real Time Pricing","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDLarge General ServiceReal Time PricingNon-Incentive CostsMarket Potential0","ID","Large General Service","Real Time Pricing","Non-Incentive Costs","Market Potential",0]
["IDLarge General ServiceReal Time PricingIncentive CostsMarket Potential0","ID","Large General Service","Real Time Pricing","Incentive Costs","Market Potential",0]
["IDLarge General ServiceReal Time PricingProgram Annual BenefitsMarket Potential0","ID","Large General Service","Real Time Pricing","Program Annual Benefits","Market Potential",0]
["IDLarge General ServiceReal Time PricingProgram Annual CostsMarket Potential0","ID","Large General Service","Real Time Pricing","Program Annual Costs","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingParticipantsMarket Potential0","ID","Extra Large General Service","Real Time Pricing","Participants","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingNew ParticipantsMarket Potential0","ID","Extra Large General Service","Real Time Pricing","New Participants","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Real Time Pricing","Summer Peak Reduction @Meter  (MW)","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Real Time Pricing","Summer Peak Reduction @Generation (MW)","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Real Time Pricing","Winter Peak Reduction @Meter  (MW)","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Real Time Pricing","Winter Peak Reduction @Generation (MW)","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Real Time Pricing","Non-Incentive Costs","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingIncentive CostsMarket Potential0","ID","Extra Large General Service","Real Time Pricing","Incentive Costs","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Real Time Pricing","Program Annual Benefits","Market Potential",0]
["IDExtra Large General ServiceReal Time PricingProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Real Time Pricing","Program Annual Costs","Market Potential",0]
["IDResidentialBehavioralParticipantsMarket Potential0","ID","Residential","Behavioral","Participants","Market Potential",0,1915.7905620249282,7449.8012386146693,17763.666132678878,20071.855108770618,19683.754276660242,19781.651865383046,19869.588196909961,19946.738913396137,20012.230659350302,20065.139130683347,20104.487187568491,20129.243062159443,20138.318697899263,20130.568263700672,20104.7868938098,20059.709712817974,19994.011215217211,19906.305080282102,19795.144516107124,19659.023241562994,19523.202364792593,19785.226295390188,20050.416163946978,20318.810703321076,22292.877363757751,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBehavioralNew ParticipantsMarket Potential0","ID","Residential","Behavioral","New Participants","Market Potential",0,1915.7905620249282,5534.0106765897408,10313.864894064209,2308.1889760917402,0,97.897588722804358,87.936331526914728,77.150716486175952,65.491745954164799,52.908471333044872,39.348056885144615,24.755874590951862,9.0756357398204273,0,0,0,0,0,0,0,0,262.02393059759561,265.18986855679032,268.3945393740978,1974.0666604366743,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBehavioralSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Behavioral","Summer Peak Reduction @Meter  (MW)","Market Potential",0,7.5143409529672786E-2,0.29080486821176194,0.69095748044556971,0.77861337398149355,0.761042922867876,0.76181486027179124,0.76218679509161891,0.76213187506850066,0.76162184322753934,0.7606269960020946,0.75911614511865955,0.75705658432315237,0.75441406220693963,0.75115276259363872,0.74723529417910539,0.74262269138082548,0.73727442865356319,0.73114845087041602,0.7242012227579826,0.71638780081737785,0.70863560616242305,0.71531709594419812,0.7220489530489681,0.72883161710243249,0.79649071143905525,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBehavioralSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Behavioral","Summer Peak Reduction @Generation (MW)","Market Potential",0,8.0076097111757019E-2,0.30989436083947353,0.73631445060269574,0.82972439682597354,0.81100055719083119,0.81182316738255678,0.81221951736106024,0.81216099218723425,0.81161747999524647,0.81055732736796104,0.8089472987197992,0.80675254083882386,0.80393655392896379,0.80046117070933365,0.79628654537415322,0.79137115449789586,0.78567181229066829,0.77914370297358915,0.77174043345906074,0.76341410999294312,0.75515303299490943,0.76227312014513871,0.76944688091322255,0.77667478378349586,0.84877526794443225,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B836&C836&D836&E836&F836&G836","v":"IDResidentialBehavioralWinter Peak Reduction @Meter  (MW)Market Potential0"},"ID","Residential","Behavioral","Winter Peak Reduction @Meter  (MW)","Market Potential",0,7.1703963154036765E-2,0.27749421653587159,0.6593311380063348,0.74297486670688195,0.72620864612764191,0.7269452505952062,0.7273001613023935,0.72724775506558925,0.7267610682814708,0.72581175696802791,0.72437006039403529,0.72240476932834008,0.7198832001096872,0.71677117593125217,0.71303301695482346,0.70863154112131765,0.70352807781117499,0.69768249683481831,0.6910532556050879,0.68359746776630459,0.67620010473232739,0.68257577094344468,0.68899949907635627,0.69547170863431884,0.76003392690088489,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBehavioralWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Behavioral","Winter Peak Reduction @Generation (MW)","Market Potential",0,7.6410872926296641E-2,0.295709949420153,0.70261203964869434,0.79174644789735926,0.77387963142331828,0.77466458929582926,0.77504279763682171,0.77498695126341566,0.77446831658298254,0.77345668901111242,0.77192035421359262,0.76982605427146211,0.76713896004868631,0.76382265124813742,0.75983910587683656,0.75514870110967358,0.74971022784652064,0.74348092160573132,0.73641651279314568,0.7284712998362155,0.72058834690145712,0.72738253510597262,0.73422794019219551,0.74112500920110702,0.80992532704697873,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialBehavioralNon-Incentive CostsMarket Potential0","ID","Residential","Behavioral","Non-Incentive Costs","Market Potential",0,62305.73,80291.259999999995,113811.32,121312.93,120051.61,120369.77,120655.57,120906.31,121119.16,121291.11,121418.99,121499.45,121528.94,121503.75,121419.96,121273.46,121059.94,120774.9,120413.63,119971.23,119529.81,120381.39,121243.26,122115.54,128531.26,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBehavioralIncentive CostsMarket Potential0","ID","Residential","Behavioral","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialBehavioralProgram Annual BenefitsMarket Potential0","ID","Residential","Behavioral","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialBehavioralProgram Annual CostsMarket Potential0","ID","Residential","Behavioral","Program Annual Costs","Market Potential",0,62305.73,80291.259999999995,113811.32,121312.93,120051.61,120369.77,120655.57,120906.31,121119.16,121291.11,121418.99,121499.45,121528.94,121503.75,121419.96,121273.46,121059.94,120774.9,120413.63,119971.23,119529.81,120381.39,121243.26,122115.54,128531.26,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingParticipantsMarket Potential0","ID","Residential","Ancillary Cooling","Participants","Market Potential",0,392.70498536057136,1262.0789608619814,3154.4141897392642,4341.0304554826607,5162.7366093027922,5525.983890998662,5914.7890497750077,6330.9503236745522,6776.3924737703974,7253.1756862561988,7763.5051008824739,8309.7410098083819,8894.4097740390698,9520.2155079374679,10190.052585851879,10907.01902870292,11674.430832443282,12495.837304659994,13375.037480251474,14316.097692102536,15270.797890160306,15457.368350538503,15646.218229250711,15837.375375013869,16030.867976785687,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingNew ParticipantsMarket Potential0","ID","Residential","Ancillary Cooling","New Participants","Market Potential",0,392.70498536057136,869.37397550141009,1892.3352288772828,1186.6162657433965,821.70615382013148,363.24728169586979,388.80515877634571,416.16127389954454,445.44215009584514,476.78321248580141,510.32941462627514,546.23590892590801,584.66876423068788,625.8057338983981,669.83707791441157,716.96644285104048,767.4118037403623,821.40647221671134,879.20017559148073,941.06021185106147,954.70019805776974,186.57046037819782,188.84987871220801,191.15714576315804,193.49260177181714,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,9.8176246340142839E-2,0.31551974021549534,0.78860354743481609,1.0852576138706651,1.290684152325698,1.3814959727496654,1.478697262443752,1.5827375809186381,1.6940981184425994,1.8132939215640498,1.9408762752206186,2.0774352524520956,2.2236024435097677,2.3800538769843671,2.5475131464629697,2.7267547571757298,2.9186077081108204,3.1239593261649983,3.3437593700628687,3.5790244230256341,3.8176994725400766,3.8643420876346259,3.911554557312678,3.9593438437534672,4.0077169941964215,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.10462089337184872,0.33623160722026357,0.84037036171655588,1.1564978834938886,1.3754093694860379,1.4721824091535223,1.5757643461676811,1.6866342507658121,1.8053049003011503,1.9323251508568304,2.0682824757252969,2.213805682493708,2.3695678213019691,2.5362892977241764,2.7147412046706836,2.9057488887209395,3.1101957673815219,3.3290274149243375,3.5632559357021192,3.8139646451679816,4.0683071958014452,4.1180116023386892,4.1683232707935609,4.2192496203681449,4.2707981609083774,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary CoolingNon-Incentive CostsMarket Potential0","ID","Residential","Ancillary Cooling","Non-Incentive Costs","Market Potential",0,37737.07,66337.210000000006,127714.89,85371.75,63477.14,35969.61,37503.08,39144.449999999997,40901.300000000003,42781.77,44794.54,46948.93,49254.9,51723.12,54365,57192.76,60219.48,63459.16,66926.78,70638.39,71456.789999999994,25369,25505.77,25644.2,25784.33,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingIncentive CostsMarket Potential0","ID","Residential","Ancillary Cooling","Incentive Costs","Market Potential",0,7854.1,25241.58,63088.28,86820.61,103254.73,110519.67999999999,118295.78,126619.01,135527.85,145063.51,155270.1,166194.82,177888.2,190404.31,203801.05,218140.38,233488.62,249916.75,267500.75,286321.95,305415.96000000002,309147.37,312924.36,316747.51,320617.36,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary CoolingProgram Annual BenefitsMarket Potential0","ID","Residential","Ancillary Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary CoolingProgram Annual CostsMarket Potential0","ID","Residential","Ancillary Cooling","Program Annual Costs","Market Potential",0,45591.17,91578.79,190803.17,172192.36,166731.87,146489.29,155798.85999999999,165763.46,176429.15,187845.28,200064.64000000001,213143.75,227143.09,242127.43,258166.05,275333.14,293708.09999999998,313375.90999999997,334427.53000000003,356960.34,376872.74,334516.37,338430.13,342391.71,346401.69,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingParticipantsMarket Potential0","ID","General Service","Ancillary Cooling","Participants","Market Potential",0,54.931808570091007,176.33163400875458,440.22011205989475,605.5895084792611,719.94767732988623,770.31281649081427,824.20335580154733,881.86616153114164,943.56539165206141,1009.5837072742656,1080.2235689625543,1155.8086238853853,1236.6851901602226,1323.2238452065528,1415.8211253950133,1514.9013447918735,1620.9185413446808,1734.3585594397609,1855.7412783881466,1985.6229970662339,2117.3097632683857,2142.4443563678947,2167.8812084627975,2193.6239233542533,2219.6761480560485,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingNew ParticipantsMarket Potential0","ID","General Service","Ancillary Cooling","New Participants","Market Potential",0,54.931808570091007,121.39982543866357,263.88847805114017,165.36939641936635,114.35816885062513,50.365139160928038,53.890539310733061,57.662805729594311,61.699230120919765,66.018315622204227,70.639861688288647,75.585054922830977,80.876566274837387,86.538655046330177,92.597280188460445,99.08021939686023,106.01719655280726,113.44001809508018,121.38271894838567,129.88171867808728,131.68676620215183,25.134593099508947,25.436852094902861,25.742714891455762,26.05222470179524,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,3.4332380356306876E-2,0.11020727125547161,0.27513757003743422,0.37849344279953817,0.44996729833117888,0.48144551030675892,0.51512709737596707,0.55116635095696342,0.5897283697825384,0.63098981704641599,0.67513973060159638,0.72238038992836573,0.77292824385013914,0.82701490325409555,0.88488820337188323,0.94681334049492094,1.0130740883404254,1.0839740996498506,1.1598382989925917,1.2410143731663961,1.323318602042741,1.3390277227299341,1.3549257552892484,1.3710149520964083,1.3872975925350304,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,3.6586083073643305E-2,0.11744167866098851,0.29319860404671166,0.40333913341809269,0.47950479361805082,0.5130493502842699,0.54894191962485839,0.58734692130963706,0.62844029175462313,0.67241029097017901,0.71945836594373014,0.76980007451871879,0.82366607400909964,0.8813031790857796,0.94297549378930434,1.0089656228633002,1.0795759679672052,1.1551301147163795,1.2359743169145265,1.3224790847894246,1.4101860635579082,1.4269263882458803,1.4438680256705545,1.4610133760618162,1.4783648684303392,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary CoolingNon-Incentive CostsMarket Potential0","ID","General Service","Ancillary Cooling","Non-Incentive Costs","Market Potential",0,8093.2,13078.3,23764.95,16376.01,12550.17,7750.7,8015.1,8298.02,8600.75,8924.68,9271.2999999999993,9642.19,10039.049999999999,10463.709999999999,10918.11,11404.33,11924.6,12481.31,13077.01,13714.44,13849.82,5858.4,5881.07,5904.01,5927.23,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingIncentive CostsMarket Potential0","ID","General Service","Ancillary Cooling","Incentive Costs","Market Potential",0,1098.6400000000001,3526.63,8804.4,12111.79,14398.95,15406.26,16484.07,17637.32,18871.310000000001,20191.669999999998,21604.47,23116.17,24733.7,26464.48,28316.42,30298.03,32418.37,34687.17,37114.83,39712.46,42346.2,42848.89,43357.62,43872.480000000003,44393.52,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary CoolingProgram Annual BenefitsMarket Potential0","ID","General Service","Ancillary Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary CoolingProgram Annual CostsMarket Potential0","ID","General Service","Ancillary Cooling","Program Annual Costs","Market Potential",0,9191.83,16604.93,32569.35,28487.8,26949.13,23156.95,24499.17,25935.34,27472.06,29116.36,30875.77,32758.36,34772.76,36928.19,39234.53,41702.35,44342.97,47168.480000000003,50191.839999999997,53426.9,56196.01,48707.29,49238.7,49776.49,50320.75,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B862&C862&D862&E862&F862&G862","v":"IDResidentialAncillary HeatingParticipantsMarket Potential0"},"ID","Residential","Ancillary Heating","Participants","Market Potential",0,121.98049412868589,370.72739719386527,876.25609978577336,1140.3793661879247,1282.5687919961611,1298.2385331393939,1314.099718818801,1330.1546880015746,1346.4058082311587,1362.8554759763804,1379.5061169848441,1396.3601866406439,1413.4201703264473,1430.6885837900002,1448.1679735151126,1465.8609170971747,1483.770023623262,1501.8979340568835,1520.2473216274316,1538.8208922243887,1557.6213847963511,1576.6515717549273,1595.9142593835725,1615.4122882514146,1635.14853363214,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary HeatingNew ParticipantsMarket Potential0","ID","Residential","Ancillary Heating","New Participants","Market Potential",0,121.98049412868589,248.74690306517937,505.52870259190809,264.12326640215133,142.18942580823636,15.669741143232841,15.861185679407072,16.054969182773675,16.251120229584103,16.449667745221632,16.650641008463708,16.854069655799776,17.059983685803445,17.268413463552861,17.479389725112469,17.692943582062071,17.909106526087271,18.127910433621537,18.34938757054806,18.573570596957097,18.800492571962423,19.030186958576223,19.262687628645153,19.498028867842095,19.73624538072545,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary HeatingSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,6.6479369300133817E-2,0.2020464314706566,0.47755957438324653,0.621506754572419,0.69899999163790782,0.70754000056096966,0.71618434675624654,0.7249343049608582,0.73379116548598156,0.74275623440712746,0.75183083375674009,0.76101630171915102,0.7703139928279138,0.77972527816555004,0.78925154556573651,0.79889419981796028,0.8086546628746778,0.8185343740610016,0.82853479028695032,0.83865738626229192,0.84890365471401141,0.85927510660643547,0.86977327136404714,0.88039969709702093,0.89115595082951637,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary HeatingWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,7.0843317668514302E-2,0.21530949645210634,0.50890832734787572,0.66230472567393328,0.74488490157492304,0.75398550784417051,0.76319730046488332,0.77252163785257688,0.78195989501916197,0.7915134637757113,0.80118375293770261,0.81097218853276964,0.82088021401099087,0.83090929045774731,0.84106089680918217,0.8513365300702902,0.86173770553567541,0.87226595701300258,0.88292283704917973,0.89370991715930514,0.90462878805840941,0.91568105989603099,0.92686836249365634,0.93819234558506071,0.94965467905958689,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary HeatingNon-Incentive CostsMarket Potential0","ID","Residential","Ancillary Heating","Non-Incentive Costs","Market Potential",0,22141.53,29747.51,45154.42,30670.09,23354.06,15762.88,15774.37,15785.99,15797.76,15809.68,15821.73,15833.94,15846.29,15858.8,15871.46,15884.27,15897.24,15910.37,15923.66,15937.11,15950.73,15964.51,15978.46,15992.58,16006.87,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary HeatingIncentive CostsMarket Potential0","ID","Residential","Ancillary Heating","Incentive Costs","Market Potential",0,2439.61,7414.55,17525.12,22807.59,25651.38,25964.77,26281.99,26603.09,26928.12,27257.11,27590.12,27927.200000000001,28268.400000000001,28613.77,28963.360000000001,29317.22,29675.4,30037.96,30404.95,30776.42,31152.43,31533.03,31918.29,32308.25,32702.97,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary HeatingProgram Annual BenefitsMarket Potential0","ID","Residential","Ancillary Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary HeatingProgram Annual CostsMarket Potential0","ID","Residential","Ancillary Heating","Program Annual Costs","Market Potential",0,24581.14,37162.06,62679.54,53477.68,49005.440000000002,41727.65,42056.36,42389.09,42725.88,43066.79,43411.86,43761.14,44114.7,44472.57,44834.82,45201.49,45572.639999999999,45948.33,46328.61,46713.53,47103.15,47497.54,47896.74,48300.82,48709.84,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingParticipantsMarket Potential0","ID","General Service","Ancillary Heating","Participants","Market Potential",0,3.56309419195125,10.816277446557002,25.536516171704992,33.221121704895545,37.349179538083746,37.791265585015992,38.238678266290869,38.691481009736229,39.149738004378129,39.61351420952866,40.082875363982915,40.557887995326041,41.038619429351698,41.525137799593466,42.017512056970411,42.51581197954809,43.0201081824166,43.530472127686863,44.046976134606687,44.56969338979799,45.098697957616601,45.634064790636153,46.175869740257575,46.724189567445592,47.27910195359383,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingNew ParticipantsMarket Potential0","ID","General Service","Ancillary Heating","New Participants","Market Potential",0,3.56309419195125,7.2531832546057524,14.72023872514799,7.6846055331905525,4.1280578331882012,0.44208604693224629,0.44741268127487643,0.45280274344536053,0.45825699464189995,0.46377620515053053,0.46936115445425486,0.47501263134312666,0.48073143402565677,0.48651837024176814,0.49237425737694451,0.49829992257767941,0.50429620286850962,0.51036394527026374,0.51650400691982412,0.52271725519130285,0.52900456781861038,0.53536683301955179,0.54180494962142234,0.54831982718801697,0.55491238614823857,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,2.4050885795670941E-3,7.3009872764259777E-3,1.7237148415900874E-2,2.2424257150804493E-2,2.5210696188206531E-2,2.5509104269885795E-2,2.5811107829746337E-2,2.6116749681571957E-2,2.642607315295524E-2,2.6739122091431845E-2,2.705594087068847E-2,2.7376574396845078E-2,2.7701068114812398E-2,2.8029468014725591E-2,2.8361820638455028E-2,2.8698173086194961E-2,2.9038573023131207E-2,2.9383068686188635E-2,2.9731708890859514E-2,3.0084543038113642E-2,3.0441621121391208E-2,3.0802993733679403E-2,3.1168712074673866E-2,3.1538827958025775E-2,3.1913393818675841E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,2.5629673695301515E-3,7.7802507208290465E-3,1.8368657732204682E-2,2.3896267211002232E-2,2.6865618273877376E-2,2.7183614950858692E-2,2.750544312632815E-2,2.7831148424522546E-2,2.816077701721573E-2,2.849437563025559E-2,2.8831991550179528E-2,2.9173672630909076E-2,2.951946730052472E-2,2.9869424568121899E-2,3.0223594030749177E-2,3.0582025880429412E-2,3.094477091126514E-2,3.1311880526628977E-2,3.1683406746440233E-2,3.2059402214528604E-2,3.2439920206086111E-2,3.2825014635208226E-2,3.3214740062525429E-2,3.360915170292602E-2,3.4008305433371529E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary HeatingNon-Incentive CostsMarket Potential0","ID","General Service","Ancillary Heating","Non-Incentive Costs","Market Potential",0,3459.77,3736.52,4296.55,3768.88,3502.14,3225.69,3226.09,3226.5,3226.9,3227.32,3227.74,3228.16,3228.59,3229.02,3229.46,3229.91,3230.36,3230.81,3231.27,3231.74,3232.21,3232.69,3233.17,3233.66,3234.15,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingIncentive CostsMarket Potential0","ID","General Service","Ancillary Heating","Incentive Costs","Market Potential",0,71.260000000000005,216.33,510.73,664.42,746.98,755.83,764.77,773.83,782.99,792.27,801.66,811.16,820.77,830.5,840.35,850.32,860.4,870.61,880.94,891.39,901.97,912.68,923.52,934.48,945.58,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary HeatingProgram Annual BenefitsMarket Potential0","ID","General Service","Ancillary Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary HeatingProgram Annual CostsMarket Potential0","ID","General Service","Ancillary Heating","Program Annual Costs","Market Potential",0,3531.03,3952.85,4807.28,4433.3,4249.12,3981.52,3990.86,4000.33,4009.9,4019.59,4029.4,4039.32,4049.36,4059.53,4069.81,4080.22,4090.76,4101.42,4112.21,4123.13,4134.18,4145.37,4156.6899999999996,4168.1400000000003,4179.74,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B882&C882&D882&E882&F882&G882","v":"IDResidentialAncillary WHParticipantsMarket Potential0"},"ID","Residential","Ancillary WH","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary WHNew ParticipantsMarket Potential0","ID","Residential","Ancillary WH","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary WHSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary WHSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary WHWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary WHWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary WHNon-Incentive CostsMarket Potential0","ID","Residential","Ancillary WH","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary WHIncentive CostsMarket Potential0","ID","Residential","Ancillary WH","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary WHProgram Annual BenefitsMarket Potential0","ID","Residential","Ancillary WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary WHProgram Annual CostsMarket Potential0","ID","Residential","Ancillary WH","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHParticipantsMarket Potential0","ID","General Service","Ancillary WH","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHNew ParticipantsMarket Potential0","ID","General Service","Ancillary WH","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary WHNon-Incentive CostsMarket Potential0","ID","General Service","Ancillary WH","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHIncentive CostsMarket Potential0","ID","General Service","Ancillary WH","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary WHProgram Annual BenefitsMarket Potential0","ID","General Service","Ancillary WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary WHProgram Annual CostsMarket Potential0","ID","General Service","Ancillary WH","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B902&C902&D902&E902&F902&G902","v":"IDResidentialAncillary DLC WHParticipantsMarket Potential0"},"ID","Residential","Ancillary DLC WH","Participants","Market Potential",0,899.08346967170064,2695.4858291558157,6284.7234413183569,8068.2103820675966,8951.2003534908981,8937.7427678109689,8924.305414793158,8910.8882640188931,8897.4912851153276,8884.1144477552753,8870.7577216571535,8857.4210765849075,8844.1044823479242,8830.8079088009999,8817.5313258442402,8804.2747034230106,8791.0380115278549,8777.8212201944425,8764.6242995034845,8751.4472195806829,8738.2899505966434,8725.1524627668277,8712.0347263514705,8698.9367116555241,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary DLC WHNew ParticipantsMarket Potential0","ID","Residential","Ancillary DLC WH","New Participants","Market Potential",0,899.08346967170064,1796.4023594841151,3589.2376121625412,1783.4869407492397,882.98997142330154,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary DLC WHSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary DLC WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.4495417348358503,1.3477429145779078,3.1423617206591783,4.0341051910337979,4.4756001767454494,4.4688713839054843,4.4621527073965792,4.4554441320094469,4.4487456425576637,4.4420572238776375,4.4353788608285765,4.4287105382924539,4.4220522411739625,4.4154039544005004,4.4087656629221197,4.402137351711505,4.3955190057639273,4.3889106100972208,4.3823121497517423,4.3757236097903416,4.3691449752983216,4.3625762313834135,4.3560173631757353,4.3494683558277618,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary DLC WHSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary DLC WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.47905129458210816,1.436213677086432,3.3486378097391074,4.2989185752704584,4.7693949027551676,4.7622244074014111,4.7550646924515974,4.7479157416980469,4.7407775389574418,4.7336500680707987,4.7265333129034275,4.7194272573448997,4.7123318853089966,4.7052471807336964,4.698173127581116,4.6911097098374945,4.6840569115131361,4.6770147166423923,4.6699831092836126,4.6629620735191191,4.6559515934551596,4.6489516532218813,4.6419622369732902,4.6349833288872144,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary DLC WHWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary DLC WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.4495417348358503,1.3477429145779078,3.1423617206591783,4.0341051910337979,4.4756001767454494,4.4688713839054843,4.4621527073965792,4.4554441320094469,4.4487456425576637,4.4420572238776375,4.4353788608285765,4.4287105382924539,4.4220522411739625,4.4154039544005004,4.4087656629221197,4.402137351711505,4.3955190057639273,4.3889106100972208,4.3823121497517423,4.3757236097903416,4.3691449752983216,4.3625762313834135,4.3560173631757353,4.3494683558277618,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary DLC WHWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary DLC WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.47905129458210816,1.436213677086432,3.3486378097391074,4.2989185752704584,4.7693949027551676,4.7622244074014111,4.7550646924515974,4.7479157416980469,4.7407775389574418,4.7336500680707987,4.7265333129034275,4.7194272573448997,4.7123318853089966,4.7052471807336964,4.698173127581116,4.6911097098374945,4.6840569115131361,4.6770147166423923,4.6699831092836126,4.6629620735191191,4.6559515934551596,4.6489516532218813,4.6419622369732902,4.6349833288872144,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary DLC WHNon-Incentive CostsMarket Potential0","ID","Residential","Ancillary DLC WH","Non-Incentive Costs","Market Potential",0,146494.59,200333.73,307903.84000000003,199558.8,145528.98000000001,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,92549.59,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary DLC WHIncentive CostsMarket Potential0","ID","Residential","Ancillary DLC WH","Incentive Costs","Market Potential",0,21578,64691.66,150833.35999999999,193637.05,214828.81,214505.83,214183.33,213861.32,213539.79,213218.75,212898.19,212578.11,212258.51,211939.39,211620.75,211302.59,210984.91,210667.71,210350.98,210034.73,209718.96,209403.66,209088.83,208774.48,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary DLC WHProgram Annual BenefitsMarket Potential0","ID","Residential","Ancillary DLC WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary DLC WHProgram Annual CostsMarket Potential0","ID","Residential","Ancillary DLC WH","Program Annual Costs","Market Potential",0,168072.6,265025.39,458737.21,393195.85,360357.79,307055.40999999997,306732.92,306410.90000000002,306089.38,305768.33,305447.77,305127.69,304808.09000000003,304488.98,304170.34000000003,303852.18,303534.5,303217.3,302900.57,302584.32000000001,302268.55,301953.25,301638.42,301324.07,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHParticipantsMarket Potential0","ID","General Service","Ancillary DLC WH","Participants","Market Potential",0,50.767095821532457,154.11071500777004,363.84521250253772,473.33575202726473,532.15247038618259,538.45132848448111,544.82608066289913,551.27763064343867,557.80689299368055,564.41479325626938,571.10226807995218,577.87026535218513,584.71974433332821,591.65167579244962,598.66704214475544,605.76683759066532,612.95206825655475,620.22375233718287,627.58292023982665,635.03061473014077,642.56789107976454,650.19581721569693,657.91547387146124,665.7279547400783,673.6343666288742,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHNew ParticipantsMarket Potential0","ID","General Service","Ancillary DLC WH","New Participants","Market Potential",0,50.767095821532457,103.34361918623759,209.73449749476768,109.49053952472701,58.816718358917853,6.2988580982985241,6.3747521784180208,6.4515499805395393,6.5292623502418792,6.6079002625888279,6.6874748236828054,6.7679972722329467,6.8494789811430792,6.9319314591214152,7.0153663523058185,7.0997954459098764,7.1852306658894349,7.2716840806281198,7.359167902643776,7.4476944903141202,7.5372763496237667,7.6279261359323982,7.7196566557643109,7.8124808686170581,7.9064118887959012,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary DLC WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,6.3966540735130903E-2,0.19417950090979025,0.45844496775319754,0.59640304755435347,0.67051211268659006,0.67844867389044627,0.6864808616352529,0.69460981461073279,0.70283668517203746,0.71116263950289937,0.71958885778073978,0.72811653434375334,0.7367468778599936,0.7454811114984865,0.75432047310239181,0.76326621536423833,0.772319606003259,0.78148192794485039,0.79075447950218158,0.80013857455997739,0.80963554276050331,0.81924672969177814,0.82897349707804124,0.83881722297249872,0.84877930195238149,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary DLC WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,6.8165537867786549E-2,0.20692615186465285,0.48853896819394454,0.63555311972970319,0.71452697430369783,0.72298452034361282,0.73154397019954487,0.74020653730896502,0.74897344967182167,0.75784595002440258,0.76682529601528104,0.77591276038336887,0.78510963113810062,0.79441721174178015,0.80383682129410894,0.81336979471892401,0.82301748295317456,0.83278125313816109,0.84266248881306649,0.85266259011080281,0.86278297395620551,0.8730250742666007,0.88339034215477541,0.89388024613437633,0.9044962723277723,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary DLC WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,6.3966540735130903E-2,0.19417950090979025,0.45844496775319754,0.59640304755435347,0.67051211268659006,0.67844867389044627,0.6864808616352529,0.69460981461073279,0.70283668517203746,0.71116263950289937,0.71958885778073978,0.72811653434375334,0.7367468778599936,0.7454811114984865,0.75432047310239181,0.76326621536423833,0.772319606003259,0.78148192794485039,0.79075447950218158,0.80013857455997739,0.80963554276050331,0.81924672969177814,0.82897349707804124,0.83881722297249872,0.84877930195238149,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary DLC WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,6.8165537867786549E-2,0.20692615186465285,0.48853896819394454,0.63555311972970319,0.71452697430369783,0.72298452034361282,0.73154397019954487,0.74020653730896502,0.74897344967182167,0.75784595002440258,0.76682529601528104,0.77591276038336887,0.78510963113810062,0.79441721174178015,0.80383682129410894,0.81336979471892401,0.82301748295317456,0.83278125313816109,0.84266248881306649,0.85266259011080281,0.86278297395620551,0.8730250742666007,0.88339034215477541,0.89388024613437633,0.9044962723277723,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary DLC WHNon-Incentive CostsMarket Potential0","ID","General Service","Ancillary DLC WH","Non-Incentive Costs","Market Potential",0,12960.79,16904.03,24883.34,17365.05,13564.51,9625.67,9631.36,9637.1200000000008,9642.9500000000007,9648.85,9654.82,9660.86,9666.9699999999993,9673.15,9679.41,9685.74,9692.15,9698.6299999999992,9705.19,9711.83,9718.5499999999993,9725.35,9732.23,9739.19,9746.24,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHIncentive CostsMarket Potential0","ID","General Service","Ancillary DLC WH","Incentive Costs","Market Potential",0,1218.4100000000001,3698.66,8732.2900000000009,11360.06,12771.66,12922.83,13075.83,13230.66,13387.37,13545.96,13706.45,13868.89,14033.27,14199.64,14368.01,14538.4,14710.85,14885.37,15061.99,15240.73,15421.63,15604.7,15789.97,15977.47,16167.22,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary DLC WHProgram Annual BenefitsMarket Potential0","ID","General Service","Ancillary DLC WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary DLC WHProgram Annual CostsMarket Potential0","ID","General Service","Ancillary DLC WH","Program Annual Costs","Market Potential",0,14179.2,20602.68,33615.629999999997,28725.1,26336.17,22548.5,22707.19,22867.79,23030.32,23194.799999999999,23361.27,23529.74,23700.240000000002,23872.79,24047.42,24224.14,24403,24584,24767.18,24952.57,25140.18,25330.05,25522.2,25716.66,25913.46,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVParticipantsMarket Potential0","ID","Residential","Ancillary EV","Participants","Market Potential",0,0,0,56.147534921456717,199.76696382635797,552.80527007123476,842.92389335515327,1110.7532058030197,1317.31396456414,1562.2877090695806,1852.8178942652046,2197.3764047301052,2606.010595541818,3090.6362739934693,3665.3851655343205,4347.0169960696712,5155.4082069746028,6114.1315537923183,7251.1434897638228,8599.5993783502836,10198.820306413674,12095.439690409152,14344.763110721977,17012.38102703229,20176.081401623207,20422.581998566762,20672.094208275154,20924.654825026195,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVNew ParticipantsMarket Potential0","ID","Residential","Ancillary EV","New Participants","Market Potential",0,0,0,56.147534921456717,143.61942890490124,353.03830624487682,290.11862328391851,267.82931244786641,206.56075876112027,244.97374450544066,290.53018519562397,344.55851046490056,408.63419081171287,484.62567845165131,574.74889154085122,681.63183053535067,808.39121090493154,958.72334681771554,1137.0119359715045,1348.4558885864608,1599.2209280633906,1896.6193839954776,2249.323420312825,2667.6179163103134,3163.7003745909169,246.50059694355514,249.51220970839131,252.56061675104138,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary EV","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,1.4036883730364179E-2,4.9941740956589493E-2,0.1382013175178087,0.21073097333878832,0.2776883014507549,0.32932849114103496,0.39057192726739515,0.46320447356630112,0.5493441011825263,0.65150264888545451,0.7726590684983673,0.91634629138358015,1.0867542490174178,1.2888520517436506,1.5285328884480796,1.8127858724409558,2.149899844587571,2.5497050766034186,3.0238599226022878,3.586190777680494,4.2530952567580727,5.0440203504058019,5.1056454996416907,5.1680235520687887,5.2311637062565488,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary EV","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,1.4958315995699252E-2,5.3220099058599202E-2,0.14727335626364951,0.22456412333630468,0.29591677477701928,0.35094681494142688,0.41621049367795732,0.49361090533493301,0.58540505241104679,0.69426965993761136,0.8233792290050802,0.97649860548122347,1.1580927632325424,1.3734570031368825,1.6288713645013635,1.9317837515355454,2.2910271148631405,2.7170770211033872,3.2223571212726849,3.8216014254907225,4.5322839479519104,5.3751282506455684,5.4407986995329187,5.5072714749241145,5.5745563792162711,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary EV","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,1.4036883730364179E-2,4.9941740956589493E-2,0.1382013175178087,0.21073097333878832,0.2776883014507549,0.32932849114103496,0.39057192726739515,0.46320447356630112,0.5493441011825263,0.65150264888545451,0.7726590684983673,0.91634629138358015,1.0867542490174178,1.2888520517436506,1.5285328884480796,1.8127858724409558,2.149899844587571,2.5497050766034186,3.0238599226022878,3.586190777680494,4.2530952567580727,5.0440203504058019,5.1056454996416907,5.1680235520687887,5.2311637062565488,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary EV","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,1.4958315995699252E-2,5.3220099058599202E-2,0.14727335626364951,0.22456412333630468,0.29591677477701928,0.35094681494142688,0.41621049367795732,0.49361090533493301,0.58540505241104679,0.69426965993761136,0.8233792290050802,0.97649860548122347,1.1580927632325424,1.3734570031368825,1.6288713645013635,1.9317837515355454,2.2910271148631405,2.7170770211033872,3.2223571212726849,3.8216014254907225,4.5322839479519104,5.3751282506455684,5.4407986995329187,5.5072714749241145,5.5745563792162711,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary EVNon-Incentive CostsMarket Potential0","ID","Residential","Ancillary EV","Non-Incentive Costs","Market Potential",0,0,0,37880.480000000003,42254.080000000002,52725.02,49579.040000000001,48464.57,45401.14,47321.79,49599.61,52301.03,55504.81,59304.39,63810.55,69154.7,75492.67,83009.27,91923.7,102495.9,115034.15,129904.07,147539.28,168454,193258.12,47398.14,47548.72,47701.14,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVIncentive CostsMarket Potential0","ID","Residential","Ancillary EV","Incentive Costs","Market Potential",0,0,0,1122.95,3995.34,11056.11,16858.48,22215.06,26346.28,31245.75,37056.36,43947.53,52120.21,61812.73,73307.7,86940.34,103108.16,122282.63,145022.87,171991.99,203976.41,241908.79,286895.26,340247.62,403521.63,408451.64,413441.88,418493.1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary EVProgram Annual BenefitsMarket Potential0","ID","Residential","Ancillary EV","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary EVProgram Annual CostsMarket Potential0","ID","Residential","Ancillary EV","Program Annual Costs","Market Potential",0,0,0,39003.43,46249.42,63781.13,66437.509999999995,70679.64,71747.42,78567.55,86655.97,96248.56,107625.03,121117.11,137118.25,156095.04000000001,178600.83,205291.9,236946.57,274487.89,319010.56,371812.87,434434.54,508701.62,596779.75,455849.78,460990.6,466194.23,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartyParticipantsMarket Potential0","ID","General Service","Ancillary Third Party","Participants","Market Potential",0,40.983947278312499,165.88344127740004,432.32969475499993,514.6409204849374,520.73119856767778,526.89486802270142,533.1328026883632,539.44588689061766,545.83501556822546,552.30109439946057,558.84503993033513,565.46777970436085,572.17025239386339,578.95340793287244,585.81820765160057,592.76562441253577,599.7966427481615,606.91225900032896,614.11348146129683,621.40133051646092,628.77683878879316,636.24105128501117,643.79502554349733,651.43983178399037,659.17655305906897,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartyNew ParticipantsMarket Potential0","ID","General Service","Ancillary Third Party","New Participants","Market Potential",0,40.983947278312499,124.89949399908754,266.4462534775999,82.311225729937462,6.0902780827403831,6.1636694550236371,6.2379346656617827,6.3130842022544584,6.3891286776078005,6.4660788312351087,6.5439455308745664,6.6227397740257175,6.7024726895025424,6.7831555390090443,6.8647997187281362,6.947416760935198,7.0310183356257312,7.115616252167456,7.2012224609678697,7.287849055164088,7.3755082723322403,7.4642124962180105,7.5539742584861642,7.6448062404930397,7.7367212750785939,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartySummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Third Party","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.1653811618091385E-2,4.7175944981664011E-2,0.12295292753832129,0.14636382719764832,0.14809762371068247,0.14985213746294698,0.15162761632309882,0.15342431112594312,0.15524247570792934,0.15708236694307159,0.15894424477929911,0.16082837227524147,0.16273501563745421,0.16466444425809013,0.16661693075302089,0.16859275100041496,0.17059218417977781,0.17261551281145845,0.17466302279662935,0.17673500345774437,0.17883174757948134,0.18095355145017403,0.1831007149037405,0.1852735413621126,0.18747233787817402,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartySummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Third Party","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.241881033470949E-2,5.0272746144143232E-2,0.13102400632813438,0.15597168286194407,0.15781929210430784,0.15968897854107736,0.16158100631191263,0.16349564271733069,0.16543315825653168,0.16739382666567731,0.16937792495662735,0.17138573345613967,0.17341753584553943,0.1754736192008633,0.17755427403348348,0.17965979433121798,0.18179047759993372,0.18394662490564626,0.18612854091712419,0.18833653394900296,0.1905709160054149,0.19283200282414112,0.19512011392129208,0.19743557263652237,0.19977870617878732,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartyWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Third Party","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.1778464145154328E-2,4.7680552482734118E-2,0.12426806747962994,0.14792937686746346,0.14968171856758705,0.15145499910450144,0.15324946899813804,0.1550653817663035,0.15690299396055493,0.15876256520250503,0.16064435822056097,0.16254863888710316,0.16447567625610923,0.16642574260122805,0.16839911345430916,0.17039606764439355,0.17241688733717098,0.17446185807490955,0.17653126881686304,0.17862541198016171,0.18074458348119263,0.1828890827774749,0.18505921291003666,0.18725528054629817,0.18947759602346911,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartyWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Third Party","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.255164550847648E-2,5.0810477922777195E-2,0.13242547685382561,0.15764000092440694,0.15950737272760768,0.16139705786924705,0.16330932331429884,0.16524443922240356,0.16720267898609861,0.16918431926950664,0.1711896400474861,0.1732189246452506,0.17527245977846251,0.17735053559380654,0.17945344571004812,0.18158148725958392,0.18373496093048911,0.18591417100906815,0.18811942542291457,0.19035103578448606,0.19260931743520102,0.19489458949006278,0.19720717488281825,0.1995474004116562,0.20191559678545301,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary Third PartyNon-Incentive CostsMarket Potential0","ID","General Service","Ancillary Third Party","Non-Incentive Costs","Market Potential",0,471.14,1907.22,4970.72,5917.18,5987.27,6058.2,6129.98,6202.62,6276.12,6350.5,6425.77,6501.95,6579.03,6657.03,6735.96,6815.84,6896.68,6978.47,7061.25,7145.02,7229.78,7315.56,7402.37,7490.21,7579.1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartyIncentive CostsMarket Potential0","ID","General Service","Ancillary Third Party","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Third PartyProgram Annual BenefitsMarket Potential0","ID","General Service","Ancillary Third Party","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary Third PartyProgram Annual CostsMarket Potential0","ID","General Service","Ancillary Third Party","Program Annual Costs","Market Potential",0,471.14,1907.22,4970.72,5917.18,5987.27,6058.2,6129.98,6202.62,6276.12,6350.5,6425.77,6501.95,6579.03,6657.03,6735.96,6815.84,6896.68,6978.47,7061.25,7145.02,7229.78,7315.56,7402.37,7490.21,7579.1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartyParticipantsMarket Potential0","ID","Large General Service","Ancillary Third Party","Participants","Market Potential",0,3.6538802204275211,14.590520780787902,37.51528144032811,44.060045858571129,43.986881689391907,43.916055702712647,43.847493340613347,43.781122422612441,43.716873069857073,43.654677631730834,43.594470614801565,43.536188614035048,43.479770246201888,43.425156085408013,43.372288600680825,43.321112095545622,43.271572649528665,43.223618061525627,43.177197794975825,43.132262924784676,43.088766085938722,43.046661423758998,43.005904545740933,42.96645247492966,42.928263604782316,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartyNew ParticipantsMarket Potential0","ID","Large General Service","Ancillary Third Party","New Participants","Market Potential",0,3.6538802204275211,10.936640560360381,22.924760659540208,6.5447644182430196,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartySummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Ancillary Third Party","Summer Peak Reduction @Meter  (MW)","Market Potential",0,5.092514149696642E-2,0.20297951477215384,0.52099514998671037,0.61084957370971549,0.60882957851374564,0.60687338453481066,0.60497895827020409,0.60314433103060205,0.60136759687427954,0.59964691060717046,0.59798048584667074,0.59636659314715357,0.59480355818523023,0.59328976000285072,0.59182362930640153,0.59040364682001834,0.58902834169137885,0.58769628994831213,0.58640611300459655,0.58515647621338374,0.58394608746672894,0.58277369583975858,0.58163809027804958,0.58053809832684811,0.57947258490079145,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartySummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Ancillary Third Party","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.4268053598642819E-2,0.21630383074611448,0.55519517262010909,0.65094796857386561,0.64879537352274685,0.64671076783334469,0.6446919845164153,0.64273692565068419,0.64084356018145727,0.63900992178939731,0.63723410682722803,0.63551427232220115,0.63384863404223168,0.63223546462366875,0.63067309175873987,0.62915989644076975,0.62769431126532271,0.62627481878549884,0.62489994991964681,0.6235682824098292,0.62227843932942128,0.62102908763827636,0.61981893678394029,0.61864673734745113,0.61751127973230124,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartyWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Ancillary Third Party","Winter Peak Reduction @Meter  (MW)","Market Potential",0,5.1469851484279093E-2,0.2051506421498335,0.52656786423348623,0.61738339676379961,0.61534179511716069,0.61336467712375808,0.61144998752995439,0.60959573658875765,0.60779999797194084,0.60606090674871027,0.60437665742879898,0.60274550206793165,0.60116574843367387,0.59963575822974113,0.59815394537690347,0.59671877434868392,0.59532875856010026,0.59398245880776479,0.59267848175970039,0.59141547849329101,0.59019214307983392,0.58900721121420174,0.5878594588881848,0.58674770110611518,0.58567079064143046,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartyWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Ancillary Third Party","Winter Peak Reduction @Generation (MW)","Market Potential",0,5.4848520337040803E-2,0.21861747884679614,0.56113370016356157,0.65791069561359716,0.65573507578555057,0.65362817255302441,0.65158779574803327,0.64961182500933257,0.64769820755748175,0.64584495604082504,0.64405014645012681,0.64231191609967142,0.64062846167271303,0.63899803732922111,0.63741895287393802,0.63588957198282603,0.63440831048604029,0.63297363470563173,0.63158405984622801,0.63023814843701087,0.62893450882335245,0.6276717937065236,0.62644869872994968,0.6252639611105234,0.62411635831354484,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceAncillary Third PartyNon-Incentive CostsMarket Potential0","ID","Large General Service","Ancillary Third Party","Non-Incentive Costs","Market Potential",0,2058.79,8206.0300000000007,21062.71,24695.34,24613.67,24534.59,24458,24383.83,24312,24242.44,24175.07,24109.82,24046.63,23985.43,23926.16,23868.75,23813.15,23759.3,23707.14,23656.62,23607.69,23560.29,23514.38,23469.91,23426.83,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartyIncentive CostsMarket Potential0","ID","Large General Service","Ancillary Third Party","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Third PartyProgram Annual BenefitsMarket Potential0","ID","Large General Service","Ancillary Third Party","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceAncillary Third PartyProgram Annual CostsMarket Potential0","ID","Large General Service","Ancillary Third Party","Program Annual Costs","Market Potential",0,2058.79,8206.0300000000007,21062.71,24695.34,24613.67,24534.59,24458,24383.83,24312,24242.44,24175.07,24109.82,24046.63,23985.43,23926.16,23868.75,23813.15,23759.3,23707.14,23656.62,23607.69,23560.29,23514.38,23469.91,23426.83,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartyParticipantsMarket Potential0","ID","Extra Large General Service","Ancillary Third Party","Participants","Market Potential",0,0.11380050000000001,0.22760100000000003,0.38692169999999998,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0.45520200000000005,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartyNew ParticipantsMarket Potential0","ID","Extra Large General Service","Ancillary Third Party","New Participants","Market Potential",0,0.11380050000000001,0.11380050000000001,0.15932069999999995,6.8280300000000071E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartySummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Ancillary Third Party","Summer Peak Reduction @Meter  (MW)","Market Potential",0,7.7700043111801412E-2,0.15466936867917436,0.2615861850736016,0.30620725222253581,0.30471359823689775,0.30326600247816687,0.30186302296034645,0.30050326284491008,0.29918536902726811,0.29790803076749195,0.29666997836390946,0.29546998186822776,0.29430684984088612,0.29317942814537667,0.29208659878031512,0.29102727874807688,0.29000041895885675,0.28900500316904104,0.28804004695281837,0.28710459670598881,0.28619772868096272,0.28531854805197382,0.28446618800955786,0.28363980888338508,0.28283859729255362,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartySummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Ancillary Third Party","Summer Peak Reduction @Generation (MW)","Market Potential",0,8.2800557450768766E-2,0.16482243039127703,0.27875765672804942,0.32630781353637661,0.32471611065313061,0.32317348942686153,0.32167841321435042,0.32022939348349327,0.31882498830697797,0.31746380090312443,0.31614447822240993,0.31486570957824783,0.31362622532063739,0.31242479555133917,0.31126022887927868,0.31013137121491569,0.30903710460236228,0.3079763460880659,0.30694804662491298,0.30595119001064452,0.30498479185950844,0.3040478986061102,0.30313958654044953,0.3022589608731725,0.30140515483008695,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartyWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Ancillary Third Party","Winter Peak Reduction @Meter  (MW)","Market Potential",0,8.0322206367305374E-2,0.15988903547805838,0.2704140010589865,0.31654090678938657,0.31499684608013917,0.31350039793657869,0.31205007170963783,0.31064442342132281,0.30928205430347655,0.30796160938229472,0.3066817761071573,0.3054412830223916,0.30423889848062075,0.30307342939639664,0.30194372003885595,0.3008486508621756,0.29978713737264834,0.29875812903122689,0.29776060819042977,0.29679358906453202,0.29585611673199758,0.29494726616914552,0.29406614131407094,0.29321187415987415,0.29238362387627981,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartyWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Ancillary Third Party","Winter Peak Reduction @Generation (MW)","Market Potential",0,8.5594849070018519E-2,0.17038473516417132,0.28816496276533088,0.33731980689406071,0.33567438840594538,0.33407970794605574,0.33253417701368054,0.33103625684284188,0.32958445684513699,0.32817733310133707,0.32681348690021023,0.3254915633230942,0.32421024987278424,0.3229682751453502,0.32176440754353786,0.32059745403045142,0.31946625892225949,0.31836970271869874,0.3173067009701937,0.31627620318044758,0.31527719174339042,0.31430868091341169,0.31336971580783346,0.31245937144061608,0.31157675178631694,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceAncillary Third PartyNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Ancillary Third Party","Non-Incentive Costs","Market Potential",0,3212.89,6395.56,10816.56,12661.64,12599.87,12540.02,12482,12425.78,12371.28,12318.46,12267.27,12217.65,12169.56,12122.94,12077.75,12033.95,11991.49,11950.33,11910.42,11871.74,11834.24,11797.89,11762.65,11728.48,11695.35,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartyIncentive CostsMarket Potential0","ID","Extra Large General Service","Ancillary Third Party","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Third PartyProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Ancillary Third Party","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceAncillary Third PartyProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Ancillary Third Party","Program Annual Costs","Market Potential",0,3212.89,6395.56,10816.56,12661.64,12599.87,12540.02,12482,12425.78,12371.28,12318.46,12267.27,12217.65,12169.56,12122.94,12077.75,12033.95,11991.49,11950.33,11910.42,11871.74,11834.24,11797.89,11762.65,11728.48,11695.35,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary Battery StorageParticipantsMarket Potential0","ID","Residential","Ancillary Battery Storage","Participants","Market Potential",0,3.9862906578001924,24.230548836200345,61.982294923023893,100.3832984474747,139.71337603444019,179.98949756339388,221.22890889205408,276.62159287020273,333.3347712990589,391.39244210056478,464.480174068971,539.2953780846218,615.86935526206855,708.40195275797191,717.05682982526866,725.81744756247519,734.68509785267486,743.66108836248941,752.74674273491371,761.94340078450625,771.25241869496494,780.67516921911636,790.21304188134911,799.86744318251863,809.63979680735792,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary Battery StorageNew ParticipantsMarket Potential0","ID","Residential","Ancillary Battery Storage","New Participants","Market Potential",0,3.9862906578001924,20.244258178400152,37.751746086823545,38.401003524450807,39.330077586965487,40.276121528953695,41.239411328660196,55.392683978148654,56.713178428856168,58.057670801505878,73.087731968406217,74.815204015650806,76.57397717744675,92.53259749590336,8.6548770672967521,8.7606177372065304,8.8676502901996628,8.9759905098145509,9.0856543724243011,9.1966580495925427,9.3090179104586923,9.4227505241514109,9.5378726622327576,9.6544013011695142,9.7723536248392975,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Residential","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,7.9725813156003855E-3,4.8461097672400692E-2,0.12396458984604779,0.20076659689494941,0.2794267520688804,0.35997899512678777,0.44245781778410814,0.55324318574040543,0.66666954259811784,0.78278488420112957,0.92896034813794204,1.0785907561692436,1.2317387105241371,1.4168039055159438,1.4341136596505373,1.4516348951249505,1.4693701957053498,1.4873221767249789,1.5054934854698274,1.5238868015690126,1.5425048373899299,1.5613503384382328,1.5804260837626982,1.5997348863650374,1.6192795936147157,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,8.4959306432229164E-3,5.1642260946718553E-2,0.1321020778410569,0.21394564886503561,0.29776934363691432,0.38360932984525553,0.47150236336754919,0.58956008710614394,0.71043216389398745,0.83416974019728218,0.98994069494665604,1.1493933889271564,1.3125945338066252,1.5098080834568881,1.5282541130120815,1.5469255063138858,1.5658250167363061,1.5849554312926033,1.6043195710462781,1.6239202915270807,1.6437604831520993,1.6638430716519956,1.684171018502449,1.7047473213608668,1.7255750145084354,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B966&C966&D966&E966&F966&G966","v":"IDResidentialAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0"},"ID","Residential","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,7.9725813156003855E-3,4.8461097672400692E-2,0.12396458984604779,0.20076659689494941,0.2794267520688804,0.35997899512678777,0.44245781778410814,0.55324318574040543,0.66666954259811784,0.78278488420112957,0.92896034813794204,1.0785907561692436,1.2317387105241371,1.4168039055159438,1.4341136596505373,1.4516348951249505,1.4693701957053498,1.4873221767249789,1.5054934854698274,1.5238868015690126,1.5425048373899299,1.5613503384382328,1.5804260837626982,1.5997348863650374,1.6192795936147157,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Residential","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,8.4959306432229164E-3,5.1642260946718553E-2,0.1321020778410569,0.21394564886503561,0.29776934363691432,0.38360932984525553,0.47150236336754919,0.58956008710614394,0.71043216389398745,0.83416974019728218,0.98994069494665604,1.1493933889271564,1.3125945338066252,1.5098080834568881,1.5282541130120815,1.5469255063138858,1.5658250167363061,1.5849554312926033,1.6043195710462781,1.6239202915270807,1.6437604831520993,1.6638430716519956,1.684171018502449,1.7047473213608668,1.7255750145084354,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary Battery StorageNon-Incentive CostsMarket Potential0","ID","Residential","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,28305.34,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary Battery StorageIncentive CostsMarket Potential0","ID","Residential","Ancillary Battery Storage","Incentive Costs","Market Potential",0,79.73,484.61,1239.6500000000001,2007.67,2794.27,3599.79,4424.58,5532.43,6666.7,7827.85,9289.6,10785.91,12317.39,14168.04,14341.14,14516.35,14693.7,14873.22,15054.93,15238.87,15425.05,15613.5,15804.26,15997.35,16192.8,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDResidentialAncillary Battery StorageProgram Annual BenefitsMarket Potential0","ID","Residential","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDResidentialAncillary Battery StorageProgram Annual CostsMarket Potential0","ID","Residential","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,28385.07,28789.95,29544.99,30313.01,31099.61,31905.13,32729.919999999998,33837.769999999997,34972.04,36133.19,37594.949999999997,39091.25,40622.730000000003,42473.38,42646.48,42821.69,42999.05,43178.559999999998,43360.28,43544.21,43730.39,43918.85,44109.599999999999,44302.69,44498.14,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageParticipantsMarket Potential0","ID","General Service","Ancillary Battery Storage","Participants","Market Potential",0,0.55760472487500001,3.3853763526000002,8.6500539166666659,14.003834571018707,19.483140082464136,25.090231810604834,30.827406958170666,38.531849063615553,46.414542140155227,54.478679379538626,64.628337951127193,75.011032001598892,85.630922126972763,98.461463934161969,99.628946879523923,100.81048034226798,102.00623175989142,103.21637057828724,104.44106827573076,105.68049838715322,106.93483652870633,108.20426042262096,109.4889499223635,110.78908703809361,112.1048559624267,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageNew ParticipantsMarket Potential0","ID","General Service","Ancillary Battery Storage","New Participants","Market Potential",0,0.55760472487500001,2.8277716277250002,5.2646775640666661,5.3537806543520414,5.4793055114454283,5.6070917281406985,5.7371751475658321,7.7044421054448868,7.8826930765396739,8.064137239383399,10.149658571588567,10.382694050471699,10.619890125373871,12.830541807189206,1.1674829453619537,1.1815334627440564,1.1957514176234412,1.2101388183958193,1.2246976974435171,1.2394301114224646,1.2543381415531059,1.2694238939146345,1.2846894997425409,1.3001371157301094,1.315768924333085,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.1152094497500001E-3,6.7707527052000005E-3,1.7300107833333331E-2,2.8007669142037415E-2,3.8966280164928271E-2,5.0180463621209669E-2,6.1654813916341332E-2,7.7063698127231101E-2,9.2829084280310448E-2,0.10895735875907725,0.1292566759022544,0.15002206400319779,0.17126184425394553,0.19692292786832394,0.19925789375904784,0.20162096068453597,0.20401246351978283,0.20643274115657448,0.20888213655146151,0.21136099677430645,0.21386967305741267,0.21640852084524193,0.21897789984472701,0.22157817407618721,0.22420971192485339,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.1884158671675192E-3,7.2152096176470596E-3,1.8435750035521451E-2,2.9846194737891532E-2,4.1524168973708732E-2,5.3474492349967678E-2,6.5702060865666378E-2,8.2122440459538676E-2,9.8922724083877284E-2,0.11610971734769528,0.13774155573556521,0.15987005967945203,0.1825040966048013,0.20984966737886182,0.21233790895039198,0.21485609621114235,0.21740458601852392,0.21998373951041611,0.2225939221562889,0.22523550380893695,0.22790885875683362,0.23061436577711203,0.23335240818918054,0.23612337390898039,0.23892765550389322,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","General Service","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.1152094497500001E-3,6.7707527052000005E-3,1.7300107833333331E-2,2.8007669142037415E-2,3.8966280164928271E-2,5.0180463621209669E-2,6.1654813916341332E-2,7.7063698127231101E-2,9.2829084280310448E-2,0.10895735875907725,0.1292566759022544,0.15002206400319779,0.17126184425394553,0.19692292786832394,0.19925789375904784,0.20162096068453597,0.20401246351978283,0.20643274115657448,0.20888213655146151,0.21136099677430645,0.21386967305741267,0.21640852084524193,0.21897789984472701,0.22157817407618721,0.22420971192485339,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","General Service","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.1884158671675192E-3,7.2152096176470596E-3,1.8435750035521451E-2,2.9846194737891532E-2,4.1524168973708732E-2,5.3474492349967678E-2,6.5702060865666378E-2,8.2122440459538676E-2,9.8922724083877284E-2,0.11610971734769528,0.13774155573556521,0.15987005967945203,0.1825040966048013,0.20984966737886182,0.21233790895039198,0.21485609621114235,0.21740458601852392,0.21998373951041611,0.2225939221562889,0.22523550380893695,0.22790885875683362,0.23061436577711203,0.23335240818918054,0.23612337390898039,0.23892765550389322,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary Battery StorageNon-Incentive CostsMarket Potential0","ID","General Service","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,4064.67,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageIncentive CostsMarket Potential0","ID","General Service","Ancillary Battery Storage","Incentive Costs","Market Potential",0,11.15,67.709999999999994,173,280.08,389.66,501.8,616.54999999999995,770.64,928.29,1089.57,1292.57,1500.22,1712.62,1969.23,1992.58,2016.21,2040.12,2064.33,2088.8200000000002,2113.61,2138.6999999999998,2164.09,2189.7800000000002,2215.7800000000002,2242.1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDGeneral ServiceAncillary Battery StorageProgram Annual BenefitsMarket Potential0","ID","General Service","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDGeneral ServiceAncillary Battery StorageProgram Annual CostsMarket Potential0","ID","General Service","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,4075.82,4132.37,4237.67,4344.74,4454.33,4566.47,4681.21,4835.3,4992.96,5154.24,5357.23,5564.89,5777.29,6033.9,6057.25,6080.88,6104.79,6128.99,6153.49,6178.28,6203.36,6228.75,6254.45,6280.45,6306.76,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageParticipantsMarket Potential0","ID","Large General Service","Ancillary Battery Storage","Participants","Market Potential",0,3.340079729811711E-2,0.2000619879444385,0.50431492782937315,0.80552211451293254,1.1057536875161365,1.4050568578042348,1.7034768197596484,2.1011096733736947,2.4976503193620068,2.8931524551400747,3.3872937540638355,3.880230714263373,4.372023151955946,4.9619676499620642,4.9559267563280809,4.9500790821730458,4.9444184662837269,4.9389389439103279,4.9336347405018302,4.9285002656411034,4.9235301071733986,4.9187190255220763,4.914061948185581,4.9095539644098976,4.9051903200308873,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageNew ParticipantsMarket Potential0","ID","Large General Service","Ancillary Battery Storage","New Participants","Market Potential",0,3.340079729811711E-2,0.1666611906463214,0.30425293988493463,0.30120718668355939,0.30023157300320391,0.29930317028809839,0.29841996195541354,0.39763285361404632,0.39654064598831207,0.39550213577806792,0.4941412989237608,0.49293696019953748,0.49179243769257308,0.58994449800611815,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,5.010119594717567E-4,3.0009298191665773E-3,7.5647239174405972E-3,1.2082831717693988E-2,1.658630531274205E-2,2.1075852867063524E-2,2.5552152296394726E-2,3.1516645100605423E-2,3.7464754790430099E-2,4.3397286827101117E-2,5.0809406310957532E-2,5.8203460713950592E-2,6.5580347279339188E-2,7.4429514749430964E-2,7.4338901344921215E-2,7.425118623259569E-2,7.4166276994255903E-2,7.4084084158654917E-2,7.4004521107527449E-2,7.3927503984616547E-2,7.385295160760097E-2,7.3780785382831143E-2,7.3710929222783717E-2,7.3643309466148471E-2,7.3577854800463319E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.3390021256581068E-4,3.1979218021809222E-3,8.0612999972725884E-3,1.2875992879043039E-2,1.7675090912981722E-2,2.2459348750067692E-2,2.7229488806899751E-2,3.3585512681804583E-2,3.9924077994916984E-2,4.6246043080883543E-2,5.4144721132733942E-2,6.20241482458979E-2,6.9885280561955657E-2,7.9315339673306659E-2,7.9218778074297974E-2,7.9125305021947659E-2,7.9034822031389493E-2,7.8947233758157417E-2,7.8862447898047153E-2,7.8780375090171079E-2,7.8700928823104185E-2,7.8624025344022963E-2,7.8549583570741391E-2,7.8477525006552085E-2,7.8407773657782731E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,5.010119594717567E-4,3.0009298191665773E-3,7.5647239174405972E-3,1.2082831717693988E-2,1.658630531274205E-2,2.1075852867063524E-2,2.5552152296394726E-2,3.1516645100605423E-2,3.7464754790430099E-2,4.3397286827101117E-2,5.0809406310957532E-2,5.8203460713950592E-2,6.5580347279339188E-2,7.4429514749430964E-2,7.4338901344921215E-2,7.425118623259569E-2,7.4166276994255903E-2,7.4084084158654917E-2,7.4004521107527449E-2,7.3927503984616547E-2,7.385295160760097E-2,7.3780785382831143E-2,7.3710929222783717E-2,7.3643309466148471E-2,7.3577854800463319E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,5.3390021256581068E-4,3.1979218021809222E-3,8.0612999972725884E-3,1.2875992879043039E-2,1.7675090912981722E-2,2.2459348750067692E-2,2.7229488806899751E-2,3.3585512681804583E-2,3.9924077994916984E-2,4.6246043080883543E-2,5.4144721132733942E-2,6.20241482458979E-2,6.9885280561955657E-2,7.9315339673306659E-2,7.9218778074297974E-2,7.9125305021947659E-2,7.9034822031389493E-2,7.8947233758157417E-2,7.8862447898047153E-2,7.8780375090171079E-2,7.8700928823104185E-2,7.8624025344022963E-2,7.8549583570741391E-2,7.8477525006552085E-2,7.8407773657782731E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceAncillary Battery StorageNon-Incentive CostsMarket Potential0","ID","Large General Service","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,1640.85,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageIncentive CostsMarket Potential0","ID","Large General Service","Ancillary Battery Storage","Incentive Costs","Market Potential",0,0.67,4,10.09,16.11,22.12,28.1,34.07,42.02,49.95,57.86,67.75,77.599999999999994,87.44,99.24,99.12,99,98.89,98.78,98.67,98.57,98.47,98.37,98.28,98.19,98.1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDLarge General ServiceAncillary Battery StorageProgram Annual BenefitsMarket Potential0","ID","Large General Service","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDLarge General ServiceAncillary Battery StorageProgram Annual CostsMarket Potential0","ID","Large General Service","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,1641.52,1644.85,1650.94,1656.96,1662.97,1668.95,1674.92,1682.87,1690.8,1698.71,1708.6,1718.45,1728.29,1740.09,1739.97,1739.85,1739.74,1739.63,1739.52,1739.42,1739.32,1739.22,1739.13,1739.04,1738.95,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageParticipantsMarket Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Participants","Market Potential",0,1.1000000000000001E-3,3.2999999999999995E-3,5.4999999999999997E-3,8.8000000000000005E-3,1.2100000000000001E-2,1.5400000000000002E-2,1.8700000000000001E-2,2.3100000000000002E-2,2.75E-2,3.1899999999999998E-2,3.7399999999999996E-2,4.2900000000000001E-2,4.8399999999999992E-2,5.4999999999999993E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,5.5E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageNew ParticipantsMarket Potential0","ID","Extra Large General Service","Ancillary Battery Storage","New Participants","Market Potential",0,1.1000000000000001E-3,2.1999999999999997E-3,2.2000000000000001E-3,3.3000000000000008E-3,3.3000000000000008E-3,3.3000000000000008E-3,3.2999999999999991E-3,4.4000000000000011E-3,4.3999999999999977E-3,4.3999999999999977E-3,5.4999999999999979E-3,5.5000000000000049E-3,5.499999999999991E-3,6.6000000000000017E-3,6.9388939039072284E-18,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.6500000000000001E-5,4.9499999999999997E-5,8.2499999999999986E-5,1.3200000000000001E-4,1.8150000000000002E-4,2.3100000000000003E-4,2.8050000000000004E-4,3.4650000000000002E-4,4.125E-4,4.7849999999999998E-4,5.6099999999999998E-4,6.4349999999999997E-4,7.2599999999999987E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.7583120204603582E-5,5.2749360613810737E-5,8.7915601023017882E-5,1.4066496163682866E-4,1.9341432225063941E-4,2.4616368286445013E-4,2.9891304347826091E-4,3.6924552429667523E-4,4.3957800511508949E-4,5.0991048593350375E-4,5.9782608695652171E-4,6.8574168797953957E-4,7.7365728900255742E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.6500000000000001E-5,4.9499999999999997E-5,8.2499999999999986E-5,1.3200000000000001E-4,1.8150000000000002E-4,2.3100000000000003E-4,2.8050000000000004E-4,3.4650000000000002E-4,4.125E-4,4.7849999999999998E-4,5.6099999999999998E-4,6.4349999999999997E-4,7.2599999999999987E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,8.25E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.7583120204603582E-5,5.2749360613810737E-5,8.7915601023017882E-5,1.4066496163682866E-4,1.9341432225063941E-4,2.4616368286445013E-4,2.9891304347826091E-4,3.6924552429667523E-4,4.3957800511508949E-4,5.0991048593350375E-4,5.9782608695652171E-4,6.8574168797953957E-4,7.7365728900255742E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,8.7915601023017898E-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceAncillary Battery StorageNon-Incentive CostsMarket Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,16.190000000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageIncentive CostsMarket Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Incentive Costs","Market Potential",0,0.02,7.0000000000000007E-2,0.11,0.18,0.24,0.31,0.37,0.46,0.55000000000000004,0.64,0.75,0.86,0.97,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["IDExtra Large General ServiceAncillary Battery StorageProgram Annual BenefitsMarket Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["IDExtra Large General ServiceAncillary Battery StorageProgram Annual CostsMarket Potential0","ID","Extra Large General Service","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,16.22,16.260000000000002,16.3,16.37,16.440000000000001,16.5,16.57,16.66,16.739999999999998,16.829999999999998,16.940000000000001,17.05,17.16,17.29,17.29,17.29,17.29,17.29,17.29,17.29,17.29,17.29,17.29,17.29,17.29,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingParticipantsMarket Potential0","WA","Residential","Ancillary Cooling","Participants","Market Potential",0,763.8068462612257,2445.2745517446924,6092.1292388414786,8358.2206265559034,9909.9525427787739,10574.791861714153,11284.233949239437,12041.271117796474,12849.096428211866,13711.117157513165,14630.969170274489,15612.532254107615,16659.946483981115,17777.629684389671,18970.296063026126,20242.9760945501,21601.037738319807,23050.209079579839,24596.602489602054,26246.740406682933,27911.492478043943,28166.150431005477,28423.13182378513,28682.457854906348,28944.14991630298,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingNew ParticipantsMarket Potential0","WA","Residential","Ancillary Cooling","New Participants","Market Potential",0,763.8068462612257,1681.4677054834667,3646.8546870967862,2266.0913877144249,1551.7319162228705,664.8393189353792,709.44208752528357,757.03716855703715,807.82531041539187,862.02072930129907,919.85201276132466,981.56308383312535,1047.4142298735005,1117.6832004085554,1192.6663786364552,1272.6800315239743,1358.0616437697063,1449.1713412600329,1546.3934100222141,1650.1379170808796,1664.7520713610102,254.65795296153374,256.98139277965311,259.32603112121797,261.6920613966322,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.19095171156530644,0.61131863793617314,1.5230323097103697,2.0895551566389758,2.4774881356946934,2.6436979654285384,2.821058487309859,3.0103177794491183,3.2122741070529663,3.4277792893782912,3.6577422925686225,3.9031330635269037,4.1649866209952791,4.4444074210974174,4.7425740157565315,5.0607440236375254,5.4002594345799517,5.7625522698949601,6.149150622400513,6.5616851016707329,6.9778731195109858,7.0415376077513692,7.1057829559462826,7.1706144637265874,7.2360374790757449,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.20348647865015604,0.65144782388765254,1.6230097077049976,2.2267211814140833,2.6401194966908497,2.8172399461088431,3.0062430597931149,3.207926022430859,3.4231395002695719,3.6527912290902504,3.8978498428906887,4.1593489594276463,4.4383915398500413,4.7361545408113992,5.0538938786834304,5.3929497268089568,5.7547521681372036,6.1408272270832907,6.5528033060534021,6.9924180537838163,7.4359261716868987,7.5037698292320645,7.5722324764985958,7.6413197610044623,7.7110373817942719,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary CoolingNon-Incentive CostsMarket Potential0","WA","Residential","Ancillary Cooling","Non-Incentive Costs","Market Potential",0,72141.67,127201.32,245124.54,162278.75,119417.18,66203.62,68879.789999999994,71735.490000000005,74782.78,78034.509999999995,81504.38,85207.05,89158.12,93374.25,97873.24,102674.06,107796.96,113263.54,119096.87,125321.54,126198.39,41592.74,41732.15,41872.82,42014.79,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingIncentive CostsMarket Potential0","WA","Residential","Ancillary Cooling","Incentive Costs","Market Potential",0,15276.14,48905.49,121842.58,167164.41,198199.05,211495.84,225684.68,240825.42,256981.93,274222.34000000003,292619.38,312250.65000000002,333198.93,355552.59,379405.92,404859.52,432020.75,461004.18,491932.05,524934.81000000006,558229.85,563323.01,568462.64,573649.16,578883,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary CoolingProgram Annual BenefitsMarket Potential0","WA","Residential","Ancillary Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary CoolingProgram Annual CostsMarket Potential0","WA","Residential","Ancillary Cooling","Program Annual Costs","Market Potential",0,87417.81,176106.82,366967.13,329443.15999999997,317616.23,277699.46000000002,294564.46999999997,312560.90999999997,331764.71000000002,352256.85,374123.77,397457.69,422357.05,448926.85,477279.17,507533.59,539817.72,574267.72,611028.92000000004,650256.35,684428.24,604915.75,610194.78,615521.98,620897.78,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingParticipantsMarket Potential0","WA","General Service","Ancillary Cooling","Participants","Market Potential",0,75.839848598524796,242.95053081477266,605.56834674166441,831.31036253123216,986.22602438325066,1053.0098787283443,1124.3166543181599,1200.4526964015383,1281.745101326173,1368.5431222725811,1461.219670222164,1560.1729166115008,1665.8280045621955,1778.6388760423542,1899.0902228141929,2027.6995695544326,2165.0194981023806,2311.6400223973228,2468.1911243147019,2635.3454613022896,2804.1674032286719,2831.4392836030297,2858.977588449764,2886.7849205229481,2914.8639080034795,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingNew ParticipantsMarket Potential0","WA","General Service","Ancillary Cooling","New Participants","Market Potential",0,75.839848598524796,167.11068221624788,362.61781592689175,225.74201578956774,154.9156618520185,66.783854345093687,71.306775589815516,76.13604208337847,81.292404924634639,86.798020946408087,92.676547949582982,98.953246389336755,105.65508795069468,112.81087148015877,120.45134677183864,128.60934674023974,137.31992854794794,146.62052429494224,156.55110191737913,167.15433698758761,168.82194192638235,27.271880374357806,27.538304846734263,27.80733207318417,28.078987480531396,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Cooling","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.7399905374077997E-2,0.15184408175923292,0.37848021671354026,0.51956897658202017,0.61639126523953169,0.65813117420521516,0.70269790894884987,0.75028293525096146,0.8010906883288581,0.85533945142036316,0.91326229388885261,0.97510807288218804,1.0411425028513723,1.1116492975264713,1.1869313892588704,1.2673122309715203,1.353137186313988,1.4447750139983269,1.5426194526966888,1.6470909133139309,1.7526046270179199,1.7696495522518936,1.7868609927811026,1.8042405753268427,1.8217899425021746,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Cooling","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.051140811389386E-2,0.16181168132910584,0.403325039123551,0.553675379989365,0.65685343695602272,0.70133330584528464,0.74882556367098241,0.79953424472608847,0.85367720410151116,0.91148705394326845,0.9732121631381635,1.0391177247252643,1.109486895621667,1.1846220135618835,1.2648458964821723,1.3505032299355502,1.4419620485016922,1.5396153175600245,1.6438826222257978,1.755211970709645,1.8676519895757884,1.8858158058950272,1.9041570681810556,1.9226775099390907,1.941378881609308,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Cooling","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Cooling","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary CoolingNon-Incentive CostsMarket Potential0","WA","General Service","Ancillary Cooling","Non-Incentive Costs","Market Potential",0,11132.72,17978.03,32641.06,22375.38,17063.400000000001,10453.52,10792.73,11154.93,11541.66,11954.58,12395.47,12866.22,13368.86,13905.54,14478.58,15090.43,15743.72,16441.27,17186.060000000001,17981.3,18106.37,7490.12,7510.1,7530.28,7550.65,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingIncentive CostsMarket Potential0","WA","General Service","Ancillary Cooling","Incentive Costs","Market Potential",0,1516.8,4859.01,12111.37,16626.21,19724.52,21060.2,22486.33,24009.05,25634.9,27370.86,29224.39,31203.46,33316.559999999998,35572.78,37981.800000000003,40553.99,43300.39,46232.800000000003,49363.82,52706.91,56083.35,56628.79,57179.55,57735.7,58297.279999999999,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary CoolingProgram Annual BenefitsMarket Potential0","WA","General Service","Ancillary Cooling","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary CoolingProgram Annual CostsMarket Potential0","WA","General Service","Ancillary Cooling","Program Annual Costs","Market Potential",0,12649.51,22837.040000000001,44752.43,39001.589999999997,36787.919999999998,31513.71,33279.07,35163.980000000003,37176.559999999998,39325.440000000002,41619.86,44069.68,46685.42,49478.32,52460.38,55644.42,59044.11,62674.07,66549.88,70688.210000000006,74189.72,64118.9,64689.65,65265.97,65847.929999999993,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary HeatingParticipantsMarket Potential0","WA","Residential","Ancillary Heating","Participants","Market Potential",0,237.25070981788457,718.28332307636174,1692.3159373244366,2195.6865860114972,2461.9105763847051,2484.3724747675897,2507.0393102768689,2529.9129527111249,2552.9952889285478,2576.2882230025825,2599.7936763789949,2623.5135880343755,2647.449914636084,2671.6046307036595,2695.9797287716947,2720.5772195542049,2745.3991321104913,2770.4475140125196,2795.7244315138241,2821.2319697199555,2846.9722327604823,2872.9473439625585,2899.1594460260831,2925.6107012004472,2952.3032914629039,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary HeatingNew ParticipantsMarket Potential0","WA","Residential","Ancillary Heating","New Participants","Market Potential",0,237.25070981788457,481.03261325847717,974.03261424807488,503.37064868706057,266.22399037320793,22.461898382884556,22.666835509279281,22.873642434255999,23.082336217422835,23.292934074034747,23.505453376412333,23.719911655380656,23.936326601708515,24.154716067575464,24.375098068035186,24.597490782510249,24.821912556286406,25.048381902028268,25.276917501304524,25.507538206131358,25.74026304052677,25.975111202076278,26.212102063524526,26.451255174364178,26.692590262456633,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary HeatingSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.12930163685074708,0.39146441107661717,0.92231218584181807,1.1966491893762661,1.3417412641296644,1.3539829987483365,1.3663364241008937,1.3788025592275632,1.3913824324660586,1.4040770815364076,1.4168875536265524,1.4298149054787348,1.442860203476666,1.4560245237334946,1.4693089521805738,1.4827145846570418,1.496242527000218,1.5098938951368235,1.5236698151750343,1.5375714234973759,1.5515998668544631,1.5657563024595944,1.5800418980842152,1.5944578321542437,1.6090052938472827,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary HeatingWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.13778946808476883,0.41716156338087934,0.98285612301984027,1.2752016084572315,1.4298180564041607,1.4428633831504012,1.4560277324178321,1.4693121901401995,1.4827178521590565,1.4962458243141599,1.5098972225346892,1.5236731729313031,1.5375748118890302,1.551603286161013,1.5657597529631007,1.5800453800693113,1.5944613459081607,1.6090088396598716,1.6236890613544697,1.6385032219707756,1.653452543536299,1.6685382592280418,1.6837616134742277,1.699123862056952,1.7146262722157743,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary HeatingNon-Incentive CostsMarket Potential0","WA","Residential","Ancillary Heating","Non-Incentive Costs","Market Potential",0,41751.07,56377.99,85957.99,57718.27,43489.47,28863.74,28876.04,28888.45,28900.97,28913.61,28926.36,28939.22,28952.21,28965.31,28978.54,28991.88,29005.34,29018.93,29032.639999999999,29046.48,29060.45,29074.54,29088.76,29103.1,29117.58,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary HeatingIncentive CostsMarket Potential0","WA","Residential","Ancillary Heating","Incentive Costs","Market Potential",0,4745.01,14365.67,33846.32,43913.73,49238.21,49687.45,50140.79,50598.26,51059.91,51525.760000000002,51995.87,52470.27,52949,53432.09,53919.59,54411.54,54907.98,55408.95,55914.49,56424.639999999999,56939.44,57458.95,57983.19,58512.21,59046.07,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B1030&C1030&D1030&E1030&F1030&G1030","v":"WAResidentialAncillary HeatingProgram Annual BenefitsMarket Potential0"},"WA","Residential","Ancillary Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary HeatingProgram Annual CostsMarket Potential0","WA","Residential","Ancillary Heating","Program Annual Costs","Market Potential",0,46496.09,70743.649999999994,119804.3,101632,92727.679999999993,78551.19,79016.83,79486.710000000006,79960.88,80439.37,80922.23,81409.5,81901.210000000006,82397.399999999994,82898.13,83403.42,83913.33,84427.88,84947.13,85471.12,85999.89,86533.48,87071.94,87615.32,88163.65,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingParticipantsMarket Potential0","WA","General Service","Ancillary Heating","Participants","Market Potential",0,4.919272295851485,14.90271647429077,35.12812217343032,45.603601683163348,51.163069219740798,51.660280263742557,52.162348662235289,52.669321867688623,53.181247796144881,53.698174831747792,54.220151831315505,54.747228128958184,55.279453540740839,55.816878369391581,56.359553409055962,56.907529950097725,57.460859783946461,58.019595207992595,58.583789030530269,59.153494575748425,59.728765688770693,60.309656740744515,60.896222633979967,61.488518807138774,62.086601240474096,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingNew ParticipantsMarket Potential0","WA","General Service","Ancillary Heating","New Participants","Market Potential",0,4.919272295851485,9.9834441784392851,20.22540569913955,10.475479509733027,5.5594675365774506,0.49721104400175875,0.50206839849273166,0.50697320545333469,0.5119259284562574,0.51692703560291164,0.5219769995677126,0.52707629764267949,0.53222541178265459,0.53742482865074237,0.54267503966438113,0.54797654104176274,0.55332983384873557,0.55873542404613374,0.56419382253767481,0.56970554521815586,0.57527111302226785,0.58089105197382196,0.58656589323545205,0.59229617315880745,0.59808243333532118,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Heating","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Heating","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Heating","Winter Peak Reduction @Meter  (MW)","Market Potential",0,3.3205087996997524E-3,1.0059333620146271E-2,2.3711482467065469E-2,3.0782431136135262E-2,3.4535071723325039E-2,3.4870689178026222E-2,3.5209585347008819E-2,3.5551792260689823E-2,3.5897342262397797E-2,3.6246268011429765E-2,3.6598602486137971E-2,3.6954378987046774E-2,3.7313631140000067E-2,3.7676392899339321E-2,3.804269855111278E-2,3.8412582716315966E-2,3.8786080354163865E-2,3.9163226765395E-2,3.9544057595607932E-2,3.992860883863019E-2,4.0316916839920218E-2,4.070901830000255E-2,4.1104950277936481E-2,4.1504750194818675E-2,4.1908455837320016E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Heating","Winter Peak Reduction @Generation (MW)","Market Potential",0,3.5384791130645271E-3,1.0719664983105575E-2,2.5267990693803782E-2,3.2803102233733228E-2,3.6802079841565472E-2,3.7159728450582075E-2,3.7520871000648784E-2,3.7885541624776024E-2,3.8253774789426466E-2,3.8625605297772557E-2,3.9001068292985899E-2,3.9380199261558793E-2,3.9763034036658214E-2,4.0149608801512492E-2,4.053996009283118E-2,4.0934124804258273E-2,4.1332140189859194E-2,4.1734043867641728E-2,4.2139873823111608E-2,4.2549668412862521E-2,4.2963466368201426E-2,4.3381306798809194E-2,4.3803229196436998E-2,4.4229273438638826E-2,4.4659479792540514E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary HeatingNon-Incentive CostsMarket Potential0","WA","General Service","Ancillary Heating","Non-Incentive Costs","Market Potential",0,4743.76,5123.57,5891.72,5160.47,4791.7700000000004,4412.1000000000004,4412.47,4412.83,4413.21,4413.58,4413.96,4414.34,4414.7299999999996,4415.12,4415.51,4415.91,4416.3100000000004,4416.72,4417.13,4417.54,4417.96,4418.38,4418.8,4419.2299999999996,4419.67,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingIncentive CostsMarket Potential0","WA","General Service","Ancillary Heating","Incentive Costs","Market Potential",0,98.39,298.05,702.56,912.07,1023.26,1033.21,1043.25,1053.3900000000001,1063.6300000000001,1073.96,1084.4000000000001,1094.94,1105.5899999999999,1116.3399999999999,1127.19,1138.1500000000001,1149.22,1160.3900000000001,1171.68,1183.07,1194.58,1206.19,1217.92,1229.77,1241.73,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary HeatingProgram Annual BenefitsMarket Potential0","WA","General Service","Ancillary Heating","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary HeatingProgram Annual CostsMarket Potential0","WA","General Service","Ancillary Heating","Program Annual Costs","Market Potential",0,4842.1400000000003,5421.62,6594.28,6072.54,5815.03,5445.31,5455.71,5466.22,5476.83,5487.54,5498.36,5509.29,5520.32,5531.46,5542.7,5554.06,5565.53,5577.11,5588.8,5600.61,5612.53,5624.57,5636.73,5649,5661.4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHParticipantsMarket Potential0","WA","Residential","Ancillary WH","Participants","Market Potential",0,81.223478302358103,491.81281650640284,1241.5057254489357,2505.665868742532,4214.2116336938188,6769.4297929861241,10787.475694178424,15766.426960499786,21731.586539070602,26098.830033606551,29379.222083309924,32717.300650097168,36113.845300565023,39569.645024472273,43085.498341795646,46662.213410954857,50300.608138219097,54001.510288307625,57765.757596197072,61594.197880148349,64186.730065662581,66821.442276759699,69498.888384410369,72219.628855167524,74984.230825413499,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHNew ParticipantsMarket Potential0","WA","Residential","Ancillary WH","New Participants","Market Potential",0,81.223478302358103,410.58933820404474,749.69290894253277,1264.1601432935963,1708.5457649512869,2555.2181592923052,4018.0459011922994,4978.9512663213627,5965.1595785708159,4367.2434945359491,3280.3920497033723,3338.0785667872442,3396.5446504678548,3455.7997239072502,3515.8533173233736,3576.7150691592105,3638.3947272642399,3700.9021500885283,3764.2473078894473,3828.4402839512768,2592.532185514232,2634.7122110971177,2677.4461076506705,2720.740470757155,2764.6019702459744,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.0611739151179049E-2,0.24590640825320143,0.62075286272446784,1.2528329343712661,2.1071058168469095,3.3847148964930622,5.3937378470892119,7.8832134802498928,10.865793269535301,13.049415016803275,14.689611041654961,16.358650325048583,18.056922650282512,19.784822512236136,21.542749170897824,23.331106705477428,25.150304069109549,27.000755144153814,28.882878798098535,30.797098940074175,32.093365032831294,33.410721138379849,34.749444192205182,36.109814427583764,37.492115412706752,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.3277641891708275E-2,0.2620486021453553,0.66150134561430929,1.3350734594749212,2.2454239309962802,3.606899932324235,5.7478024798478389,8.4006963770778906,11.579063586461318,13.906026232740063,15.653890709350982,17.432491821236766,19.242244938493727,21.083570452084544,22.956893830880034,24.862645679323773,26.801261795726287,28.773183231195453,30.77885634920986,32.818732885842046,34.200090614696606,35.603922781734703,37.030524501497425,38.480194402795995,39.95323466827233,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.0611739151179049E-2,0.24590640825320143,0.62075286272446784,1.2528329343712661,2.1071058168469095,3.3847148964930622,5.3937378470892119,7.8832134802498928,10.865793269535301,13.049415016803275,14.689611041654961,16.358650325048583,18.056922650282512,19.784822512236136,21.542749170897824,23.331106705477428,25.150304069109549,27.000755144153814,28.882878798098535,30.797098940074175,32.093365032831294,33.410721138379849,34.749444192205182,36.109814427583764,37.492115412706752,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,4.3277641891708275E-2,0.2620486021453553,0.66150134561430929,1.3350734594749212,2.2454239309962802,3.606899932324235,5.7478024798478389,8.4006963770778906,11.579063586461318,13.906026232740063,15.653890709350982,17.432491821236766,19.242244938493727,21.083570452084544,22.956893830880034,24.862645679323773,26.801261795726287,28.773183231195453,30.77885634920986,32.818732885842046,34.200090614696606,35.603922781734703,37.030524501497425,38.480194402795995,39.95323466827233,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary WHNon-Incentive CostsMarket Potential0","WA","Residential","Ancillary WH","Non-Incentive Costs","Market Potential",0,97423,117184.95,137531.16,168399.2,195062.33,245862.68,333632.34000000003,391286.66,450459.16,354584.2,289373.11,292834.3,296342.27,299897.57,303500.78999999998,307152.49,310853.27,314603.71999999997,318404.42,322256,248101.52,250632.32000000001,253196.35,255794.01,258425.7,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHIncentive CostsMarket Potential0","WA","Residential","Ancillary WH","Incentive Costs","Market Potential",0,1949.36,11803.51,29796.14,60135.98,101141.08,162466.32,258899.42,378394.25,521558.08,626371.92000000004,705101.33,785215.22,866732.29,949671.48,1034051.96,1119893.1200000001,1207214.6000000001,1296036.25,1386378.18,1478260.75,1540481.52,1603714.61,1667973.32,1733271.09,1799621.54,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary WHProgram Annual BenefitsMarket Potential0","WA","Residential","Ancillary WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary WHProgram Annual CostsMarket Potential0","WA","Residential","Ancillary WH","Program Annual Costs","Market Potential",0,99372.36,128988.45,167327.29999999999,228535.18,296203.40999999997,408328.99,592531.76,769680.91,972017.24,980956.12,994474.44,1078049.52,1163074.55,1249569.05,1337552.75,1427045.61,1518067.87,1610639.96,1704782.61,1800516.75,1788583.04,1854346.93,1921169.67,1989065.11,2058047.24,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHParticipantsMarket Potential0","WA","General Service","Ancillary WH","Participants","Market Potential",0,8.0648351441846877,48.864118242463242,123.4078497279866,249.21404863475183,419.39304628012889,671.27643049437745,1067.4563437341569,1558.101959656949,2145.8566905152543,2575.8316978759526,2898.8180517589435,3227.8417375788331,3562.9900303907057,3904.3513342781184,4252.0151960832236,4606.0723192973946,4966.6145781142013,5333.7350316465581,5707.5279383099378,6088.088770373507,6487.3010789993705,6893.7052237882954,7307.4037671981741,7728.5005892240351,8157.100903352336,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHNew ParticipantsMarket Potential0","WA","General Service","Ancillary WH","New Participants","Market Potential",0,8.0648351441846877,40.799283098278551,74.543731485523352,125.80619890676523,170.17899764537705,251.88338421424857,396.17991323977947,490.6456159227921,587.75473085830527,429.97500736069833,322.9863538829909,329.02368581988958,335.14829281187258,341.36130388741276,347.66386180510517,354.05712321417104,360.54225881680668,367.12045353235681,373.79290666337965,380.56083206356925,399.21230862586344,406.4041447889249,413.69854340987877,421.096822025861,428.60031412830085,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,1.0161692281672708E-2,6.1568788985503685E-2,0.1554938906572631,0.31400970127978728,0.52843523831296235,0.8458083024229156,1.3449949931050378,1.9632084691677558,2.7037794300492206,3.2455479393237003,3.6525107452162686,4.06708058934933,4.4893674382922892,4.9194826811904298,5.3575391470648617,5.8036511223147169,6.2579343684238937,6.7205061398746633,7.1914852022705213,7.6709918506706192,8.1739993595392075,8.6860685819732524,9.2073287466697007,9.7379107424222831,10.277947138223942,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,1.082874284065719E-2,6.5610388944483886E-2,0.1657010770004935,0.33462244381904016,0.56312365549122156,0.90133024554871655,1.4332853720215661,2.092080636368026,2.8812653772903034,3.4585975482989135,3.8922748776814458,4.3340585990508629,4.784065897583428,5.2424154744143543,5.7092275650733821,6.1846239581358873,6.6687280140919585,7.161664684435916,7.663560530978816,8.1745437453864227,8.7105705024927609,9.2562538171070461,9.8117314009694159,10.377142734891606,10.952629090178966,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,1.0161692281672708E-2,6.1568788985503685E-2,0.1554938906572631,0.31400970127978728,0.52843523831296235,0.8458083024229156,1.3449949931050378,1.9632084691677558,2.7037794300492206,3.2455479393237003,3.6525107452162686,4.06708058934933,4.4893674382922892,4.9194826811904298,5.3575391470648617,5.8036511223147169,6.2579343684238937,6.7205061398746633,7.1914852022705213,7.6709918506706192,8.1739993595392075,8.6860685819732524,9.2073287466697007,9.7379107424222831,10.277947138223942,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,1.082874284065719E-2,6.5610388944483886E-2,0.1657010770004935,0.33462244381904016,0.56312365549122156,0.90133024554871655,1.4332853720215661,2.092080636368026,2.8812653772903034,3.4585975482989135,3.8922748776814458,4.3340585990508629,4.784065897583428,5.2424154744143543,5.7092275650733821,6.1846239581358873,6.6687280140919585,7.161664684435916,7.663560530978816,8.1745437453864227,8.7105705024927609,9.2562538171070461,9.8117314009694159,10.377142734891606,10.952629090178966,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary WHNon-Incentive CostsMarket Potential0","WA","General Service","Ancillary WH","Non-Incentive Costs","Market Potential",0,9758.1200000000008,12213.2,14744.04,18588.72,21916.68,28044.51,38866.75,45951.68,53234.86,41401.379999999997,33377.230000000003,33830.03,34289.379999999997,34755.35,35228.050000000003,35707.54,36193.93,36687.29,37187.72,37695.32,39094.18,39633.57,40180.65,40735.519999999997,41298.28,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHIncentive CostsMarket Potential0","WA","General Service","Ancillary WH","Incentive Costs","Market Potential",0,193.56,1172.74,2961.79,5981.14,10065.43,16110.63,25618.95,37394.449999999997,51500.56,61819.96,69571.63,77468.2,85511.76,93704.43,102048.36,110545.74,119198.75,128009.64,136980.67000000001,146114.13,155695.23000000001,165448.93,175377.69,185484.01,195770.42,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary WHProgram Annual BenefitsMarket Potential0","WA","General Service","Ancillary WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary WHProgram Annual CostsMarket Potential0","WA","General Service","Ancillary WH","Program Annual Costs","Market Potential",0,9951.67,13385.94,17705.82,24569.86,31982.11,44155.14,64485.7,83346.12,104735.42,103221.34,102948.87,111298.23,119801.14,128459.79,137276.41,146253.28,155392.68,164696.93,174168.39,183809.45,194789.4,205082.49,215558.34,226219.53,237068.7,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHParticipantsMarket Potential0","WA","Residential","Ancillary DLC WH","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHNew ParticipantsMarket Potential0","WA","Residential","Ancillary DLC WH","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary DLC WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary DLC WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary DLC WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary DLC WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary DLC WHNon-Incentive CostsMarket Potential0","WA","Residential","Ancillary DLC WH","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHIncentive CostsMarket Potential0","WA","Residential","Ancillary DLC WH","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary DLC WHProgram Annual BenefitsMarket Potential0","WA","Residential","Ancillary DLC WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary DLC WHProgram Annual CostsMarket Potential0","WA","Residential","Ancillary DLC WH","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHParticipantsMarket Potential0","WA","General Service","Ancillary DLC WH","Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHNew ParticipantsMarket Potential0","WA","General Service","Ancillary DLC WH","New Participants","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary DLC WH","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary DLC WH","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary DLC WH","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary DLC WH","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary DLC WHNon-Incentive CostsMarket Potential0","WA","General Service","Ancillary DLC WH","Non-Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHIncentive CostsMarket Potential0","WA","General Service","Ancillary DLC WH","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary DLC WHProgram Annual BenefitsMarket Potential0","WA","General Service","Ancillary DLC WH","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary DLC WHProgram Annual CostsMarket Potential0","WA","General Service","Ancillary DLC WH","Program Annual Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVParticipantsMarket Potential0","WA","Residential","Ancillary EV","Participants","Market Potential",0,0,0,108.4378964235363,384.6313391902396,1061.1182414250179,1613.0602085207281,2119.0948533702572,2505.4902950762039,2962.3410243940675,3502.4938480319229,4141.1380575302674,4896.2325575994128,5789.0108769746712,6844.5782628760726,8092.6176495834243,9568.224353216794,11312.892964639643,13375.684192267749,15814.604466823066,18698.2371030141,22107.670886995493,26138.780322179318,30904.921654729886,36540.120491948037,36873.504036119564,37209.929294057438,37549.424017649246,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVNew ParticipantsMarket Potential0","WA","Residential","Ancillary EV","New Participants","Market Potential",0,0,0,108.4378964235363,276.1934427667033,676.48690223477831,551.9419670957102,506.03464484952906,386.39544170594672,456.85072931786362,540.15282363785536,638.64420949834448,755.0945000691454,892.77831937525843,1055.5673859014014,1248.0393867073517,1475.6067036333698,1744.6686114228487,2062.7912276281058,2438.9202745553175,2883.6326361910342,3409.4337839813925,4031.1094351838256,4766.1413325505673,5635.1988372181513,333.38354417152732,336.42525793787354,339.494723591808,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary EV","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0,0,2.7109474105884074E-2,9.6157834797559905E-2,0.2652795603562545,0.40326505213018204,0.52977371334256429,0.62637257376905098,0.74058525609851689,0.87562346200798069,1.0352845143825669,1.2240581393998531,1.4472527192436677,1.7111445657190181,2.023154412395856,2.3920560883041984,2.8282232411599106,3.343921048066937,3.9536511167057666,4.6745592757535253,5.5269177217488732,6.5346950805448296,7.7262304136824715,9.1350301229870094,9.2183760090298907,9.3024823235143597,9.387356004412311,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary EV","Summer Peak Reduction @Generation (MW)","Market Potential",0,0,0,2.8889038902263506E-2,0.10246998593090356,0.28269347864050992,0.42973684157095271,0.56454999290554586,0.66748995499685737,0.78919997452953627,0.93310258099742183,1.1032443674153525,1.3044097819691529,1.5422556684182307,1.8234703385752538,2.1559616500382099,2.5490793779882761,3.0138781342283787,3.5634282268402995,4.2131832019456166,4.9814144029769025,5.8897247674220727,6.9636563091909949,8.2334083692268454,9.7346868318275881,9.823503845939781,9.9131312057910907,10.003576304787202,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary EV","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0,0,2.7109474105884074E-2,9.6157834797559905E-2,0.2652795603562545,0.40326505213018204,0.52977371334256429,0.62637257376905098,0.74058525609851689,0.87562346200798069,1.0352845143825669,1.2240581393998531,1.4472527192436677,1.7111445657190181,2.023154412395856,2.3920560883041984,2.8282232411599106,3.343921048066937,3.9536511167057666,4.6745592757535253,5.5269177217488732,6.5346950805448296,7.7262304136824715,9.1350301229870094,9.2183760090298907,9.3024823235143597,9.387356004412311,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary EV","Winter Peak Reduction @Generation (MW)","Market Potential",0,0,0,2.8889038902263506E-2,0.10246998593090356,0.28269347864050992,0.42973684157095271,0.56454999290554586,0.66748995499685737,0.78919997452953627,0.93310258099742183,1.1032443674153525,1.3044097819691529,1.5422556684182307,1.8234703385752538,2.1559616500382099,2.5490793779882761,3.0138781342283787,3.5634282268402995,4.2131832019456166,4.9814144029769025,5.8897247674220727,6.9636563091909949,8.2334083692268454,9.7346868318275881,9.823503845939781,9.9131312057910907,10.003576304787202,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary EVNon-Incentive CostsMarket Potential0","WA","Residential","Ancillary EV","Non-Incentive Costs","Market Potential",0,0,0,72051.63,80439.41,100454.08,94226.84,91931.47,85949.51,89472.27,93637.38,98561.95,104384.46,111268.65,119408.11,129031.71,140410.07,153863.17000000001,169769.3,188575.75,210811.37,237101.43,268185.21000000002,304936.8,348389.68,83298.91,83451,83604.47,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVIncentive CostsMarket Potential0","WA","Residential","Ancillary EV","Incentive Costs","Market Potential",0,0,0,2168.7600000000002,7692.63,21222.36,32261.200000000001,42381.9,50109.81,59246.82,70049.88,82822.759999999995,97924.65,115780.22,136891.57,161852.35,191364.49,226257.86,267513.68,316292.09000000003,373964.74,442153.42,522775.61,618098.43000000005,730802.41,737470.08,744198.59,750988.48,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary EVProgram Annual BenefitsMarket Potential0","WA","Residential","Ancillary EV","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary EVProgram Annual CostsMarket Potential0","WA","Residential","Ancillary EV","Program Annual Costs","Market Potential",0,0,0,74220.39,88132.04,121676.45,126488.04,134313.37,136059.31,148719.09,163687.26,181384.71,202309.11,227048.87,256299.67,290884.06,331774.56,380121.03,437282.98,504867.84000000003,584776.11,679254.84,790960.82,923035.24,1079192.0900000001,820768.99,827649.59,834592.95,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartyParticipantsMarket Potential0","WA","General Service","Ancillary Third Party","Participants","Market Potential",0,171.464178757094,346.29539870073864,594.71426072531062,706.46258594552853,713.3277540951201,720.25998945038702,727.25994720430481,734.3282889505598,741.46568274608035,748.67280317417612,755.95033140829707,763.29895527641236,770.71936932602125,778.21227488979594,785.77838015186865,793.41840021476412,801.13305716698721,808.92308015126969,816.78920543348511,824.73217647223589,832.75274398912052,840.85166603968753,849.02970808508132,857.28764306439041,865.62625146769983,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartyNew ParticipantsMarket Potential0","WA","General Service","Ancillary Third Party","New Participants","Market Potential",0,171.464178757094,174.83121994364464,248.41886202457198,111.74832522021791,6.8651681495915682,6.9322353552669256,6.9999577539177835,7.0683417462549869,7.137393795520552,7.2071204280957772,7.2775282341209504,7.3486238681152827,7.4204140496088939,7.4929055637746842,7.5661052620727105,7.6400200628954735,7.7146569522230948,7.7900229842824729,7.8661252822154211,7.9429710387507839,8.0205675168846255,8.0989220505670119,8.178042045393795,8.2579349793090842,8.3386084033094221,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartySummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Third Party","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.5507475611936257E-2,9.1971840291838469E-2,0.15798451545687148,0.18768468356482124,0.18952315547988358,0.19137972821115032,0.19325458013390379,0.19514789138151811,0.19705984386278802,0.19899062127942768,0.20094040914374289,0.20290939479647677,0.20489776742483182,0.20690571808066924,0.20893343969888784,0.21098112711598435,0.21304897708879592,0.21513718831342815,0.21724596144436906,0.21937549911379225,0.22152600595104921,0.22369768860235495,0.22589075575066647,0.22810541813575841,0.23034188857449536,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartySummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Third Party","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.8494752357135823E-2,9.8009207472121135E-2,0.16835519549964992,0.20000499101110533,0.20196414693082224,0.20394259187036479,0.20594051591421972,0.20795811102037309,0.20999557103877667,0.2120530917299954,0.21413087078403975,0.21622910783938273,0.21834800450216518,0.22048776436558956,0.22264859302950538,0.22483069812018794,0.22703428931031108,0.22925957833911781,0.23150677903278885,0.23377610732501306,0.23606778127775918,0.23838202110225379,0.2407190491801646,0.24307909008499404,0.24546237060368217,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartyWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Third Party","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.5268011894120212E-2,9.1487877634835152E-2,0.15715318919849416,0.1866970728151762,0.18852587055442541,0.19037267386203921,0.19223766017467614,0.19412100867783497,0.19602290032309289,0.19794351784551195,0.19988304578121843,0.20184167048515456,0.20381958014900572,0.20581696481930403,0.2078340164157105,0.20987092874947774,0.21192789754209382,0.21400512044411066,0.21610279705415744,0.21822112893814224,0.22036031964864169,0.22252057474448314,0.22470210181051822,0.22690511047759329,0.22912981244271474,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartyWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Third Party","Winter Peak Reduction @Generation (MW)","Market Potential",0,4.8239569367135776E-2,9.7493475740446658E-2,0.16746929795235951,0.19895254988829517,0.2009013965839998,0.20286943079927452,0.20485684161836759,0.2068638199891677,0.20889055874157383,0.21093725260604429,0.21300409823232996,0.21509129420839146,0.21719904107950311,0.21932754136754479,0.22147699959048434,0.22364762228205215,0.22583961801160893,0.22805319740420998,0.23028857316086684,0.23254596007900921,0.23482557507314758,0.23712763719574076,0.2394523676582675,0.24179998985250778,0.24417072937203191,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary Third PartyNon-Incentive CostsMarket Potential0","WA","General Service","Ancillary Third Party","Non-Incentive Costs","Market Potential",0,1820.3,3678.87,6319.38,7507.39,7580.93,7655.19,7730.18,7805.92,7882.39,7959.62,8037.62,8116.38,8195.91,8276.23,8357.34,8439.25,8521.9599999999991,8605.49,8689.84,8775.02,8861.0400000000009,8947.91,9035.6299999999992,9124.2199999999993,9213.68,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartyIncentive CostsMarket Potential0","WA","General Service","Ancillary Third Party","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Third PartyProgram Annual BenefitsMarket Potential0","WA","General Service","Ancillary Third Party","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary Third PartyProgram Annual CostsMarket Potential0","WA","General Service","Ancillary Third Party","Program Annual Costs","Market Potential",0,1820.3,3678.87,6319.38,7507.39,7580.93,7655.19,7730.18,7805.92,7882.39,7959.62,8037.62,8116.38,8195.91,8276.23,8357.34,8439.25,8521.9599999999991,8605.49,8689.84,8775.02,8861.0400000000009,8947.91,9035.6299999999992,9124.2199999999993,9213.68,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartyParticipantsMarket Potential0","WA","Large General Service","Ancillary Third Party","Participants","Market Potential",0,20.204856597887463,40.359732966574846,68.52735548158978,80.521926380911708,80.426853393060867,80.335080582893468,80.246493402126717,80.160981278418021,80.078437477361192,79.998758969272671,79.921846300601544,79.847603469803033,79.775937807520279,79.70675986092489,79.639983282072208,79.575524720131583,79.513303717357346,79.453242608670621,79.3952664247266,79.339302798346338,79.285281874196286,79.233136221602777,79.182800750392786,79.134212629655693,79.087311209324994,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartyNew ParticipantsMarket Potential0","WA","Large General Service","Ancillary Third Party","New Participants","Market Potential",0,20.204856597887463,20.154876368687383,28.167622515014934,11.994570899321928,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartySummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Ancillary Third Party","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.32053381976391787,0.64012488211465768,1.0865300430895191,1.2763493310308445,1.2744892654751105,1.2726884902980011,1.2709451157503779,1.2692573123146611,1.2676233087850797,1.266041390409113,1.2645098970881681,1.2630272216356078,1.2615918080903006,1.2602021500839191,1.2588567892602813,1.2575543137450698,1.2562933566643244,1.2550725947101578,1.2538907467521818,1.2527465724931941,1.2516388711677127,1.2505664802819856,1.2495282743941696,1.2485231639333796,1.2475500940563831,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartySummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Ancillary Third Party","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.34157482924543675,0.68214501504119529,1.157853839609462,1.3601335582170124,1.3581513911712602,1.3562324065409219,1.3543745905268307,1.3525759935151973,1.3508347280318411,1.3491489667616294,1.3475169406310401,1.3459369369518412,1.344407297623935,1.3429264173954807,1.3414927421784755,1.3401047674180198,1.3387610365135596,1.3374601392904495,1.3362007105202278,1.3349814284880586,1.3338010136058318,1.3326582270694647,1.3315518695590043,1.3304807799801572,1.3294438342459325,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartyWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Ancillary Third Party","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.31884714698907574,0.63675649742452722,1.0808126412750181,1.2696330860198712,1.2677828082672919,1.2659915089029596,1.2642573081217368,1.2625783860331001,1.2609529807514954,1.259379386547558,1.2578559520582555,1.2563810785540874,1.2549532182615051,1.2535708727388033,1.2522325913037777,1.2509369695114991,1.2496826476806002,1.2484683094665374,1.2472926804803264,1.2461545269513001,1.2450526544324938,1.2439859065472849,1.2429531637759879,1.2419533422811209,1.2409853927701149,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartyWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Ancillary Third Party","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.33977743711538333,0.67855551728956442,1.151761126678408,1.3529764343775268,1.3510046976420418,1.3490958108514062,1.3472477708032147,1.3454586381426898,1.3437265353276806,1.3420496446585231,1.34042620637069,1.3388545167882433,1.3373329265361307,1.3358598388094665,1.3344337076979729,1.3330530365638311,1.3317163764712279,1.3304223246659606,1.3291695231035021,1.3279566570239771,1.3267824535725636,1.3256456804638586,1.324545144688819,1.3234796912629165,1.322448202014189,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceAncillary Third PartyNon-Incentive CostsMarket Potential0","WA","Large General Service","Ancillary Third Party","Non-Incentive Costs","Market Potential",0,12821.35,25605,43461.2,51053.97,50979.57,50907.54,50837.8,50770.29,50704.93,50641.66,50580.4,50521.09,50463.67,50408.09,50354.27,50302.17,50251.73,50202.9,50155.63,50109.86,50065.55,50022.66,49981.13,49940.93,49902,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartyIncentive CostsMarket Potential0","WA","Large General Service","Ancillary Third Party","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Third PartyProgram Annual BenefitsMarket Potential0","WA","Large General Service","Ancillary Third Party","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceAncillary Third PartyProgram Annual CostsMarket Potential0","WA","Large General Service","Ancillary Third Party","Program Annual Costs","Market Potential",0,12821.35,25605,43461.2,51053.97,50979.57,50907.54,50837.8,50770.29,50704.93,50641.66,50580.4,50521.09,50463.67,50408.09,50354.27,50302.17,50251.73,50202.9,50155.63,50109.86,50065.55,50022.66,49981.13,49940.93,49902,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Third PartyParticipantsMarket Potential0","WA","Extra Large General Service","Ancillary Third Party","Participants","Market Potential",0,0.22760100000000003,0.45520200000000005,0.77384339999999996,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0.9104040000000001,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Third PartyNew ParticipantsMarket Potential0","WA","Extra Large General Service","Ancillary Third Party","New Participants","Market Potential",0,0.22760100000000003,0.22760100000000003,0.31864139999999991,0.13656060000000014,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B1114&C1114&D1114&E1114&F1114&G1114","v":"WAExtra Large General ServiceAncillary Third PartySummer Peak Reduction @Meter  (MW)Market Potential0"},"WA","Extra Large General Service","Ancillary Third Party","Summer Peak Reduction @Meter  (MW)","Market Potential",0,0.12081891525864465,0.24202491971421858,0.41172807182828286,0.48454757619759442,0.484709323464524,0.48487120875890766,0.48503323218213662,0.48519539383567778,0.48535769382107402,0.48552013223994367,0.48568270919398138,0.48584542478495762,0.48600827911471856,0.48617127228518719,0.48633440439836173,0.48649767555631734,0.48666108586120466,0.48682463541525151,0.48698832432076145,0.48715215268011447,0.48731612059576729,0.4874802281702531,0.48764447550618129,0.48780886270623869,0.48797338987318795,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Third PartySummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Ancillary Third Party","Summer Peak Reduction @Generation (MW)","Market Potential",0,0.12874990969591288,0.25791231853603858,0.43875540476159725,0.5163550470988858,0.51652741204659425,0.51669992408238241,0.51687258331429731,0.51704538985046655,0.51721834379909848,0.51739144526848213,0.51756469436698782,0.51773809120306646,0.51791163588524991,0.51808532852215172,0.51825916922246562,0.51843315809496737,0.51860729524851301,0.51878158079204129,0.51895601483457099,0.51913059748520296,0.51930532885311942,0.5194802090475843,0.51965523817794257,0.51983041635362182,0.52000574368413033,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Third PartyWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Ancillary Third Party","Winter Peak Reduction @Meter  (MW)","Market Potential",0,0.13515406945919187,0.27074115621618583,0.46057957314922449,0.5420391056276016,0.54222004419423786,0.54240113716527383,0.54258238465413133,0.5427637867743158,0.5429453436394186,0.5431270553631149,0.54330892205916503,0.54349094384141516,0.54367312082379526,0.54385545312032124,0.54403794084509349,0.54422058411229868,0.54440338303620717,0.5445863377311766,0.54476944831164853,0.54495271489215025,0.54513613758729507,0.54531971651178179,0.5455034517803945,0.5456873435080033,0.54587139180956423,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Third PartyWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Ancillary Third Party","Winter Peak Reduction @Generation (MW)","Market Potential",0,0.14402607572377649,0.28851359358076067,0.49081369687683768,0.57762053029369309,0.57781334632804549,0.57800632690246567,0.57819947213782108,0.57839278215506795,0.57858625707525424,0.57877989701951715,0.57897370210908461,0.57916767246527612,0.57936180820950045,0.57955610946325797,0.57975057634813887,0.57994520898582558,0.58014000749808947,0.58033497200679518,0.58053010263389659,0.58072539950143887,0.58092086273155907,0.58111649244648533,0.58131228876853636,0.58150825182012289,0.58170438172374705,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceAncillary Third PartyNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Ancillary Third Party","Non-Incentive Costs","Market Potential",0,5406.16,10829.65,18423.18,21681.56,21688.799999999999,21696.05,21703.3,21710.55,21717.81,21725.08,21732.36,21739.64,21746.92,21754.22,21761.52,21768.82,21776.14,21783.45,21790.78,21798.11,21805.45,21812.79,21820.14,21827.49,21834.86,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Third PartyIncentive CostsMarket Potential0","WA","Extra Large General Service","Ancillary Third Party","Incentive Costs","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Third PartyProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Ancillary Third Party","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceAncillary Third PartyProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Ancillary Third Party","Program Annual Costs","Market Potential",0,5406.16,10829.65,18423.18,21681.56,21688.799999999999,21696.05,21703.3,21710.55,21717.81,21725.08,21732.36,21739.64,21746.92,21754.22,21761.52,21768.82,21776.14,21783.45,21790.78,21798.11,21805.45,21812.79,21820.14,21827.49,21834.86,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageParticipantsMarket Potential0","WA","Residential","Ancillary Battery Storage","Participants","Market Potential",0,23.494821728845764,71.131246095896373,119.70658527321089,193.27801641790427,268.18197999833387,344.43666712959265,422.06048994560086,526.12568832376337,632.05468630633493,739.8728309276579,875.35140618821379,1013.2405420215947,1153.5729475538492,1322.8384980707363,1334.9077682569293,1347.0871556517156,1359.3776649388451,1371.7803099685677,1384.2961138412677,1396.9261089918577,1409.6713372749466,1422.5328500507817,1435.5117082719762,1448.6089825710276,1461.8257533486353,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageNew ParticipantsMarket Potential0","WA","Residential","Ancillary Battery Storage","New Participants","Market Potential",0,23.494821728845764,47.636424367050608,48.575339177314518,73.571431144693378,74.903963580429604,76.254687131258777,77.623822816008214,104.06519837816251,105.92899798257156,107.81814462132297,135.47857526055589,137.88913583338092,140.33240553225448,169.26555051688706,12.06927018619308,12.179387394786318,12.290509287129453,12.402645029722635,12.515803872699962,12.629995150590048,12.745228283088863,12.861512775835081,12.978858221194514,13.097274299051378,13.216770777607735,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.6989643457691528E-2,0.14226249219179274,0.23941317054642178,0.38655603283580853,0.53636395999666775,0.68887333425918529,0.84412097989120172,1.0522513766475268,1.2641093726126698,1.4797456618553158,1.7507028123764277,2.0264810840431893,2.3071458951076984,2.6456769961414723,2.6698155365138585,2.6941743113034313,2.7187553298776903,2.7435606199371354,2.7685922276825354,2.7938522179837153,2.8193426745498931,2.8450657001015633,2.8710234165439523,2.8972179651420551,2.9236515066972708,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,5.0074215108366932E-2,0.15160112126150121,0.25512912462321163,0.4119309812828309,0.57157284739627845,0.73409349345607977,0.89953216100937949,1.1213249964274581,1.3470901242675508,1.5768815663419817,1.8656253328819561,2.159506696550713,2.4585953698931142,2.8193488876187898,2.8450719698570528,2.8710297435032301,2.8972243498270358,2.9236579496346287,2.9503327234468619,2.9772508716791508,3.0044146148229891,3.0318261936291169,3.0594878692923619,3.0874019236381662,3.115570659310817,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Residential","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.6989643457691528E-2,0.14226249219179274,0.23941317054642178,0.38655603283580853,0.53636395999666775,0.68887333425918529,0.84412097989120172,1.0522513766475268,1.2641093726126698,1.4797456618553158,1.7507028123764277,2.0264810840431893,2.3071458951076984,2.6456769961414723,2.6698155365138585,2.6941743113034313,2.7187553298776903,2.7435606199371354,2.7685922276825354,2.7938522179837153,2.8193426745498931,2.8450657001015633,2.8710234165439523,2.8972179651420551,2.9236515066972708,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Residential","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,5.0074215108366932E-2,0.15160112126150121,0.25512912462321163,0.4119309812828309,0.57157284739627845,0.73409349345607977,0.89953216100937949,1.1213249964274581,1.3470901242675508,1.5768815663419817,1.8656253328819561,2.159506696550713,2.4585953698931142,2.8193488876187898,2.8450719698570528,2.8710297435032301,2.8972243498270358,2.9236579496346287,2.9503327234468619,2.9772508716791508,3.0044146148229891,3.0318261936291169,3.0594878692923619,3.0874019236381662,3.115570659310817,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary Battery StorageNon-Incentive CostsMarket Potential0","WA","Residential","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,52544.47,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageIncentive CostsMarket Potential0","WA","Residential","Ancillary Battery Storage","Incentive Costs","Market Potential",0,469.9,1422.62,2394.13,3865.56,5363.64,6888.73,8441.2099999999991,10522.51,12641.09,14797.46,17507.03,20264.810000000001,23071.46,26456.77,26698.16,26941.74,27187.55,27435.61,27685.919999999998,27938.52,28193.43,28450.66,28710.23,28972.18,29236.52,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAResidentialAncillary Battery StorageProgram Annual BenefitsMarket Potential0","WA","Residential","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAResidentialAncillary Battery StorageProgram Annual CostsMarket Potential0","WA","Residential","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,53014.36,53967.09,54938.6,56410.03,57908.11,59433.2,60985.68,63066.98,65185.56,67341.919999999998,70051.5,72809.279999999999,75615.929999999993,79001.240000000005,79242.62,79486.210000000006,79732.02,79980.070000000007,80230.39,80482.990000000005,80737.89,80995.12,81254.7,81516.649999999994,81780.98,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageParticipantsMarket Potential0","WA","General Service","Ancillary Battery Storage","Participants","Market Potential",0,2.3328459694842727,7.0672530347089522,11.89904483243919,19.223471726408942,26.68913365662014,34.298094735732725,42.052445926779541,52.452020639325717,63.049802954598675,73.848677864119423,87.422827441775851,101.25394304687104,115.34575595355417,132.34902634180202,133.63577893739264,134.93510207734084,136.24711856581416,137.57195240667852,138.90972881521859,140.26057422997209,141.62461632468037,143.00198402035502,144.39280749746283,145.79721820822968,147.21534888906461,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageNew ParticipantsMarket Potential0","WA","General Service","Ancillary Battery Storage","New Participants","Market Potential",0,2.3328459694842727,4.7344070652246799,4.8317917977302374,7.3244268939697523,7.4656619302111977,7.6089610791125857,7.7543511910468155,10.399574712546176,10.597782315272958,10.798874909520748,13.574149577656428,13.831115605095192,14.091812906683131,17.003270388247842,1.2867525955906274,1.2993231399481999,1.3120164884733185,1.3248338408643576,1.3377764085400656,1.3508454147535076,1.3640420947082816,1.3773676956746499,1.3908234771078014,1.4044107107668538,1.4181306808349348,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,4.6656919389685457E-3,1.4134506069417904E-2,2.3798089664878379E-2,3.8446943452817885E-2,5.3378267313240281E-2,6.8596189471465452E-2,8.4104891853559086E-2,0.10490404127865144,0.12609960590919736,0.14769735572823886,0.17484565488355169,0.2025078860937421,0.23069151190710835,0.26469805268360402,0.26727155787478529,0.26987020415468171,0.27249423713162835,0.27514390481335704,0.27781945763043719,0.28052114845994419,0.28324923264936075,0.28600396804071004,0.28878561499492567,0.29159443641645938,0.29443069777812925,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,4.971964981850539E-3,1.5062346621289326E-2,2.5360283104090345E-2,4.0970741104878396E-2,5.6882211544373701E-2,7.3099093639669072E-2,8.9625843833715996E-2,0.111790325318256,0.13437724414876104,0.15739274907101328,0.18632316164061349,0.21580124264039013,0.24583494448754087,0.28207379868244248,0.28481623814448559,0.28758546904804105,0.29038175312407111,0.29320535466044018,0.29605654052689384,0.29893558020028155,0.30184274579002635,0.30477831206384276,0.30774255647370596,0.31073575918207519,0.31375820308837304,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","General Service","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,4.6656919389685457E-3,1.4134506069417904E-2,2.3798089664878379E-2,3.8446943452817885E-2,5.3378267313240281E-2,6.8596189471465452E-2,8.4104891853559086E-2,0.10490404127865144,0.12609960590919736,0.14769735572823886,0.17484565488355169,0.2025078860937421,0.23069151190710835,0.26469805268360402,0.26727155787478529,0.26987020415468171,0.27249423713162835,0.27514390481335704,0.27781945763043719,0.28052114845994419,0.28324923264936075,0.28600396804071004,0.28878561499492567,0.29159443641645938,0.29443069777812925,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","General Service","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,4.971964981850539E-3,1.5062346621289326E-2,2.5360283104090345E-2,4.0970741104878396E-2,5.6882211544373701E-2,7.3099093639669072E-2,8.9625843833715996E-2,0.111790325318256,0.13437724414876104,0.15739274907101328,0.18632316164061349,0.21580124264039013,0.24583494448754087,0.28207379868244248,0.28481623814448559,0.28758546904804105,0.29038175312407111,0.29320535466044018,0.29605654052689384,0.29893558020028155,0.30184274579002635,0.30477831206384276,0.30774255647370596,0.31073575918207519,0.31375820308837304,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary Battery StorageNon-Incentive CostsMarket Potential0","WA","General Service","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,5569.91,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageIncentive CostsMarket Potential0","WA","General Service","Ancillary Battery Storage","Incentive Costs","Market Potential",0,46.66,141.35,237.98,384.47,533.78,685.96,841.05,1049.04,1261,1476.97,1748.46,2025.08,2306.92,2646.98,2672.72,2698.7,2724.94,2751.44,2778.19,2805.21,2832.49,2860.04,2887.86,2915.94,2944.31,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAGeneral ServiceAncillary Battery StorageProgram Annual BenefitsMarket Potential0","WA","General Service","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAGeneral ServiceAncillary Battery StorageProgram Annual CostsMarket Potential0","WA","General Service","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,5616.57,5711.26,5807.9,5954.38,6103.7,6255.88,6410.96,6618.96,6830.91,7046.89,7318.37,7594.99,7876.83,8216.9,8242.6299999999992,8268.6200000000008,8294.86,8321.35,8348.11,8375.1299999999992,8402.41,8429.9500000000007,8457.77,8485.86,8514.2199999999993,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageParticipantsMarket Potential0","WA","Large General Service","Ancillary Battery Storage","Participants","Market Potential",0,0.18469634442056276,0.55340371543363276,0.9212077587370886,1.4721317497310062,2.021791186351455,2.5702525896076343,3.1175793862520091,3.8470236456117246,4.5750741280086604,5.3018054072601739,6.2099336674904055,7.1165421987346731,8.0217132033705649,9.1076785800224958,9.100048366249851,9.0926830202627613,9.0855733485713852,9.0787104767894569,9.0720858385582748,9.065691164855151,9.059518473672961,9.053560060057908,9.0478084864930732,9.0422565736157612,9.0368973912570265,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageNew ParticipantsMarket Potential0","WA","Large General Service","Ancillary Battery Storage","New Participants","Market Potential",0,0.18469634442056276,0.36870737101307,0.36780404330345584,0.55092399099391764,0.5496594366204488,0.5484614032561792,0.54732679664437489,0.72944425935971546,0.72805048239693582,0.72673127925151348,0.90812826023023163,0.90660853124426755,0.90517100463589184,1.0859653766519308,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,2.7704451663084413E-3,8.3010557315044906E-3,1.3818116381056329E-2,2.2081976245965095E-2,3.0326867795271828E-2,3.8553788844114513E-2,4.6763690793780135E-2,5.7705354684175869E-2,6.8626111920129906E-2,7.9527081108902609E-2,9.3149005012356081E-2,0.10674813298102009,0.12032569805055847,0.13661517870033743,0.13650072549374778,0.13639024530394142,0.13628360022857078,0.13618065715184186,0.13608128757837412,0.13598536747282727,0.1358927771050944,0.13580340090086862,0.1357171272973961,0.13563384860423641,0.13555346086885542,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,2.952307295725108E-3,8.8459673183125427E-3,1.4725187959352438E-2,2.353151773866698E-2,3.2317634052932469E-2,4.1084600217513333E-2,4.9833430087148481E-2,6.1493344718857493E-2,7.3130980307043805E-2,8.4747528888429888E-2,9.9263645580089599E-2,0.11375546992862329,0.12822431591065481,0.14558309750675344,0.14546113117407053,0.14534339866148915,0.14522975301424848,0.1451200523783481,0.14501415982350183,0.14491194317223707,0.14481327483492581,0.14471803165054201,0.14462609473294555,0.14453734932250256,0.14445168464285529,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,2.7704451663084413E-3,8.3010557315044906E-3,1.3818116381056329E-2,2.2081976245965095E-2,3.0326867795271828E-2,3.8553788844114513E-2,4.6763690793780135E-2,5.7705354684175869E-2,6.8626111920129906E-2,7.9527081108902609E-2,9.3149005012356081E-2,0.10674813298102009,0.12032569805055847,0.13661517870033743,0.13650072549374778,0.13639024530394142,0.13628360022857078,0.13618065715184186,0.13608128757837412,0.13598536747282727,0.1358927771050944,0.13580340090086862,0.1357171272973961,0.13563384860423641,0.13555346086885542,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,2.952307295725108E-3,8.8459673183125427E-3,1.4725187959352438E-2,2.353151773866698E-2,3.2317634052932469E-2,4.1084600217513333E-2,4.9833430087148481E-2,6.1493344718857493E-2,7.3130980307043805E-2,8.4747528888429888E-2,9.9263645580089599E-2,0.11375546992862329,0.12822431591065481,0.14558309750675344,0.14546113117407053,0.14534339866148915,0.14522975301424848,0.1451200523783481,0.14501415982350183,0.14491194317223707,0.14481327483492581,0.14471803165054201,0.14462609473294555,0.14453734932250256,0.14445168464285529,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceAncillary Battery StorageNon-Incentive CostsMarket Potential0","WA","Large General Service","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,2714.89,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageIncentive CostsMarket Potential0","WA","Large General Service","Ancillary Battery Storage","Incentive Costs","Market Potential",0,3.69,11.07,18.420000000000002,29.44,40.44,51.41,62.35,76.94,91.5,106.04,124.2,142.33000000000001,160.43,182.15,182,181.85,181.71,181.57,181.44,181.31,181.19,181.07,180.96,180.85,180.74,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WALarge General ServiceAncillary Battery StorageProgram Annual BenefitsMarket Potential0","WA","Large General Service","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WALarge General ServiceAncillary Battery StorageProgram Annual CostsMarket Potential0","WA","Large General Service","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,2718.58,2725.96,2733.31,2744.33,2755.33,2766.29,2777.24,2791.83,2806.39,2820.93,2839.09,2857.22,2875.32,2897.04,2896.89,2896.74,2896.6,2896.46,2896.33,2896.2,2896.08,2895.96,2895.85,2895.74,2895.63,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageParticipantsMarket Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Participants","Market Potential",0,2.2000000000000001E-3,6.5999999999999991E-3,1.0999999999999999E-2,1.7600000000000001E-2,2.4200000000000003E-2,3.0800000000000004E-2,3.7400000000000003E-2,4.6200000000000005E-2,5.5E-2,6.3799999999999996E-2,7.4799999999999991E-2,8.5800000000000001E-2,9.6799999999999983E-2,0.10999999999999999,0.11,0.11,0.11,0.11,0.11,0.11,0.11,0.11,0.11,0.11,0.11,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageNew ParticipantsMarket Potential0","WA","Extra Large General Service","Ancillary Battery Storage","New Participants","Market Potential",0,2.2000000000000001E-3,4.3999999999999994E-3,4.4000000000000003E-3,6.6000000000000017E-3,6.6000000000000017E-3,6.6000000000000017E-3,6.5999999999999982E-3,8.8000000000000023E-3,8.7999999999999953E-3,8.7999999999999953E-3,1.0999999999999996E-2,1.100000000000001E-2,1.0999999999999982E-2,1.3200000000000003E-2,1.3877787807814457E-17,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageSummer Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Meter  (MW)","Market Potential",0,3.3000000000000003E-5,9.8999999999999994E-5,1.6499999999999997E-4,2.6400000000000002E-4,3.6300000000000004E-4,4.6200000000000006E-4,5.6100000000000008E-4,6.9300000000000004E-4,8.25E-4,9.5699999999999995E-4,1.122E-3,1.2869999999999999E-3,1.4519999999999997E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageSummer Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Summer Peak Reduction @Generation (MW)","Market Potential",0,3.5166240409207165E-5,1.0549872122762147E-4,1.7583120204603576E-4,2.8132992327365732E-4,3.8682864450127882E-4,4.9232736572890027E-4,5.9782608695652182E-4,7.3849104859335045E-4,8.7915601023017898E-4,1.0198209718670075E-3,1.1956521739130434E-3,1.3714833759590791E-3,1.5473145780051148E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageWinter Peak Reduction @Meter  (MW)Market Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Meter  (MW)","Market Potential",0,3.3000000000000003E-5,9.8999999999999994E-5,1.6499999999999997E-4,2.6400000000000002E-4,3.6300000000000004E-4,4.6200000000000006E-4,5.6100000000000008E-4,6.9300000000000004E-4,8.25E-4,9.5699999999999995E-4,1.122E-3,1.2869999999999999E-3,1.4519999999999997E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,1.65E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageWinter Peak Reduction @Generation (MW)Market Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Winter Peak Reduction @Generation (MW)","Market Potential",0,3.5166240409207165E-5,1.0549872122762147E-4,1.7583120204603576E-4,2.8132992327365732E-4,3.8682864450127882E-4,4.9232736572890027E-4,5.9782608695652182E-4,7.3849104859335045E-4,8.7915601023017898E-4,1.0198209718670075E-3,1.1956521739130434E-3,1.3714833759590791E-3,1.5473145780051148E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,1.758312020460358E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceAncillary Battery StorageNon-Incentive CostsMarket Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Non-Incentive Costs","Market Potential",0,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,29.41,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageIncentive CostsMarket Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Incentive Costs","Market Potential",0,0.04,0.13,0.22,0.35,0.48,0.62,0.75,0.92,1.1000000000000001,1.28,1.5,1.72,1.94,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WAExtra Large General ServiceAncillary Battery StorageProgram Annual BenefitsMarket Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Program Annual Benefits","Market Potential",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["WAExtra Large General ServiceAncillary Battery StorageProgram Annual CostsMarket Potential0","WA","Extra Large General Service","Ancillary Battery Storage","Program Annual Costs","Market Potential",0,29.45,29.54,29.63,29.76,29.89,30.02,30.15,30.33,30.51,30.68,30.9,31.12,31.34,31.61,31.61,31.61,31.61,31.61,31.61,31.61,31.61,31.61,31.61,31.61,31.61,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"Translator","index":9,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Range","Type",null,null,null,"<---- Cells and Variable Names that will be written to Results Tab."]
[{"$f":"\"C\"&CELL(\"row\",DR!$C$19)&\":AU\"&CELL(\"row\",DR!$C$19)","v":"C19:AU19"},"Participants"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C$20)&\":AU\"&CELL(\"row\",DR!$C$20)","v":"C20:AU20"},"New Participants"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C$26)&\":AU\"&CELL(\"row\",DR!$C$26)","v":"C26:AU26"},"Summer Peak Reduction @Meter  (MW)"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C30)&\":AV\"&CELL(\"row\",DR!$C30)","v":"C30:AV30"},"Summer Peak Reduction @Generation (MW)"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C$39)&\":AU\"&CELL(\"row\",DR!$C$39)","v":"C39:AU39"},"Winter Peak Reduction @Meter  (MW)"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C43)&\":AV\"&CELL(\"row\",DR!$C43)","v":"C43:AV43"},"Winter Peak Reduction @Generation (MW)"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C65)&\":AV\"&CELL(\"row\",DR!$C65)","v":"C65:AV65"},"Non-Incentive Costs"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C66)&\":AV\"&CELL(\"row\",DR!$C66)","v":"C66:AV66"},"Incentive Costs"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C72)&\":AV\"&CELL(\"row\",DR!$C72)","v":"C72:AV72"},"Program Annual Benefits"]
[{"$f":"\"C\"&CELL(\"row\",DR!$C73)&\":AU\"&CELL(\"row\",DR!$C73)","v":"C73:AU73"},"Program Annual Costs"]